Fitter report for DC_Motor_Main
Fri Aug 04 19:03:47 2006
Version 4.2 Build 157 12/07/2004 SJ Full Version


---------------------
; Table of Contents ;
---------------------
  1. Legal Notice
  2. Fitter Summary
  3. Fitter Settings
  4. Fitter Device Options
  5. Fitter Equations
  6. Pin-Out File
  7. Fitter Resource Usage Summary
  8. Input Pins
  9. Output Pins
 10. All Package Pins
 11. I/O Standard
 12. Dedicated Inputs I/O
 13. Output Pin Default Load For Reported TCO
 14. Fitter Resource Utilization by Entity
 15. Control Signals
 16. Global & Other Fast Signals
 17. Non-Global High Fan-Out Signals
 18. Interconnect Usage Summary
 19. LAB External Interconnect
 20. LAB Macrocells
 21. Shareable Expander
 22. Logic Cell Interconnection
 23. Fitter Messages



----------------
; Legal Notice ;
----------------
Copyright (C) 1991-2004 Altera Corporation
Any  megafunction  design,  and related netlist (encrypted  or  decrypted),
support information,  device programming or simulation file,  and any other
associated  documentation or information  provided by  Altera  or a partner
under  Altera's   Megafunction   Partnership   Program  may  be  used  only
to program  PLD  devices (but not masked  PLD  devices) from  Altera.   Any
other  use  of such  megafunction  design,  netlist,  support  information,
device programming or simulation file,  or any other  related documentation
or information  is prohibited  for  any  other purpose,  including, but not
limited to  modification,  reverse engineering,  de-compiling, or use  with
any other  silicon devices,  unless such use is  explicitly  licensed under
a separate agreement with  Altera  or a megafunction partner.  Title to the
intellectual property,  including patents,  copyrights,  trademarks,  trade
secrets,  or maskworks,  embodied in any such megafunction design, netlist,
support  information,  device programming or simulation file,  or any other
related documentation or information provided by  Altera  or a megafunction
partner, remains with Altera, the megafunction partner, or their respective
licensors. No other licenses, including any licenses needed under any third
party's intellectual property, are provided herein.



+------------------------------------------------------------------+
; Fitter Summary                                                   ;
+-----------------------+------------------------------------------+
; Fitter Status         ; Successful - Fri Aug 04 19:03:47 2006    ;
; Quartus II Version    ; 4.2 Build 157 12/07/2004 SJ Full Version ;
; Revision Name         ; DC_Motor_Main                            ;
; Top-level Entity Name ; DC_Motor_Main                            ;
; Family                ; MAX7000S                                 ;
; Device                ; EPM7128STC100-6                          ;
; Timing Models         ; Final                                    ;
; Total macrocells      ; 77 / 128 ( 60 % )                        ;
; Total pins            ; 77 / 84 ( 91 % )                         ;
+-----------------------+------------------------------------------+


+--------------------------------------------------------------------------------------+
; Fitter Settings                                                                      ;
+--------------------------------------------+--------------------+--------------------+
; Option                                     ; Setting            ; Default Value      ;
+--------------------------------------------+--------------------+--------------------+
; Device                                     ; AUTO               ;                    ;
; Use smart compilation                      ; Normal             ; Normal             ;
; Optimize Timing                            ; Normal compilation ; Normal compilation ;
; Optimize IOC Register Placement for Timing ; On                 ; On                 ;
; Limit to One Fitting Attempt               ; Off                ; Off                ;
; Fitter Initial Placement Seed              ; 1                  ; 1                  ;
; Slow Slew Rate                             ; Off                ; Off                ;
; Fitter Effort                              ; Auto Fit           ; Auto Fit           ;
+--------------------------------------------+--------------------+--------------------+


+----------------------------------------------------------------------------------------+
; Fitter Device Options                                                                  ;
+----------------------------------------------+-----------------------------------------+
; Option                                       ; Setting                                 ;
+----------------------------------------------+-----------------------------------------+
; Enable user-supplied start-up clock (CLKUSR) ; Off                                     ;
; Enable device-wide reset (DEV_CLRn)          ; Off                                     ;
; Enable device-wide output enable (DEV_OE)    ; Off                                     ;
; Enable INIT_DONE output                      ; Off                                     ;
; Configuration scheme                         ; Passive Serial                          ;
; Reserve all unused pins                      ; As output driving an unspecified signal ;
; Security bit                                 ; Off                                     ;
; Base pin-out file on sameframe device        ; Off                                     ;
+----------------------------------------------+-----------------------------------------+


+------------------+
; Fitter Equations ;
+------------------+
The equations can be found in E:/戴仙金/资料/Verilog书/源代码/DC_Motor/DC_Motor_Main/DC_Motor_Main.fit.eqn.


+--------------+
; Pin-Out File ;
+--------------+
The pin-out file can be found in E:/戴仙金/资料/Verilog书/源代码/DC_Motor/DC_Motor_Main/DC_Motor_Main.pin.


+---------------------------------------------------+
; Fitter Resource Usage Summary                     ;
+-------------------------------+-------------------+
; Resource                      ; Usage             ;
+-------------------------------+-------------------+
; Logic cells                   ; 77 / 128 ( 60 % ) ;
; Registers                     ; 57 / 128 ( 44 % ) ;
; Number of pterms used         ; 251               ;
; User inserted logic elements  ; 0                 ;
; I/O pins                      ; 77 / 84 ( 91 % )  ;
;     -- Clock pins             ; 2 / 2 ( 100 % )   ;
;     -- Dedicated input pins   ; 2 / 2 ( 100 % )   ;
; Global signals                ; 2                 ;
; Shareable expanders           ; 50 / 128 ( 39 % ) ;
; Parallel expanders            ; 0 / 120 ( 0 % )   ;
; Cells using turbo bit         ; 77 / 128 ( 60 % ) ;
; Maximum fan-out node          ; Reset             ;
; Maximum fan-out               ; 32                ;
; Total fan-out                 ; 631               ;
; Average fan-out               ; 3.09              ;
+-------------------------------+-------------------+


+---------------------------------------------------------------------------------------------------------------------------------------------------------+
; Input Pins                                                                                                                                              ;
+-------------------+-------+----------+-----+-----------------------+--------------------+--------+----------------+--------------+----------------------+
; Name              ; Pin # ; I/O Bank ; LAB ; Combinational Fan-Out ; Registered Fan-Out ; Global ; Input Register ; I/O Standard ; Location assigned by ;
+-------------------+-------+----------+-----+-----------------------+--------------------+--------+----------------+--------------+----------------------+
; AD7492_Busy       ; 81    ; --       ; 8   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; AD7492_Data[0]    ; 98    ; --       ; 1   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; AD7492_Data[10]   ; 42    ; --       ; 5   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; AD7492_Data[11]   ; 100   ; --       ; 1   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; AD7492_Data[1]    ; 21    ; --       ; 3   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; AD7492_Data[2]    ; 56    ; --       ; 6   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; AD7492_Data[3]    ; 45    ; --       ; 5   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; AD7492_Data[4]    ; 33    ; --       ; 4   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; AD7492_Data[5]    ; 67    ; --       ; 7   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; AD7492_Data[6]    ; 55    ; --       ; 6   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; AD7492_Data[7]    ; 77    ; --       ; 8   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; AD7492_Data[8]    ; 23    ; --       ; 3   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; AD7492_Data[9]    ; 54    ; --       ; 6   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; AD7895_Busy       ; 16    ; --       ; 3   ; 8                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; AD7895_Data       ; 5     ; --       ; 2   ; 12                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Clk_SCL           ; 87    ; --       ; --  ; 11                    ; 0                  ; yes    ; no             ; TTL          ; Fitter               ;
; Clock             ; 90    ; --       ; --  ; 4                     ; 0                  ; yes    ; no             ; TTL          ; Fitter               ;
; Current_SW        ; 85    ; --       ; 8   ; 9                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Current_Set[0]    ; 83    ; --       ; 8   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Current_Set[10]   ; 79    ; --       ; 8   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Current_Set[11]   ; 46    ; --       ; 5   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Current_Set[1]    ; 71    ; --       ; 7   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Current_Set[2]    ; 72    ; --       ; 7   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Current_Set[3]    ; 49    ; --       ; 5   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Current_Set[4]    ; 30    ; --       ; 4   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Current_Set[5]    ; 64    ; --       ; 7   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Current_Set[6]    ; 58    ; --       ; 6   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Current_Set[7]    ; 19    ; --       ; 3   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Current_Set[8]    ; 29    ; --       ; 4   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Current_Set[9]    ; 32    ; --       ; 4   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Position_SW       ; 92    ; --       ; 1   ; 5                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Position_Set[0]   ; 88    ; --       ; --  ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Position_Set[10]  ; 97    ; --       ; 1   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Position_Set[11]  ; 99    ; --       ; 1   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Position_Set[1]   ; 24    ; --       ; 3   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Position_Set[2]   ; 89    ; --       ; --  ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Position_Set[3]   ; 65    ; --       ; 7   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Position_Set[4]   ; 96    ; --       ; 1   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Position_Set[5]   ; 25    ; --       ; 3   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Position_Set[6]   ; 20    ; --       ; 3   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Position_Set[7]   ; 69    ; --       ; 7   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Position_Set[8]   ; 80    ; --       ; 8   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Position_Set[9]   ; 31    ; --       ; 4   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Measure_Ctrl ; 68    ; --       ; 7   ; 17                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Pulse        ; 60    ; --       ; 6   ; 17                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_SW           ; 50    ; --       ; 5   ; 18                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[0]       ; 35    ; --       ; 4   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[10]      ; 6     ; --       ; 2   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[11]      ; 28    ; --       ; 4   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[12]      ; 84    ; --       ; 8   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[13]      ; 93    ; --       ; 1   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[14]      ; 9     ; --       ; 2   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[15]      ; 17    ; --       ; 3   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[1]       ; 78    ; --       ; 8   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[2]       ; 22    ; --       ; 3   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[3]       ; 44    ; --       ; 5   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[4]       ; 70    ; --       ; 7   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[5]       ; 47    ; --       ; 5   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[6]       ; 7     ; --       ; 2   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[7]       ; 48    ; --       ; 5   ; 2                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[8]       ; 61    ; --       ; 6   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Rate_Set[9]       ; 94    ; --       ; 1   ; 1                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; Reset             ; 27    ; --       ; 4   ; 32                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
+-------------------+-------+----------+-----+-----------------------+--------------------+--------+----------------+--------------+----------------------+


+------------------------------------------------------------------------------------------------------------------------------------------------------+
; Output Pins                                                                                                                                          ;
+-----------------------+-------+----------+-----+-----------------+----------------+------------+---------------+--------------+----------------------+
; Name                  ; Pin # ; I/O Bank ; LAB ; Output Register ; Slow Slew Rate ; Open Drain ; TRI Primitive ; I/O Standard ; Location assigned by ;
+-----------------------+-------+----------+-----+-----------------+----------------+------------+---------------+--------------+----------------------+
; AD7492_CS             ; 14    ; --       ; 2   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; AD7492_Conv           ; 10    ; --       ; 2   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; AD7492_Mode           ; 13    ; --       ; 2   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; AD7492_RD             ; 12    ; --       ; 2   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; AD7895_Conv           ; 37    ; --       ; 4   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; AD7895_SCL            ; 40    ; --       ; 5   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; Current_Adjust_Drive  ; 52    ; --       ; 6   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; Position_Adjust_Drive ; 63    ; --       ; 7   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; Rate_Adjust_Drive     ; 75    ; --       ; 8   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; Rate_Over             ; 2     ; --       ; 1   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
+-----------------------+-------+----------+-----+-----------------+----------------+------------+---------------+--------------+----------------------+


+--------------------------------------------------------------------------------------------------------------+
; All Package Pins                                                                                             ;
+----------+------------+----------+-----------------------+--------+--------------+---------+-----------------+
; Location ; Pad Number ; I/O Bank ; Pin Name/Usage        ; Dir.   ; I/O Standard ; Voltage ; User Assignment ;
+----------+------------+----------+-----------------------+--------+--------------+---------+-----------------+
; 1        ; 12         ; --       ; RESERVED              ;        ;              ;         ;                 ;
; 2        ; 13         ; --       ; Rate_Over             ; output ; TTL          ;         ; N               ;
; 3        ; 14         ; --       ; VCCIO                 ; power  ;              ; 5.0V    ;                 ;
; 4        ; 15         ; --       ; +TDI                  ; input  ; TTL          ;         ; N               ;
; 5        ; 16         ; --       ; AD7895_Data           ; input  ; TTL          ;         ; N               ;
; 6        ; 17         ; --       ; Rate_Set[10]          ; input  ; TTL          ;         ; N               ;
; 7        ; 18         ; --       ; Rate_Set[6]           ; input  ; TTL          ;         ; N               ;
; 8        ; 19         ; --       ; RESERVED              ;        ;              ;         ;                 ;
; 9        ; 20         ; --       ; Rate_Set[14]          ; input  ; TTL          ;         ; N               ;
; 10       ; 21         ; --       ; AD7492_Conv           ; output ; TTL          ;         ; N               ;
; 11       ; 22         ; --       ; GND                   ; gnd    ;              ;         ;                 ;
; 12       ; 23         ; --       ; AD7492_RD             ; output ; TTL          ;         ; N               ;
; 13       ; 24         ; --       ; AD7492_Mode           ; output ; TTL          ;         ; N               ;
; 14       ; 25         ; --       ; AD7492_CS             ; output ; TTL          ;         ; N               ;
; 15       ; 26         ; --       ; +TMS                  ; input  ; TTL          ;         ; N               ;
; 16       ; 27         ; --       ; AD7895_Busy           ; input  ; TTL          ;         ; N               ;
; 17       ; 28         ; --       ; Rate_Set[15]          ; input  ; TTL          ;         ; N               ;
; 18       ; 29         ; --       ; VCCIO                 ; power  ;              ; 5.0V    ;                 ;
; 19       ; 30         ; --       ; Current_Set[7]        ; input  ; TTL          ;         ; N               ;
; 20       ; 31         ; --       ; Position_Set[6]       ; input  ; TTL          ;         ; N               ;
; 21       ; 32         ; --       ; AD7492_Data[1]        ; input  ; TTL          ;         ; N               ;
; 22       ; 33         ; --       ; Rate_Set[2]           ; input  ; TTL          ;         ; N               ;
; 23       ; 34         ; --       ; AD7492_Data[8]        ; input  ; TTL          ;         ; N               ;
; 24       ; 35         ; --       ; Position_Set[1]       ; input  ; TTL          ;         ; N               ;
; 25       ; 36         ; --       ; Position_Set[5]       ; input  ; TTL          ;         ; N               ;
; 26       ; 37         ; --       ; GND                   ; gnd    ;              ;         ;                 ;
; 27       ; 38         ; --       ; Reset                 ; input  ; TTL          ;         ; N               ;
; 28       ; 39         ; --       ; Rate_Set[11]          ; input  ; TTL          ;         ; N               ;
; 29       ; 40         ; --       ; Current_Set[8]        ; input  ; TTL          ;         ; N               ;
; 30       ; 41         ; --       ; Current_Set[4]        ; input  ; TTL          ;         ; N               ;
; 31       ; 42         ; --       ; Position_Set[9]       ; input  ; TTL          ;         ; N               ;
; 32       ; 43         ; --       ; Current_Set[9]        ; input  ; TTL          ;         ; N               ;
; 33       ; 44         ; --       ; AD7492_Data[4]        ; input  ; TTL          ;         ; N               ;
; 34       ; 45         ; --       ; VCCIO                 ; power  ;              ; 5.0V    ;                 ;
; 35       ; 46         ; --       ; Rate_Set[0]           ; input  ; TTL          ;         ; N               ;
; 36       ; 47         ; --       ; RESERVED              ;        ;              ;         ;                 ;
; 37       ; 48         ; --       ; AD7895_Conv           ; output ; TTL          ;         ; N               ;
; 38       ; 49         ; --       ; GND                   ; gnd    ;              ;         ;                 ;
; 39       ; 50         ; --       ; VCCINT                ; power  ;              ; 5.0V    ;                 ;
; 40       ; 51         ; --       ; AD7895_SCL            ; output ; TTL          ;         ; N               ;
; 41       ; 52         ; --       ; RESERVED              ;        ;              ;         ;                 ;
; 42       ; 53         ; --       ; AD7492_Data[10]       ; input  ; TTL          ;         ; N               ;
; 43       ; 54         ; --       ; GND                   ; gnd    ;              ;         ;                 ;
; 44       ; 55         ; --       ; Rate_Set[3]           ; input  ; TTL          ;         ; N               ;
; 45       ; 56         ; --       ; AD7492_Data[3]        ; input  ; TTL          ;         ; N               ;
; 46       ; 57         ; --       ; Current_Set[11]       ; input  ; TTL          ;         ; N               ;
; 47       ; 58         ; --       ; Rate_Set[5]           ; input  ; TTL          ;         ; N               ;
; 48       ; 59         ; --       ; Rate_Set[7]           ; input  ; TTL          ;         ; N               ;
; 49       ; 60         ; --       ; Current_Set[3]        ; input  ; TTL          ;         ; N               ;
; 50       ; 61         ; --       ; Rate_SW               ; input  ; TTL          ;         ; N               ;
; 51       ; 62         ; --       ; VCCIO                 ; power  ;              ; 5.0V    ;                 ;
; 52       ; 63         ; --       ; Current_Adjust_Drive  ; output ; TTL          ;         ; N               ;
; 53       ; 64         ; --       ; RESERVED              ;        ;              ;         ;                 ;
; 54       ; 65         ; --       ; AD7492_Data[9]        ; input  ; TTL          ;         ; N               ;
; 55       ; 66         ; --       ; AD7492_Data[6]        ; input  ; TTL          ;         ; N               ;
; 56       ; 67         ; --       ; AD7492_Data[2]        ; input  ; TTL          ;         ; N               ;
; 57       ; 68         ; --       ; RESERVED              ;        ;              ;         ;                 ;
; 58       ; 69         ; --       ; Current_Set[6]        ; input  ; TTL          ;         ; N               ;
; 59       ; 70         ; --       ; GND                   ; gnd    ;              ;         ;                 ;
; 60       ; 71         ; --       ; Rate_Pulse            ; input  ; TTL          ;         ; N               ;
; 61       ; 72         ; --       ; Rate_Set[8]           ; input  ; TTL          ;         ; N               ;
; 62       ; 73         ; --       ; +TCK                  ; input  ; TTL          ;         ; N               ;
; 63       ; 74         ; --       ; Position_Adjust_Drive ; output ; TTL          ;         ; N               ;
; 64       ; 75         ; --       ; Current_Set[5]        ; input  ; TTL          ;         ; N               ;
; 65       ; 76         ; --       ; Position_Set[3]       ; input  ; TTL          ;         ; N               ;
; 66       ; 77         ; --       ; VCCIO                 ; power  ;              ; 5.0V    ;                 ;
; 67       ; 78         ; --       ; AD7492_Data[5]        ; input  ; TTL          ;         ; N               ;
; 68       ; 79         ; --       ; Rate_Measure_Ctrl     ; input  ; TTL          ;         ; N               ;
; 69       ; 80         ; --       ; Position_Set[7]       ; input  ; TTL          ;         ; N               ;
; 70       ; 81         ; --       ; Rate_Set[4]           ; input  ; TTL          ;         ; N               ;
; 71       ; 82         ; --       ; Current_Set[1]        ; input  ; TTL          ;         ; N               ;
; 72       ; 83         ; --       ; Current_Set[2]        ; input  ; TTL          ;         ; N               ;
; 73       ; 84         ; --       ; *TDO                  ; output ; TTL          ;         ; N               ;
; 74       ; 85         ; --       ; GND                   ; gnd    ;              ;         ;                 ;
; 75       ; 86         ; --       ; Rate_Adjust_Drive     ; output ; TTL          ;         ; N               ;
; 76       ; 87         ; --       ; RESERVED              ;        ;              ;         ;                 ;
; 77       ; 88         ; --       ; AD7492_Data[7]        ; input  ; TTL          ;         ; N               ;
; 78       ; 89         ; --       ; Rate_Set[1]           ; input  ; TTL          ;         ; N               ;
; 79       ; 90         ; --       ; Current_Set[10]       ; input  ; TTL          ;         ; N               ;
; 80       ; 91         ; --       ; Position_Set[8]       ; input  ; TTL          ;         ; N               ;
; 81       ; 92         ; --       ; AD7492_Busy           ; input  ; TTL          ;         ; N               ;
; 82       ; 93         ; --       ; VCCIO                 ; power  ;              ; 5.0V    ;                 ;
; 83       ; 94         ; --       ; Current_Set[0]        ; input  ; TTL          ;         ; N               ;
; 84       ; 95         ; --       ; Rate_Set[12]          ; input  ; TTL          ;         ; N               ;
; 85       ; 96         ; --       ; Current_SW            ; input  ; TTL          ;         ; N               ;
; 86       ; 97         ; --       ; GND                   ; gnd    ;              ;         ;                 ;
; 87       ; 98         ; --       ; Clk_SCL               ; input  ; TTL          ;         ; N               ;
; 88       ; 99         ; --       ; Position_Set[0]       ; input  ; TTL          ;         ; N               ;
; 89       ; 0          ; --       ; Position_Set[2]       ; input  ; TTL          ;         ; N               ;
; 90       ; 1          ; --       ; Clock                 ; input  ; TTL          ;         ; N               ;
; 91       ; 2          ; --       ; VCCINT                ; power  ;              ; 5.0V    ;                 ;
; 92       ; 3          ; --       ; Position_SW           ; input  ; TTL          ;         ; N               ;
; 93       ; 4          ; --       ; Rate_Set[13]          ; input  ; TTL          ;         ; N               ;
; 94       ; 5          ; --       ; Rate_Set[9]           ; input  ; TTL          ;         ; N               ;
; 95       ; 6          ; --       ; GND                   ; gnd    ;              ;         ;                 ;
; 96       ; 7          ; --       ; Position_Set[4]       ; input  ; TTL          ;         ; N               ;
; 97       ; 8          ; --       ; Position_Set[10]      ; input  ; TTL          ;         ; N               ;
; 98       ; 9          ; --       ; AD7492_Data[0]        ; input  ; TTL          ;         ; N               ;
; 99       ; 10         ; --       ; Position_Set[11]      ; input  ; TTL          ;         ; N               ;
; 100      ; 11         ; --       ; AD7492_Data[11]       ; input  ; TTL          ;         ; N               ;
+----------+------------+----------+-----------------------+--------+--------------+---------+-----------------+


+--------------------------------------------------------------------------------------------------+
; I/O Standard                                                                                     ;
+--------------+------------+----------------------+-------------------+-------------------+-------+
; I/O Standard ; Input Vref ; Dedicated Input Pins ; Pins in I/O Bank1 ; Pins in I/O Bank2 ; Total ;
+--------------+------------+----------------------+-------------------+-------------------+-------+
; TTL          ; -          ; 4                    ; 0                 ; 0                 ; 4     ;
+--------------+------------+----------------------+-------------------+-------------------+-------+


+-------------------------------------------------------------------------------+
; Dedicated Inputs I/O                                                          ;
+-----------------+-------+-------+-------+--------------+------------+---------+
; Name            ; Pin # ; Type  ; VCCIO ; I/O Standard ; Input Vref ; Current ;
+-----------------+-------+-------+-------+--------------+------------+---------+
; Clk_SCL         ; 87    ; Input ; --    ; TTL          ; -          ; 0 mA    ;
; Clock           ; 90    ; Input ; --    ; TTL          ; -          ; 0 mA    ;
; Position_Set[0] ; 88    ; Input ; --    ; TTL          ; -          ; 0 mA    ;
; Position_Set[2] ; 89    ; Input ; --    ; TTL          ; -          ; 0 mA    ;
+-----------------+-------+-------+-------+--------------+------------+---------+


+-----------------------------------------------+
; Output Pin Default Load For Reported TCO      ;
+--------------+-------+------------------------+
; I/O Standard ; Load  ; Termination Resistance ;
+--------------+-------+------------------------+
; LVTTL        ; 10 pF ; Not Available          ;
; LVCMOS       ; 10 pF ; Not Available          ;
; TTL          ; 0 pF  ; Not Available          ;
+--------------+-------+------------------------+


+-------------------------------------------------------------------------------------------------------------------------------------+
; Fitter Resource Utilization by Entity                                                                                               ;
+-------------------------------------------+------------+------+---------------------------------------------------------------------+
; Compilation Hierarchy Node                ; Macrocells ; Pins ; Full Hierarchy Name                                                 ;
+-------------------------------------------+------------+------+---------------------------------------------------------------------+
; |DC_Motor_Main                            ; 77         ; 77   ; |DC_Motor_Main                                                      ;
;    |Current_Adjust:inst5|                 ; 5          ; 0    ; |DC_Motor_Main|Current_Adjust:inst5                                 ;
;    |Position_Adjust:inst8|                ; 5          ; 0    ; |DC_Motor_Main|Position_Adjust:inst8                                ;
;    |Position_adc_ctrl:inst6|              ; 16         ; 0    ; |DC_Motor_Main|Position_adc_ctrl:inst6                              ;
;    |Rate_Adjust:inst11|                   ; 9          ; 0    ; |DC_Motor_Main|Rate_Adjust:inst11                                   ;
;    |Rate_Measure:inst2|                   ; 17         ; 0    ; |DC_Motor_Main|Rate_Measure:inst2                                   ;
;       |lpm_counter:Rate_Pulse_Data_rtl_0| ; 16         ; 0    ; |DC_Motor_Main|Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0 ;
;    |main:inst3|                           ; 25         ; 0    ; |DC_Motor_Main|main:inst3                                           ;
;       |Data_Read:b2v_inst1|               ; 16         ; 0    ; |DC_Motor_Main|main:inst3|Data_Read:b2v_inst1                       ;
;          |lpm_counter:cnt_rtl_1|          ; 4          ; 0    ; |DC_Motor_Main|main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1 ;
;       |Data_drive:b2v_inst|               ; 9          ; 0    ; |DC_Motor_Main|main:inst3|Data_drive:b2v_inst                       ;
+-------------------------------------------+------------+------+---------------------------------------------------------------------+


+----------------------------------------------------------------------------------------------------------------------------------+
; Control Signals                                                                                                                  ;
+-------------------------------------------+----------+---------+--------------+--------+----------------------+------------------+
; Name                                      ; Location ; Fan-Out ; Usage        ; Global ; Global Resource Used ; Global Line Name ;
+-------------------------------------------+----------+---------+--------------+--------+----------------------+------------------+
; AD7895_Busy                               ; PIN_16   ; 8       ; Clock enable ; no     ; --                   ; --               ;
; Clk_SCL                                   ; PIN_87   ; 11      ; Clock        ; yes    ; On                   ; --               ;
; Clock                                     ; PIN_90   ; 4       ; Clock        ; yes    ; On                   ; --               ;
; Current_SW                                ; PIN_85   ; 9       ; Clock enable ; no     ; --                   ; --               ;
; Position_adc_ctrl:inst6|Adc_Rd            ; LC21     ; 13      ; Clock        ; no     ; --                   ; --               ;
; Rate_Measure_Ctrl                         ; PIN_68   ; 17      ; Clock        ; no     ; --                   ; --               ;
; Rate_Pulse                                ; PIN_60   ; 17      ; Clock        ; no     ; --                   ; --               ;
; Reset                                     ; PIN_27   ; 32      ; Clock enable ; no     ; --                   ; --               ;
; main:inst3|Data_drive:b2v_inst|Adc_SCL~42 ; SEXP50   ; 14      ; Clock        ; no     ; --                   ; --               ;
; main:inst3|Data_drive:b2v_inst|Adc_SCL~58 ; SEXP65   ; 2       ; Clock        ; no     ; --                   ; --               ;
+-------------------------------------------+----------+---------+--------------+--------+----------------------+------------------+


+------------------------------------------------------------------------+
; Global & Other Fast Signals                                            ;
+---------+----------+---------+----------------------+------------------+
; Name    ; Location ; Fan-Out ; Global Resource Used ; Global Line Name ;
+---------+----------+---------+----------------------+------------------+
; Clk_SCL ; PIN_87   ; 11      ; On                   ; --               ;
; Clock   ; PIN_90   ; 4       ; On                   ; --               ;
+---------+----------+---------+----------------------+------------------+


+-------------------------------------------------------------------------+
; Non-Global High Fan-Out Signals                                         ;
+---------------------------------------------------------------+---------+
; Name                                                          ; Fan-Out ;
+---------------------------------------------------------------+---------+
; Reset                                                         ; 32      ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; 19      ;
; Rate_SW                                                       ; 18      ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; 18      ;
; Rate_Measure_Ctrl                                             ; 17      ;
; Rate_Pulse                                                    ; 17      ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; 17      ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; 16      ;
; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0]  ; 15      ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; 15      ;
; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1]  ; 14      ;
; main:inst3|Data_drive:b2v_inst|Adc_SCL~42                     ; 14      ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; 14      ;
; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2]  ; 13      ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; 13      ;
; Position_adc_ctrl:inst6|Adc_Rd                                ; 13      ;
; AD7895_Data                                                   ; 12      ;
; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3]  ; 12      ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; 12      ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; 10      ;
; Current_SW                                                    ; 9       ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; 9       ;
; AD7895_Busy                                                   ; 8       ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; 8       ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; 7       ;
; main:inst3|Data_drive:b2v_inst|cnt1[1]                        ; 7       ;
; main:inst3|Data_drive:b2v_inst|cnt1[0]                        ; 7       ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; 6       ;
; main:inst3|Data_drive:b2v_inst|cnt1[2]                        ; 6       ;
; Position_SW                                                   ; 5       ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; 5       ;
; main:inst3|Data_drive:b2v_inst|cnt1[3]                        ; 5       ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; 4       ;
; main:inst3|Data_drive:b2v_inst|cnt1[4]                        ; 4       ;
; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; 3       ;
; main:inst3|Data_Read:b2v_inst1|Data[8]                        ; 3       ;
; main:inst3|Data_Read:b2v_inst1|Data[10]                       ; 3       ;
; main:inst3|Data_Read:b2v_inst1|Data[4]                        ; 3       ;
; main:inst3|Data_Read:b2v_inst1|Data[5]                        ; 3       ;
; main:inst3|Data_Read:b2v_inst1|Data[6]                        ; 3       ;
; main:inst3|Data_Read:b2v_inst1|Data[7]                        ; 3       ;
; main:inst3|Data_Read:b2v_inst1|Data[9]                        ; 3       ;
; main:inst3|Data_Read:b2v_inst1|Data[11]                       ; 3       ;
; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select                 ; 3       ;
; main:inst3|Data_drive:b2v_inst|cnt1[5]                        ; 3       ;
; main:inst3|Data_drive:b2v_inst|Adc_SCL~58                     ; 2       ;
; Position_Set[0]                                               ; 2       ;
; Position_Set[1]                                               ; 2       ;
; Position_Set[2]                                               ; 2       ;
; Position_Set[3]                                               ; 2       ;
+---------------------------------------------------------------+---------+


+-------------------------------------------------+
; Interconnect Usage Summary                      ;
+----------------------------+--------------------+
; Interconnect Resource Type ; Usage              ;
+----------------------------+--------------------+
; Output enables             ; 0 / 6 ( 0 % )      ;
; PIA buffers                ; 168 / 288 ( 58 % ) ;
; PIAs                       ; 186 / 288 ( 64 % ) ;
+----------------------------+--------------------+


+-----------------------------------------------------------------------------+
; LAB External Interconnect                                                   ;
+-----------------------------------------------+-----------------------------+
; LAB External Interconnects  (Average = 23.25) ; Number of LABs  (Total = 8) ;
+-----------------------------------------------+-----------------------------+
; 0 - 2                                         ; 0                           ;
; 3 - 5                                         ; 0                           ;
; 6 - 8                                         ; 0                           ;
; 9 - 11                                        ; 0                           ;
; 12 - 14                                       ; 0                           ;
; 15 - 17                                       ; 2                           ;
; 18 - 20                                       ; 1                           ;
; 21 - 23                                       ; 1                           ;
; 24 - 26                                       ; 1                           ;
; 27 - 29                                       ; 1                           ;
; 30 - 32                                       ; 2                           ;
+-----------------------------------------------+-----------------------------+


+----------------------------------------------------------------------+
; LAB Macrocells                                                       ;
+----------------------------------------+-----------------------------+
; Number of Macrocells  (Average = 9.63) ; Number of LABs  (Total = 8) ;
+----------------------------------------+-----------------------------+
; 0                                      ; 0                           ;
; 1                                      ; 2                           ;
; 2                                      ; 0                           ;
; 3                                      ; 0                           ;
; 4                                      ; 0                           ;
; 5                                      ; 1                           ;
; 6                                      ; 0                           ;
; 7                                      ; 0                           ;
; 8                                      ; 0                           ;
; 9                                      ; 0                           ;
; 10                                     ; 0                           ;
; 11                                     ; 0                           ;
; 12                                     ; 1                           ;
; 13                                     ; 1                           ;
; 14                                     ; 1                           ;
; 15                                     ; 1                           ;
; 16                                     ; 1                           ;
+----------------------------------------+-----------------------------+


+-------------------------------------------------------------------------------+
; Shareable Expander                                                            ;
+-------------------------------------------------+-----------------------------+
; Number of shareable expanders  (Average = 6.25) ; Number of LABs  (Total = 5) ;
+-------------------------------------------------+-----------------------------+
; 0                                               ; 3                           ;
; 1                                               ; 2                           ;
; 2                                               ; 0                           ;
; 3                                               ; 0                           ;
; 4                                               ; 0                           ;
; 5                                               ; 0                           ;
; 6                                               ; 0                           ;
; 7                                               ; 0                           ;
; 8                                               ; 0                           ;
; 9                                               ; 0                           ;
; 10                                              ; 0                           ;
; 11                                              ; 0                           ;
; 12                                              ; 0                           ;
; 13                                              ; 0                           ;
; 14                                              ; 0                           ;
; 15                                              ; 0                           ;
; 16                                              ; 3                           ;
+-------------------------------------------------+-----------------------------+


+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Logic Cell Interconnection                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ;
+-----+------------+-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; LAB ; Logic Cell ; Input                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                               ; Output                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
+-----+------------+-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
;  A  ; LC1        ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Pulse, Rate_Measure_Ctrl ; Rate_Over                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ;
;  A  ; LC2        ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Pulse, Rate_Measure_Ctrl ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~191                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ;
;  A  ; LC7        ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Pulse, Rate_Measure_Ctrl                                                                ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~187                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ;
;  A  ; LC5        ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Pulse, Rate_Measure_Ctrl                                                                                                                               ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~183                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ;
;  A  ; LC4        ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Pulse, Rate_Measure_Ctrl                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~139sexp, Rate_Adjust:inst11|always0~197                                                                                                                             ;
;  A  ; LC8        ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Pulse, Rate_Measure_Ctrl                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                               ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~143sexp, Rate_Adjust:inst11|always0~198                                                                                                                                                                                           ;
;  A  ; LC9        ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Pulse, Rate_Measure_Ctrl                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~147sexp, Rate_Adjust:inst11|always0~199                                                                                                                                                                                                                                                         ;
;  A  ; LC10       ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Pulse, Rate_Measure_Ctrl                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~151sexp, Rate_Adjust:inst11|always0~200                                                                                                                                                                                                                                                                                                                       ;
;  A  ; LC11       ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Pulse, Rate_Measure_Ctrl                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~155sexp, Rate_Adjust:inst11|always0~201                                                                                                                                                                                                                                                                                                                                                                                     ;
;  A  ; LC12       ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Pulse, Rate_Measure_Ctrl                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                       ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~159sexp, Rate_Adjust:inst11|always0~202                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  A  ; LC13       ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Pulse, Rate_Measure_Ctrl                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~163                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ;
;  A  ; LC3        ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Pulse, Rate_Measure_Ctrl                                                                                                                                                                                              ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~179                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                               ;
;  A  ; LC15       ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Pulse, Rate_Measure_Ctrl                                                                                                                                                                                                                                                                                                                                                                                           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~167                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  A  ; LC16       ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Pulse, Rate_Measure_Ctrl                                                                                                                                                                                                                                                                                                                            ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~171                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 ;
;  A  ; LC14       ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Pulse, Rate_Measure_Ctrl                                                                                                                                                                                                                                                             ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~175                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  B  ; LC28       ; Clk_SCL, main:inst3|Data_drive:b2v_inst|cnt1[3], main:inst3|Data_drive:b2v_inst|cnt1[1], main:inst3|Data_drive:b2v_inst|cnt1[0], main:inst3|Data_drive:b2v_inst|cnt1[2], main:inst3|Data_drive:b2v_inst|cnt1[4], Current_SW, Reset, AD7895_Busy                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; main:inst3|Data_drive:b2v_inst|cnt1[4], main:inst3|Data_drive:b2v_inst|cnt1[5], main:inst3|Data_drive:b2v_inst|Adc_SCL_Select, main:inst3|Data_drive:b2v_inst|Adc_Conv                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  B  ; LC27       ; Clk_SCL, main:inst3|Data_drive:b2v_inst|cnt1[1], main:inst3|Data_drive:b2v_inst|cnt1[0], main:inst3|Data_drive:b2v_inst|cnt1[2], main:inst3|Data_drive:b2v_inst|cnt1[3], Current_SW, Reset, AD7895_Busy                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; main:inst3|Data_drive:b2v_inst|cnt1[3], main:inst3|Data_drive:b2v_inst|cnt1[4], main:inst3|Data_drive:b2v_inst|cnt1[5], main:inst3|Data_drive:b2v_inst|Adc_SCL_Select, main:inst3|Data_drive:b2v_inst|Adc_Conv                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  B  ; LC29       ; Clk_SCL, main:inst3|Data_drive:b2v_inst|cnt1[4], main:inst3|Data_drive:b2v_inst|cnt1[3], main:inst3|Data_drive:b2v_inst|cnt1[1], main:inst3|Data_drive:b2v_inst|cnt1[0], main:inst3|Data_drive:b2v_inst|cnt1[2], main:inst3|Data_drive:b2v_inst|cnt1[5], Current_SW, Reset, AD7895_Busy                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; main:inst3|Data_drive:b2v_inst|cnt1[5], main:inst3|Data_drive:b2v_inst|Adc_SCL_Select, main:inst3|Data_drive:b2v_inst|Adc_Conv                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  B  ; LC26       ; Clk_SCL, main:inst3|Data_drive:b2v_inst|cnt1[1], main:inst3|Data_drive:b2v_inst|cnt1[0], main:inst3|Data_drive:b2v_inst|cnt1[2], Current_SW, Reset, AD7895_Busy                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; main:inst3|Data_drive:b2v_inst|cnt1[2], main:inst3|Data_drive:b2v_inst|cnt1[3], main:inst3|Data_drive:b2v_inst|cnt1[4], main:inst3|Data_drive:b2v_inst|cnt1[5], main:inst3|Data_drive:b2v_inst|Adc_SCL_Select, main:inst3|Data_drive:b2v_inst|Adc_Conv                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  B  ; LC25       ; Clk_SCL, main:inst3|Data_drive:b2v_inst|cnt1[1], main:inst3|Data_drive:b2v_inst|cnt1[0], Current_SW, Reset, AD7895_Busy                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; main:inst3|Data_drive:b2v_inst|cnt1[1], main:inst3|Data_drive:b2v_inst|cnt1[2], main:inst3|Data_drive:b2v_inst|cnt1[3], main:inst3|Data_drive:b2v_inst|cnt1[4], main:inst3|Data_drive:b2v_inst|cnt1[5], main:inst3|Data_drive:b2v_inst|Adc_SCL_Select, main:inst3|Data_drive:b2v_inst|Adc_Conv                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  B  ; LC18       ; Position_adc_ctrl:inst6|Position_Data[9], Position_Set[9]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           ; Position_Adjust:inst8|Position_Adjust_Out~10                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  ;
;  B  ; LC19       ; Clock, Reset, Position_SW                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           ; AD7492_Mode                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  B  ; LC24       ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Set[8]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           ; Rate_Adjust:inst11|Rate_Adjust_Out~14                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  B  ; LC17       ; Clock, Reset, Position_SW                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           ; AD7492_CS                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ;
;  B  ; LC30       ; Clk_SCL, Current_SW, Reset, AD7895_Busy                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; main:inst3|Data_drive:b2v_inst|cnt1[1], main:inst3|Data_drive:b2v_inst|cnt1[2], main:inst3|Data_drive:b2v_inst|cnt1[3], main:inst3|Data_drive:b2v_inst|cnt1[4], main:inst3|Data_drive:b2v_inst|cnt1[5], main:inst3|Data_drive:b2v_inst|Adc_SCL_Select, main:inst3|Data_drive:b2v_inst|Adc_Conv                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  B  ; LC22       ; Clock, Reset, Position_SW, AD7492_Busy                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ; AD7492_Conv                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  B  ; LC21       ; Clock, Reset, Position_SW, AD7492_Busy                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ; AD7492_RD, Position_adc_ctrl:inst6|Position_Data[11], Position_adc_ctrl:inst6|Position_Data[10], Position_adc_ctrl:inst6|Position_Data[9], Position_adc_ctrl:inst6|Position_Data[8], Position_adc_ctrl:inst6|Position_Data[7], Position_adc_ctrl:inst6|Position_Data[6], Position_adc_ctrl:inst6|Position_Data[5], Position_adc_ctrl:inst6|Position_Data[4], Position_adc_ctrl:inst6|Position_Data[3], Position_adc_ctrl:inst6|Position_Data[2], Position_adc_ctrl:inst6|Position_Data[1], Position_adc_ctrl:inst6|Position_Data[0]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           ;
;  C  ; LC41       ; AD7492_Data[11], Position_adc_ctrl:inst6|Adc_Rd                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; Position_Adjust:inst8|always0~143                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ;
;  C  ; LC48       ; AD7492_Data[10], Position_adc_ctrl:inst6|Adc_Rd                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; Position_Adjust:inst8|always0~139                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ;
;  C  ; LC33       ; AD7492_Data[9], Position_adc_ctrl:inst6|Adc_Rd                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ; Position_Adjust:inst8|always0~135                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ;
;  C  ; LC34       ; AD7492_Data[8], Position_adc_ctrl:inst6|Adc_Rd                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ; Position_Adjust:inst8|always0~131                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ;
;  C  ; LC35       ; AD7492_Data[7], Position_adc_ctrl:inst6|Adc_Rd                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ; Position_Adjust:inst8|always0~127sexp, Position_Adjust:inst8|always0~154                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ;
;  C  ; LC36       ; AD7492_Data[6], Position_adc_ctrl:inst6|Adc_Rd                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ; Position_Adjust:inst8|always0~123sexp, Position_Adjust:inst8|always0~153                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ;
;  C  ; LC37       ; AD7492_Data[5], Position_adc_ctrl:inst6|Adc_Rd                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ; Position_Adjust:inst8|always0~119sexp, Position_Adjust:inst8|always0~152                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ;
;  C  ; LC46       ; AD7492_Data[4], Position_adc_ctrl:inst6|Adc_Rd                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ; Position_Adjust:inst8|always0~115sexp, Position_Adjust:inst8|always0~151                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ;
;  C  ; LC45       ; AD7492_Data[3], Position_adc_ctrl:inst6|Adc_Rd                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ; Position_Adjust:inst8|always0~111sexp, Position_Adjust:inst8|always0~150                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ;
;  C  ; LC44       ; AD7492_Data[2], Position_adc_ctrl:inst6|Adc_Rd                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ; Position_Adjust:inst8|always0~107sexp, Position_Adjust:inst8|always0~149                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ;
;  C  ; LC40       ; Position_adc_ctrl:inst6|Position_Data[8], Position_Set[8]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           ; Position_Adjust:inst8|Position_Adjust_Out~10                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  ;
;  C  ; LC43       ; AD7492_Data[1], Position_adc_ctrl:inst6|Adc_Rd                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ; Position_Adjust:inst8|always0~103sexp, Position_Adjust:inst8|always0~148                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ;
;  C  ; LC42       ; AD7492_Data[0], Position_adc_ctrl:inst6|Adc_Rd                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ; Position_Adjust:inst8|always0~99sexp, Position_Adjust:inst8|always0~147                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                       ;
;  D  ; LC52       ; AD7895_Data, main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_Read:b2v_inst1|Data[11], main:inst3|Data_drive:b2v_inst|Adc_SCL~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; main:inst3|Data_Read:b2v_inst1|Data[11], Current_Adjust:inst5|always0~127sexp, Current_Adjust:inst5|always0~154                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                               ;
;  D  ; LC53       ; AD7895_Data, main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|Data[9], main:inst3|Data_drive:b2v_inst|Adc_SCL~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ; main:inst3|Data_Read:b2v_inst1|Data[9], Current_Adjust:inst5|always0~119sexp, Current_Adjust:inst5|always0~152                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  D  ; LC54       ; AD7895_Data, main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_Read:b2v_inst1|Data[7], main:inst3|Data_drive:b2v_inst|Adc_SCL~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ; main:inst3|Data_Read:b2v_inst1|Data[7], Current_Adjust:inst5|always0~111sexp, Current_Adjust:inst5|always0~150                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  D  ; LC55       ; AD7895_Data, main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|Data[6], main:inst3|Data_drive:b2v_inst|Adc_SCL~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ; main:inst3|Data_Read:b2v_inst1|Data[6], Current_Adjust:inst5|always0~107sexp, Current_Adjust:inst5|always0~149                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  D  ; LC56       ; AD7895_Data, main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|Data[5], main:inst3|Data_drive:b2v_inst|Adc_SCL~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ; main:inst3|Data_Read:b2v_inst1|Data[5], Current_Adjust:inst5|always0~103sexp, Current_Adjust:inst5|always0~148                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  D  ; LC57       ; AD7895_Data, main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|Data[4], main:inst3|Data_drive:b2v_inst|Adc_SCL~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ; main:inst3|Data_Read:b2v_inst1|Data[4], Current_Adjust:inst5|always0~99sexp, Current_Adjust:inst5|always0~147                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 ;
;  D  ; LC58       ; AD7895_Data, main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_Read:b2v_inst1|Data[10], main:inst3|Data_drive:b2v_inst|Adc_SCL~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; main:inst3|Data_Read:b2v_inst1|Data[10], Current_Adjust:inst5|always0~123sexp, Current_Adjust:inst5|always0~153                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                               ;
;  D  ; LC59       ; AD7895_Data, main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|Data[8], main:inst3|Data_drive:b2v_inst|Adc_SCL~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ; main:inst3|Data_Read:b2v_inst1|Data[8], Current_Adjust:inst5|always0~115sexp, Current_Adjust:inst5|always0~151                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  D  ; LC51       ; AD7895_Data, main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|Data[13], main:inst3|Data_drive:b2v_inst|Adc_SCL~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; main:inst3|Data_Read:b2v_inst1|Data[13], Current_Adjust:inst5|always0~135                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ;
;  D  ; LC50       ; AD7895_Data, main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|Data[14], main:inst3|Data_drive:b2v_inst|Adc_SCL~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; main:inst3|Data_Read:b2v_inst1|Data[14], Current_Adjust:inst5|always0~139                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ;
;  D  ; LC64       ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_drive:b2v_inst|Adc_SCL~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 ; main:inst3|Data_Read:b2v_inst1|Data[14], main:inst3|Data_Read:b2v_inst1|Data[13], main:inst3|Data_Read:b2v_inst1|Data[12], main:inst3|Data_Read:b2v_inst1|Data[11], main:inst3|Data_Read:b2v_inst1|Data[9], main:inst3|Data_Read:b2v_inst1|Data[7], main:inst3|Data_Read:b2v_inst1|Data[6], main:inst3|Data_Read:b2v_inst1|Data[5], main:inst3|Data_Read:b2v_inst1|Data[4], main:inst3|Data_Read:b2v_inst1|Data[15], main:inst3|Data_Read:b2v_inst1|Data[10], main:inst3|Data_Read:b2v_inst1|Data[8]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                          ;
;  D  ; LC63       ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_drive:b2v_inst|Adc_SCL~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                               ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|Data[14], main:inst3|Data_Read:b2v_inst1|Data[13], main:inst3|Data_Read:b2v_inst1|Data[12], main:inst3|Data_Read:b2v_inst1|Data[11], main:inst3|Data_Read:b2v_inst1|Data[9], main:inst3|Data_Read:b2v_inst1|Data[7], main:inst3|Data_Read:b2v_inst1|Data[6], main:inst3|Data_Read:b2v_inst1|Data[5], main:inst3|Data_Read:b2v_inst1|Data[4], main:inst3|Data_Read:b2v_inst1|Data[15], main:inst3|Data_Read:b2v_inst1|Data[10], main:inst3|Data_Read:b2v_inst1|Data[8]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ;
;  D  ; LC62       ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_drive:b2v_inst|Adc_SCL~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|Data[14], main:inst3|Data_Read:b2v_inst1|Data[13], main:inst3|Data_Read:b2v_inst1|Data[12], main:inst3|Data_Read:b2v_inst1|Data[11], main:inst3|Data_Read:b2v_inst1|Data[9], main:inst3|Data_Read:b2v_inst1|Data[7], main:inst3|Data_Read:b2v_inst1|Data[6], main:inst3|Data_Read:b2v_inst1|Data[5], main:inst3|Data_Read:b2v_inst1|Data[4], main:inst3|Data_Read:b2v_inst1|Data[15], main:inst3|Data_Read:b2v_inst1|Data[10], main:inst3|Data_Read:b2v_inst1|Data[8]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ;
;  D  ; LC61       ; main:inst3|Data_drive:b2v_inst|Adc_SCL~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|Data[14], main:inst3|Data_Read:b2v_inst1|Data[13], main:inst3|Data_Read:b2v_inst1|Data[12], main:inst3|Data_Read:b2v_inst1|Data[11], main:inst3|Data_Read:b2v_inst1|Data[9], main:inst3|Data_Read:b2v_inst1|Data[7], main:inst3|Data_Read:b2v_inst1|Data[6], main:inst3|Data_Read:b2v_inst1|Data[5], main:inst3|Data_Read:b2v_inst1|Data[4], main:inst3|Data_Read:b2v_inst1|Data[15], main:inst3|Data_Read:b2v_inst1|Data[10], main:inst3|Data_Read:b2v_inst1|Data[8]                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  D  ; LC49       ; Clk_SCL, main:inst3|Data_drive:b2v_inst|Adc_Conv, Current_SW, Reset, AD7895_Busy, main:inst3|Data_drive:b2v_inst|cnt1[1], main:inst3|Data_drive:b2v_inst|cnt1[5], main:inst3|Data_drive:b2v_inst|cnt1[0], main:inst3|Data_drive:b2v_inst|cnt1[4], main:inst3|Data_drive:b2v_inst|cnt1[3], main:inst3|Data_drive:b2v_inst|cnt1[2]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ; main:inst3|Data_drive:b2v_inst|Adc_Conv, AD7895_Conv                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                          ;
;  D  ; LC60       ; Clk_SCL, main:inst3|Data_drive:b2v_inst|cnt1[1], main:inst3|Data_drive:b2v_inst|cnt1[5], main:inst3|Data_drive:b2v_inst|cnt1[4], main:inst3|Data_drive:b2v_inst|cnt1[0], main:inst3|Data_drive:b2v_inst|cnt1[3], main:inst3|Data_drive:b2v_inst|cnt1[2], Current_SW, Reset, AD7895_Busy                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; main:inst3|Data_drive:b2v_inst|Adc_SCL~41, main:inst3|Data_drive:b2v_inst|Adc_SCL~42, main:inst3|Data_drive:b2v_inst|Adc_SCL~58                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                               ;
;  E  ; LC76       ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Set[14]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; Rate_Adjust:inst11|Rate_Adjust_Out~14                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  E  ; LC80       ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Set[13]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; Rate_Adjust:inst11|Rate_Adjust_Out~14                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  E  ; LC69       ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Set[12]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; Rate_Adjust:inst11|Rate_Adjust_Out~14                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  E  ; LC79       ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Set[11]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; Rate_Adjust:inst11|Rate_Adjust_Out~14                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  E  ; LC71       ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Set[10]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; Rate_Adjust:inst11|Rate_Adjust_Out~14                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  E  ; LC72       ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Set[9]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           ; Rate_Adjust:inst11|Rate_Adjust_Out~14                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  E  ; LC67       ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Reset, Rate_SW, Rate_Pulse, Rate_Measure_Ctrl                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~131sexp, Rate_Adjust:inst11|always0~195 ;
;  E  ; LC68       ; Position_adc_ctrl:inst6|Position_Data[10], Position_Set[10]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; Position_Adjust:inst8|Position_Adjust_Out~10                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  ;
;  E  ; LC66       ; Reset, Rate_SW, Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0], Rate_Pulse, Rate_Measure_Ctrl                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14], Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Measure:inst2|Rate_Pulse_Alarm, Rate_Adjust:inst11|always0~135sexp, Rate_Adjust:inst11|always0~196                                                               ;
;  E  ; LC74       ; main:inst3|Data_Read:b2v_inst1|Data[15], Current_Set[11]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ; Current_Adjust:inst5|Current_Adjust_Out~14                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  E  ; LC75       ; main:inst3|Data_Read:b2v_inst1|Data[12], Current_Set[8]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; Current_Adjust:inst5|Current_Adjust_Out~14                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  E  ; LC65       ; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select, Clk_SCL                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ; AD7895_SCL                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  E  ; LC73       ; AD7895_Data, main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_Read:b2v_inst1|Data[15], main:inst3|Data_drive:b2v_inst|Adc_SCL~58                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; main:inst3|Data_Read:b2v_inst1|Data[15], Current_Adjust:inst5|always0~143                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ;
;  E  ; LC77       ; AD7895_Data, main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0], main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2], main:inst3|Data_Read:b2v_inst1|Data[12], main:inst3|Data_drive:b2v_inst|Adc_SCL~58                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; main:inst3|Data_Read:b2v_inst1|Data[12], Current_Adjust:inst5|always0~131                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ;
;  F  ; LC84       ; Position_adc_ctrl:inst6|Position_Data[11], Position_Set[11]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; Position_Adjust:inst8|Position_Adjust_Out~10                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  ;
;  F  ; LC81       ; Current_Adjust:inst5|always0~131, Current_Adjust:inst5|always0~135, Current_Adjust:inst5|always0~139, Current_Adjust:inst5|always0~143, Current_SW, Reset, Current_Adjust:inst5|always0~99sexp, Current_Adjust:inst5|always0~147, Current_Adjust:inst5|always0~103sexp, Current_Adjust:inst5|always0~148, Current_Adjust:inst5|always0~107sexp, Current_Adjust:inst5|always0~149, Current_Adjust:inst5|always0~111sexp, Current_Adjust:inst5|always0~150, Current_Adjust:inst5|always0~115sexp, Current_Adjust:inst5|always0~151, Current_Adjust:inst5|always0~119sexp, Current_Adjust:inst5|always0~152, Current_Adjust:inst5|always0~123sexp, Current_Adjust:inst5|always0~153, Current_Adjust:inst5|always0~127sexp, Current_Adjust:inst5|always0~154                                                                                                                                                                                                                                                                                                                            ; Current_Adjust_Drive                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                          ;
;  F  ; LC89       ; main:inst3|Data_Read:b2v_inst1|Data[14], Current_Set[10]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ; Current_Adjust:inst5|Current_Adjust_Out~14                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  F  ; LC90       ; main:inst3|Data_Read:b2v_inst1|Data[13], Current_Set[9]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; Current_Adjust:inst5|Current_Adjust_Out~14                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  F  ; LC91       ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15], Rate_Set[15]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; Rate_Adjust:inst11|Rate_Adjust_Out~14                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  G  ; LC97       ; Position_Adjust:inst8|always0~131, Position_Adjust:inst8|always0~135, Position_Adjust:inst8|always0~139, Position_Adjust:inst8|always0~143, Reset, Position_SW, Position_Adjust:inst8|always0~99sexp, Position_Adjust:inst8|always0~147, Position_Adjust:inst8|always0~103sexp, Position_Adjust:inst8|always0~148, Position_Adjust:inst8|always0~107sexp, Position_Adjust:inst8|always0~149, Position_Adjust:inst8|always0~111sexp, Position_Adjust:inst8|always0~150, Position_Adjust:inst8|always0~115sexp, Position_Adjust:inst8|always0~151, Position_Adjust:inst8|always0~119sexp, Position_Adjust:inst8|always0~152, Position_Adjust:inst8|always0~123sexp, Position_Adjust:inst8|always0~153, Position_Adjust:inst8|always0~127sexp, Position_Adjust:inst8|always0~154                                                                                                                                                                                                                                                                                                       ; Position_Adjust_Drive                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  H  ; LC113      ; Rate_Adjust:inst11|always0~163, Rate_Adjust:inst11|always0~167, Rate_Adjust:inst11|always0~171, Rate_Adjust:inst11|always0~175, Rate_Adjust:inst11|always0~179, Rate_Adjust:inst11|always0~183, Rate_Adjust:inst11|always0~187, Rate_Adjust:inst11|always0~191, Reset, Rate_SW, Rate_Adjust:inst11|always0~131sexp, Rate_Adjust:inst11|always0~195, Rate_Adjust:inst11|always0~135sexp, Rate_Adjust:inst11|always0~196, Rate_Adjust:inst11|always0~139sexp, Rate_Adjust:inst11|always0~197, Rate_Adjust:inst11|always0~143sexp, Rate_Adjust:inst11|always0~198, Rate_Adjust:inst11|always0~147sexp, Rate_Adjust:inst11|always0~199, Rate_Adjust:inst11|always0~151sexp, Rate_Adjust:inst11|always0~200, Rate_Adjust:inst11|always0~155sexp, Rate_Adjust:inst11|always0~201, Rate_Adjust:inst11|always0~159sexp, Rate_Adjust:inst11|always0~202                                                                                                                                                                                                                                      ; Rate_Adjust_Drive                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ;
+-----+------------+-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+


+-----------------+
; Fitter Messages ;
+-----------------+
Info: *******************************************************************
Info: Running Quartus II Fitter
    Info: Version 4.2 Build 157 12/07/2004 SJ Full Version
    Info: Processing started: Fri Aug 04 19:03:45 2006
Info: Command: quartus_fit --import_settings_files=off --export_settings_files=off DC_Motor_Main -c DC_Motor_Main
Info: Automatically selected device EPM7128STC100-6 for design DC_Motor_Main
Info: Fitting design with smaller device may be possible, but smaller device must be specified
Info: Quartus II Fitter was successful. 0 errors, 0 warnings
    Info: Processing ended: Fri Aug 04 19:03:47 2006
    Info: Elapsed time: 00:00:04


