--A1L5Q is Q~reg0
A1L5Q_reg_input = VCC;
A1L5Q = TFFE(A1L5Q_reg_input, GLOBAL(T), , , EN);


--A1L4Q is QN~reg0
A1L4Q_or_out = A1L5Q;
A1L4Q_reg_input = A1L4Q_or_out;
A1L4Q = DFFE(A1L4Q_reg_input, GLOBAL(T), , , EN);


--EN is EN
--operation mode is input

EN = INPUT();


--T is T
--operation mode is input

T = INPUT();


--Q is Q
--operation mode is output

Q = OUTPUT(A1L5Q);


--QN is QN
--operation mode is output

QN = OUTPUT(A1L4Q);


