--A1L63 is pulse_16_out~232
A1L63_p1_out = !Reset & counter_data[0];
A1L63_or_out = A1L63_p1_out;
A1L63 = A1L63_or_out;


--A1L73 is pulse_16_out~234
A1L73_p1_out = counter_data[1] & !Reset & !counter_data[0];
A1L73_or_out = A1L73_p1_out;
A1L73 = A1L73_or_out;


--A1L83 is pulse_16_out~236
A1L83_p1_out = counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L83_or_out = A1L83_p1_out;
A1L83 = A1L83_or_out;


--A1L93 is pulse_16_out~238
A1L93_p1_out = counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L93_or_out = A1L93_p1_out;
A1L93 = A1L93_or_out;


--A1L04 is pulse_16_out~240
A1L04_p1_out = counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L04_or_out = A1L04_p1_out;
A1L04 = A1L04_or_out;


--A1L14 is pulse_16_out~242
A1L14_p1_out = counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L14_or_out = A1L14_p1_out;
A1L14 = A1L14_or_out;


--A1L24 is pulse_16_out~244
A1L24_p1_out = counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L24_or_out = A1L24_p1_out;
A1L24 = A1L24_or_out;


--A1L34 is pulse_16_out~246
A1L34_p1_out = counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L34_or_out = A1L34_p1_out;
A1L34 = A1L34_or_out;


--A1L44 is pulse_16_out~248
A1L44_p1_out = counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L44_or_out = A1L44_p1_out;
A1L44 = A1L44_or_out;


--A1L54 is pulse_16_out~250
A1L54_p1_out = counter_data[9] & !counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L54_or_out = A1L54_p1_out;
A1L54 = A1L54_or_out;


--A1L64 is pulse_16_out~252
A1L64_p1_out = counter_data[10] & !counter_data[9] & !counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L64_or_out = A1L64_p1_out;
A1L64 = A1L64_or_out;


--A1L74 is pulse_16_out~254
A1L74_p1_out = counter_data[11] & !counter_data[10] & !counter_data[9] & !counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L74_or_out = A1L74_p1_out;
A1L74 = A1L74_or_out;


--A1L84 is pulse_16_out~256
A1L84_p1_out = counter_data[12] & !counter_data[11] & !counter_data[10] & !counter_data[9] & !counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L84_or_out = A1L84_p1_out;
A1L84 = A1L84_or_out;


--A1L94 is pulse_16_out~258
A1L94_p1_out = counter_data[13] & !counter_data[12] & !counter_data[11] & !counter_data[10] & !counter_data[9] & !counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L94_or_out = A1L94_p1_out;
A1L94 = A1L94_or_out;


--A1L05 is pulse_16_out~260
A1L05_p1_out = counter_data[14] & !counter_data[13] & !counter_data[12] & !counter_data[11] & !counter_data[10] & !counter_data[9] & !counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L05_or_out = A1L05_p1_out;
A1L05 = A1L05_or_out;


--A1L15 is pulse_16_out~262
A1L15_p1_out = !counter_data[14] & !counter_data[13] & !counter_data[12] & !counter_data[11] & !counter_data[10] & !counter_data[9] & !counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0] & counter_data[15];
A1L15_or_out = A1L15_p1_out;
A1L15 = A1L15_or_out;


--Reset is Reset
--operation mode is input

Reset = INPUT();


--counter_data[15] is counter_data[15]
--operation mode is input

counter_data[15] = INPUT();


--counter_data[14] is counter_data[14]
--operation mode is input

counter_data[14] = INPUT();


--counter_data[13] is counter_data[13]
--operation mode is input

counter_data[13] = INPUT();


--counter_data[12] is counter_data[12]
--operation mode is input

counter_data[12] = INPUT();


--counter_data[11] is counter_data[11]
--operation mode is input

counter_data[11] = INPUT();


--counter_data[10] is counter_data[10]
--operation mode is input

counter_data[10] = INPUT();


--counter_data[9] is counter_data[9]
--operation mode is input

counter_data[9] = INPUT();


--counter_data[8] is counter_data[8]
--operation mode is input

counter_data[8] = INPUT();


--counter_data[7] is counter_data[7]
--operation mode is input

counter_data[7] = INPUT();


--counter_data[6] is counter_data[6]
--operation mode is input

counter_data[6] = INPUT();


--counter_data[5] is counter_data[5]
--operation mode is input

counter_data[5] = INPUT();


--counter_data[4] is counter_data[4]
--operation mode is input

counter_data[4] = INPUT();


--counter_data[3] is counter_data[3]
--operation mode is input

counter_data[3] = INPUT();


--counter_data[2] is counter_data[2]
--operation mode is input

counter_data[2] = INPUT();


--counter_data[1] is counter_data[1]
--operation mode is input

counter_data[1] = INPUT();


--counter_data[0] is counter_data[0]
--operation mode is input

counter_data[0] = INPUT();


--pulse_16_out[15] is pulse_16_out[15]
--operation mode is output

pulse_16_out[15] = OUTPUT(A1L63);


--pulse_16_out[14] is pulse_16_out[14]
--operation mode is output

pulse_16_out[14] = OUTPUT(A1L73);


--pulse_16_out[13] is pulse_16_out[13]
--operation mode is output

pulse_16_out[13] = OUTPUT(A1L83);


--pulse_16_out[12] is pulse_16_out[12]
--operation mode is output

pulse_16_out[12] = OUTPUT(A1L93);


--pulse_16_out[11] is pulse_16_out[11]
--operation mode is output

pulse_16_out[11] = OUTPUT(A1L04);


--pulse_16_out[10] is pulse_16_out[10]
--operation mode is output

pulse_16_out[10] = OUTPUT(A1L14);


--pulse_16_out[9] is pulse_16_out[9]
--operation mode is output

pulse_16_out[9] = OUTPUT(A1L24);


--pulse_16_out[8] is pulse_16_out[8]
--operation mode is output

pulse_16_out[8] = OUTPUT(A1L34);


--pulse_16_out[7] is pulse_16_out[7]
--operation mode is output

pulse_16_out[7] = OUTPUT(A1L44);


--pulse_16_out[6] is pulse_16_out[6]
--operation mode is output

pulse_16_out[6] = OUTPUT(A1L54);


--pulse_16_out[5] is pulse_16_out[5]
--operation mode is output

pulse_16_out[5] = OUTPUT(A1L64);


--pulse_16_out[4] is pulse_16_out[4]
--operation mode is output

pulse_16_out[4] = OUTPUT(A1L74);


--pulse_16_out[3] is pulse_16_out[3]
--operation mode is output

pulse_16_out[3] = OUTPUT(A1L84);


--pulse_16_out[2] is pulse_16_out[2]
--operation mode is output

pulse_16_out[2] = OUTPUT(A1L94);


--pulse_16_out[1] is pulse_16_out[1]
--operation mode is output

pulse_16_out[1] = OUTPUT(A1L05);


--pulse_16_out[0] is pulse_16_out[0]
--operation mode is output

pulse_16_out[0] = OUTPUT(A1L15);


