--A1L4Q is Adc_Cs~reg0
--operation mode is normal

A1L4Q_lut_out = Reset # En;
A1L4Q = DFFEA(A1L4Q_lut_out, Clk, , , , , );


--A1L2Q is Adc_Conv~reg0
--operation mode is normal

A1L2Q_lut_out = Reset # En # !Adc_Over;
A1L2Q = DFFEA(A1L2Q_lut_out, Clk, , , , , );


--A1L91Q is Adc_Mode~reg0
--operation mode is normal

A1L91Q_lut_out = !Reset & !En;
A1L91Q = DFFEA(A1L91Q_lut_out, Clk, , , , , );


--A1L22Q is Adc_Rd~reg0
--operation mode is normal

A1L22Q_lut_out = Reset # En # Adc_Over;
A1L22Q = DFFEA(A1L22Q_lut_out, Clk, , , , , );


--A1L94Q is Position_Data[11]~reg0
--operation mode is normal

A1L94Q_lut_out = Adc_Data[11];
A1L94Q = DFFEA(A1L94Q_lut_out, !A1L22Q, , , , , );


--A1L74Q is Position_Data[10]~reg0
--operation mode is normal

A1L74Q_lut_out = Adc_Data[10];
A1L74Q = DFFEA(A1L74Q_lut_out, !A1L22Q, , , , , );


--A1L54Q is Position_Data[9]~reg0
--operation mode is normal

A1L54Q_lut_out = Adc_Data[9];
A1L54Q = DFFEA(A1L54Q_lut_out, !A1L22Q, , , , , );


--A1L34Q is Position_Data[8]~reg0
--operation mode is normal

A1L34Q_lut_out = Adc_Data[8];
A1L34Q = DFFEA(A1L34Q_lut_out, !A1L22Q, , , , , );


--A1L14Q is Position_Data[7]~reg0
--operation mode is normal

A1L14Q_lut_out = Adc_Data[7];
A1L14Q = DFFEA(A1L14Q_lut_out, !A1L22Q, , , , , );


--A1L93Q is Position_Data[6]~reg0
--operation mode is normal

A1L93Q_lut_out = Adc_Data[6];
A1L93Q = DFFEA(A1L93Q_lut_out, !A1L22Q, , , , , );


--A1L73Q is Position_Data[5]~reg0
--operation mode is normal

A1L73Q_lut_out = Adc_Data[5];
A1L73Q = DFFEA(A1L73Q_lut_out, !A1L22Q, , , , , );


--A1L53Q is Position_Data[4]~reg0
--operation mode is normal

A1L53Q_lut_out = Adc_Data[4];
A1L53Q = DFFEA(A1L53Q_lut_out, !A1L22Q, , , , , );


--A1L33Q is Position_Data[3]~reg0
--operation mode is normal

A1L33Q_lut_out = Adc_Data[3];
A1L33Q = DFFEA(A1L33Q_lut_out, !A1L22Q, , , , , );


--A1L13Q is Position_Data[2]~reg0
--operation mode is normal

A1L13Q_lut_out = Adc_Data[2];
A1L13Q = DFFEA(A1L13Q_lut_out, !A1L22Q, , , , , );


--A1L92Q is Position_Data[1]~reg0
--operation mode is normal

A1L92Q_lut_out = Adc_Data[1];
A1L92Q = DFFEA(A1L92Q_lut_out, !A1L22Q, , , , , );


--A1L72Q is Position_Data[0]~reg0
--operation mode is normal

A1L72Q_lut_out = Adc_Data[0];
A1L72Q = DFFEA(A1L72Q_lut_out, !A1L22Q, , , , , );


--Reset is Reset
--operation mode is input

Reset = INPUT();


--En is En
--operation mode is input

En = INPUT();


--Clk is Clk
--operation mode is input

Clk = INPUT();


--Adc_Over is Adc_Over
--operation mode is input

Adc_Over = INPUT();


--Adc_Data[11] is Adc_Data[11]
--operation mode is input

Adc_Data[11] = INPUT();


--Adc_Data[10] is Adc_Data[10]
--operation mode is input

Adc_Data[10] = INPUT();


--Adc_Data[9] is Adc_Data[9]
--operation mode is input

Adc_Data[9] = INPUT();


--Adc_Data[8] is Adc_Data[8]
--operation mode is input

Adc_Data[8] = INPUT();


--Adc_Data[7] is Adc_Data[7]
--operation mode is input

Adc_Data[7] = INPUT();


--Adc_Data[6] is Adc_Data[6]
--operation mode is input

Adc_Data[6] = INPUT();


--Adc_Data[5] is Adc_Data[5]
--operation mode is input

Adc_Data[5] = INPUT();


--Adc_Data[4] is Adc_Data[4]
--operation mode is input

Adc_Data[4] = INPUT();


--Adc_Data[3] is Adc_Data[3]
--operation mode is input

Adc_Data[3] = INPUT();


--Adc_Data[2] is Adc_Data[2]
--operation mode is input

Adc_Data[2] = INPUT();


--Adc_Data[1] is Adc_Data[1]
--operation mode is input

Adc_Data[1] = INPUT();


--Adc_Data[0] is Adc_Data[0]
--operation mode is input

Adc_Data[0] = INPUT();


--Adc_Cs is Adc_Cs
--operation mode is output

Adc_Cs = OUTPUT(A1L4Q);


--Adc_Conv is Adc_Conv
--operation mode is output

Adc_Conv = OUTPUT(A1L2Q);


--Adc_Mode is Adc_Mode
--operation mode is output

Adc_Mode = OUTPUT(A1L91Q);


--Adc_Rd is Adc_Rd
--operation mode is output

Adc_Rd = OUTPUT(A1L22Q);


--Position_Data[11] is Position_Data[11]
--operation mode is output

Position_Data[11] = OUTPUT(A1L94Q);


--Position_Data[10] is Position_Data[10]
--operation mode is output

Position_Data[10] = OUTPUT(A1L74Q);


--Position_Data[9] is Position_Data[9]
--operation mode is output

Position_Data[9] = OUTPUT(A1L54Q);


--Position_Data[8] is Position_Data[8]
--operation mode is output

Position_Data[8] = OUTPUT(A1L34Q);


--Position_Data[7] is Position_Data[7]
--operation mode is output

Position_Data[7] = OUTPUT(A1L14Q);


--Position_Data[6] is Position_Data[6]
--operation mode is output

Position_Data[6] = OUTPUT(A1L93Q);


--Position_Data[5] is Position_Data[5]
--operation mode is output

Position_Data[5] = OUTPUT(A1L73Q);


--Position_Data[4] is Position_Data[4]
--operation mode is output

Position_Data[4] = OUTPUT(A1L53Q);


--Position_Data[3] is Position_Data[3]
--operation mode is output

Position_Data[3] = OUTPUT(A1L33Q);


--Position_Data[2] is Position_Data[2]
--operation mode is output

Position_Data[2] = OUTPUT(A1L13Q);


--Position_Data[1] is Position_Data[1]
--operation mode is output

Position_Data[1] = OUTPUT(A1L92Q);


--Position_Data[0] is Position_Data[0]
--operation mode is output

Position_Data[0] = OUTPUT(A1L72Q);


