Fitter report for second_pulse_latch
Wed Jul 19 23:02:13 2006
Version 4.2 Build 157 12/07/2004 SJ Full Version


---------------------
; Table of Contents ;
---------------------
  1. Legal Notice
  2. Fitter Summary
  3. Fitter Settings
  4. Fitter Device Options
  5. Fitter Equations
  6. Pin-Out File
  7. Fitter Resource Usage Summary
  8. Input Pins
  9. Output Pins
 10. All Package Pins
 11. I/O Standard
 12. Dedicated Inputs I/O
 13. Output Pin Default Load For Reported TCO
 14. Fitter Resource Utilization by Entity
 15. Control Signals
 16. Global & Other Fast Signals
 17. Non-Global High Fan-Out Signals
 18. Interconnect Usage Summary
 19. LAB External Interconnect
 20. LAB Macrocells
 21. Parallel Expander
 22. Shareable Expander
 23. Logic Cell Interconnection
 24. Fitter Messages



----------------
; Legal Notice ;
----------------
Copyright (C) 1991-2004 Altera Corporation
Any  megafunction  design,  and related netlist (encrypted  or  decrypted),
support information,  device programming or simulation file,  and any other
associated  documentation or information  provided by  Altera  or a partner
under  Altera's   Megafunction   Partnership   Program  may  be  used  only
to program  PLD  devices (but not masked  PLD  devices) from  Altera.   Any
other  use  of such  megafunction  design,  netlist,  support  information,
device programming or simulation file,  or any other  related documentation
or information  is prohibited  for  any  other purpose,  including, but not
limited to  modification,  reverse engineering,  de-compiling, or use  with
any other  silicon devices,  unless such use is  explicitly  licensed under
a separate agreement with  Altera  or a megafunction partner.  Title to the
intellectual property,  including patents,  copyrights,  trademarks,  trade
secrets,  or maskworks,  embodied in any such megafunction design, netlist,
support  information,  device programming or simulation file,  or any other
related documentation or information provided by  Altera  or a megafunction
partner, remains with Altera, the megafunction partner, or their respective
licensors. No other licenses, including any licenses needed under any third
party's intellectual property, are provided herein.



+------------------------------------------------------------------+
; Fitter Summary                                                   ;
+-----------------------+------------------------------------------+
; Fitter Status         ; Successful - Wed Jul 19 23:02:13 2006    ;
; Quartus II Version    ; 4.2 Build 157 12/07/2004 SJ Full Version ;
; Revision Name         ; second_pulse_latch                       ;
; Top-level Entity Name ; second_pulse_latch                       ;
; Family                ; MAX7000S                                 ;
; Device                ; EPM7128SLC84-6                           ;
; Timing Models         ; Final                                    ;
; Total macrocells      ; 93 / 128 ( 72 % )                        ;
; Total pins            ; 55 / 68 ( 80 % )                         ;
+-----------------------+------------------------------------------+


+--------------------------------------------------------------------------------------+
; Fitter Settings                                                                      ;
+--------------------------------------------+--------------------+--------------------+
; Option                                     ; Setting            ; Default Value      ;
+--------------------------------------------+--------------------+--------------------+
; Device                                     ; AUTO               ;                    ;
; Use smart compilation                      ; Normal             ; Normal             ;
; Optimize Timing                            ; Normal compilation ; Normal compilation ;
; Optimize IOC Register Placement for Timing ; On                 ; On                 ;
; Limit to One Fitting Attempt               ; Off                ; Off                ;
; Fitter Initial Placement Seed              ; 1                  ; 1                  ;
; Slow Slew Rate                             ; Off                ; Off                ;
; Fitter Effort                              ; Auto Fit           ; Auto Fit           ;
+--------------------------------------------+--------------------+--------------------+


+----------------------------------------------------------------------------------------+
; Fitter Device Options                                                                  ;
+----------------------------------------------+-----------------------------------------+
; Option                                       ; Setting                                 ;
+----------------------------------------------+-----------------------------------------+
; Enable user-supplied start-up clock (CLKUSR) ; Off                                     ;
; Enable device-wide reset (DEV_CLRn)          ; Off                                     ;
; Enable device-wide output enable (DEV_OE)    ; Off                                     ;
; Enable INIT_DONE output                      ; Off                                     ;
; Configuration scheme                         ; Passive Serial                          ;
; Reserve all unused pins                      ; As output driving an unspecified signal ;
; Security bit                                 ; Off                                     ;
; Base pin-out file on sameframe device        ; Off                                     ;
+----------------------------------------------+-----------------------------------------+


+------------------+
; Fitter Equations ;
+------------------+
The equations can be found in E:/戴仙金/资料/Verilog书/源代码/step_motor/second_pulse_latch/second_pulse_latch.fit.eqn.


+--------------+
; Pin-Out File ;
+--------------+
The pin-out file can be found in E:/戴仙金/资料/Verilog书/源代码/step_motor/second_pulse_latch/second_pulse_latch.pin.


+---------------------------------------------------+
; Fitter Resource Usage Summary                     ;
+-------------------------------+-------------------+
; Resource                      ; Usage             ;
+-------------------------------+-------------------+
; Logic cells                   ; 93 / 128 ( 72 % ) ;
; Registers                     ; 16 / 128 ( 12 % ) ;
; Number of pterms used         ; 414               ;
; User inserted logic elements  ; 0                 ;
; I/O pins                      ; 55 / 68 ( 80 % )  ;
;     -- Clock pins             ; 1 / 2 ( 50 % )    ;
;     -- Dedicated input pins   ; 0 / 2 ( 0 % )     ;
; Global signals                ; 1                 ;
; Shareable expanders           ; 77 / 128 ( 60 % ) ;
; Parallel expanders            ; 26 / 120 ( 21 % ) ;
; Cells using turbo bit         ; 93 / 128 ( 72 % ) ;
; Maximum fan-out node          ; acceleration[1]   ;
; Maximum fan-out               ; 24                ;
; Total fan-out                 ; 846               ;
; Average fan-out               ; 3.76              ;
+-------------------------------+-------------------+


+--------------------------------------------------------------------------------------------------------------------------------------------------------+
; Input Pins                                                                                                                                             ;
+------------------+-------+----------+-----+-----------------------+--------------------+--------+----------------+--------------+----------------------+
; Name             ; Pin # ; I/O Bank ; LAB ; Combinational Fan-Out ; Registered Fan-Out ; Global ; Input Register ; I/O Standard ; Location assigned by ;
+------------------+-------+----------+-----+-----------------------+--------------------+--------+----------------+--------------+----------------------+
; Clk_1Hz          ; 83    ; --       ; --  ; 16                    ; 0                  ; yes    ; no             ; TTL          ; Fitter               ;
; Reset            ; 5     ; --       ; 1   ; 22                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[0]  ; 57    ; --       ; 6   ; 19                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[10] ; 45    ; --       ; 5   ; 16                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[11] ; 61    ; --       ; 6   ; 14                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[12] ; 54    ; --       ; 6   ; 14                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[13] ; 68    ; --       ; 7   ; 13                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[14] ; 81    ; --       ; 8   ; 9                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[15] ; 15    ; --       ; 2   ; 4                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[16] ; 52    ; --       ; 5   ; 23                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[1]  ; 48    ; --       ; 5   ; 24                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[2]  ; 18    ; --       ; 2   ; 20                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[3]  ; 49    ; --       ; 5   ; 17                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[4]  ; 76    ; --       ; 8   ; 14                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[5]  ; 16    ; --       ; 2   ; 14                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[6]  ; 29    ; --       ; 3   ; 11                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[7]  ; 51    ; --       ; 5   ; 17                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[8]  ; 11    ; --       ; 1   ; 20                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; acceleration[9]  ; 4     ; --       ; 1   ; 19                    ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[0]         ; 6     ; --       ; 1   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[10]        ; 67    ; --       ; 7   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[11]        ; 56    ; --       ; 6   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[12]        ; 75    ; --       ; 8   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[13]        ; 74    ; --       ; 8   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[14]        ; 65    ; --       ; 7   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[15]        ; 80    ; --       ; 8   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[1]         ; 79    ; --       ; 8   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[2]         ; 60    ; --       ; 6   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[3]         ; 70    ; --       ; 7   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[4]         ; 8     ; --       ; 1   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[5]         ; 77    ; --       ; 8   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[6]         ; 69    ; --       ; 7   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[7]         ; 35    ; --       ; 4   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[8]         ; 58    ; --       ; 6   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
; speed[9]         ; 17    ; --       ; 2   ; 0                     ; 0                  ; no     ; no             ; TTL          ; Fitter               ;
+------------------+-------+----------+-----+-----------------------+--------------------+--------+----------------+--------------+----------------------+


+-----------------------------------------------------------------------------------------------------------------------------------------------------+
; Output Pins                                                                                                                                         ;
+----------------------+-------+----------+-----+-----------------+----------------+------------+---------------+--------------+----------------------+
; Name                 ; Pin # ; I/O Bank ; LAB ; Output Register ; Slow Slew Rate ; Open Drain ; TRI Primitive ; I/O Standard ; Location assigned by ;
+----------------------+-------+----------+-----+-----------------+----------------+------------+---------------+--------------+----------------------+
; second_pulse_out[0]  ; 27    ; --       ; 3   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[10] ; 25    ; --       ; 3   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[11] ; 24    ; --       ; 3   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[12] ; 33    ; --       ; 4   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[13] ; 34    ; --       ; 4   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[14] ; 39    ; --       ; 4   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[15] ; 36    ; --       ; 4   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[1]  ; 73    ; --       ; 8   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[2]  ; 10    ; --       ; 1   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[3]  ; 12    ; --       ; 1   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[4]  ; 9     ; --       ; 1   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[5]  ; 28    ; --       ; 3   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[6]  ; 37    ; --       ; 4   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[7]  ; 50    ; --       ; 5   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[8]  ; 46    ; --       ; 5   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
; second_pulse_out[9]  ; 30    ; --       ; 3   ; no              ; no             ; no         ; no            ; TTL          ; Fitter               ;
+----------------------+-------+----------+-----+-----------------+----------------+------------+---------------+--------------+----------------------+


+-------------------------------------------------------------------------------------------------------------+
; All Package Pins                                                                                            ;
+----------+------------+----------+----------------------+--------+--------------+---------+-----------------+
; Location ; Pad Number ; I/O Bank ; Pin Name/Usage       ; Dir.   ; I/O Standard ; Voltage ; User Assignment ;
+----------+------------+----------+----------------------+--------+--------------+---------+-----------------+
; 1        ; 0          ; --       ; GND+                 ;        ;              ;         ;                 ;
; 2        ; 1          ; --       ; GND+                 ;        ;              ;         ;                 ;
; 3        ; 2          ; --       ; VCCINT               ; power  ;              ; 5.0V    ;                 ;
; 4        ; 3          ; --       ; acceleration[9]      ; input  ; TTL          ;         ; N               ;
; 5        ; 4          ; --       ; Reset                ; input  ; TTL          ;         ; N               ;
; 6        ; 5          ; --       ; speed[0]             ; input  ; TTL          ;         ; N               ;
; 7        ; 6          ; --       ; GND                  ; gnd    ;              ;         ;                 ;
; 8        ; 7          ; --       ; speed[4]             ; input  ; TTL          ;         ; N               ;
; 9        ; 8          ; --       ; second_pulse_out[4]  ; output ; TTL          ;         ; N               ;
; 10       ; 9          ; --       ; second_pulse_out[2]  ; output ; TTL          ;         ; N               ;
; 11       ; 10         ; --       ; acceleration[8]      ; input  ; TTL          ;         ; N               ;
; 12       ; 11         ; --       ; second_pulse_out[3]  ; output ; TTL          ;         ; N               ;
; 13       ; 12         ; --       ; VCCIO                ; power  ;              ; 5.0V    ;                 ;
; 14       ; 13         ; --       ; +TDI                 ; input  ; TTL          ;         ; N               ;
; 15       ; 14         ; --       ; acceleration[15]     ; input  ; TTL          ;         ; N               ;
; 16       ; 15         ; --       ; acceleration[5]      ; input  ; TTL          ;         ; N               ;
; 17       ; 16         ; --       ; speed[9]             ; input  ; TTL          ;         ; N               ;
; 18       ; 17         ; --       ; acceleration[2]      ; input  ; TTL          ;         ; N               ;
; 19       ; 18         ; --       ; GND                  ; gnd    ;              ;         ;                 ;
; 20       ; 19         ; --       ; RESERVED             ;        ;              ;         ;                 ;
; 21       ; 20         ; --       ; RESERVED             ;        ;              ;         ;                 ;
; 22       ; 21         ; --       ; RESERVED             ;        ;              ;         ;                 ;
; 23       ; 22         ; --       ; +TMS                 ; input  ; TTL          ;         ; N               ;
; 24       ; 23         ; --       ; second_pulse_out[11] ; output ; TTL          ;         ; N               ;
; 25       ; 24         ; --       ; second_pulse_out[10] ; output ; TTL          ;         ; N               ;
; 26       ; 25         ; --       ; VCCIO                ; power  ;              ; 5.0V    ;                 ;
; 27       ; 26         ; --       ; second_pulse_out[0]  ; output ; TTL          ;         ; N               ;
; 28       ; 27         ; --       ; second_pulse_out[5]  ; output ; TTL          ;         ; N               ;
; 29       ; 28         ; --       ; acceleration[6]      ; input  ; TTL          ;         ; N               ;
; 30       ; 29         ; --       ; second_pulse_out[9]  ; output ; TTL          ;         ; N               ;
; 31       ; 30         ; --       ; RESERVED             ;        ;              ;         ;                 ;
; 32       ; 31         ; --       ; GND                  ; gnd    ;              ;         ;                 ;
; 33       ; 32         ; --       ; second_pulse_out[12] ; output ; TTL          ;         ; N               ;
; 34       ; 33         ; --       ; second_pulse_out[13] ; output ; TTL          ;         ; N               ;
; 35       ; 34         ; --       ; speed[7]             ; input  ; TTL          ;         ; N               ;
; 36       ; 35         ; --       ; second_pulse_out[15] ; output ; TTL          ;         ; N               ;
; 37       ; 36         ; --       ; second_pulse_out[6]  ; output ; TTL          ;         ; N               ;
; 38       ; 37         ; --       ; VCCIO                ; power  ;              ; 5.0V    ;                 ;
; 39       ; 38         ; --       ; second_pulse_out[14] ; output ; TTL          ;         ; N               ;
; 40       ; 39         ; --       ; RESERVED             ;        ;              ;         ;                 ;
; 41       ; 40         ; --       ; RESERVED             ;        ;              ;         ;                 ;
; 42       ; 41         ; --       ; GND                  ; gnd    ;              ;         ;                 ;
; 43       ; 42         ; --       ; VCCINT               ; power  ;              ; 5.0V    ;                 ;
; 44       ; 43         ; --       ; RESERVED             ;        ;              ;         ;                 ;
; 45       ; 44         ; --       ; acceleration[10]     ; input  ; TTL          ;         ; N               ;
; 46       ; 45         ; --       ; second_pulse_out[8]  ; output ; TTL          ;         ; N               ;
; 47       ; 46         ; --       ; GND                  ; gnd    ;              ;         ;                 ;
; 48       ; 47         ; --       ; acceleration[1]      ; input  ; TTL          ;         ; N               ;
; 49       ; 48         ; --       ; acceleration[3]      ; input  ; TTL          ;         ; N               ;
; 50       ; 49         ; --       ; second_pulse_out[7]  ; output ; TTL          ;         ; N               ;
; 51       ; 50         ; --       ; acceleration[7]      ; input  ; TTL          ;         ; N               ;
; 52       ; 51         ; --       ; acceleration[16]     ; input  ; TTL          ;         ; N               ;
; 53       ; 52         ; --       ; VCCIO                ; power  ;              ; 5.0V    ;                 ;
; 54       ; 53         ; --       ; acceleration[12]     ; input  ; TTL          ;         ; N               ;
; 55       ; 54         ; --       ; RESERVED             ;        ;              ;         ;                 ;
; 56       ; 55         ; --       ; speed[11]            ; input  ; TTL          ;         ; N               ;
; 57       ; 56         ; --       ; acceleration[0]      ; input  ; TTL          ;         ; N               ;
; 58       ; 57         ; --       ; speed[8]             ; input  ; TTL          ;         ; N               ;
; 59       ; 58         ; --       ; GND                  ; gnd    ;              ;         ;                 ;
; 60       ; 59         ; --       ; speed[2]             ; input  ; TTL          ;         ; N               ;
; 61       ; 60         ; --       ; acceleration[11]     ; input  ; TTL          ;         ; N               ;
; 62       ; 61         ; --       ; +TCK                 ; input  ; TTL          ;         ; N               ;
; 63       ; 62         ; --       ; RESERVED             ;        ;              ;         ;                 ;
; 64       ; 63         ; --       ; RESERVED             ;        ;              ;         ;                 ;
; 65       ; 64         ; --       ; speed[14]            ; input  ; TTL          ;         ; N               ;
; 66       ; 65         ; --       ; VCCIO                ; power  ;              ; 5.0V    ;                 ;
; 67       ; 66         ; --       ; speed[10]            ; input  ; TTL          ;         ; N               ;
; 68       ; 67         ; --       ; acceleration[13]     ; input  ; TTL          ;         ; N               ;
; 69       ; 68         ; --       ; speed[6]             ; input  ; TTL          ;         ; N               ;
; 70       ; 69         ; --       ; speed[3]             ; input  ; TTL          ;         ; N               ;
; 71       ; 70         ; --       ; *TDO                 ; output ; TTL          ;         ; N               ;
; 72       ; 71         ; --       ; GND                  ; gnd    ;              ;         ;                 ;
; 73       ; 72         ; --       ; second_pulse_out[1]  ; output ; TTL          ;         ; N               ;
; 74       ; 73         ; --       ; speed[13]            ; input  ; TTL          ;         ; N               ;
; 75       ; 74         ; --       ; speed[12]            ; input  ; TTL          ;         ; N               ;
; 76       ; 75         ; --       ; acceleration[4]      ; input  ; TTL          ;         ; N               ;
; 77       ; 76         ; --       ; speed[5]             ; input  ; TTL          ;         ; N               ;
; 78       ; 77         ; --       ; VCCIO                ; power  ;              ; 5.0V    ;                 ;
; 79       ; 78         ; --       ; speed[1]             ; input  ; TTL          ;         ; N               ;
; 80       ; 79         ; --       ; speed[15]            ; input  ; TTL          ;         ; N               ;
; 81       ; 80         ; --       ; acceleration[14]     ; input  ; TTL          ;         ; N               ;
; 82       ; 81         ; --       ; GND                  ; gnd    ;              ;         ;                 ;
; 83       ; 82         ; --       ; Clk_1Hz              ; input  ; TTL          ;         ; N               ;
; 84       ; 83         ; --       ; GND+                 ;        ;              ;         ;                 ;
+----------+------------+----------+----------------------+--------+--------------+---------+-----------------+


+--------------------------------------------------------------------------------------------------+
; I/O Standard                                                                                     ;
+--------------+------------+----------------------+-------------------+-------------------+-------+
; I/O Standard ; Input Vref ; Dedicated Input Pins ; Pins in I/O Bank1 ; Pins in I/O Bank2 ; Total ;
+--------------+------------+----------------------+-------------------+-------------------+-------+
; TTL          ; -          ; 1                    ; 0                 ; 0                 ; 1     ;
+--------------+------------+----------------------+-------------------+-------------------+-------+


+-----------------------------------------------------------------------+
; Dedicated Inputs I/O                                                  ;
+---------+-------+-------+-------+--------------+------------+---------+
; Name    ; Pin # ; Type  ; VCCIO ; I/O Standard ; Input Vref ; Current ;
+---------+-------+-------+-------+--------------+------------+---------+
; Clk_1Hz ; 83    ; Input ; --    ; TTL          ; -          ; 0 mA    ;
+---------+-------+-------+-------+--------------+------------+---------+


+-----------------------------------------------+
; Output Pin Default Load For Reported TCO      ;
+--------------+-------+------------------------+
; I/O Standard ; Load  ; Termination Resistance ;
+--------------+-------+------------------------+
; LVTTL        ; 10 pF ; Not Available          ;
; LVCMOS       ; 10 pF ; Not Available          ;
; TTL          ; 0 pF  ; Not Available          ;
+--------------+-------+------------------------+


+---------------------------------------------------------------------------------------------------------------------------------------------+
; Fitter Resource Utilization by Entity                                                                                                       ;
+------------------------------------+------------+------+------------------------------------------------------------------------------------+
; Compilation Hierarchy Node         ; Macrocells ; Pins ; Full Hierarchy Name                                                                ;
+------------------------------------+------------+------+------------------------------------------------------------------------------------+
; |second_pulse_latch                ; 93         ; 55   ; |second_pulse_latch                                                                ;
;    |lpm_add_sub:add_rtl_0|         ; 37         ; 0    ; |second_pulse_latch|lpm_add_sub:add_rtl_0                                          ;
;       |addcore:adder[0]|           ; 10         ; 0    ; |second_pulse_latch|lpm_add_sub:add_rtl_0|addcore:adder[0]                         ;
;          |a_csnbuffer:result_node| ; 7          ; 0    ; |second_pulse_latch|lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node ;
;       |addcore:adder[1]|           ; 25         ; 0    ; |second_pulse_latch|lpm_add_sub:add_rtl_0|addcore:adder[1]                         ;
;          |a_csnbuffer:result_node| ; 7          ; 0    ; |second_pulse_latch|lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node ;
;       |addcore:adder[2]|           ; 2          ; 0    ; |second_pulse_latch|lpm_add_sub:add_rtl_0|addcore:adder[2]                         ;
;          |a_csnbuffer:result_node| ; 2          ; 0    ; |second_pulse_latch|lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node ;
;    |lpm_add_sub:add_rtl_1|         ; 31         ; 0    ; |second_pulse_latch|lpm_add_sub:add_rtl_1                                          ;
;       |addcore:adder[0]|           ; 15         ; 0    ; |second_pulse_latch|lpm_add_sub:add_rtl_1|addcore:adder[0]                         ;
;          |a_csnbuffer:result_node| ; 7          ; 0    ; |second_pulse_latch|lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node ;
;       |addcore:adder[1]|           ; 16         ; 0    ; |second_pulse_latch|lpm_add_sub:add_rtl_1|addcore:adder[1]                         ;
;          |a_csnbuffer:result_node| ; 7          ; 0    ; |second_pulse_latch|lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node ;
+------------------------------------+------------+------+------------------------------------------------------------------------------------+


+-----------------------------------------------------------------------------------------+
; Control Signals                                                                         ;
+---------+----------+---------+-------+--------+----------------------+------------------+
; Name    ; Location ; Fan-Out ; Usage ; Global ; Global Resource Used ; Global Line Name ;
+---------+----------+---------+-------+--------+----------------------+------------------+
; Clk_1Hz ; PIN_83   ; 16      ; Clock ; yes    ; On                   ; --               ;
+---------+----------+---------+-------+--------+----------------------+------------------+


+------------------------------------------------------------------------+
; Global & Other Fast Signals                                            ;
+---------+----------+---------+----------------------+------------------+
; Name    ; Location ; Fan-Out ; Global Resource Used ; Global Line Name ;
+---------+----------+---------+----------------------+------------------+
; Clk_1Hz ; PIN_83   ; 16      ; On                   ; --               ;
+---------+----------+---------+----------------------+------------------+


+---------------------------------------------------------------------------------------------+
; Non-Global High Fan-Out Signals                                                             ;
+-----------------------------------------------------------------------------------+---------+
; Name                                                                              ; Fan-Out ;
+-----------------------------------------------------------------------------------+---------+
; acceleration[1]                                                                   ; 24      ;
; acceleration[16]                                                                  ; 23      ;
; second_pulse_out[2]~reg0                                                          ; 23      ;
; second_pulse_out[1]~reg0                                                          ; 23      ;
; Reset                                                                             ; 22      ;
; second_pulse_out[8]~reg0                                                          ; 21      ;
; acceleration[2]                                                                   ; 20      ;
; acceleration[8]                                                                   ; 20      ;
; second_pulse_out[9]~reg0                                                          ; 20      ;
; second_pulse_out[0]~reg0                                                          ; 20      ;
; acceleration[0]                                                                   ; 19      ;
; acceleration[9]                                                                   ; 19      ;
; second_pulse_out[7]~reg0                                                          ; 18      ;
; second_pulse_out[3]~reg0                                                          ; 18      ;
; acceleration[3]                                                                   ; 17      ;
; acceleration[7]                                                                   ; 17      ;
; second_pulse_out[10]~reg0                                                         ; 17      ;
; acceleration[10]                                                                  ; 16      ;
; second_pulse_out[12]~reg0                                                         ; 15      ;
; second_pulse_out[11]~reg0                                                         ; 15      ;
; second_pulse_out[5]~reg0                                                          ; 15      ;
; second_pulse_out[4]~reg0                                                          ; 15      ;
; acceleration[4]                                                                   ; 14      ;
; acceleration[5]                                                                   ; 14      ;
; acceleration[11]                                                                  ; 14      ;
; acceleration[12]                                                                  ; 14      ;
; second_pulse_out[13]~reg0                                                         ; 14      ;
; acceleration[13]                                                                  ; 13      ;
; second_pulse_out[6]~reg0                                                          ; 12      ;
; acceleration[6]                                                                   ; 11      ;
; lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39                                  ; 11      ;
; lpm_add_sub:add_rtl_0|addcore:adder[0]|genr_node[3]~82                            ; 11      ;
; lpm_add_sub:add_rtl_0|addcore:adder[0]|prop_node[3]~77                            ; 11      ;
; second_pulse_out[14]~reg0                                                         ; 10      ;
; acceleration[14]                                                                  ; 9       ;
; lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39                                  ; 9       ;
; lpm_add_sub:add_rtl_1|addcore:adder[0]|genr_node[3]~88                            ; 9       ;
; lpm_add_sub:add_rtl_1|addcore:adder[0]|prop_node[3]~77                            ; 9       ;
; lpm_add_sub:add_rtl_1|addcore:adder[1]|ps[0]~29sexpbal                            ; 7       ;
; lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~16bal ; 7       ;
; lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[0]~23sexpbal                            ; 7       ;
; lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[1]~21sexpbal                            ; 6       ;
; second_pulse_out[15]~reg0                                                         ; 5       ;
; lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~67    ; 4       ;
; acceleration[15]                                                                  ; 4       ;
; lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~33    ; 4       ;
; lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~17                                      ; 4       ;
; lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~17                                      ; 4       ;
; lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~70    ; 3       ;
; lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~69    ; 3       ;
+-----------------------------------------------------------------------------------+---------+


+-------------------------------------------------+
; Interconnect Usage Summary                      ;
+----------------------------+--------------------+
; Interconnect Resource Type ; Usage              ;
+----------------------------+--------------------+
; Output enables             ; 0 / 6 ( 0 % )      ;
; PIA buffers                ; 155 / 288 ( 53 % ) ;
; PIAs                       ; 182 / 288 ( 63 % ) ;
+----------------------------+--------------------+


+-----------------------------------------------------------------------------+
; LAB External Interconnect                                                   ;
+-----------------------------------------------+-----------------------------+
; LAB External Interconnects  (Average = 22.75) ; Number of LABs  (Total = 8) ;
+-----------------------------------------------+-----------------------------+
; 0 - 2                                         ; 0                           ;
; 3 - 5                                         ; 0                           ;
; 6 - 8                                         ; 0                           ;
; 9 - 11                                        ; 1                           ;
; 12 - 14                                       ; 1                           ;
; 15 - 17                                       ; 0                           ;
; 18 - 20                                       ; 0                           ;
; 21 - 23                                       ; 1                           ;
; 24 - 26                                       ; 2                           ;
; 27 - 29                                       ; 2                           ;
; 30 - 32                                       ; 1                           ;
+-----------------------------------------------+-----------------------------+


+-----------------------------------------------------------------------+
; LAB Macrocells                                                        ;
+-----------------------------------------+-----------------------------+
; Number of Macrocells  (Average = 11.63) ; Number of LABs  (Total = 8) ;
+-----------------------------------------+-----------------------------+
; 0                                       ; 0                           ;
; 1                                       ; 0                           ;
; 2                                       ; 0                           ;
; 3                                       ; 0                           ;
; 4                                       ; 1                           ;
; 5                                       ; 0                           ;
; 6                                       ; 0                           ;
; 7                                       ; 1                           ;
; 8                                       ; 0                           ;
; 9                                       ; 1                           ;
; 10                                      ; 1                           ;
; 11                                      ; 0                           ;
; 12                                      ; 0                           ;
; 13                                      ; 0                           ;
; 14                                      ; 0                           ;
; 15                                      ; 1                           ;
; 16                                      ; 3                           ;
+-----------------------------------------+-----------------------------+


+---------------------------------------------------------+
; Parallel Expander                                       ;
+--------------------------+------------------------------+
; Parallel Expander Length ; Number of Parallel Expanders ;
+--------------------------+------------------------------+
; 0                        ; 0                            ;
; 1                        ; 15                           ;
; 2                        ; 4                            ;
; 3                        ; 1                            ;
+--------------------------+------------------------------+


+-------------------------------------------------------------------------------+
; Shareable Expander                                                            ;
+-------------------------------------------------+-----------------------------+
; Number of shareable expanders  (Average = 9.63) ; Number of LABs  (Total = 8) ;
+-------------------------------------------------+-----------------------------+
; 0                                               ; 0                           ;
; 1                                               ; 0                           ;
; 2                                               ; 1                           ;
; 3                                               ; 0                           ;
; 4                                               ; 1                           ;
; 5                                               ; 0                           ;
; 6                                               ; 0                           ;
; 7                                               ; 0                           ;
; 8                                               ; 0                           ;
; 9                                               ; 0                           ;
; 10                                              ; 0                           ;
; 11                                              ; 3                           ;
; 12                                              ; 1                           ;
; 13                                              ; 2                           ;
+-------------------------------------------------+-----------------------------+


+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Logic Cell Interconnection                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
+-----+------------+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; LAB ; Logic Cell ; Input                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ; Output                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           ;
+-----+------------+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
;  A  ; LC3        ; Clk_1Hz, Reset, acceleration[16], lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~17, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~17                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~15, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~16, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~24, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~29, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~56, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~27, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~34, second_pulse_out[3], lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~30, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~43, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[7]~57, lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~89, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~92, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~95, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~96                                                                                                                                                                                                                                      ;
;  A  ; LC8        ; Clk_1Hz, Reset, acceleration[16], lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~30, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~29                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; lpm_add_sub:add_rtl_1|addcore:adder[0]|g2cp[2]~23, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~27, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~28, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~30, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~34, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~28, second_pulse_out[4], lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~84, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~86, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~80, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[7]~82, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~42, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~98                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 ;
;  A  ; LC6        ; Clk_1Hz, Reset, second_pulse_out~1202                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ; lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~17, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~25, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~29, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~56, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~28, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~34, second_pulse_out~1202, second_pulse_out[2], lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~17, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~27, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~30, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~40, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~43, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[7]~57, lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~80, second_pulse_out~1262, second_pulse_out~1267, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~76, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~90, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~93 ;
;  A  ; LC2        ; lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_1|addcore:adder[0]|genr_node[3]~88, lpm_add_sub:add_rtl_1|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[1]|g2cp[2]~23, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~58, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~59, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~58, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~50, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~41, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~33, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~67, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~16bal, lpm_add_sub:add_rtl_1|addcore:adder[1]|ps[0]~29sexpbal ; second_pulse_out[15]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  A  ; LC12       ; lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_1|addcore:adder[0]|genr_node[3]~88, lpm_add_sub:add_rtl_1|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[1]|g2cp[1]~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~49, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~50, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~50, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~41, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~33, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~67, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~16bal, lpm_add_sub:add_rtl_1|addcore:adder[1]|ps[0]~29sexpbal                                                                                 ; second_pulse_out[14]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  A  ; LC7        ; lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_1|addcore:adder[0]|genr_node[3]~88, lpm_add_sub:add_rtl_1|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~40, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~41, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~41, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~33, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~67, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~16bal, lpm_add_sub:add_rtl_1|addcore:adder[1]|ps[0]~29sexpbal, second_pulse_out[12]~reg0, acceleration[12]                                                                                                                                                                       ; second_pulse_out[13]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  A  ; LC15       ; lpm_add_sub:add_rtl_1|addcore:adder[0]|genr_node[3]~88, lpm_add_sub:add_rtl_1|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~23, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~24, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~33, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~67, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~16bal, lpm_add_sub:add_rtl_1|addcore:adder[1]|ps[0]~29sexpbal                                                                                                                                                                                                                                                                                                    ; second_pulse_out[12]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  A  ; LC16       ; second_pulse_out[10]~reg0, second_pulse_out[9]~reg0, acceleration[9], acceleration[10]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                       ; lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~2                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  A  ; LC14       ; second_pulse_out[10]~reg0, acceleration[10], second_pulse_out[9]~reg0, acceleration[9]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                       ; lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~2                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  A  ; LC10       ; second_pulse_out[12]~reg0, second_pulse_out[11]~reg0, acceleration[11], acceleration[12]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~2                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  A  ; LC9        ; second_pulse_out[12]~reg0, acceleration[12], second_pulse_out[11]~reg0, acceleration[11]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~9                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  A  ; LC5        ; second_pulse_out[12]~reg0, acceleration[12], second_pulse_out[11]~reg0, acceleration[11]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  A  ; LC4        ; second_pulse_out[14]~reg0, acceleration[14], second_pulse_out[13]~reg0, acceleration[13]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~9                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  A  ; LC11       ; second_pulse_out[13]~reg0, acceleration[13], second_pulse_out[12]~reg0, acceleration[12]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  A  ; LC13       ; acceleration[9], second_pulse_out[9]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ; lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~25, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~33, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  A  ; LC1        ; second_pulse_out[14]~reg0, second_pulse_out[13]~reg0, acceleration[13], acceleration[14]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~2, lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~9                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ;
;  B  ; LC28       ; lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_0|addcore:adder[0]|genr_node[3]~82, lpm_add_sub:add_rtl_0|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_0|addcore:adder[1]|g2cp[1]~17, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~49, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~70, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~68, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[1]~21sexpbal, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[0]~23sexpbal, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~69, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~70, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~71                                                                                                            ; second_pulse_out[13]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  B  ; LC20       ; lpm_add_sub:add_rtl_0|addcore:adder[1]|g2cp[2]~24, second_pulse_out[13]~reg0, second_pulse_out[12]~reg0, second_pulse_out[11]~reg0, acceleration[11], acceleration[12], acceleration[13]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  B  ; LC27       ; lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_0|addcore:adder[0]|genr_node[3]~82, lpm_add_sub:add_rtl_0|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_0|addcore:adder[1]|g2cp[2]~23, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~71, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~59, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~72, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~68, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[1]~21sexpbal, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[0]~23sexpbal, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~69, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~70, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~71                            ; second_pulse_out[14]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  B  ; LC31       ; lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_0|addcore:adder[0]|genr_node[3]~82, lpm_add_sub:add_rtl_0|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~40, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~69, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~68, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[1]~21sexpbal, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[0]~23sexpbal, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~69, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~70, second_pulse_out[11]~reg0, acceleration[11]                                                                                                                                                                                                  ; second_pulse_out[12]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  B  ; LC17       ; second_pulse_out[14]~reg0, acceleration[14], second_pulse_out[13]~reg0, acceleration[13]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; lpm_add_sub:add_rtl_1|addcore:adder[1]|g2cp[2]~23                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  B  ; LC19       ; second_pulse_out[13]~reg0, acceleration[13], second_pulse_out[12]~reg0, acceleration[12]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; lpm_add_sub:add_rtl_0|addcore:adder[1]|g2cp[2]~23                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  B  ; LC32       ; second_pulse_out[8]~reg0, acceleration[8], second_pulse_out[7]~reg0, acceleration[7]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~2                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  B  ; LC22       ; second_pulse_out[7]~reg0, second_pulse_out[8]~reg0, acceleration[8], acceleration[7]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~2                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  B  ; LC21       ; second_pulse_out[7]~reg0, acceleration[7]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ; lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~17, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~26, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~34, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60, second_pulse_out~1284                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ;
;  B  ; LC25       ; second_pulse_out[6]~reg0, acceleration[6], second_pulse_out[5]~reg0, acceleration[5]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~17, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~26, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~34, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60, lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~2, second_pulse_out~1273, second_pulse_out~1278, second_pulse_out~1284, second_pulse_out~1290                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  B  ; LC24       ; second_pulse_out[8]~reg0, acceleration[8]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ; lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~9, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~25, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~33, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  B  ; LC23       ; second_pulse_out[8]~reg0, acceleration[8]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ; lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~17, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~26, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~34, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  B  ; LC26       ; second_pulse_out[6]~reg0, second_pulse_out[5]~reg0, acceleration[5], acceleration[6]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~17, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~26, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~34, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60, lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~2, second_pulse_out~1273, second_pulse_out~1278, second_pulse_out~1284, second_pulse_out~1290                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  B  ; LC29       ; second_pulse_out[7]~reg0, second_pulse_out[6]~reg0, acceleration[6], acceleration[7]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~9, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~25, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~33, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60, second_pulse_out[8]~reg0, second_pulse_out~1296                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  B  ; LC30       ; second_pulse_out[7]~reg0, acceleration[7], second_pulse_out[6]~reg0, acceleration[6]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~9, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~25, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~33, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60, second_pulse_out[8]~reg0, second_pulse_out~1296                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  B  ; LC18       ; lpm_add_sub:add_rtl_1|addcore:adder[1]|g2cp[2]~24, second_pulse_out[14]~reg0, second_pulse_out[13]~reg0, second_pulse_out[12]~reg0, acceleration[12], acceleration[13], acceleration[14]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  C  ; LC47       ; acceleration[2], second_pulse_out[1]~reg0, second_pulse_out[0]~reg0, acceleration[0], acceleration[1], second_pulse_out[2]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ; lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~17                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  C  ; LC38       ; second_pulse_out[6]~reg0, acceleration[6], second_pulse_out[5]~reg0, acceleration[5]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~34                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 ;
;  C  ; LC41       ; second_pulse_out[5]~reg0, acceleration[5], lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~29, second_pulse_out[4]~reg0, acceleration[4]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                       ; lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~56                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  C  ; LC33       ; second_pulse_out[5]~reg0, acceleration[5]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ; lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 ;
;  C  ; LC35       ; second_pulse_out[6]~reg0, acceleration[6], second_pulse_out[5]~reg0, acceleration[5]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; lpm_add_sub:add_rtl_1|addcore:adder[0]|g2cp[2]~23                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  C  ; LC36       ; lpm_add_sub:add_rtl_1|addcore:adder[0]|g2cp[2]~24, second_pulse_out[6]~reg0, second_pulse_out[5]~reg0, second_pulse_out[4]~reg0, acceleration[4], acceleration[5], acceleration[6]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                           ; second_pulse_out[7]~reg0, second_pulse_out~1278                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  ;
;  C  ; LC43       ; Clk_1Hz, Reset, acceleration[0], second_pulse_out[0]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ; second_pulse_out[0]~reg0, second_pulse_out[0], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~17, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~29, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~56, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~25, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~26, second_pulse_out[1]~reg0, second_pulse_out~1202, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~17, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~24, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~26, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~43, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[7]~57, second_pulse_out~1256, second_pulse_out~1262, second_pulse_out~1267, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~76                                                                                                                                                                                                                                                                                                                                                                                        ;
;  C  ; LC34       ; lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~40, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~29, second_pulse_out[4]~reg0, acceleration[4], lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~30, second_pulse_out[3]~reg0, acceleration[3], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~89, second_pulse_out[2]~reg0, acceleration[2], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~90, second_pulse_out[1]~reg0, acceleration[1], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~91, second_pulse_out[0]~reg0, acceleration[0]                                                                                                                                                                                                                                                                                                                                                                  ; lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~9, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~25, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~33, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60, second_pulse_out[8]~reg0, second_pulse_out~1296                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  C  ; LC42       ; lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~86, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~29, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~30, acceleration[3], second_pulse_out[3]~reg0, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~89, second_pulse_out[2]~reg0, acceleration[2], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~90, second_pulse_out[1]~reg0, acceleration[1], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~91, second_pulse_out[0]~reg0, acceleration[0], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~54, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~55                                                                                                                                                                                                               ; second_pulse_out[6]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  C  ; LC46       ; Clk_1Hz, Reset, acceleration[16], lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~34, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~17                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~15, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~16, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~32, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~33, second_pulse_out[11], lpm_add_sub:add_rtl_0|addcore:adder[1]|prop_node[2]~115, lpm_add_sub:add_rtl_0|addcore:adder[1]|genr_node[2]~99, lpm_add_sub:add_rtl_0|addcore:adder[1]|g2cp[1]~17, lpm_add_sub:add_rtl_0|addcore:adder[1]|g2cp[2]~23, lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~24, lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~30, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~68, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~70                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ;
;  C  ; LC45       ; Clk_1Hz, Reset, acceleration[16], lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~26, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~33                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; lpm_add_sub:add_rtl_1|addcore:adder[1]|gcp[2]~12, lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~31, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~32, lpm_add_sub:add_rtl_0|addcore:adder[1]|prop_node[1]~110, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~24, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~25, second_pulse_out[10], lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_0|addcore:adder[1]|genr_node[1]~95, lpm_add_sub:add_rtl_1|addcore:adder[1]|gcp[2]~13, lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~24, lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~30, lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~24, lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~30, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~67, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~68                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  C  ; LC39       ; lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~35, second_pulse_out[4]~reg0, acceleration[4], acceleration[3], second_pulse_out[3]~reg0, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~27, second_pulse_out[2]~reg0, acceleration[2], lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~28, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~25, second_pulse_out[1]~reg0, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~26, acceleration[1]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; second_pulse_out[7]~reg0, second_pulse_out~1278                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                  ;
;  C  ; LC48       ; lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~76, acceleration[2], second_pulse_out[0]~reg0, acceleration[1], acceleration[0], second_pulse_out[1]~reg0, second_pulse_out[2]~reg0, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~27, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~89                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ; second_pulse_out[3]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  C  ; LC37       ; Clk_1Hz, Reset, acceleration[16], lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~9                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ; lpm_add_sub:add_rtl_1|addcore:adder[1]|gcp[2]~12, lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~7, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~8, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~15, second_pulse_out[9], lpm_add_sub:add_rtl_0|addcore:adder[1]|prop_node[1]~110, lpm_add_sub:add_rtl_0|addcore:adder[1]|gcp[2]~12, lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_0|addcore:adder[1]|genr_node[1]~95, lpm_add_sub:add_rtl_1|addcore:adder[1]|gcp[2]~13, lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~24, lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~30, lpm_add_sub:add_rtl_0|addcore:adder[1]|gcp[2]~13, lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~24, lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~30, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~33, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~16bal, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~67, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~69                                                                                                                                                                                                                                                                                                                                ;
;  C  ; LC40       ; Clk_1Hz, Reset, acceleration[16], lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~43, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; lpm_add_sub:add_rtl_0|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_1|addcore:adder[0]|g2cp[2]~23, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~29, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~40, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~41, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~41, second_pulse_out[5], lpm_add_sub:add_rtl_0|addcore:adder[0]|genr_node[3]~82, lpm_add_sub:add_rtl_1|addcore:adder[0]|g2cp[2]~24, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~40, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~86, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~35, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[7]~82, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~43, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~97                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ;
;  D  ; LC57       ; Clk_1Hz, lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~2, acceleration[16], Reset, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ; lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~58, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~59, second_pulse_out[15], lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~73, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~74                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ;
;  D  ; LC53       ; Clk_1Hz, Reset, acceleration[16], lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; lpm_add_sub:add_rtl_0|addcore:adder[1]|prop_node[3]~100, lpm_add_sub:add_rtl_1|addcore:adder[1]|g2cp[2]~23, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~49, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~50, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~58, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~59, second_pulse_out[14], lpm_add_sub:add_rtl_0|addcore:adder[1]|genr_node[3]~103, lpm_add_sub:add_rtl_1|addcore:adder[1]|g2cp[2]~24, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~71                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ;
;  D  ; LC61       ; Clk_1Hz, Reset, acceleration[16], lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; lpm_add_sub:add_rtl_0|addcore:adder[1]|prop_node[3]~100, lpm_add_sub:add_rtl_1|addcore:adder[1]|g2cp[1]~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|g2cp[2]~23, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~40, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~41, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~49, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~50, second_pulse_out[13], lpm_add_sub:add_rtl_0|addcore:adder[1]|g2cp[2]~23, lpm_add_sub:add_rtl_0|addcore:adder[1]|genr_node[3]~103, lpm_add_sub:add_rtl_1|addcore:adder[1]|g2cp[2]~24, lpm_add_sub:add_rtl_0|addcore:adder[1]|g2cp[2]~24, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~70, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~72                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ;
;  D  ; LC63       ; acceleration[3], second_pulse_out[3]~reg0, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~24, second_pulse_out[2]~reg0, acceleration[2], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~25, second_pulse_out[1]~reg0, acceleration[1], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~26, second_pulse_out[0]~reg0, acceleration[0], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~27, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~28                                                                                                                                                                                                                                                                                                                                                                                                   ; second_pulse_out[4]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  D  ; LC64       ; Clk_1Hz, Reset, acceleration[16], lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~25                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; lpm_add_sub:add_rtl_1|addcore:adder[1]|g2cp[1]~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|g2cp[2]~23, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~23, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~24, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~40, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~41, second_pulse_out[12], lpm_add_sub:add_rtl_0|addcore:adder[1]|prop_node[2]~115, lpm_add_sub:add_rtl_0|addcore:adder[1]|genr_node[2]~99, lpm_add_sub:add_rtl_0|addcore:adder[1]|g2cp[1]~17, lpm_add_sub:add_rtl_0|addcore:adder[1]|g2cp[2]~23, lpm_add_sub:add_rtl_0|addcore:adder[1]|g2cp[2]~24, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~69, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~71                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ;
;  D  ; LC51       ; second_pulse_out[5]~reg0, acceleration[5], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~97, second_pulse_out[4]~reg0, acceleration[4]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[7]~57                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  D  ; LC50       ; lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~80, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~27, second_pulse_out[3]~reg0, acceleration[3], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~96, acceleration[2], second_pulse_out[2]~reg0, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~40, second_pulse_out[1]~reg0, acceleration[1], lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~39, second_pulse_out[0]~reg0, acceleration[0], lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~41, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~43                                                                                                                                                                                                                                                                 ; second_pulse_out[5]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  D  ; LC49       ; second_pulse_out[4]~reg0, acceleration[4]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ; lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~43                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  D  ; LC56       ; Clk_1Hz, Reset, acceleration[16], lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[7]~57, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~56                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; lpm_add_sub:add_rtl_0|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_1|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_1|addcore:adder[0]|genr_node[3]~88, lpm_add_sub:add_rtl_1|addcore:adder[0]|g2cp[2]~23, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~54, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~55, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[7]~55, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[7]~56, second_pulse_out[6], lpm_add_sub:add_rtl_0|addcore:adder[0]|genr_node[3]~82, lpm_add_sub:add_rtl_1|addcore:adder[0]|g2cp[2]~24, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~35                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ;
;  D  ; LC52       ; lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[7]~82, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~97, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~27, second_pulse_out[3]~reg0, acceleration[3], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~96, acceleration[2], second_pulse_out[2]~reg0, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~40, second_pulse_out[1]~reg0, acceleration[1], lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~39, second_pulse_out[0]~reg0, acceleration[0], lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[7]~55, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[7]~56                                                                                                                                                   ; second_pulse_out[6]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  E  ; LC73       ; lpm_add_sub:add_rtl_0|addcore:adder[0]|genr_node[3]~82, lpm_add_sub:add_rtl_0|addcore:adder[0]|prop_node[3]~77, Reset, acceleration[16], acceleration[7], second_pulse_out[7]~reg0, lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; second_pulse_out~1278                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ;
;  E  ; LC74       ; second_pulse_out~1273, lpm_add_sub:add_rtl_0|addcore:adder[0]|genr_node[3]~82, Reset, acceleration[16], acceleration[7], second_pulse_out[7]~reg0, lpm_add_sub:add_rtl_0|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[0]|g2cp[2]~23, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~34                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; second_pulse_out[7]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  E  ; LC66       ; lpm_add_sub:add_rtl_0|addcore:adder[0]|genr_node[3]~82, Reset, acceleration[16], second_pulse_out[8]~reg0, acceleration[8], lpm_add_sub:add_rtl_0|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[0]~23sexpbal, second_pulse_out[7]~reg0, acceleration[7]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ; second_pulse_out~1290                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ;
;  E  ; LC67       ; second_pulse_out~1284, Reset, acceleration[16], second_pulse_out[8]~reg0, acceleration[8], lpm_add_sub:add_rtl_0|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_0|addcore:adder[0]|genr_node[3]~82, lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39, second_pulse_out[7]~reg0, acceleration[7], lpm_add_sub:add_rtl_0|addcore:adder[1]|_~143sexp                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; second_pulse_out~1296                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ;
;  E  ; LC75       ; Clk_1Hz, second_pulse_out~1278, lpm_add_sub:add_rtl_1|addcore:adder[0]|g2cp[2]~23, Reset, acceleration[16], acceleration[7], second_pulse_out[7]~reg0, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~34                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ; lpm_add_sub:add_rtl_1|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_1|addcore:adder[0]|genr_node[3]~88, second_pulse_out[7]~reg0, second_pulse_out[7], lpm_add_sub:add_rtl_0|addcore:adder[1]|prop_node[0]~105, lpm_add_sub:add_rtl_0|addcore:adder[1]|genr_node[0]~91, lpm_add_sub:add_rtl_0|addcore:adder[1]|gcp[2]~12, lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~17, second_pulse_out~1273, second_pulse_out~1278, lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~24, lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~30, second_pulse_out~1296, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~17, second_pulse_out~1284, second_pulse_out~1290, lpm_add_sub:add_rtl_0|addcore:adder[1]|_~143sexp, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[0]~23sexpbal                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                          ;
;  E  ; LC77       ; second_pulse_out[10]~reg0, acceleration[10], second_pulse_out[9]~reg0, acceleration[9]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                       ; lpm_add_sub:add_rtl_1|addcore:adder[1]|gcp[2]~12                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 ;
;  E  ; LC68       ; second_pulse_out~1290, Reset, acceleration[16], second_pulse_out[8]~reg0, acceleration[8], lpm_add_sub:add_rtl_1|addcore:adder[0]|genr_node[3]~88, lpm_add_sub:add_rtl_1|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39, second_pulse_out[7]~reg0, acceleration[7], lpm_add_sub:add_rtl_0|addcore:adder[1]|_~143sexp                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; second_pulse_out[8]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  E  ; LC79       ; second_pulse_out[9]~reg0, acceleration[9], second_pulse_out[8]~reg0, acceleration[8]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; lpm_add_sub:add_rtl_0|addcore:adder[1]|gcp[2]~12                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 ;
;  E  ; LC69       ; Clk_1Hz, second_pulse_out~1296, lpm_add_sub:add_rtl_1|addcore:adder[0]|genr_node[3]~88, Reset, acceleration[16], lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39, second_pulse_out[8]~reg0, acceleration[8], lpm_add_sub:add_rtl_1|addcore:adder[0]|prop_node[3]~77                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; lpm_add_sub:add_rtl_1|addcore:adder[1]|gcp[2]~12, lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_0|addcore:adder[1]|prop_node[0]~105, second_pulse_out[8]~reg0, second_pulse_out[8], lpm_add_sub:add_rtl_0|addcore:adder[1]|genr_node[0]~91, lpm_add_sub:add_rtl_0|addcore:adder[1]|gcp[2]~12, lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~24, lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~30, second_pulse_out~1284, second_pulse_out~1290, second_pulse_out~1296, lpm_add_sub:add_rtl_0|addcore:adder[1]|gcp[2]~13, lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~24, lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~30, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~9, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~33, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~17, lpm_add_sub:add_rtl_1|addcore:adder[1]|ps[0]~29sexpbal, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[1]~21sexpbal                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ;
;  E  ; LC70       ; second_pulse_out[9]~reg0, acceleration[10], second_pulse_out[10]~reg0, acceleration[9], second_pulse_out[8]~reg0, acceleration[8], second_pulse_out[7]~reg0, acceleration[7]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 ; lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~30                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ;
;  E  ; LC71       ; lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~24, second_pulse_out[8]~reg0, acceleration[10], second_pulse_out[10]~reg0, acceleration[9], second_pulse_out[7]~reg0, acceleration[7], acceleration[8], second_pulse_out[9]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ; lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~17                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ;
;  E  ; LC78       ; lpm_add_sub:add_rtl_1|addcore:adder[1]|gcp[2]~13, second_pulse_out[10]~reg0, second_pulse_out[9]~reg0, second_pulse_out[8]~reg0, acceleration[8], acceleration[9], acceleration[10]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                          ; lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~17                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  E  ; LC76       ; lpm_add_sub:add_rtl_1|addcore:adder[0]|genr_node[3]~88, lpm_add_sub:add_rtl_1|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~7, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~8, lpm_add_sub:add_rtl_1|addcore:adder[1]|ps[0]~29sexpbal, second_pulse_out[8]~reg0, acceleration[8]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ; second_pulse_out[9]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  E  ; LC65       ; lpm_add_sub:add_rtl_0|addcore:adder[0]|genr_node[3]~82, lpm_add_sub:add_rtl_0|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~15, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~16bal, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[1]~21sexpbal, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[0]~23sexpbal, second_pulse_out[7]~reg0, acceleration[7], second_pulse_out[8]~reg0, acceleration[8]                                                                                                                                                                                                                                                                                                                                                                                                                                                    ; second_pulse_out[9]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  E  ; LC72       ; lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~30, second_pulse_out[9]~reg0, acceleration[10], second_pulse_out[10]~reg0, acceleration[8], second_pulse_out[7]~reg0, acceleration[7], second_pulse_out[8]~reg0, acceleration[9]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ; lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~34, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  E  ; LC80       ; lpm_add_sub:add_rtl_0|addcore:adder[1]|gcp[2]~13, second_pulse_out[9]~reg0, second_pulse_out[8]~reg0, second_pulse_out[7]~reg0, acceleration[7], acceleration[8], acceleration[9]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ; lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~26                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  F  ; LC91       ; second_pulse_out[3]~reg0, acceleration[3], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~95, acceleration[2], second_pulse_out[2]~reg0, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~27, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~24, second_pulse_out[1]~reg0, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~26, acceleration[1], lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~28, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~42                                                                                                                                                                                                                                                                                                                                                                                            ; second_pulse_out[4]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  F  ; LC82       ; lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~84, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~42, acceleration[3], second_pulse_out[3]~reg0, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~92, second_pulse_out[2]~reg0, acceleration[2], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~93, second_pulse_out[1]~reg0, acceleration[1], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~94, second_pulse_out[0]~reg0, acceleration[0], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~40, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~41                                                                                                                                                                                                                                                                 ; second_pulse_out[5]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  F  ; LC81       ; second_pulse_out[4]~reg0, acceleration[4]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ; lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~42                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  F  ; LC89       ; second_pulse_out[4]~reg0, acceleration[4], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~98, second_pulse_out[3]~reg0, acceleration[3], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~95, second_pulse_out[2]~reg0, acceleration[2], lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~27, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~24, second_pulse_out[1]~reg0, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~26, acceleration[1]                                                                                                                                                                                                                                                                                                                                                                                                   ; lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~17, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~26, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~34, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60, lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~2, second_pulse_out~1273, second_pulse_out~1278, second_pulse_out~1284, second_pulse_out~1290                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  G  ; LC103      ; lpm_add_sub:add_rtl_0|addcore:adder[0]|genr_node[3]~82, lpm_add_sub:add_rtl_0|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_0|addcore:adder[1]|gcp[2]~12, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~24, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~25, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[1]~21sexpbal, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[0]~23sexpbal, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~67                                                                                                                                                                                                                                                                                                                                                                                                           ; second_pulse_out[10]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  G  ; LC105      ; lpm_add_sub:add_rtl_1|addcore:adder[0]|genr_node[3]~88, lpm_add_sub:add_rtl_1|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[1]|gcp[2]~12, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~15, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~16, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[3]~25, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~16bal, lpm_add_sub:add_rtl_1|addcore:adder[1]|ps[0]~29sexpbal                                                                                                                                                                                                                                                                                                                                                                                ; second_pulse_out[11]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  G  ; LC101      ; lpm_add_sub:add_rtl_0|addcore:adder[0]|genr_node[3]~82, lpm_add_sub:add_rtl_0|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_0|addcore:adder[1]|g4~17, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~32, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~68, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~32, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[1]~21sexpbal, lpm_add_sub:add_rtl_0|addcore:adder[1]|ps[0]~23sexpbal, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[1]~67                                                                                                                                                                                                                                                                                                                               ; second_pulse_out[11]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  G  ; LC108      ; lpm_add_sub:add_rtl_0|addcore:adder[1]|genr_node[3]~103, lpm_add_sub:add_rtl_0|addcore:adder[1]|genr_node[2]~99, lpm_add_sub:add_rtl_0|addcore:adder[1]|prop_node[3]~100                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~2                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
;  G  ; LC98       ; lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~24, second_pulse_out[9]~reg0, acceleration[11], second_pulse_out[11]~reg0, acceleration[10], second_pulse_out[8]~reg0, acceleration[8], acceleration[9], second_pulse_out[10]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 ; lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~17                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ;
;  G  ; LC97       ; second_pulse_out[10]~reg0, acceleration[11], second_pulse_out[11]~reg0, acceleration[10], second_pulse_out[9]~reg0, acceleration[9], second_pulse_out[8]~reg0, acceleration[8]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                               ; lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~30                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ;
;  G  ; LC106      ; lpm_add_sub:add_rtl_1|addcore:adder[0]|genr_node[3]~88, lpm_add_sub:add_rtl_1|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~31, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~32, lpm_add_sub:add_rtl_0|addcore:adder[1]|a_csnbuffer:result_node|sout_node[2]~16bal, lpm_add_sub:add_rtl_1|addcore:adder[1]|ps[0]~29sexpbal, second_pulse_out[8]~reg0, acceleration[8], second_pulse_out[9]~reg0, acceleration[9]                                                                                                                                                                                                                                                                                                                                                                                                                            ; second_pulse_out[10]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  G  ; LC109      ; lpm_add_sub:add_rtl_0|addcore:adder[2]|a_csnbuffer:result_node|sout_node[0]~9, lpm_add_sub:add_rtl_0|addcore:adder[1]|genr_node[1]~95, lpm_add_sub:add_rtl_0|addcore:adder[1]|prop_node[3]~100, lpm_add_sub:add_rtl_0|addcore:adder[1]|prop_node[2]~115, lpm_add_sub:add_rtl_0|addcore:adder[1]|genr_node[0]~91, lpm_add_sub:add_rtl_0|addcore:adder[1]|prop_node[1]~110, lpm_add_sub:add_rtl_0|addcore:adder[0]|genr_node[3]~82, lpm_add_sub:add_rtl_0|addcore:adder[1]|prop_node[0]~105, lpm_add_sub:add_rtl_0|addcore:adder[0]|prop_node[3]~77, lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~73, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~74                                                                                                                                                                                                                          ; second_pulse_out[15]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                        ;
;  G  ; LC99       ; lpm_add_sub:add_rtl_1|addcore:adder[1]|g4~30, second_pulse_out[10]~reg0, acceleration[11], second_pulse_out[11]~reg0, acceleration[9], second_pulse_out[8]~reg0, acceleration[8], second_pulse_out[9]~reg0, acceleration[10]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                 ; lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[4]~25, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[6]~51, lpm_add_sub:add_rtl_1|addcore:adder[1]|a_csnbuffer:result_node|sout_node[7]~60                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  H  ; LC117      ; lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~80, second_pulse_out[1]~reg0, second_pulse_out[2]~reg0, second_pulse_out[0]~reg0, acceleration[0], acceleration[2], acceleration[1], lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~15, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~16                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              ; second_pulse_out[3]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  H  ; LC115      ; Clk_1Hz, second_pulse_out~1256, second_pulse_out[0]~reg0, acceleration[16], Reset, acceleration[0], acceleration[1], second_pulse_out[1]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ; lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~17, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~26, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~29, lpm_add_sub:add_rtl_1|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~42, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~56, lpm_add_sub:add_rtl_1|addcore:adder[0]|p2c[2]~34, second_pulse_out[1]~reg0, second_pulse_out[1], second_pulse_out~1202, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~17, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[5]~30, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~39, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[6]~43, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[7]~57, lpm_add_sub:add_rtl_0|addcore:adder[0]|bg_out~39, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~80, second_pulse_out~1256, second_pulse_out~1262, second_pulse_out~1267, lpm_add_sub:add_rtl_0|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~76, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~91, lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[4]~94                                                                                  ;
;  H  ; LC116      ; second_pulse_out[2]~reg0, acceleration[2], second_pulse_out[1]~reg0, acceleration[1]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ; lpm_add_sub:add_rtl_1|addcore:adder[0]|a_csnbuffer:result_node|sout_node[3]~17                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                   ;
;  H  ; LC120      ; second_pulse_out~1267, acceleration[16], second_pulse_out[1]~reg0, acceleration[0], second_pulse_out[2]~reg0, acceleration[1], second_pulse_out[0]~reg0, acceleration[2]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     ; second_pulse_out[2]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  H  ; LC114      ; second_pulse_out[0]~reg0, acceleration[16], Reset, acceleration[1], second_pulse_out[1]~reg0, acceleration[0]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                ; second_pulse_out[1]~reg0                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
;  H  ; LC119      ; second_pulse_out~1262, acceleration[1], second_pulse_out[1]~reg0, second_pulse_out[0]~reg0, acceleration[0], second_pulse_out[2]~reg0, acceleration[16]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                      ; second_pulse_out~1202                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ;
;  H  ; LC118      ; acceleration[16], second_pulse_out[1]~reg0, second_pulse_out[0]~reg0, acceleration[0], second_pulse_out[2]~reg0, acceleration[1]                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             ; second_pulse_out~1267                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                            ;
+-----+------------+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+


+-----------------+
; Fitter Messages ;
+-----------------+
Info: *******************************************************************
Info: Running Quartus II Fitter
    Info: Version 4.2 Build 157 12/07/2004 SJ Full Version
    Info: Processing started: Wed Jul 19 23:02:08 2006
Info: Command: quartus_fit --import_settings_files=off --export_settings_files=off second_pulse_latch -c second_pulse_latch
Info: Automatically selected device EPM7128SLC84-6 for design second_pulse_latch
Info: Fitting design with smaller device may be possible, but smaller device must be specified
Info: Quartus II Fitter was successful. 0 errors, 0 warnings
    Info: Processing ended: Wed Jul 19 23:02:13 2006
    Info: Elapsed time: 00:00:06


