--A1L5Q is Q~reg0 at LC1
A1L5Q_reg_input = VCC;
A1L5Q = TFFE(A1L5Q_reg_input, GLOBAL(T), , , EN);


--A1L4Q is QN~reg0 at LC2
A1L4Q_or_out = A1L5Q;
A1L4Q_reg_input = A1L4Q_or_out;
A1L4Q = DFFE(A1L4Q_reg_input, GLOBAL(T), , , EN);


--EN is EN at PIN_24
--operation mode is input

EN = INPUT();


--T is T at PIN_43
--operation mode is input

T = INPUT();


--Q is Q at PIN_4
--operation mode is output

Q = OUTPUT(A1L5Q);


--QN is QN at PIN_5
--operation mode is output

QN = OUTPUT(A1L4Q);






