--A1L11 is Y3~13
A1L11_p1_out = I1 & EN & I0;
A1L11_or_out = A1L11_p1_out;
A1L11 = A1L11_or_out;


--A1L9 is Y2~10
A1L9_p1_out = I1 & EN & !I0;
A1L9_or_out = A1L9_p1_out;
A1L9 = A1L9_or_out;


--A1L7 is Y1~12
A1L7_p1_out = !I1 & EN & I0;
A1L7_or_out = A1L7_p1_out;
A1L7 = A1L7_or_out;


--A1L5 is Y0~12
A1L5_p1_out = !I1 & EN & !I0;
A1L5_or_out = A1L5_p1_out;
A1L5 = A1L5_or_out;


--EN is EN
--operation mode is input

EN = INPUT();


--I1 is I1
--operation mode is input

I1 = INPUT();


--I0 is I0
--operation mode is input

I0 = INPUT();


--Y3 is Y3
--operation mode is output

Y3 = OUTPUT(A1L11);


--Y2 is Y2
--operation mode is output

Y2 = OUTPUT(A1L9);


--Y1 is Y1
--operation mode is output

Y1 = OUTPUT(A1L7);


--Y0 is Y0
--operation mode is output

Y0 = OUTPUT(A1L5);


