--A1L04 is always0~131
A1L04_or_out = Current_Set[8];
A1L04 = Current_Data[8] $ A1L04_or_out;


--A1L14 is always0~135
A1L14_or_out = Current_Set[9];
A1L14 = Current_Data[9] $ A1L14_or_out;


--A1L24 is always0~139
A1L24_or_out = Current_Set[10];
A1L24 = Current_Data[10] $ A1L24_or_out;


--A1L34 is always0~143
A1L34_or_out = Current_Set[11];
A1L34 = Current_Data[11] $ A1L34_or_out;


--A1L2 is Current_Adjust_Out~10
A1L2_p1_out = !A1L04 & !A1L14 & !A1L24 & !A1L34 & A1L23 & A1L25 & A1L33 & A1L35 & A1L43 & A1L45 & A1L53 & A1L55 & A1L63 & A1L65 & A1L73 & A1L75 & A1L83 & A1L85 & A1L93 & A1L95;
A1L2_or_out = A1L2_p1_out # !Current_Adjust_Select # En # Reset;
A1L2 = !(A1L2_or_out);


--A1L23 is always0~99sexp
A1L23 = EXP(Current_Data[0] & !Current_Set[0]);


--A1L25 is always0~155
A1L25 = EXP(!Current_Data[0] & Current_Set[0]);


--A1L33 is always0~103sexp
A1L33 = EXP(Current_Data[1] & !Current_Set[1]);


--A1L35 is always0~156
A1L35 = EXP(!Current_Data[1] & Current_Set[1]);


--A1L43 is always0~107sexp
A1L43 = EXP(Current_Data[2] & !Current_Set[2]);


--A1L45 is always0~157
A1L45 = EXP(!Current_Data[2] & Current_Set[2]);


--A1L53 is always0~111sexp
A1L53 = EXP(Current_Data[3] & !Current_Set[3]);


--A1L55 is always0~158
A1L55 = EXP(!Current_Data[3] & Current_Set[3]);


--A1L63 is always0~115sexp
A1L63 = EXP(Current_Data[4] & !Current_Set[4]);


--A1L65 is always0~159
A1L65 = EXP(!Current_Data[4] & Current_Set[4]);


--A1L73 is always0~119sexp
A1L73 = EXP(Current_Data[5] & !Current_Set[5]);


--A1L75 is always0~160
A1L75 = EXP(!Current_Data[5] & Current_Set[5]);


--A1L83 is always0~123sexp
A1L83 = EXP(Current_Data[6] & !Current_Set[6]);


--A1L85 is always0~161
A1L85 = EXP(!Current_Data[6] & Current_Set[6]);


--A1L93 is always0~127sexp
A1L93 = EXP(Current_Data[7] & !Current_Set[7]);


--A1L95 is always0~162
A1L95 = EXP(!Current_Data[7] & Current_Set[7]);


--En is En
--operation mode is input

En = INPUT();


--Reset is Reset
--operation mode is input

Reset = INPUT();


--Current_Adjust_Select is Current_Adjust_Select
--operation mode is input

Current_Adjust_Select = INPUT();


--Current_Data[11] is Current_Data[11]
--operation mode is input

Current_Data[11] = INPUT();


--Current_Data[10] is Current_Data[10]
--operation mode is input

Current_Data[10] = INPUT();


--Current_Data[9] is Current_Data[9]
--operation mode is input

Current_Data[9] = INPUT();


--Current_Data[8] is Current_Data[8]
--operation mode is input

Current_Data[8] = INPUT();


--Current_Data[7] is Current_Data[7]
--operation mode is input

Current_Data[7] = INPUT();


--Current_Data[6] is Current_Data[6]
--operation mode is input

Current_Data[6] = INPUT();


--Current_Data[5] is Current_Data[5]
--operation mode is input

Current_Data[5] = INPUT();


--Current_Data[4] is Current_Data[4]
--operation mode is input

Current_Data[4] = INPUT();


--Current_Data[3] is Current_Data[3]
--operation mode is input

Current_Data[3] = INPUT();


--Current_Data[2] is Current_Data[2]
--operation mode is input

Current_Data[2] = INPUT();


--Current_Data[1] is Current_Data[1]
--operation mode is input

Current_Data[1] = INPUT();


--Current_Data[0] is Current_Data[0]
--operation mode is input

Current_Data[0] = INPUT();


--Current_Set[11] is Current_Set[11]
--operation mode is input

Current_Set[11] = INPUT();


--Current_Set[10] is Current_Set[10]
--operation mode is input

Current_Set[10] = INPUT();


--Current_Set[9] is Current_Set[9]
--operation mode is input

Current_Set[9] = INPUT();


--Current_Set[8] is Current_Set[8]
--operation mode is input

Current_Set[8] = INPUT();


--Current_Set[7] is Current_Set[7]
--operation mode is input

Current_Set[7] = INPUT();


--Current_Set[6] is Current_Set[6]
--operation mode is input

Current_Set[6] = INPUT();


--Current_Set[5] is Current_Set[5]
--operation mode is input

Current_Set[5] = INPUT();


--Current_Set[4] is Current_Set[4]
--operation mode is input

Current_Set[4] = INPUT();


--Current_Set[3] is Current_Set[3]
--operation mode is input

Current_Set[3] = INPUT();


--Current_Set[2] is Current_Set[2]
--operation mode is input

Current_Set[2] = INPUT();


--Current_Set[1] is Current_Set[1]
--operation mode is input

Current_Set[1] = INPUT();


--Current_Set[0] is Current_Set[0]
--operation mode is input

Current_Set[0] = INPUT();


--Current_Adjust_Out is Current_Adjust_Out
--operation mode is output

Current_Adjust_Out = OUTPUT(A1L2);


