--A1L4Q is Adc_Cs~reg0 at LC3_A20
--operation mode is normal

A1L4Q_lut_out = Reset # En;
A1L4Q = DFFEA(A1L4Q_lut_out, GLOBAL(Clk), , , , , );


--A1L2Q is Adc_Conv~reg0 at LC2_A20
--operation mode is normal

A1L2Q_lut_out = Reset # En # !Adc_Over;
A1L2Q = DFFEA(A1L2Q_lut_out, GLOBAL(Clk), , , , , );


--A1L91Q is Adc_Mode~reg0 at LC6_A20
--operation mode is normal

A1L91Q_lut_out = !Reset & !En;
A1L91Q = DFFEA(A1L91Q_lut_out, GLOBAL(Clk), , , , , );


--A1L22Q is Adc_Rd~reg0 at LC1_A20
--operation mode is normal

A1L22Q_lut_out = Reset # En # Adc_Over;
A1L22Q = DFFEA(A1L22Q_lut_out, GLOBAL(Clk), , , , , );


--A1L94Q is Position_Data[11]~reg0 at LC2_B20
--operation mode is normal

A1L94Q_lut_out = Adc_Data[11];
A1L94Q = DFFEA(A1L94Q_lut_out, !GLOBAL(A1L22Q), , , , , );


--A1L74Q is Position_Data[10]~reg0 at LC8_C10
--operation mode is normal

A1L74Q_lut_out = Adc_Data[10];
A1L74Q = DFFEA(A1L74Q_lut_out, !GLOBAL(A1L22Q), , , , , );


--A1L54Q is Position_Data[9]~reg0 at LC7_B14
--operation mode is normal

A1L54Q_lut_out = Adc_Data[9];
A1L54Q = DFFEA(A1L54Q_lut_out, !GLOBAL(A1L22Q), , , , , );


--A1L34Q is Position_Data[8]~reg0 at LC2_A10
--operation mode is normal

A1L34Q_lut_out = Adc_Data[8];
A1L34Q = DFFEA(A1L34Q_lut_out, !GLOBAL(A1L22Q), , , , , );


--A1L14Q is Position_Data[7]~reg0 at LC8_B10
--operation mode is normal

A1L14Q_lut_out = Adc_Data[7];
A1L14Q = DFFEA(A1L14Q_lut_out, !GLOBAL(A1L22Q), , , , , );


--A1L93Q is Position_Data[6]~reg0 at LC1_C12
--operation mode is normal

A1L93Q_lut_out = Adc_Data[6];
A1L93Q = DFFEA(A1L93Q_lut_out, !GLOBAL(A1L22Q), , , , , );


--A1L73Q is Position_Data[5]~reg0 at LC8_A14
--operation mode is normal

A1L73Q_lut_out = Adc_Data[5];
A1L73Q = DFFEA(A1L73Q_lut_out, !GLOBAL(A1L22Q), , , , , );


--A1L53Q is Position_Data[4]~reg0 at LC1_B22
--operation mode is normal

A1L53Q_lut_out = Adc_Data[4];
A1L53Q = DFFEA(A1L53Q_lut_out, !GLOBAL(A1L22Q), , , , , );


--A1L33Q is Position_Data[3]~reg0 at LC2_B6
--operation mode is normal

A1L33Q_lut_out = Adc_Data[3];
A1L33Q = DFFEA(A1L33Q_lut_out, !GLOBAL(A1L22Q), , , , , );


--A1L13Q is Position_Data[2]~reg0 at LC1_A6
--operation mode is normal

A1L13Q_lut_out = Adc_Data[2];
A1L13Q = DFFEA(A1L13Q_lut_out, !GLOBAL(A1L22Q), , , , , );


--A1L92Q is Position_Data[1]~reg0 at LC7_C20
--operation mode is normal

A1L92Q_lut_out = Adc_Data[1];
A1L92Q = DFFEA(A1L92Q_lut_out, !GLOBAL(A1L22Q), , , , , );


--A1L72Q is Position_Data[0]~reg0 at LC4_C13
--operation mode is normal

A1L72Q_lut_out = Adc_Data[0];
A1L72Q = DFFEA(A1L72Q_lut_out, !GLOBAL(A1L22Q), , , , , );


--Reset is Reset at PIN_89
--operation mode is input

Reset = INPUT();


--En is En at PIN_38
--operation mode is input

En = INPUT();


--Clk is Clk at PIN_39
--operation mode is input

Clk = INPUT();


--Adc_Over is Adc_Over at PIN_40
--operation mode is input

Adc_Over = INPUT();


--Adc_Data[11] is Adc_Data[11] at PIN_90
--operation mode is input

Adc_Data[11] = INPUT();


--Adc_Data[10] is Adc_Data[10] at PIN_57
--operation mode is input

Adc_Data[10] = INPUT();


--Adc_Data[9] is Adc_Data[9] at PIN_65
--operation mode is input

Adc_Data[9] = INPUT();


--Adc_Data[8] is Adc_Data[8] at PIN_8
--operation mode is input

Adc_Data[8] = INPUT();


--Adc_Data[7] is Adc_Data[7] at PIN_62
--operation mode is input

Adc_Data[7] = INPUT();


--Adc_Data[6] is Adc_Data[6] at PIN_19
--operation mode is input

Adc_Data[6] = INPUT();


--Adc_Data[5] is Adc_Data[5] at PIN_69
--operation mode is input

Adc_Data[5] = INPUT();


--Adc_Data[4] is Adc_Data[4] at PIN_63
--operation mode is input

Adc_Data[4] = INPUT();


--Adc_Data[3] is Adc_Data[3] at PIN_15
--operation mode is input

Adc_Data[3] = INPUT();


--Adc_Data[2] is Adc_Data[2] at PIN_68
--operation mode is input

Adc_Data[2] = INPUT();


--Adc_Data[1] is Adc_Data[1] at PIN_20
--operation mode is input

Adc_Data[1] = INPUT();


--Adc_Data[0] is Adc_Data[0] at PIN_55
--operation mode is input

Adc_Data[0] = INPUT();


--Adc_Cs is Adc_Cs at PIN_7
--operation mode is output

Adc_Cs = OUTPUT(A1L4Q);


--Adc_Conv is Adc_Conv at PIN_6
--operation mode is output

Adc_Conv = OUTPUT(A1L2Q);


--Adc_Mode is Adc_Mode at PIN_9
--operation mode is output

Adc_Mode = OUTPUT(A1L91Q);


--Adc_Rd is Adc_Rd at PIN_29
--operation mode is output

Adc_Rd = OUTPUT(A1L22Q);


--Position_Data[11] is Position_Data[11] at PIN_14
--operation mode is output

Position_Data[11] = OUTPUT(A1L94Q);


--Position_Data[10] is Position_Data[10] at PIN_56
--operation mode is output

Position_Data[10] = OUTPUT(A1L74Q);


--Position_Data[9] is Position_Data[9] at PIN_16
--operation mode is output

Position_Data[9] = OUTPUT(A1L54Q);


--Position_Data[8] is Position_Data[8] at PIN_70
--operation mode is output

Position_Data[8] = OUTPUT(A1L34Q);


--Position_Data[7] is Position_Data[7] at PIN_61
--operation mode is output

Position_Data[7] = OUTPUT(A1L14Q);


--Position_Data[6] is Position_Data[6] at PIN_58
--operation mode is output

Position_Data[6] = OUTPUT(A1L93Q);


--Position_Data[5] is Position_Data[5] at PIN_10
--operation mode is output

Position_Data[5] = OUTPUT(A1L73Q);


--Position_Data[4] is Position_Data[4] at PIN_13
--operation mode is output

Position_Data[4] = OUTPUT(A1L53Q);


--Position_Data[3] is Position_Data[3] at PIN_64
--operation mode is output

Position_Data[3] = OUTPUT(A1L33Q);


--Position_Data[2] is Position_Data[2] at PIN_71
--operation mode is output

Position_Data[2] = OUTPUT(A1L13Q);


--Position_Data[1] is Position_Data[1] at PIN_23
--operation mode is output

Position_Data[1] = OUTPUT(A1L92Q);


--Position_Data[0] is Position_Data[0] at PIN_21
--operation mode is output

Position_Data[0] = OUTPUT(A1L72Q);


