--A1L5Q is QN~reg0
A1L5Q_or_out = !D;
A1L5Q_reg_input = A1L5Q_or_out;
A1L5Q = DFFE(A1L5Q_reg_input, GLOBAL(CLK), , , );


--A1L6Q is Q~reg0
A1L6Q_or_out = D;
A1L6Q_reg_input = A1L6Q_or_out;
A1L6Q = DFFE(A1L6Q_reg_input, GLOBAL(CLK), , , );


--D is D
--operation mode is input

D = INPUT();


--CLK is CLK
--operation mode is input

CLK = INPUT();


--Q is Q
--operation mode is output

Q = OUTPUT(A1L6Q);


--QN is QN
--operation mode is output

QN = OUTPUT(A1L5Q);


