--S22_safe_q[0] is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|safe_q[0] at LC_X35_Y10_N0
--operation mode is arithmetic

S22_safe_q[0]_lut_out = !S22_safe_q[0];
S22_safe_q[0] = DFFEAS(S22_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , J1L4, , , J1L8, );

--S22L2 is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|counter_cella0~COUT at LC_X35_Y10_N0
--operation mode is arithmetic

S22L2_cout_0 = S22_safe_q[0];
S22L2 = CARRY(S22L2_cout_0);

--S22L3 is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X35_Y10_N0
--operation mode is arithmetic

S22L3_cout_1 = S22_safe_q[0];
S22L3 = CARRY(S22L3_cout_1);


--S9_safe_q[0] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|safe_q[0] at LC_X35_Y7_N5
--operation mode is arithmetic

S9_safe_q[0]_lut_out = !S9_safe_q[0];
S9_safe_q[0] = DFFEAS(S9_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , M1L5, , , M1L8, );

--S9L2 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|counter_cella0~COUT at LC_X35_Y7_N5
--operation mode is arithmetic

S9L2_cout_0 = S9_safe_q[0];
S9L2 = CARRY(S9L2_cout_0);

--S9L3 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X35_Y7_N5
--operation mode is arithmetic

S9L3_cout_1 = S9_safe_q[0];
S9L3 = CARRY(S9L3_cout_1);


--S3_safe_q[0] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|safe_q[0] at LC_X35_Y9_N0
--operation mode is arithmetic

S3_safe_q[0]_lut_out = !S3_safe_q[0];
S3_safe_q[0] = DFFEAS(S3_safe_q[0]_lut_out, GLOBAL(Q1_EO), VCC, , D1_Timepiece_EN, , , P1L2, );

--S3L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|counter_cella0~COUT at LC_X35_Y9_N0
--operation mode is arithmetic

S3L2_cout_0 = S3_safe_q[0];
S3L2 = CARRY(S3L2_cout_0);

--S3L3 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X35_Y9_N0
--operation mode is arithmetic

S3L3_cout_1 = S3_safe_q[0];
S3L3 = CARRY(S3L3_cout_1);


--D1_TimeSet_EN is maincontrol:inst3|TimeSet_EN at LC_X36_Y6_N1
--operation mode is normal

D1_TimeSet_EN_lut_out = !D1_Function[1] & D1_Function[0] & !D1_Function[2];
D1_TimeSet_EN = DFFEAS(D1_TimeSet_EN_lut_out, GLOBAL(SW3), VCC, , , , , , );


--L1L9 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_0[0]~36 at LC_X35_Y9_N4
--operation mode is normal

L1L9 = D1_TimeSet_EN & S9_safe_q[0] # !D1_TimeSet_EN & S3_safe_q[0];


--S02_safe_q[0] is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|safe_q[0] at LC_X36_Y11_N6
--operation mode is arithmetic

S02_safe_q[0]_lut_out = !S02_safe_q[0];
S02_safe_q[0] = DFFEAS(S02_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , J1L2, , , J1L14, );

--S02L2 is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|counter_cella0~COUT at LC_X36_Y11_N6
--operation mode is arithmetic

S02L2_cout_0 = S02_safe_q[0];
S02L2 = CARRY(S02L2_cout_0);

--S02L3 is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X36_Y11_N6
--operation mode is arithmetic

S02L3_cout_1 = S02_safe_q[0];
S02L3 = CARRY(S02L3_cout_1);


--S7_safe_q[0] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|safe_q[0] at LC_X33_Y12_N1
--operation mode is arithmetic

S7_safe_q[0]_lut_out = !S7_safe_q[0];
S7_safe_q[0] = DFFEAS(S7_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , M1L2, , , M1L9, );

--S7L2 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|counter_cella0~COUT at LC_X33_Y12_N1
--operation mode is arithmetic

S7L2_cout_0 = S7_safe_q[0];
S7L2 = CARRY(S7L2_cout_0);

--S7L3 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X33_Y12_N1
--operation mode is arithmetic

S7L3_cout_1 = S7_safe_q[0];
S7L3 = CARRY(S7L3_cout_1);


--S1_safe_q[0] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|safe_q[0] at LC_X33_Y11_N5
--operation mode is arithmetic

S1_safe_q[0]_lut_out = !S1_safe_q[0];
S1_safe_q[0] = DFFEAS(S1_safe_q[0]_lut_out, GLOBAL(P1_EO), VCC, , D1_Timepiece_EN, , , N1L6, );

--S1L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|counter_cella0~COUT at LC_X33_Y11_N5
--operation mode is arithmetic

S1L2_cout_0 = S1_safe_q[0];
S1L2 = CARRY(S1L2_cout_0);

--S1L3 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X33_Y11_N5
--operation mode is arithmetic

S1L3_cout_1 = S1_safe_q[0];
S1L3 = CARRY(S1L3_cout_1);


--L1L1 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_0[0]~36 at LC_X33_Y11_N2
--operation mode is normal

L1L1 = D1_TimeSet_EN & S7_safe_q[0] # !D1_TimeSet_EN & S1_safe_q[0];


--J1L02 is alarmclock:inst11|alarm~459 at LC_X36_Y11_N1
--operation mode is normal

J1L02 = S22_safe_q[0] & L1L1 $ S02_safe_q[0] # !L1L9 # !S22_safe_q[0] & L1L9 # L1L1 $ S02_safe_q[0];


--S22_safe_q[1] is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|safe_q[1] at LC_X35_Y10_N1
--operation mode is arithmetic

S22_safe_q[1]_lut_out = S22_safe_q[1] $ S22L2;
S22_safe_q[1] = DFFEAS(S22_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , J1L4, , , J1L8, );

--S22L5 is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|counter_cella1~COUT at LC_X35_Y10_N1
--operation mode is arithmetic

S22L5_cout_0 = !S22L2 # !S22_safe_q[1];
S22L5 = CARRY(S22L5_cout_0);

--S22L6 is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X35_Y10_N1
--operation mode is arithmetic

S22L6_cout_1 = !S22L3 # !S22_safe_q[1];
S22L6 = CARRY(S22L6_cout_1);


--S9_safe_q[1] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|safe_q[1] at LC_X35_Y7_N6
--operation mode is arithmetic

S9_safe_q[1]_lut_out = S9_safe_q[1] $ S9L2;
S9_safe_q[1] = DFFEAS(S9_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , M1L5, , , M1L8, );

--S9L5 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|counter_cella1~COUT at LC_X35_Y7_N6
--operation mode is arithmetic

S9L5_cout_0 = !S9L2 # !S9_safe_q[1];
S9L5 = CARRY(S9L5_cout_0);

--S9L6 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X35_Y7_N6
--operation mode is arithmetic

S9L6_cout_1 = !S9L3 # !S9_safe_q[1];
S9L6 = CARRY(S9L6_cout_1);


--S3_safe_q[1] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|safe_q[1] at LC_X35_Y9_N1
--operation mode is arithmetic

S3_safe_q[1]_lut_out = S3_safe_q[1] $ S3L2;
S3_safe_q[1] = DFFEAS(S3_safe_q[1]_lut_out, GLOBAL(Q1_EO), VCC, , D1_Timepiece_EN, , , P1L2, );

--S3L5 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|counter_cella1~COUT at LC_X35_Y9_N1
--operation mode is arithmetic

S3L5_cout_0 = !S3L2 # !S3_safe_q[1];
S3L5 = CARRY(S3L5_cout_0);

--S3L6 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X35_Y9_N1
--operation mode is arithmetic

S3L6_cout_1 = !S3L3 # !S3_safe_q[1];
S3L6 = CARRY(S3L6_cout_1);


--L1L01 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_0[1]~37 at LC_X35_Y9_N8
--operation mode is normal

L1L01 = D1_TimeSet_EN & S9_safe_q[1] # !D1_TimeSet_EN & S3_safe_q[1];


--S32_safe_q[0] is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|safe_q[0] at LC_X34_Y10_N1
--operation mode is arithmetic

S32_safe_q[0]_lut_out = !S32_safe_q[0];
S32_safe_q[0] = DFFEAS(S32_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , J1L3, , , J1L01, );

--S32L2 is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|counter_cella0~COUT at LC_X34_Y10_N1
--operation mode is arithmetic

S32L2_cout_0 = S32_safe_q[0];
S32L2 = CARRY(S32L2_cout_0);

--S32L3 is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X34_Y10_N1
--operation mode is arithmetic

S32L3_cout_1 = S32_safe_q[0];
S32L3 = CARRY(S32L3_cout_1);


--S01_safe_q[0] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|safe_q[0] at LC_X39_Y9_N5
--operation mode is arithmetic

S01_safe_q[0]_lut_out = !S01_safe_q[0];
S01_safe_q[0] = DFFEAS(S01_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , M1L3, , , M1L01, );

--S01L2 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|counter_cella0~COUT at LC_X39_Y9_N5
--operation mode is arithmetic

S01L2_cout_0 = S01_safe_q[0];
S01L2 = CARRY(S01L2_cout_0);

--S01L3 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X39_Y9_N5
--operation mode is arithmetic

S01L3_cout_1 = S01_safe_q[0];
S01L3 = CARRY(S01L3_cout_1);


--S4_safe_q[0] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|safe_q[0] at LC_X36_Y9_N5
--operation mode is arithmetic

S4_safe_q[0]_lut_out = !S4_safe_q[0];
S4_safe_q[0] = DFFEAS(S4_safe_q[0]_lut_out, GLOBAL(Q1_EO), VCC, , P1L4, , , P1L3, );

--S4L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|counter_cella0~COUT at LC_X36_Y9_N5
--operation mode is arithmetic

S4L2_cout_0 = S4_safe_q[0];
S4L2 = CARRY(S4L2_cout_0);

--S4L3 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X36_Y9_N5
--operation mode is arithmetic

S4L3_cout_1 = S4_safe_q[0];
S4L3 = CARRY(S4L3_cout_1);


--L1L31 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_1[0]~36 at LC_X36_Y9_N9
--operation mode is normal

L1L31 = D1_TimeSet_EN & S01_safe_q[0] # !D1_TimeSet_EN & S4_safe_q[0];


--J1L12 is alarmclock:inst11|alarm~460 at LC_X35_Y10_N5
--operation mode is normal

J1L12 = L1L31 & L1L01 $ S22_safe_q[1] # !S32_safe_q[0] # !L1L31 & S32_safe_q[0] # L1L01 $ S22_safe_q[1];


--S22_safe_q[3] is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|safe_q[3] at LC_X35_Y10_N3
--operation mode is normal

S22_safe_q[3]_lut_out = S22_safe_q[3] $ (S22L8);
S22_safe_q[3] = DFFEAS(S22_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , J1L4, , , J1L8, );


--S9_safe_q[3] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|safe_q[3] at LC_X35_Y7_N8
--operation mode is normal

S9_safe_q[3]_lut_out = S9L8 $ S9_safe_q[3];
S9_safe_q[3] = DFFEAS(S9_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , M1L5, , , M1L8, );


--S3_safe_q[3] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|safe_q[3] at LC_X35_Y9_N3
--operation mode is normal

S3_safe_q[3]_lut_out = S3_safe_q[3] $ (S3L8);
S3_safe_q[3] = DFFEAS(S3_safe_q[3]_lut_out, GLOBAL(Q1_EO), VCC, , D1_Timepiece_EN, , , P1L2, );


--L1L21 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_0[3]~38 at LC_X35_Y9_N5
--operation mode is normal

L1L21 = D1_TimeSet_EN & S9_safe_q[3] # !D1_TimeSet_EN & S3_safe_q[3];


--S42_safe_q[1] is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|safe_q[1] at LC_X36_Y10_N1
--operation mode is arithmetic

S42_safe_q[1]_lut_out = S42_safe_q[1] $ S42L2;
S42_safe_q[1] = DFFEAS(S42_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , J1L6, , , J1L7, );

--S42L5 is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|counter_cella1~COUT at LC_X36_Y10_N1
--operation mode is arithmetic

S42L5_cout_0 = !S42L2 # !S42_safe_q[1];
S42L5 = CARRY(S42L5_cout_0);

--S42L6 is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X36_Y10_N1
--operation mode is arithmetic

S42L6_cout_1 = !S42L3 # !S42_safe_q[1];
S42L6 = CARRY(S42L6_cout_1);


--S11_safe_q[1] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|safe_q[1] at LC_X36_Y7_N6
--operation mode is arithmetic

S11_safe_q[1]_lut_out = S11_safe_q[1] $ S11L2;
S11_safe_q[1] = DFFEAS(S11_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , M1L4, , , M1L7, );

--S11L5 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|counter_cella1~COUT at LC_X36_Y7_N6
--operation mode is arithmetic

S11L5_cout_0 = !S11L2 # !S11_safe_q[1];
S11L5 = CARRY(S11L5_cout_0);

--S11L6 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X36_Y7_N6
--operation mode is arithmetic

S11L6_cout_1 = !S11L3 # !S11_safe_q[1];
S11L6 = CARRY(S11L6_cout_1);


--S5_safe_q[1] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|safe_q[1] at LC_X36_Y8_N1
--operation mode is arithmetic

S5_safe_q[1]_lut_out = S5_safe_q[1] $ S5L2;
S5_safe_q[1] = DFFEAS(S5_safe_q[1]_lut_out, GLOBAL(C1L1), VCC, , D1_Timepiece_EN, , , Q1L2, );

--S5L5 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|counter_cella1~COUT at LC_X36_Y8_N1
--operation mode is arithmetic

S5L5_cout_0 = !S5L2 # !S5_safe_q[1];
S5L5 = CARRY(S5L5_cout_0);

--S5L6 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X36_Y8_N1
--operation mode is arithmetic

S5L6_cout_1 = !S5L3 # !S5_safe_q[1];
S5L6 = CARRY(S5L6_cout_1);


--L1L81 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_0[1]~36 at LC_X36_Y8_N7
--operation mode is normal

L1L81 = D1_TimeSet_EN & S11_safe_q[1] # !D1_TimeSet_EN & S5_safe_q[1];


--J1L22 is alarmclock:inst11|alarm~461 at LC_X35_Y9_N9
--operation mode is normal

J1L22 = L1L81 & L1L21 $ S22_safe_q[3] # !S42_safe_q[1] # !L1L81 & S42_safe_q[1] # L1L21 $ S22_safe_q[3];


--S32_safe_q[2] is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|safe_q[2] at LC_X34_Y10_N3
--operation mode is arithmetic

S32_safe_q[2]_lut_out = S32_safe_q[2] $ (!S32L5);
S32_safe_q[2] = DFFEAS(S32_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , J1L3, , , J1L01, );

--S32L8 is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|counter_cella2~COUT at LC_X34_Y10_N3
--operation mode is arithmetic

S32L8_cout_0 = S32_safe_q[2] & !S32L5;
S32L8 = CARRY(S32L8_cout_0);

--S32L9 is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X34_Y10_N3
--operation mode is arithmetic

S32L9_cout_1 = S32_safe_q[2] & !S32L6;
S32L9 = CARRY(S32L9_cout_1);


--S01_safe_q[2] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|safe_q[2] at LC_X39_Y9_N7
--operation mode is arithmetic

S01_safe_q[2]_lut_out = S01_safe_q[2] $ (!S01L5);
S01_safe_q[2] = DFFEAS(S01_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , M1L3, , , M1L01, );

--S01L8 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|counter_cella2~COUT at LC_X39_Y9_N7
--operation mode is arithmetic

S01L8_cout_0 = S01_safe_q[2] & !S01L5;
S01L8 = CARRY(S01L8_cout_0);

--S01L9 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X39_Y9_N7
--operation mode is arithmetic

S01L9_cout_1 = S01_safe_q[2] & !S01L6;
S01L9 = CARRY(S01L9_cout_1);


--S4_safe_q[2] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|safe_q[2] at LC_X36_Y9_N7
--operation mode is arithmetic

S4_safe_q[2]_lut_out = S4_safe_q[2] $ (!S4L5);
S4_safe_q[2] = DFFEAS(S4_safe_q[2]_lut_out, GLOBAL(Q1_EO), VCC, , P1L4, , , P1L3, );

--S4L8 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|counter_cella2~COUT at LC_X36_Y9_N7
--operation mode is arithmetic

S4L8_cout_0 = S4_safe_q[2] & !S4L5;
S4L8 = CARRY(S4L8_cout_0);

--S4L9 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X36_Y9_N7
--operation mode is arithmetic

S4L9_cout_1 = S4_safe_q[2] & !S4L6;
S4L9 = CARRY(S4L9_cout_1);


--L1L51 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_1[2]~37 at LC_X36_Y9_N2
--operation mode is normal

L1L51 = D1_TimeSet_EN & S01_safe_q[2] # !D1_TimeSet_EN & S4_safe_q[2];


--S52_safe_q[2] is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|safe_q[2] at LC_X33_Y10_N8
--operation mode is arithmetic

S52_safe_q[2]_lut_out = S52_safe_q[2] $ (!S52L5);
S52_safe_q[2] = DFFEAS(S52_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , J1L5, , , J1L11, );

--S52L8 is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|counter_cella2~COUT at LC_X33_Y10_N8
--operation mode is arithmetic

S52L8_cout_0 = S52_safe_q[2] & !S52L5;
S52L8 = CARRY(S52L8_cout_0);

--S52L9 is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X33_Y10_N8
--operation mode is arithmetic

S52L9_cout_1 = S52_safe_q[2] & !S52L6;
S52L9 = CARRY(S52L9_cout_1);


--S21_safe_q[2] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|safe_q[2] at LC_X33_Y7_N3
--operation mode is arithmetic

S21_safe_q[2]_lut_out = S21_safe_q[2] $ (!S21L5);
S21_safe_q[2] = DFFEAS(S21_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , M1L6, , , M1L11, );

--S21L8 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|counter_cella2~COUT at LC_X33_Y7_N3
--operation mode is arithmetic

S21L8_cout_0 = S21_safe_q[2] & !S21L5;
S21L8 = CARRY(S21L8_cout_0);

--S21L9 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X33_Y7_N3
--operation mode is arithmetic

S21L9_cout_1 = S21_safe_q[2] & !S21L6;
S21L9 = CARRY(S21L9_cout_1);


--S6_safe_q[2] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|safe_q[2] at LC_X33_Y9_N3
--operation mode is arithmetic

S6_safe_q[2]_lut_out = S6_safe_q[2] $ (!S6L5);
S6_safe_q[2] = DFFEAS(S6_safe_q[2]_lut_out, GLOBAL(C1L1), VCC, , Q1L4, , , Q1L3, );

--S6L8 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|counter_cella2~COUT at LC_X33_Y9_N3
--operation mode is arithmetic

S6L8_cout_0 = S6_safe_q[2] & !S6L5;
S6L8 = CARRY(S6L8_cout_0);

--S6L9 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X33_Y9_N3
--operation mode is arithmetic

S6L9_cout_1 = S6_safe_q[2] & !S6L6;
S6L9 = CARRY(S6L9_cout_1);


--L1L32 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_1[2]~36 at LC_X33_Y9_N7
--operation mode is normal

L1L32 = D1_TimeSet_EN & S21_safe_q[2] # !D1_TimeSet_EN & S6_safe_q[2];


--J1L32 is alarmclock:inst11|alarm~462 at LC_X35_Y10_N7
--operation mode is normal

J1L32 = S32_safe_q[2] & S52_safe_q[2] $ L1L32 # !L1L51 # !S32_safe_q[2] & L1L51 # S52_safe_q[2] $ L1L32;


--J1L42 is alarmclock:inst11|alarm~463 at LC_X35_Y10_N9
--operation mode is normal

J1L42 = J1L32 # J1L12 # J1L22 # J1L02;


--S12_safe_q[2] is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|safe_q[2] at LC_X39_Y11_N8
--operation mode is arithmetic

S12_safe_q[2]_lut_out = S12_safe_q[2] $ (!S12L5);
S12_safe_q[2] = DFFEAS(S12_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , J1L1, , , J1L9, );

--S12L8 is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|counter_cella2~COUT at LC_X39_Y11_N8
--operation mode is arithmetic

S12L8_cout_0 = S12_safe_q[2] & !S12L5;
S12L8 = CARRY(S12L8_cout_0);

--S12L9 is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X39_Y11_N8
--operation mode is arithmetic

S12L9_cout_1 = S12_safe_q[2] & !S12L6;
S12L9 = CARRY(S12L9_cout_1);


--S8_safe_q[2] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|safe_q[2] at LC_X34_Y11_N2
--operation mode is arithmetic

S8_safe_q[2]_lut_out = S8_safe_q[2] $ (!S8L5);
S8_safe_q[2] = DFFEAS(S8_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , M1L1, , , M1L21, );

--S8L8 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|counter_cella2~COUT at LC_X34_Y11_N2
--operation mode is arithmetic

S8L8_cout_0 = S8_safe_q[2] & !S8L5;
S8L8 = CARRY(S8L8_cout_0);

--S8L9 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X34_Y11_N2
--operation mode is arithmetic

S8L9_cout_1 = S8_safe_q[2] & !S8L6;
S8L9 = CARRY(S8L9_cout_1);


--S2_safe_q[2] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|safe_q[2] at LC_X33_Y13_N2
--operation mode is arithmetic

S2_safe_q[2]_lut_out = S2_safe_q[2] $ (!S2L5);
S2_safe_q[2] = DFFEAS(S2_safe_q[2]_lut_out, GLOBAL(P1_EO), VCC, , N1L4, , , N1L2, );

--S2L8 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|counter_cella2~COUT at LC_X33_Y13_N2
--operation mode is arithmetic

S2L8_cout_0 = S2_safe_q[2] & !S2L5;
S2L8 = CARRY(S2L8_cout_0);

--S2L9 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X33_Y13_N2
--operation mode is arithmetic

S2L9_cout_1 = S2_safe_q[2] & !S2L6;
S2L9 = CARRY(S2L9_cout_1);


--L1L7 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_1[2]~36 at LC_X33_Y13_N8
--operation mode is normal

L1L7 = D1_TimeSet_EN & S8_safe_q[2] # !D1_TimeSet_EN & S2_safe_q[2];


--S22_safe_q[2] is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|safe_q[2] at LC_X35_Y10_N2
--operation mode is arithmetic

S22_safe_q[2]_lut_out = S22_safe_q[2] $ (!S22L5);
S22_safe_q[2] = DFFEAS(S22_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , J1L4, , , J1L8, );

--S22L8 is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|counter_cella2~COUT at LC_X35_Y10_N2
--operation mode is arithmetic

S22L8_cout_0 = S22_safe_q[2] & !S22L5;
S22L8 = CARRY(S22L8_cout_0);

--S22L9 is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X35_Y10_N2
--operation mode is arithmetic

S22L9_cout_1 = S22_safe_q[2] & !S22L6;
S22L9 = CARRY(S22L9_cout_1);


--S9_safe_q[2] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|safe_q[2] at LC_X35_Y7_N7
--operation mode is arithmetic

S9_safe_q[2]_lut_out = S9_safe_q[2] $ (!S9L5);
S9_safe_q[2] = DFFEAS(S9_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , M1L5, , , M1L8, );

--S9L8 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|counter_cella2~COUT at LC_X35_Y7_N7
--operation mode is arithmetic

S9L8_cout_0 = S9_safe_q[2] & !S9L5;
S9L8 = CARRY(S9L8_cout_0);

--S9L9 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X35_Y7_N7
--operation mode is arithmetic

S9L9_cout_1 = S9_safe_q[2] & !S9L6;
S9L9 = CARRY(S9L9_cout_1);


--S3_safe_q[2] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|safe_q[2] at LC_X35_Y9_N2
--operation mode is arithmetic

S3_safe_q[2]_lut_out = S3_safe_q[2] $ (!S3L5);
S3_safe_q[2] = DFFEAS(S3_safe_q[2]_lut_out, GLOBAL(Q1_EO), VCC, , D1_Timepiece_EN, , , P1L2, );

--S3L8 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|counter_cella2~COUT at LC_X35_Y9_N2
--operation mode is arithmetic

S3L8_cout_0 = S3_safe_q[2] & !S3L5;
S3L8 = CARRY(S3L8_cout_0);

--S3L9 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X35_Y9_N2
--operation mode is arithmetic

S3L9_cout_1 = S3_safe_q[2] & !S3L6;
S3L9 = CARRY(S3L9_cout_1);


--L1L11 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_0[2]~39 at LC_X35_Y9_N7
--operation mode is normal

L1L11 = D1_TimeSet_EN & S9_safe_q[2] # !D1_TimeSet_EN & S3_safe_q[2];


--J1L52 is alarmclock:inst11|alarm~464 at LC_X35_Y10_N4
--operation mode is normal

J1L52 = S22_safe_q[2] & S12_safe_q[2] $ L1L7 # !L1L11 # !S22_safe_q[2] & L1L11 # S12_safe_q[2] $ L1L7;


--S02_safe_q[1] is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|safe_q[1] at LC_X36_Y11_N7
--operation mode is arithmetic

S02_safe_q[1]_lut_out = S02_safe_q[1] $ (S02L2);
S02_safe_q[1] = DFFEAS(S02_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , J1L2, , , J1L14, );

--S02L5 is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|counter_cella1~COUT at LC_X36_Y11_N7
--operation mode is arithmetic

S02L5_cout_0 = !S02L2 # !S02_safe_q[1];
S02L5 = CARRY(S02L5_cout_0);

--S02L6 is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X36_Y11_N7
--operation mode is arithmetic

S02L6_cout_1 = !S02L3 # !S02_safe_q[1];
S02L6 = CARRY(S02L6_cout_1);


--S7_safe_q[1] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|safe_q[1] at LC_X33_Y12_N2
--operation mode is arithmetic

S7_safe_q[1]_lut_out = S7_safe_q[1] $ (S7L2);
S7_safe_q[1] = DFFEAS(S7_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , M1L2, , , M1L9, );

--S7L5 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|counter_cella1~COUT at LC_X33_Y12_N2
--operation mode is arithmetic

S7L5_cout_0 = !S7L2 # !S7_safe_q[1];
S7L5 = CARRY(S7L5_cout_0);

--S7L6 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X33_Y12_N2
--operation mode is arithmetic

S7L6_cout_1 = !S7L3 # !S7_safe_q[1];
S7L6 = CARRY(S7L6_cout_1);


--S1_safe_q[1] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|safe_q[1] at LC_X33_Y11_N6
--operation mode is arithmetic

S1_safe_q[1]_lut_out = S1_safe_q[1] $ S1L2;
S1_safe_q[1] = DFFEAS(S1_safe_q[1]_lut_out, GLOBAL(P1_EO), VCC, , D1_Timepiece_EN, , , N1L6, );

--S1L5 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|counter_cella1~COUT at LC_X33_Y11_N6
--operation mode is arithmetic

S1L5_cout_0 = !S1L2 # !S1_safe_q[1];
S1L5 = CARRY(S1L5_cout_0);

--S1L6 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X33_Y11_N6
--operation mode is arithmetic

S1L6_cout_1 = !S1L3 # !S1_safe_q[1];
S1L6 = CARRY(S1L6_cout_1);


--L1L2 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_0[1]~37 at LC_X33_Y11_N3
--operation mode is normal

L1L2 = D1_TimeSet_EN & S7_safe_q[1] # !D1_TimeSet_EN & S1_safe_q[1];


--S52_safe_q[3] is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|safe_q[3] at LC_X33_Y10_N9
--operation mode is normal

S52_safe_q[3]_lut_out = S52L8 $ S52_safe_q[3];
S52_safe_q[3] = DFFEAS(S52_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , J1L5, , , J1L11, );


--S21_safe_q[3] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|safe_q[3] at LC_X33_Y7_N4
--operation mode is normal

S21_safe_q[3]_lut_out = S21L8 $ S21_safe_q[3];
S21_safe_q[3] = DFFEAS(S21_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , M1L6, , , M1L11, );


--S6_safe_q[3] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|safe_q[3] at LC_X33_Y9_N4
--operation mode is normal

S6_safe_q[3]_lut_out = S6L8 $ S6_safe_q[3];
S6_safe_q[3] = DFFEAS(S6_safe_q[3]_lut_out, GLOBAL(C1L1), VCC, , Q1L4, , , Q1L3, );


--L1L42 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_1[3]~37 at LC_X33_Y9_N0
--operation mode is normal

L1L42 = D1_TimeSet_EN & S21_safe_q[3] # !D1_TimeSet_EN & S6_safe_q[3];


--J1L62 is alarmclock:inst11|alarm~465 at LC_X33_Y11_N4
--operation mode is normal

J1L62 = S02_safe_q[1] & S52_safe_q[3] $ L1L42 # !L1L2 # !S02_safe_q[1] & L1L2 # S52_safe_q[3] $ L1L42;


--S42_safe_q[2] is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|safe_q[2] at LC_X36_Y10_N2
--operation mode is arithmetic

S42_safe_q[2]_lut_out = S42_safe_q[2] $ (!S42L5);
S42_safe_q[2] = DFFEAS(S42_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , J1L6, , , J1L7, );

--S42L8 is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|counter_cella2~COUT at LC_X36_Y10_N2
--operation mode is arithmetic

S42L8_cout_0 = S42_safe_q[2] & !S42L5;
S42L8 = CARRY(S42L8_cout_0);

--S42L9 is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X36_Y10_N2
--operation mode is arithmetic

S42L9_cout_1 = S42_safe_q[2] & !S42L6;
S42L9 = CARRY(S42L9_cout_1);


--S11_safe_q[2] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|safe_q[2] at LC_X36_Y7_N7
--operation mode is arithmetic

S11_safe_q[2]_lut_out = S11_safe_q[2] $ (!S11L5);
S11_safe_q[2] = DFFEAS(S11_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , M1L4, , , M1L7, );

--S11L8 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|counter_cella2~COUT at LC_X36_Y7_N7
--operation mode is arithmetic

S11L8_cout_0 = S11_safe_q[2] & !S11L5;
S11L8 = CARRY(S11L8_cout_0);

--S11L9 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X36_Y7_N7
--operation mode is arithmetic

S11L9_cout_1 = S11_safe_q[2] & !S11L6;
S11L9 = CARRY(S11L9_cout_1);


--S5_safe_q[2] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|safe_q[2] at LC_X36_Y8_N2
--operation mode is arithmetic

S5_safe_q[2]_lut_out = S5_safe_q[2] $ (!S5L5);
S5_safe_q[2] = DFFEAS(S5_safe_q[2]_lut_out, GLOBAL(C1L1), VCC, , D1_Timepiece_EN, , , Q1L2, );

--S5L8 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|counter_cella2~COUT at LC_X36_Y8_N2
--operation mode is arithmetic

S5L8_cout_0 = S5_safe_q[2] & !S5L5;
S5L8 = CARRY(S5L8_cout_0);

--S5L9 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X36_Y8_N2
--operation mode is arithmetic

S5L9_cout_1 = S5_safe_q[2] & !S5L6;
S5L9 = CARRY(S5L9_cout_1);


--L1L91 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_0[2]~37 at LC_X36_Y8_N9
--operation mode is normal

L1L91 = D1_TimeSet_EN & S11_safe_q[2] # !D1_TimeSet_EN & S5_safe_q[2];


--S42_safe_q[0] is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|safe_q[0] at LC_X36_Y10_N0
--operation mode is arithmetic

S42_safe_q[0]_lut_out = !S42_safe_q[0];
S42_safe_q[0] = DFFEAS(S42_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , J1L6, , , J1L7, );

--S42L2 is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|counter_cella0~COUT at LC_X36_Y10_N0
--operation mode is arithmetic

S42L2_cout_0 = S42_safe_q[0];
S42L2 = CARRY(S42L2_cout_0);

--S42L3 is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X36_Y10_N0
--operation mode is arithmetic

S42L3_cout_1 = S42_safe_q[0];
S42L3 = CARRY(S42L3_cout_1);


--S11_safe_q[0] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|safe_q[0] at LC_X36_Y7_N5
--operation mode is arithmetic

S11_safe_q[0]_lut_out = !S11_safe_q[0];
S11_safe_q[0] = DFFEAS(S11_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , M1L4, , , M1L7, );

--S11L2 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|counter_cella0~COUT at LC_X36_Y7_N5
--operation mode is arithmetic

S11L2_cout_0 = S11_safe_q[0];
S11L2 = CARRY(S11L2_cout_0);

--S11L3 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X36_Y7_N5
--operation mode is arithmetic

S11L3_cout_1 = S11_safe_q[0];
S11L3 = CARRY(S11L3_cout_1);


--S5_safe_q[0] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|safe_q[0] at LC_X36_Y8_N0
--operation mode is arithmetic

S5_safe_q[0]_lut_out = !S5_safe_q[0];
S5_safe_q[0] = DFFEAS(S5_safe_q[0]_lut_out, GLOBAL(C1L1), VCC, , D1_Timepiece_EN, , , Q1L2, );

--S5L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|counter_cella0~COUT at LC_X36_Y8_N0
--operation mode is arithmetic

S5L2_cout_0 = S5_safe_q[0];
S5L2 = CARRY(S5L2_cout_0);

--S5L3 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X36_Y8_N0
--operation mode is arithmetic

S5L3_cout_1 = S5_safe_q[0];
S5L3 = CARRY(S5L3_cout_1);


--L1L71 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_0[0]~38 at LC_X36_Y8_N5
--operation mode is normal

L1L71 = D1_TimeSet_EN & S11_safe_q[0] # !D1_TimeSet_EN & S5_safe_q[0];


--J1L72 is alarmclock:inst11|alarm~466 at LC_X36_Y10_N7
--operation mode is normal

J1L72 = S42_safe_q[2] & S42_safe_q[0] $ L1L71 # !L1L91 # !S42_safe_q[2] & L1L91 # S42_safe_q[0] $ L1L71;


--S52_safe_q[0] is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|safe_q[0] at LC_X33_Y10_N6
--operation mode is arithmetic

S52_safe_q[0]_lut_out = !S52_safe_q[0];
S52_safe_q[0] = DFFEAS(S52_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , J1L5, , , J1L11, );

--S52L2 is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|counter_cella0~COUT at LC_X33_Y10_N6
--operation mode is arithmetic

S52L2_cout_0 = S52_safe_q[0];
S52L2 = CARRY(S52L2_cout_0);

--S52L3 is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X33_Y10_N6
--operation mode is arithmetic

S52L3_cout_1 = S52_safe_q[0];
S52L3 = CARRY(S52L3_cout_1);


--S21_safe_q[0] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|safe_q[0] at LC_X33_Y7_N1
--operation mode is arithmetic

S21_safe_q[0]_lut_out = !S21_safe_q[0];
S21_safe_q[0] = DFFEAS(S21_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , M1L6, , , M1L11, );

--S21L2 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|counter_cella0~COUT at LC_X33_Y7_N1
--operation mode is arithmetic

S21L2_cout_0 = S21_safe_q[0];
S21L2 = CARRY(S21L2_cout_0);

--S21L3 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X33_Y7_N1
--operation mode is arithmetic

S21L3_cout_1 = S21_safe_q[0];
S21L3 = CARRY(S21L3_cout_1);


--S6_safe_q[0] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|safe_q[0] at LC_X33_Y9_N1
--operation mode is arithmetic

S6_safe_q[0]_lut_out = !S6_safe_q[0];
S6_safe_q[0] = DFFEAS(S6_safe_q[0]_lut_out, GLOBAL(C1L1), VCC, , Q1L4, , , Q1L3, );

--S6L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|counter_cella0~COUT at LC_X33_Y9_N1
--operation mode is arithmetic

S6L2_cout_0 = S6_safe_q[0];
S6L2 = CARRY(S6L2_cout_0);

--S6L3 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X33_Y9_N1
--operation mode is arithmetic

S6L3_cout_1 = S6_safe_q[0];
S6L3 = CARRY(S6L3_cout_1);


--L1L12 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_1[0]~38 at LC_X33_Y9_N5
--operation mode is normal

L1L12 = D1_TimeSet_EN & S21_safe_q[0] # !D1_TimeSet_EN & S6_safe_q[0];


--S32_safe_q[3] is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|safe_q[3] at LC_X34_Y10_N4
--operation mode is normal

S32_safe_q[3]_lut_out = S32L8 $ S32_safe_q[3];
S32_safe_q[3] = DFFEAS(S32_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , J1L3, , , J1L01, );


--S01_safe_q[3] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|safe_q[3] at LC_X39_Y9_N8
--operation mode is normal

S01_safe_q[3]_lut_out = S01L8 $ S01_safe_q[3];
S01_safe_q[3] = DFFEAS(S01_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , M1L3, , , M1L01, );


--S4_safe_q[3] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|safe_q[3] at LC_X36_Y9_N8
--operation mode is normal

S4_safe_q[3]_lut_out = S4L8 $ S4_safe_q[3];
S4_safe_q[3] = DFFEAS(S4_safe_q[3]_lut_out, GLOBAL(Q1_EO), VCC, , P1L4, , , P1L3, );


--L1L61 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_1[3]~38 at LC_X33_Y10_N5
--operation mode is normal

L1L61 = D1_TimeSet_EN & S01_safe_q[3] # !D1_TimeSet_EN & S4_safe_q[3];


--J1L82 is alarmclock:inst11|alarm~467 at LC_X33_Y10_N2
--operation mode is normal

J1L82 = L1L12 & L1L61 $ S32_safe_q[3] # !S52_safe_q[0] # !L1L12 & S52_safe_q[0] # L1L61 $ S32_safe_q[3];


--J1L92 is alarmclock:inst11|alarm~468 at LC_X39_Y10_N2
--operation mode is normal

J1L92 = J1L72 # J1L52 # J1L62 # J1L82;


--S32_safe_q[1] is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|safe_q[1] at LC_X34_Y10_N2
--operation mode is arithmetic

S32_safe_q[1]_lut_out = S32_safe_q[1] $ (S32L2);
S32_safe_q[1] = DFFEAS(S32_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , J1L3, , , J1L01, );

--S32L5 is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|counter_cella1~COUT at LC_X34_Y10_N2
--operation mode is arithmetic

S32L5_cout_0 = !S32L2 # !S32_safe_q[1];
S32L5 = CARRY(S32L5_cout_0);

--S32L6 is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X34_Y10_N2
--operation mode is arithmetic

S32L6_cout_1 = !S32L3 # !S32_safe_q[1];
S32L6 = CARRY(S32L6_cout_1);


--S01_safe_q[1] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|safe_q[1] at LC_X39_Y9_N6
--operation mode is arithmetic

S01_safe_q[1]_lut_out = S01_safe_q[1] $ S01L2;
S01_safe_q[1] = DFFEAS(S01_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , M1L3, , , M1L01, );

--S01L5 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|counter_cella1~COUT at LC_X39_Y9_N6
--operation mode is arithmetic

S01L5_cout_0 = !S01L2 # !S01_safe_q[1];
S01L5 = CARRY(S01L5_cout_0);

--S01L6 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X39_Y9_N6
--operation mode is arithmetic

S01L6_cout_1 = !S01L3 # !S01_safe_q[1];
S01L6 = CARRY(S01L6_cout_1);


--S4_safe_q[1] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|safe_q[1] at LC_X36_Y9_N6
--operation mode is arithmetic

S4_safe_q[1]_lut_out = S4_safe_q[1] $ S4L2;
S4_safe_q[1] = DFFEAS(S4_safe_q[1]_lut_out, GLOBAL(Q1_EO), VCC, , P1L4, , , P1L3, );

--S4L5 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|counter_cella1~COUT at LC_X36_Y9_N6
--operation mode is arithmetic

S4L5_cout_0 = !S4L2 # !S4_safe_q[1];
S4L5 = CARRY(S4L5_cout_0);

--S4L6 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X36_Y9_N6
--operation mode is arithmetic

S4L6_cout_1 = !S4L3 # !S4_safe_q[1];
S4L6 = CARRY(S4L6_cout_1);


--L1L41 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_1[1]~39 at LC_X36_Y9_N1
--operation mode is normal

L1L41 = D1_TimeSet_EN & S01_safe_q[1] # !D1_TimeSet_EN & S4_safe_q[1];


--S12_safe_q[1] is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|safe_q[1] at LC_X39_Y11_N7
--operation mode is arithmetic

S12_safe_q[1]_lut_out = S12_safe_q[1] $ (S12L2);
S12_safe_q[1] = DFFEAS(S12_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , J1L1, , , J1L9, );

--S12L5 is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|counter_cella1~COUT at LC_X39_Y11_N7
--operation mode is arithmetic

S12L5_cout_0 = !S12L2 # !S12_safe_q[1];
S12L5 = CARRY(S12L5_cout_0);

--S12L6 is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X39_Y11_N7
--operation mode is arithmetic

S12L6_cout_1 = !S12L3 # !S12_safe_q[1];
S12L6 = CARRY(S12L6_cout_1);


--S8_safe_q[1] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|safe_q[1] at LC_X34_Y11_N1
--operation mode is arithmetic

S8_safe_q[1]_lut_out = S8_safe_q[1] $ S8L2;
S8_safe_q[1] = DFFEAS(S8_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , M1L1, , , M1L21, );

--S8L5 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|counter_cella1~COUT at LC_X34_Y11_N1
--operation mode is arithmetic

S8L5_cout_0 = !S8L2 # !S8_safe_q[1];
S8L5 = CARRY(S8L5_cout_0);

--S8L6 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X34_Y11_N1
--operation mode is arithmetic

S8L6_cout_1 = !S8L3 # !S8_safe_q[1];
S8L6 = CARRY(S8L6_cout_1);


--S2_safe_q[1] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|safe_q[1] at LC_X33_Y13_N1
--operation mode is arithmetic

S2_safe_q[1]_lut_out = S2_safe_q[1] $ S2L2;
S2_safe_q[1] = DFFEAS(S2_safe_q[1]_lut_out, GLOBAL(P1_EO), VCC, , N1L4, , , N1L2, );

--S2L5 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|counter_cella1~COUT at LC_X33_Y13_N1
--operation mode is arithmetic

S2L5_cout_0 = !S2L2 # !S2_safe_q[1];
S2L5 = CARRY(S2L5_cout_0);

--S2L6 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X33_Y13_N1
--operation mode is arithmetic

S2L6_cout_1 = !S2L3 # !S2_safe_q[1];
S2L6 = CARRY(S2L6_cout_1);


--L1L6 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_1[1]~37 at LC_X34_Y11_N9
--operation mode is normal

L1L6 = D1_TimeSet_EN & S8_safe_q[1] # !D1_TimeSet_EN & S2_safe_q[1];


--J1L03 is alarmclock:inst11|alarm~469 at LC_X34_Y10_N8
--operation mode is normal

J1L03 = S32_safe_q[1] & S12_safe_q[1] $ L1L6 # !L1L41 # !S32_safe_q[1] & L1L41 # S12_safe_q[1] $ L1L6;


--S12_safe_q[0] is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|safe_q[0] at LC_X39_Y11_N6
--operation mode is arithmetic

S12_safe_q[0]_lut_out = !S12_safe_q[0];
S12_safe_q[0] = DFFEAS(S12_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , J1L1, , , J1L9, );

--S12L2 is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|counter_cella0~COUT at LC_X39_Y11_N6
--operation mode is arithmetic

S12L2_cout_0 = S12_safe_q[0];
S12L2 = CARRY(S12L2_cout_0);

--S12L3 is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X39_Y11_N6
--operation mode is arithmetic

S12L3_cout_1 = S12_safe_q[0];
S12L3 = CARRY(S12L3_cout_1);


--S8_safe_q[0] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|safe_q[0] at LC_X34_Y11_N0
--operation mode is arithmetic

S8_safe_q[0]_lut_out = !S8_safe_q[0];
S8_safe_q[0] = DFFEAS(S8_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , M1L1, , , M1L21, );

--S8L2 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|counter_cella0~COUT at LC_X34_Y11_N0
--operation mode is arithmetic

S8L2_cout_0 = S8_safe_q[0];
S8L2 = CARRY(S8L2_cout_0);

--S8L3 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X34_Y11_N0
--operation mode is arithmetic

S8L3_cout_1 = S8_safe_q[0];
S8L3 = CARRY(S8L3_cout_1);


--S2_safe_q[0] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|safe_q[0] at LC_X33_Y13_N0
--operation mode is arithmetic

S2_safe_q[0]_lut_out = !S2_safe_q[0];
S2_safe_q[0] = DFFEAS(S2_safe_q[0]_lut_out, GLOBAL(P1_EO), VCC, , N1L4, , , N1L2, );

--S2L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|counter_cella0~COUT at LC_X33_Y13_N0
--operation mode is arithmetic

S2L2_cout_0 = S2_safe_q[0];
S2L2 = CARRY(S2L2_cout_0);

--S2L3 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X33_Y13_N0
--operation mode is arithmetic

S2L3_cout_1 = S2_safe_q[0];
S2L3 = CARRY(S2L3_cout_1);


--L1L5 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_1[0]~38 at LC_X34_Y11_N4
--operation mode is normal

L1L5 = D1_TimeSet_EN & S8_safe_q[0] # !D1_TimeSet_EN & S2_safe_q[0];


--S02_safe_q[2] is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|safe_q[2] at LC_X36_Y11_N8
--operation mode is arithmetic

S02_safe_q[2]_lut_out = S02_safe_q[2] $ (!S02L5);
S02_safe_q[2] = DFFEAS(S02_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , J1L2, , , J1L14, );

--S02L8 is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|counter_cella2~COUT at LC_X36_Y11_N8
--operation mode is arithmetic

S02L8_cout_0 = S02_safe_q[2] & !S02L5;
S02L8 = CARRY(S02L8_cout_0);

--S02L9 is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X36_Y11_N8
--operation mode is arithmetic

S02L9_cout_1 = S02_safe_q[2] & !S02L6;
S02L9 = CARRY(S02L9_cout_1);


--S7_safe_q[2] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|safe_q[2] at LC_X33_Y12_N3
--operation mode is arithmetic

S7_safe_q[2]_lut_out = S7_safe_q[2] $ (!S7L5);
S7_safe_q[2] = DFFEAS(S7_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , M1L2, , , M1L9, );

--S7L8 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|counter_cella2~COUT at LC_X33_Y12_N3
--operation mode is arithmetic

S7L8_cout_0 = S7_safe_q[2] & !S7L5;
S7L8 = CARRY(S7L8_cout_0);

--S7L9 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X33_Y12_N3
--operation mode is arithmetic

S7L9_cout_1 = S7_safe_q[2] & !S7L6;
S7L9 = CARRY(S7L9_cout_1);


--S1_safe_q[2] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|safe_q[2] at LC_X33_Y11_N7
--operation mode is arithmetic

S1_safe_q[2]_lut_out = S1_safe_q[2] $ (!S1L5);
S1_safe_q[2] = DFFEAS(S1_safe_q[2]_lut_out, GLOBAL(P1_EO), VCC, , D1_Timepiece_EN, , , N1L6, );

--S1L8 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|counter_cella2~COUT at LC_X33_Y11_N7
--operation mode is arithmetic

S1L8_cout_0 = S1_safe_q[2] & !S1L5;
S1L8 = CARRY(S1L8_cout_0);

--S1L9 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X33_Y11_N7
--operation mode is arithmetic

S1L9_cout_1 = S1_safe_q[2] & !S1L6;
S1L9 = CARRY(S1L9_cout_1);


--L1L3 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_0[2]~38 at LC_X33_Y11_N9
--operation mode is normal

L1L3 = D1_TimeSet_EN & S7_safe_q[2] # !D1_TimeSet_EN & S1_safe_q[2];


--J1L13 is alarmclock:inst11|alarm~470 at LC_X36_Y11_N3
--operation mode is normal

J1L13 = S02_safe_q[2] & L1L5 $ S12_safe_q[0] # !L1L3 # !S02_safe_q[2] & L1L3 # L1L5 $ S12_safe_q[0];


--S52_safe_q[1] is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|safe_q[1] at LC_X33_Y10_N7
--operation mode is arithmetic

S52_safe_q[1]_lut_out = S52_safe_q[1] $ (S52L2);
S52_safe_q[1] = DFFEAS(S52_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , J1L5, , , J1L11, );

--S52L5 is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|counter_cella1~COUT at LC_X33_Y10_N7
--operation mode is arithmetic

S52L5_cout_0 = !S52L2 # !S52_safe_q[1];
S52L5 = CARRY(S52L5_cout_0);

--S52L6 is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X33_Y10_N7
--operation mode is arithmetic

S52L6_cout_1 = !S52L3 # !S52_safe_q[1];
S52L6 = CARRY(S52L6_cout_1);


--S21_safe_q[1] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|safe_q[1] at LC_X33_Y7_N2
--operation mode is arithmetic

S21_safe_q[1]_lut_out = S21_safe_q[1] $ (S21L2);
S21_safe_q[1] = DFFEAS(S21_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , M1L6, , , M1L11, );

--S21L5 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|counter_cella1~COUT at LC_X33_Y7_N2
--operation mode is arithmetic

S21L5_cout_0 = !S21L2 # !S21_safe_q[1];
S21L5 = CARRY(S21L5_cout_0);

--S21L6 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X33_Y7_N2
--operation mode is arithmetic

S21L6_cout_1 = !S21L3 # !S21_safe_q[1];
S21L6 = CARRY(S21L6_cout_1);


--S6_safe_q[1] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|safe_q[1] at LC_X33_Y9_N2
--operation mode is arithmetic

S6_safe_q[1]_lut_out = S6_safe_q[1] $ (S6L2);
S6_safe_q[1] = DFFEAS(S6_safe_q[1]_lut_out, GLOBAL(C1L1), VCC, , Q1L4, , , Q1L3, );

--S6L5 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|counter_cella1~COUT at LC_X33_Y9_N2
--operation mode is arithmetic

S6L5_cout_0 = !S6L2 # !S6_safe_q[1];
S6L5 = CARRY(S6L5_cout_0);

--S6L6 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X33_Y9_N2
--operation mode is arithmetic

S6L6_cout_1 = !S6L3 # !S6_safe_q[1];
S6L6 = CARRY(S6L6_cout_1);


--L1L22 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_1[1]~39 at LC_X33_Y9_N6
--operation mode is normal

L1L22 = D1_TimeSet_EN & S21_safe_q[1] # !D1_TimeSet_EN & S6_safe_q[1];


--S02_safe_q[3] is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|safe_q[3] at LC_X36_Y11_N9
--operation mode is normal

S02_safe_q[3]_lut_out = S02L8 $ S02_safe_q[3];
S02_safe_q[3] = DFFEAS(S02_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , J1L2, , , J1L14, );


--S7_safe_q[3] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|safe_q[3] at LC_X33_Y12_N4
--operation mode is normal

S7_safe_q[3]_lut_out = S7L8 $ S7_safe_q[3];
S7_safe_q[3] = DFFEAS(S7_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , M1L2, , , M1L9, );


--S1_safe_q[3] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|safe_q[3] at LC_X33_Y11_N8
--operation mode is normal

S1_safe_q[3]_lut_out = S1L8 $ S1_safe_q[3];
S1_safe_q[3] = DFFEAS(S1_safe_q[3]_lut_out, GLOBAL(P1_EO), VCC, , D1_Timepiece_EN, , , N1L6, );


--L1L4 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_0[3]~39 at LC_X33_Y11_N1
--operation mode is normal

L1L4 = D1_TimeSet_EN & S7_safe_q[3] # !D1_TimeSet_EN & S1_safe_q[3];


--J1L23 is alarmclock:inst11|alarm~471 at LC_X33_Y10_N1
--operation mode is normal

J1L23 = L1L22 & L1L4 $ S02_safe_q[3] # !S52_safe_q[1] # !L1L22 & S52_safe_q[1] # L1L4 $ S02_safe_q[3];


--S12_safe_q[3] is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|safe_q[3] at LC_X39_Y11_N9
--operation mode is normal

S12_safe_q[3]_lut_out = S12L8 $ S12_safe_q[3];
S12_safe_q[3] = DFFEAS(S12_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , J1L1, , , J1L9, );


--S8_safe_q[3] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|safe_q[3] at LC_X34_Y11_N3
--operation mode is normal

S8_safe_q[3]_lut_out = S8_safe_q[3] $ (S8L8);
S8_safe_q[3] = DFFEAS(S8_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , M1L1, , , M1L21, );


--S2_safe_q[3] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|safe_q[3] at LC_X33_Y13_N3
--operation mode is normal

S2_safe_q[3]_lut_out = S2_safe_q[3] $ (S2L8);
S2_safe_q[3] = DFFEAS(S2_safe_q[3]_lut_out, GLOBAL(P1_EO), VCC, , N1L4, , , N1L2, );


--L1L8 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_1[3]~39 at LC_X34_Y11_N8
--operation mode is normal

L1L8 = D1_TimeSet_EN & S8_safe_q[3] # !D1_TimeSet_EN & S2_safe_q[3];


--S42_safe_q[3] is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|safe_q[3] at LC_X36_Y10_N3
--operation mode is normal

S42_safe_q[3]_lut_out = S42_safe_q[3] $ (S42L8);
S42_safe_q[3] = DFFEAS(S42_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , J1L6, , , J1L7, );


--S11_safe_q[3] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|safe_q[3] at LC_X36_Y7_N8
--operation mode is normal

S11_safe_q[3]_lut_out = S11L8 $ S11_safe_q[3];
S11_safe_q[3] = DFFEAS(S11_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , M1L4, , , M1L7, );


--S5_safe_q[3] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|safe_q[3] at LC_X36_Y8_N3
--operation mode is normal

S5_safe_q[3]_lut_out = S5_safe_q[3] $ (S5L8);
S5_safe_q[3] = DFFEAS(S5_safe_q[3]_lut_out, GLOBAL(C1L1), VCC, , D1_Timepiece_EN, , , Q1L2, );


--L1L02 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_0[3]~39 at LC_X36_Y8_N8
--operation mode is normal

L1L02 = D1_TimeSet_EN & S11_safe_q[3] # !D1_TimeSet_EN & S5_safe_q[3];


--J1L33 is alarmclock:inst11|alarm~472 at LC_X36_Y10_N4
--operation mode is normal

J1L33 = S42_safe_q[3] & S12_safe_q[3] $ L1L8 # !L1L02 # !S42_safe_q[3] & L1L02 # S12_safe_q[3] $ L1L8;


--J1L43 is alarmclock:inst11|alarm~473 at LC_X36_Y10_N5
--operation mode is normal

J1L43 = J1L03 # J1L33 # J1L13 # J1L23;


--J1_alarm is alarmclock:inst11|alarm at LC_X36_Y10_N6
--operation mode is normal

J1_alarm = J1L43 # J1L42 # J1L92;


--H1L68 is disp_data_mux:inst8|reduce_or~38 at LC_X36_Y1_N3
--operation mode is normal

H1L68 = H1_Data[1] & H1_Data[3] # !H1_Data[1] & H1_Data[2] $ (!H1_Data[3] & H1_Data[0]);


--H1L78 is disp_data_mux:inst8|reduce_or~40 at LC_X36_Y1_N6
--operation mode is normal

H1L78 = H1_Data[2] & H1_Data[3] # H1_Data[0] $ H1_Data[1] # !H1_Data[2] & H1_Data[3] & H1_Data[1];


--H1L88 is disp_data_mux:inst8|reduce_or~42 at LC_X36_Y1_N4
--operation mode is normal

H1L88 = H1_Data[2] & H1_Data[3] # !H1_Data[2] & H1_Data[1] & H1_Data[3] # !H1_Data[0];


--H1L66 is disp_data_mux:inst8|disp_data[3]~32 at LC_X36_Y1_N5
--operation mode is normal

H1L66 = H1_Data[1] & H1_Data[3] # H1_Data[2] & H1_Data[0] # !H1_Data[1] & H1_Data[2] $ (!H1_Data[3] & H1_Data[0]);


--H1L56 is disp_data_mux:inst8|disp_data[2]~34 at LC_X36_Y1_N7
--operation mode is normal

H1L56 = H1_Data[0] # H1_Data[1] & H1_Data[3] # !H1_Data[1] & H1_Data[2];


--H1L46 is disp_data_mux:inst8|disp_data[1]~36 at LC_X36_Y1_N2
--operation mode is normal

H1L46 = H1_Data[2] & H1_Data[3] # H1_Data[0] & H1_Data[1] # !H1_Data[2] & H1_Data[1] # !H1_Data[3] & H1_Data[0];


--H1L36 is disp_data_mux:inst8|disp_data[0]~38 at LC_X36_Y1_N0
--operation mode is normal

H1L36 = H1_Data[2] & !H1_Data[3] & !H1_Data[1] # !H1_Data[0] # !H1_Data[2] & H1_Data[3] $ (H1_Data[1]);


--J1L8 is alarmclock:inst11|LessThan~164 at LC_X35_Y10_N8
--operation mode is normal

J1L8 = S22_safe_q[3] & S22_safe_q[0] # S22_safe_q[1] # S22_safe_q[2];


--J1_disp_drive[1] is alarmclock:inst11|disp_drive[1] at LC_X34_Y7_N3
--operation mode is normal

J1_disp_drive[1]_lut_out = J1_disp_drive[0] & !J1_disp_drive[2] & !J1_disp_drive[1] # !J1_disp_drive[0] & J1_disp_drive[1];
J1_disp_drive[1] = DFFEAS(J1_disp_drive[1]_lut_out, GLOBAL(SW1), VCC, , D1_Alarmclock_EN, , , , );


--J1_disp_drive[0] is alarmclock:inst11|disp_drive[0] at LC_X34_Y7_N1
--operation mode is normal

J1_disp_drive[0]_lut_out = !J1_disp_drive[0];
J1_disp_drive[0] = DFFEAS(J1_disp_drive[0]_lut_out, GLOBAL(SW1), VCC, , D1_Alarmclock_EN, , , , );


--J1_disp_drive[2] is alarmclock:inst11|disp_drive[2] at LC_X34_Y7_N7
--operation mode is normal

J1_disp_drive[2]_lut_out = J1_disp_drive[2] & !J1_disp_drive[0] # !J1_disp_drive[2] & J1_disp_drive[0] & J1_disp_drive[1];
J1_disp_drive[2] = DFFEAS(J1_disp_drive[2]_lut_out, GLOBAL(SW1), VCC, , D1_Alarmclock_EN, , , , );


--J1L4 is alarmclock:inst11|Decoder~20 at LC_X35_Y10_N6
--operation mode is normal

J1L4 = J1_disp_drive[0] & J1_disp_drive[1] & !J1_disp_drive[2];

--J1_alarmclock_disp_select[2] is alarmclock:inst11|alarmclock_disp_select[2] at LC_X35_Y10_N6
--operation mode is normal

J1_alarmclock_disp_select[2] = DFFEAS(J1L4, GLOBAL(F1_f200hz), VCC, , , , , , );


--M1L8 is time_auto_and_set:inst1|timeset:b2v_inst3|LessThan~160 at LC_X35_Y9_N6
--operation mode is normal

M1L8 = S9_safe_q[3] & S9_safe_q[0] # S9_safe_q[2] # S9_safe_q[1];


--M1_disp_drive[1] is time_auto_and_set:inst1|timeset:b2v_inst3|disp_drive[1] at LC_X35_Y7_N9
--operation mode is normal

M1_disp_drive[1]_lut_out = !M1_disp_drive[2] & M1_disp_drive[0] $ M1_disp_drive[1];
M1_disp_drive[1] = DFFEAS(M1_disp_drive[1]_lut_out, GLOBAL(SW1), VCC, , D1_TimeSet_EN, , , , );


--M1_disp_drive[0] is time_auto_and_set:inst1|timeset:b2v_inst3|disp_drive[0] at LC_X35_Y7_N2
--operation mode is normal

M1_disp_drive[0]_lut_out = !M1_disp_drive[0] & !M1_disp_drive[2] # !M1_disp_drive[1];
M1_disp_drive[0] = DFFEAS(M1_disp_drive[0]_lut_out, GLOBAL(SW1), VCC, , D1_TimeSet_EN, , , , );


--M1_disp_drive[2] is time_auto_and_set:inst1|timeset:b2v_inst3|disp_drive[2] at LC_X35_Y7_N0
--operation mode is normal

M1_disp_drive[2]_lut_out = M1_disp_drive[0] & M1_disp_drive[1] & !M1_disp_drive[2] # !M1_disp_drive[0] & !M1_disp_drive[1] & M1_disp_drive[2];
M1_disp_drive[2] = DFFEAS(M1_disp_drive[2]_lut_out, GLOBAL(SW1), VCC, , D1_TimeSet_EN, , , , );


--M1L5 is time_auto_and_set:inst1|timeset:b2v_inst3|Decoder~95 at LC_X35_Y7_N3
--operation mode is normal

M1L5 = M1_disp_drive[0] & M1_disp_drive[1] & !M1_disp_drive[2];


--P1L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|LessThan~47 at LC_X36_Y9_N4
--operation mode is normal

P1L2 = S3_safe_q[3] & S3_safe_q[0] # S3_safe_q[2] # S3_safe_q[1];


--D1_Timepiece_EN is maincontrol:inst3|Timepiece_EN at LC_X36_Y6_N6
--operation mode is normal

D1_Timepiece_EN_lut_out = !D1_Function[1] & !D1_Function[0] & !D1_Function[2];
D1_Timepiece_EN = DFFEAS(D1_Timepiece_EN_lut_out, GLOBAL(SW3), VCC, , , , , , );


--D1_Function[0] is maincontrol:inst3|Function[0] at LC_X34_Y13_N7
--operation mode is normal

D1_Function[0]_lut_out = !D1_Function[0] & !D1_Function[1] # !D1_Function[2];
D1_Function[0] = DFFEAS(D1_Function[0]_lut_out, GLOBAL(SW3), VCC, , , , , , );


--D1_Function[2] is maincontrol:inst3|Function[2] at LC_X34_Y13_N6
--operation mode is normal

D1_Function[2]_lut_out = D1_Function[0] & !D1_Function[2] & D1_Function[1] # !D1_Function[0] & D1_Function[2] & !D1_Function[1];
D1_Function[2] = DFFEAS(D1_Function[2]_lut_out, GLOBAL(SW3), VCC, , , , , , );


--D1_Function[1] is maincontrol:inst3|Function[1] at LC_X33_Y8_N7
--operation mode is normal

D1_Function[1]_lut_out = !D1_Function[2] & D1_Function[1] $ D1_Function[0];
D1_Function[1] = DFFEAS(D1_Function[1]_lut_out, GLOBAL(SW3), VCC, , , , , , );


--J1L53 is alarmclock:inst11|always2~26 at LC_X36_Y11_N2
--operation mode is normal

J1L53 = !S12_safe_q[0] & S12_safe_q[1] & !S12_safe_q[2] & !S12_safe_q[3];


--J1L9 is alarmclock:inst11|LessThan~214 at LC_X36_Y11_N4
--operation mode is normal

J1L9 = S12_safe_q[1] # S12_safe_q[2] # S12_safe_q[3];


--J1L04 is alarmclock:inst11|hour_set0[2]~117 at LC_X36_Y11_N5
--operation mode is normal

J1L04 = S02_safe_q[2] # S02_safe_q[3] & S02_safe_q[0] # S02_safe_q[1];


--J1L14 is alarmclock:inst11|hour_set0[2]~118 at LC_X36_Y11_N0
--operation mode is normal

J1L14 = J1L04 & J1L9 # S02_safe_q[3] # !J1L04 & J1L9 & S02_safe_q[3] # !J1L53;


--J1L2 is alarmclock:inst11|Decoder~18 at LC_X34_Y10_N6
--operation mode is normal

J1L2 = J1_disp_drive[0] & !J1_disp_drive[2] & !J1_disp_drive[1];

--J1_alarmclock_disp_select[4] is alarmclock:inst11|alarmclock_disp_select[4] at LC_X34_Y10_N6
--operation mode is normal

J1_alarmclock_disp_select[4] = DFFEAS(J1L2, GLOBAL(F1_f200hz), VCC, , , , , , );


--M1L9 is time_auto_and_set:inst1|timeset:b2v_inst3|LessThan~192 at LC_X33_Y11_N0
--operation mode is normal

M1L9 = S7_safe_q[3] & S7_safe_q[1] # S7_safe_q[2] # S7_safe_q[0];


--M1L2 is time_auto_and_set:inst1|timeset:b2v_inst3|Decoder~18 at LC_X35_Y7_N1
--operation mode is normal

M1L2 = M1_disp_drive[0] & !M1_disp_drive[1] & !M1_disp_drive[2];


--N1L3 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|always0~86 at LC_X33_Y13_N9
--operation mode is normal

N1L3 = !S2_safe_q[2] & S2_safe_q[1] & !S2_safe_q[3] & !S2_safe_q[0];


--N1L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|LessThan~82 at LC_X33_Y13_N4
--operation mode is normal

N1L2 = S2_safe_q[1] # S2_safe_q[3] # S2_safe_q[2];

--N1_EO is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|EO at LC_X33_Y13_N4
--operation mode is normal

N1_EO = DFFEAS(N1L2, GLOBAL(P1_EO), VCC, , N1L4, , , , );


--N1L5 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|hour_data1[0]~71 at LC_X33_Y13_N5
--operation mode is normal

N1L5 = S1_safe_q[2] # S1_safe_q[3] & S1_safe_q[0] # S1_safe_q[1];


--N1L6 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|hour_data1[0]~72 at LC_X33_Y13_N6
--operation mode is normal

N1L6 = N1L2 & S1_safe_q[3] # N1L5 # !N1L3 # !N1L2 & S1_safe_q[3] & N1L5;


--J1L01 is alarmclock:inst11|LessThan~290 at LC_X34_Y10_N0
--operation mode is normal

J1L01 = S32_safe_q[3] # S32_safe_q[2] & S32_safe_q[0] # S32_safe_q[1];


--J1L3 is alarmclock:inst11|Decoder~19 at LC_X34_Y10_N5
--operation mode is normal

J1L3 = !J1_disp_drive[0] & !J1_disp_drive[2] & J1_disp_drive[1];

--J1_alarmclock_disp_select[3] is alarmclock:inst11|alarmclock_disp_select[3] at LC_X34_Y10_N5
--operation mode is normal

J1_alarmclock_disp_select[3] = DFFEAS(J1L3, GLOBAL(F1_f200hz), VCC, , , , , , );


--M1L01 is time_auto_and_set:inst1|timeset:b2v_inst3|LessThan~312 at LC_X39_Y9_N2
--operation mode is normal

M1L01 = S01_safe_q[3] # S01_safe_q[2] & S01_safe_q[0] # S01_safe_q[1];


--M1L3 is time_auto_and_set:inst1|timeset:b2v_inst3|Decoder~19 at LC_X35_Y7_N4
--operation mode is normal

M1L3 = !M1_disp_drive[0] & M1_disp_drive[1] & !M1_disp_drive[2];


--P1L3 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|LessThan~92 at LC_X36_Y9_N0
--operation mode is normal

P1L3 = S4_safe_q[3] # S4_safe_q[2] & S4_safe_q[1] # S4_safe_q[0];

--P1_EO is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|EO at LC_X36_Y9_N0
--operation mode is normal

P1_EO = DFFEAS(P1L3, GLOBAL(Q1_EO), VCC, , P1L4, , , , );


--P1L4 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|minute_data1[0]~11 at LC_X36_Y9_N3
--operation mode is normal

P1L4 = D1_Timepiece_EN & P1L2;


--J1L7 is alarmclock:inst11|LessThan~132 at LC_X36_Y10_N9
--operation mode is normal

J1L7 = S42_safe_q[3] & S42_safe_q[2] # S42_safe_q[1] # S42_safe_q[0];


--J1L6 is alarmclock:inst11|Decoder~22 at LC_X36_Y10_N8
--operation mode is normal

J1L6 = J1_disp_drive[0] & !J1_disp_drive[1] & J1_disp_drive[2];

--J1_alarmclock_disp_select[0] is alarmclock:inst11|alarmclock_disp_select[0] at LC_X36_Y10_N8
--operation mode is normal

J1_alarmclock_disp_select[0] = DFFEAS(J1L6, GLOBAL(F1_f200hz), VCC, , , , , , );


--M1L7 is time_auto_and_set:inst1|timeset:b2v_inst3|LessThan~128 at LC_X36_Y8_N4
--operation mode is normal

M1L7 = S11_safe_q[3] & S11_safe_q[1] # S11_safe_q[2] # S11_safe_q[0];


--M1L4 is time_auto_and_set:inst1|timeset:b2v_inst3|Decoder~22 at LC_X33_Y7_N6
--operation mode is normal

M1L4 = !M1_disp_drive[1] & M1_disp_drive[0] & M1_disp_drive[2];


--D1_Stopwatch_EN is maincontrol:inst3|Stopwatch_EN at LC_X33_Y8_N9
--operation mode is normal

D1_Stopwatch_EN_lut_out = D1_Function[1] & !D1_Function[0] & !D1_Function[2];
D1_Stopwatch_EN = DFFEAS(D1_Stopwatch_EN_lut_out, GLOBAL(SW3), VCC, , , , , , );


--C1L1 is stopwatch:inst2|F_out~8 at LC_X32_Y5_N9
--operation mode is normal

C1L1 = D1_Stopwatch_EN & F1_f60hz # !D1_Stopwatch_EN & F1_f1hz;


--Q1L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|LessThan~47 at LC_X36_Y8_N6
--operation mode is normal

Q1L2 = S5_safe_q[3] & S5_safe_q[0] # S5_safe_q[1] # S5_safe_q[2];


--J1L11 is alarmclock:inst11|LessThan~291 at LC_X33_Y10_N0
--operation mode is normal

J1L11 = S52_safe_q[3] # S52_safe_q[2] & S52_safe_q[1] # S52_safe_q[0];


--J1L5 is alarmclock:inst11|Decoder~21 at LC_X33_Y10_N3
--operation mode is normal

J1L5 = !J1_disp_drive[1] & !J1_disp_drive[0] & J1_disp_drive[2];

--J1_alarmclock_disp_select[1] is alarmclock:inst11|alarmclock_disp_select[1] at LC_X33_Y10_N3
--operation mode is normal

J1_alarmclock_disp_select[1] = DFFEAS(J1L5, GLOBAL(F1_f200hz), VCC, , , , , , );


--M1L11 is time_auto_and_set:inst1|timeset:b2v_inst3|LessThan~313 at LC_X33_Y9_N9
--operation mode is normal

M1L11 = S21_safe_q[3] # S21_safe_q[2] & S21_safe_q[0] # S21_safe_q[1];


--M1L6 is time_auto_and_set:inst1|timeset:b2v_inst3|Decoder~96 at LC_X33_Y7_N7
--operation mode is normal

M1L6 = !M1_disp_drive[1] & !M1_disp_drive[0] & M1_disp_drive[2];


--Q1L3 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|LessThan~92 at LC_X33_Y9_N8
--operation mode is normal

Q1L3 = S6_safe_q[3] # S6_safe_q[2] & S6_safe_q[0] # S6_safe_q[1];

--Q1_EO is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|EO at LC_X33_Y9_N8
--operation mode is normal

Q1_EO = DFFEAS(Q1L3, GLOBAL(C1L1), VCC, , Q1L4, , , , );


--Q1L4 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|second_data1[0]~11 at LC_X36_Y6_N9
--operation mode is normal

Q1L4 = D1_Timepiece_EN & Q1L2;


--J1L1 is alarmclock:inst11|Decoder~17 at LC_X34_Y10_N9
--operation mode is normal

J1L1 = !J1_disp_drive[0] & !J1_disp_drive[2] & !J1_disp_drive[1];

--J1_alarmclock_disp_select[5] is alarmclock:inst11|alarmclock_disp_select[5] at LC_X34_Y10_N9
--operation mode is normal

J1_alarmclock_disp_select[5] = DFFEAS(J1L1, GLOBAL(F1_f200hz), VCC, , , , , , );


--M1L21 is time_auto_and_set:inst1|timeset:b2v_inst3|LessThan~314 at LC_X34_Y11_N6
--operation mode is normal

M1L21 = S8_safe_q[1] # S8_safe_q[3] # S8_safe_q[2];


--M1L1 is time_auto_and_set:inst1|timeset:b2v_inst3|Decoder~17 at LC_X33_Y7_N9
--operation mode is normal

M1L1 = !M1_disp_drive[1] & !M1_disp_drive[0] & !M1_disp_drive[2];


--N1L4 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|hour_data1[0]~11 at LC_X33_Y13_N7
--operation mode is normal

N1L4 = D1_Timepiece_EN & N1L6;


--D1_Alarmclock_EN is maincontrol:inst3|Alarmclock_EN at LC_X33_Y8_N0
--operation mode is normal

D1_Alarmclock_EN_lut_out = D1_Function[1] & D1_Function[0] & !D1_Function[2];
D1_Alarmclock_EN = DFFEAS(D1_Alarmclock_EN_lut_out, GLOBAL(SW3), VCC, , , , , , );


--H1L23 is disp_data_mux:inst8|Data~1512 at LC_X34_Y8_N4
--operation mode is normal

H1L23 = !J1_alarmclock_disp_select[4] & !J1_alarmclock_disp_select[5];


--H1L16 is disp_data_mux:inst8|always0~1 at LC_X33_Y8_N8
--operation mode is normal

H1L16 = D1_TimeSet_EN # D1_Stopwatch_EN # D1_Timepiece_EN;


--H1L33 is disp_data_mux:inst8|Data~1513 at LC_X34_Y7_N5
--operation mode is normal

H1L33 = !J1_alarmclock_disp_select[1] & D1_Alarmclock_EN & !H1L16 & H1L23;


--H1L43 is disp_data_mux:inst8|Data~1514 at LC_X34_Y7_N0
--operation mode is normal

H1L43 = J1_alarmclock_disp_select[0] & !J1_alarmclock_disp_select[2] & !J1_alarmclock_disp_select[3] & H1L33;


--G1_time_disp_select[5] is time_disp_select:inst6|time_disp_select[5] at LC_X35_Y6_N9
--operation mode is normal

G1_time_disp_select[5]_lut_out = !G1_disp_drive[2] & !G1_disp_drive[0] & !G1_disp_drive[1];
G1_time_disp_select[5] = DFFEAS(G1_time_disp_select[5]_lut_out, GLOBAL(G1_clk), VCC, , , , , , );


--G1_time_disp_select[3] is time_disp_select:inst6|time_disp_select[3] at LC_X35_Y6_N4
--operation mode is normal

G1_time_disp_select[3]_lut_out = !G1_disp_drive[2] & !G1_disp_drive[0] & G1_disp_drive[1];
G1_time_disp_select[3] = DFFEAS(G1_time_disp_select[3]_lut_out, GLOBAL(G1_clk), VCC, , , , , , );


--G1_time_disp_select[2] is time_disp_select:inst6|time_disp_select[2] at LC_X35_Y6_N6
--operation mode is normal

G1_time_disp_select[2]_lut_out = !G1_disp_drive[2] & G1_disp_drive[0] & G1_disp_drive[1];
G1_time_disp_select[2] = DFFEAS(G1_time_disp_select[2]_lut_out, GLOBAL(G1_clk), VCC, , , , , , );


--H1L53 is disp_data_mux:inst8|Data~1515 at LC_X34_Y6_N7
--operation mode is normal

H1L53 = !G1_time_disp_select[3] & H1L16 & !G1_time_disp_select[2] & !G1_time_disp_select[5];


--G1_time_disp_select[0] is time_disp_select:inst6|time_disp_select[0] at LC_X35_Y6_N8
--operation mode is normal

G1_time_disp_select[0]_lut_out = G1_disp_drive[2] & G1_disp_drive[0] & !G1_disp_drive[1];
G1_time_disp_select[0] = DFFEAS(G1_time_disp_select[0]_lut_out, GLOBAL(G1_clk), VCC, , , , , , );


--G1_time_disp_select[4] is time_disp_select:inst6|time_disp_select[4] at LC_X34_Y6_N8
--operation mode is normal

G1_time_disp_select[4]_lut_out = G1_disp_drive[0] & !G1_disp_drive[1] & !G1_disp_drive[2];
G1_time_disp_select[4] = DFFEAS(G1_time_disp_select[4]_lut_out, GLOBAL(G1_clk), VCC, , , , , , );


--H1L63 is disp_data_mux:inst8|Data~1516 at LC_X34_Y6_N5
--operation mode is normal

H1L63 = G1_time_disp_select[0] & !G1_time_disp_select[4];


--G1_time_disp_select[1] is time_disp_select:inst6|time_disp_select[1] at LC_X34_Y6_N0
--operation mode is normal

G1_time_disp_select[1]_lut_out = !G1_disp_drive[0] & !G1_disp_drive[1] & G1_disp_drive[2];
G1_time_disp_select[1] = DFFEAS(G1_time_disp_select[1]_lut_out, GLOBAL(G1_clk), VCC, , , , , , );


--H1L73 is disp_data_mux:inst8|Data~1517 at LC_X34_Y6_N1
--operation mode is normal

H1L73 = H1L43 # H1L53 & H1L63 & !G1_time_disp_select[1];


--H1L83 is disp_data_mux:inst8|Data~1518 at LC_X34_Y6_N6
--operation mode is normal

H1L83 = !G1_time_disp_select[0] & G1_time_disp_select[1] & H1L53 & !G1_time_disp_select[4];


--H1L93 is disp_data_mux:inst8|Data~1519 at LC_X33_Y8_N4
--operation mode is normal

H1L93 = !J1_alarmclock_disp_select[5] & D1_Alarmclock_EN & !J1_alarmclock_disp_select[4] & !H1L16;


--H1L04 is disp_data_mux:inst8|Data~1520 at LC_X34_Y7_N2
--operation mode is normal

H1L04 = !J1_alarmclock_disp_select[2] & !J1_alarmclock_disp_select[3] & !J1_alarmclock_disp_select[0];


--H1L14 is disp_data_mux:inst8|Data~1521 at LC_X34_Y7_N4
--operation mode is normal

H1L14 = H1L83 # H1L04 & H1L93 & J1_alarmclock_disp_select[1];


--H1L41 is disp_data_mux:inst8|Data~386 at LC_X35_Y8_N9
--operation mode is normal

H1L41 = H1L14 # H1L73;


--H1L24 is disp_data_mux:inst8|Data~1522 at LC_X34_Y6_N4
--operation mode is normal

H1L24 = !G1_time_disp_select[0] & !G1_time_disp_select[5] & H1L16 & !G1_time_disp_select[4];


--H1L34 is disp_data_mux:inst8|Data~1523 at LC_X34_Y6_N9
--operation mode is normal

H1L34 = H1L24 & G1_time_disp_select[2] & !G1_time_disp_select[3] & !G1_time_disp_select[1];


--H1L44 is disp_data_mux:inst8|Data~1524 at LC_X34_Y7_N8
--operation mode is normal

H1L44 = !J1_alarmclock_disp_select[0] & J1_alarmclock_disp_select[2] & !J1_alarmclock_disp_select[3] & H1L33;


--H1L54 is disp_data_mux:inst8|Data~1525 at LC_X35_Y5_N2
--operation mode is normal

H1L54 = H1L73 # !H1L14 & H1L44 # H1L34;


--U1_day0[0] is date_main:inst4|datecontrol:b2v_inst1|day0[0] at LC_X35_Y14_N6
--operation mode is normal

U1_day0[0]_lut_out = T1_EO1 & D1_Date_EN & S31_safe_q[0] # !D1_Date_EN & S61_safe_q[0] # !T1_EO1 & S61_safe_q[0];
U1_day0[0] = DFFEAS(U1_day0[0]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--U1_disp_select[4] is date_main:inst4|datecontrol:b2v_inst1|disp_select[4] at LC_X35_Y14_N8
--operation mode is normal

U1_disp_select[4]_lut_out = V1_disp_drive[0] & !V1_disp_drive[1] & !D1_Date_EN # !T1_EO1;
U1_disp_select[4] = DFFEAS(U1_disp_select[4]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--U1_disp_select[2] is date_main:inst4|datecontrol:b2v_inst1|disp_select[2] at LC_X35_Y14_N9
--operation mode is normal

U1_disp_select[2]_lut_out = T1_EO1 & D1_Date_EN # V1_disp_drive[0] & V1_disp_drive[1] # !T1_EO1 & V1_disp_drive[0] & V1_disp_drive[1];
U1_disp_select[2] = DFFEAS(U1_disp_select[2]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--U1_disp_select[5] is date_main:inst4|datecontrol:b2v_inst1|disp_select[5] at LC_X35_Y14_N1
--operation mode is normal

U1_disp_select[5]_lut_out = !V1_disp_drive[0] & !V1_disp_drive[1] & !D1_Date_EN # !T1_EO1;
U1_disp_select[5] = DFFEAS(U1_disp_select[5]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--U1_disp_select[3] is date_main:inst4|datecontrol:b2v_inst1|disp_select[3] at LC_X35_Y14_N0
--operation mode is normal

U1_disp_select[3]_lut_out = !V1_disp_drive[0] & V1_disp_drive[1] & !D1_Date_EN # !T1_EO1;
U1_disp_select[3] = DFFEAS(U1_disp_select[3]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--H1L64 is disp_data_mux:inst8|Data~1526 at LC_X34_Y8_N8
--operation mode is normal

H1L64 = !U1_disp_select[5] & !U1_disp_select[3] & U1_disp_select[4] $ U1_disp_select[2];


--U1_month1[0] is date_main:inst4|datecontrol:b2v_inst1|month1[0] at LC_X35_Y14_N4
--operation mode is normal

U1_month1[0]_lut_out = T1_EO1 & D1_Date_EN & T1_month1[0] # !D1_Date_EN & S91_safe_q[0] # !T1_EO1 & S91_safe_q[0];
U1_month1[0] = DFFEAS(U1_month1[0]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--H1L74 is disp_data_mux:inst8|Data~1527 at LC_X34_Y8_N9
--operation mode is normal

H1L74 = U1_disp_select[4] # U1_disp_select[5] # U1_disp_select[2] $ !U1_disp_select[3];


--U1_day1[0] is date_main:inst4|datecontrol:b2v_inst1|day1[0] at LC_X35_Y14_N7
--operation mode is normal

U1_day1[0]_lut_out = T1_EO1 & D1_Date_EN & S41_safe_q[0] # !D1_Date_EN & S71_safe_q[0] # !T1_EO1 & S71_safe_q[0];
U1_day1[0] = DFFEAS(U1_day1[0]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--H1L61 is disp_data_mux:inst8|Data~403 at LC_X35_Y11_N0
--operation mode is normal

H1L61 = H1L74 & U1_month1[0] # H1L64 # !H1L74 & !H1L64 & U1_day1[0];


--U1_month0[0] is date_main:inst4|datecontrol:b2v_inst1|month0[0] at LC_X35_Y14_N5
--operation mode is normal

U1_month0[0]_lut_out = D1_Date_EN & T1_EO1 & S51_safe_q[0] # !T1_EO1 & S81_safe_q[0] # !D1_Date_EN & S81_safe_q[0];
U1_month0[0] = DFFEAS(U1_month0[0]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--H1L71 is disp_data_mux:inst8|Data~404 at LC_X35_Y11_N7
--operation mode is normal

H1L71 = H1L64 & H1L61 & U1_month0[0] # !H1L61 & U1_day0[0] # !H1L64 & H1L61;


--H1L84 is disp_data_mux:inst8|Data~1528 at LC_X34_Y6_N2
--operation mode is normal

H1L84 = !G1_time_disp_select[0] & H1L16 & !G1_time_disp_select[4];


--H1L94 is disp_data_mux:inst8|Data~1529 at LC_X34_Y9_N0
--operation mode is normal

H1L94 = !G1_time_disp_select[2] & !G1_time_disp_select[1];


--H1L05 is disp_data_mux:inst8|Data~1530 at LC_X34_Y9_N1
--operation mode is normal

H1L05 = H1L84 & G1_time_disp_select[5] & !G1_time_disp_select[3] & H1L94;


--H1L15 is disp_data_mux:inst8|Data~1531 at LC_X34_Y7_N6
--operation mode is normal

H1L15 = !J1_alarmclock_disp_select[1] & !H1L16 & D1_Alarmclock_EN & H1L04;


--H1L25 is disp_data_mux:inst8|Data~1532 at LC_X34_Y9_N2
--operation mode is normal

H1L25 = H1L05 # J1_alarmclock_disp_select[5] & !J1_alarmclock_disp_select[4] & H1L15;


--H1L35 is disp_data_mux:inst8|Data~1533 at LC_X34_Y8_N0
--operation mode is normal

H1L35 = U1_disp_select[4] & !U1_disp_select[5] & !U1_disp_select[2] & !U1_disp_select[3] # !U1_disp_select[4] & U1_disp_select[5] & !U1_disp_select[2] & !U1_disp_select[3] # !U1_disp_select[5] & U1_disp_select[2] $ U1_disp_select[3];


--H1L45 is disp_data_mux:inst8|Data~1534 at LC_X34_Y8_N1
--operation mode is normal

H1L45 = !D1_Alarmclock_EN & !H1L16 & H1L35;


--H1L55 is disp_data_mux:inst8|Data~1535 at LC_X34_Y8_N3
--operation mode is normal

H1L55 = !J1_alarmclock_disp_select[0] & !J1_alarmclock_disp_select[2] & J1_alarmclock_disp_select[3] & H1L33;


--H1L65 is disp_data_mux:inst8|Data~1536 at LC_X34_Y9_N7
--operation mode is normal

H1L65 = H1L55 # H1L24 & G1_time_disp_select[3] & H1L94;


--H1L75 is disp_data_mux:inst8|Data~1537 at LC_X34_Y6_N3
--operation mode is normal

H1L75 = !G1_time_disp_select[0] & !G1_time_disp_select[1] & H1L53 & G1_time_disp_select[4];


--H1L85 is disp_data_mux:inst8|Data~1538 at LC_X34_Y9_N6
--operation mode is normal

H1L85 = H1L75 # !J1_alarmclock_disp_select[5] & J1_alarmclock_disp_select[4] & H1L15;


--H1L95 is disp_data_mux:inst8|Data~1539 at LC_X34_Y9_N9
--operation mode is normal

H1L95 = !H1L85 & !H1L65 & H1L45 # H1L25;


--H1L51 is disp_data_mux:inst8|Data~390 at LC_X35_Y11_N1
--operation mode is normal

H1L51 = H1L65 # H1L85;


--H1L06 is disp_data_mux:inst8|Data~1540 at LC_X34_Y9_N4
--operation mode is normal

H1L06 = H1L65 # !H1L85 & H1L25;


--H1L21 is disp_data_mux:inst8|Data~7adv_mux_opt_ptn_431 at LC_X35_Y11_N8
--operation mode is normal

H1L21 = H1L51 & H1L06 & L1L31 # !H1L06 & L1L1 # !H1L51 & H1L06;


--H1L31 is disp_data_mux:inst8|Data~7adv_mux_opt_ptn_432 at LC_X35_Y11_N6
--operation mode is normal

H1L31 = H1L21 & L1L5 # !H1L95 # !H1L21 & H1L95 & H1L71;


--H1L81 is disp_data_mux:inst8|Data~405 at LC_X35_Y8_N0
--operation mode is normal

H1L81 = H1L41 & H1L54 # !H1L41 & H1L54 & L1L9 # !H1L54 & H1L31;


--H1L91 is disp_data_mux:inst8|Data~406 at LC_X35_Y8_N7
--operation mode is normal

H1L91 = H1L41 & H1L81 & L1L71 # !H1L81 & L1L12 # !H1L41 & H1L81;


--D1_DateSet_EN is maincontrol:inst3|DateSet_EN at LC_X34_Y13_N9
--operation mode is normal

D1_DateSet_EN_lut_out = D1_Function[0] & D1_Function[2] & !D1_Function[1];
D1_DateSet_EN = DFFEAS(D1_DateSet_EN_lut_out, GLOBAL(SW3), VCC, , , , , , );


--D1_Date_EN is maincontrol:inst3|Date_EN at LC_X33_Y8_N2
--operation mode is normal

D1_Date_EN_lut_out = !D1_Function[1] & !D1_Function[0] & D1_Function[2];
D1_Date_EN = DFFEAS(D1_Date_EN_lut_out, GLOBAL(SW3), VCC, , , , , , );


--H1L26 is disp_data_mux:inst8|always0~4 at LC_X33_Y8_N1
--operation mode is normal

H1L26 = H1L16 # D1_Alarmclock_EN # D1_Date_EN # D1_DateSet_EN;


--H1_Data[0] is disp_data_mux:inst8|Data[0] at LC_X35_Y8_N8
--operation mode is normal

H1_Data[0] = H1L26 & H1L91 # !H1L26 & H1_Data[0];


--U1_month1[1] is date_main:inst4|datecontrol:b2v_inst1|month1[1] at LC_X34_Y12_N1
--operation mode is normal

U1_month1[1]_lut_out = S91_safe_q[1] & !D1_Date_EN # !T1_EO1;
U1_month1[1] = DFFEAS(U1_month1[1]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--U1_day0[1] is date_main:inst4|datecontrol:b2v_inst1|day0[1] at LC_X34_Y12_N2
--operation mode is normal

U1_day0[1]_lut_out = T1_EO1 & D1_Date_EN & S31_safe_q[1] # !D1_Date_EN & S61_safe_q[1] # !T1_EO1 & S61_safe_q[1];
U1_day0[1] = DFFEAS(U1_day0[1]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--U1_day1[1] is date_main:inst4|datecontrol:b2v_inst1|day1[1] at LC_X34_Y12_N4
--operation mode is normal

U1_day1[1]_lut_out = T1_EO1 & D1_Date_EN & S41_safe_q[1] # !D1_Date_EN & S71_safe_q[1] # !T1_EO1 & S71_safe_q[1];
U1_day1[1] = DFFEAS(U1_day1[1]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--H1L02 is disp_data_mux:inst8|Data~407 at LC_X35_Y11_N4
--operation mode is normal

H1L02 = H1L74 & H1L64 # !H1L74 & H1L64 & U1_day0[1] # !H1L64 & U1_day1[1];


--U1_month0[1] is date_main:inst4|datecontrol:b2v_inst1|month0[1] at LC_X36_Y14_N4
--operation mode is normal

U1_month0[1]_lut_out = T1_EO1 & D1_Date_EN & S51_safe_q[1] # !D1_Date_EN & S81_safe_q[1] # !T1_EO1 & S81_safe_q[1];
U1_month0[1] = DFFEAS(U1_month0[1]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--H1L12 is disp_data_mux:inst8|Data~408 at LC_X34_Y11_N7
--operation mode is normal

H1L12 = H1L74 & H1L02 & U1_month0[1] # !H1L02 & U1_month1[1] # !H1L74 & H1L02;


--H1L01 is disp_data_mux:inst8|Data~6adv_mux_opt_ptn_435 at LC_X34_Y10_N7
--operation mode is normal

H1L01 = H1L06 & L1L41 # !H1L51 # !H1L06 & L1L2 & H1L51;


--H1L11 is disp_data_mux:inst8|Data~6adv_mux_opt_ptn_436 at LC_X34_Y11_N5
--operation mode is normal

H1L11 = H1L95 & H1L01 & L1L6 # !H1L01 & H1L12 # !H1L95 & H1L01;


--H1L22 is disp_data_mux:inst8|Data~409 at LC_X35_Y8_N6
--operation mode is normal

H1L22 = H1L41 & H1L54 # L1L22 # !H1L41 & H1L11 & !H1L54;


--H1L32 is disp_data_mux:inst8|Data~410 at LC_X35_Y8_N3
--operation mode is normal

H1L32 = H1L22 & L1L81 # !H1L54 # !H1L22 & H1L54 & L1L01;


--H1_Data[1] is disp_data_mux:inst8|Data[1] at LC_X36_Y1_N9
--operation mode is normal

H1_Data[1] = H1L26 & H1L32 # !H1L26 & H1_Data[1];


--U1_day0[2] is date_main:inst4|datecontrol:b2v_inst1|day0[2] at LC_X36_Y14_N9
--operation mode is normal

U1_day0[2]_lut_out = D1_Date_EN & T1_EO1 & S31_safe_q[2] # !T1_EO1 & S61_safe_q[2] # !D1_Date_EN & S61_safe_q[2];
U1_day0[2] = DFFEAS(U1_day0[2]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--U1_month1[2] is date_main:inst4|datecontrol:b2v_inst1|month1[2] at LC_X34_Y12_N3
--operation mode is normal

U1_month1[2]_lut_out = S91_safe_q[2] & !T1_EO1 # !D1_Date_EN;
U1_month1[2] = DFFEAS(U1_month1[2]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--U1_day1[2] is date_main:inst4|datecontrol:b2v_inst1|day1[2] at LC_X36_Y13_N5
--operation mode is normal

U1_day1[2]_lut_out = D1_Date_EN & T1_EO1 & S41_safe_q[2] # !T1_EO1 & S71_safe_q[2] # !D1_Date_EN & S71_safe_q[2];
U1_day1[2] = DFFEAS(U1_day1[2]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--H1L42 is disp_data_mux:inst8|Data~411 at LC_X35_Y11_N9
--operation mode is normal

H1L42 = H1L74 & H1L64 # U1_month1[2] # !H1L74 & !H1L64 & U1_day1[2];


--U1_month0[2] is date_main:inst4|datecontrol:b2v_inst1|month0[2] at LC_X35_Y13_N5
--operation mode is normal

U1_month0[2]_lut_out = D1_Date_EN & T1_EO1 & S51_safe_q[2] # !T1_EO1 & S81_safe_q[2] # !D1_Date_EN & S81_safe_q[2];
U1_month0[2] = DFFEAS(U1_month0[2]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--H1L52 is disp_data_mux:inst8|Data~412 at LC_X35_Y11_N3
--operation mode is normal

H1L52 = H1L64 & H1L42 & U1_month0[2] # !H1L42 & U1_day0[2] # !H1L64 & H1L42;


--H1L8 is disp_data_mux:inst8|Data~5adv_mux_opt_ptn_439 at LC_X35_Y11_N2
--operation mode is normal

H1L8 = H1L06 & L1L51 # !H1L51 # !H1L06 & L1L3 & H1L51;


--H1L9 is disp_data_mux:inst8|Data~5adv_mux_opt_ptn_440 at LC_X35_Y11_N5
--operation mode is normal

H1L9 = H1L95 & H1L8 & L1L7 # !H1L8 & H1L52 # !H1L95 & H1L8;


--H1L62 is disp_data_mux:inst8|Data~413 at LC_X35_Y8_N5
--operation mode is normal

H1L62 = H1L41 & H1L54 # !H1L41 & H1L54 & L1L11 # !H1L54 & H1L9;


--H1L72 is disp_data_mux:inst8|Data~414 at LC_X35_Y8_N4
--operation mode is normal

H1L72 = H1L62 & L1L91 # !H1L41 # !H1L62 & L1L32 & H1L41;


--H1_Data[2] is disp_data_mux:inst8|Data[2] at LC_X36_Y1_N8
--operation mode is normal

H1_Data[2] = H1L26 & H1L72 # !H1L26 & H1_Data[2];


--U1_month1[3] is date_main:inst4|datecontrol:b2v_inst1|month1[3] at LC_X34_Y12_N9
--operation mode is normal

U1_month1[3]_lut_out = S91_safe_q[3] & !D1_Date_EN # !T1_EO1;
U1_month1[3] = DFFEAS(U1_month1[3]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--U1_day0[3] is date_main:inst4|datecontrol:b2v_inst1|day0[3] at LC_X35_Y12_N2
--operation mode is normal

U1_day0[3]_lut_out = T1_EO1 & D1_Date_EN & S31_safe_q[3] # !D1_Date_EN & S61_safe_q[3] # !T1_EO1 & S61_safe_q[3];
U1_day0[3] = DFFEAS(U1_day0[3]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--U1_day1[3] is date_main:inst4|datecontrol:b2v_inst1|day1[3] at LC_X36_Y14_N6
--operation mode is normal

U1_day1[3]_lut_out = T1_EO1 & D1_Date_EN & S41_safe_q[3] # !D1_Date_EN & S71_safe_q[3] # !T1_EO1 & S71_safe_q[3];
U1_day1[3] = DFFEAS(U1_day1[3]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--H1L82 is disp_data_mux:inst8|Data~415 at LC_X34_Y9_N5
--operation mode is normal

H1L82 = H1L64 & U1_day0[3] # H1L74 # !H1L64 & !H1L74 & U1_day1[3];


--U1_month0[3] is date_main:inst4|datecontrol:b2v_inst1|month0[3] at LC_X36_Y14_N5
--operation mode is normal

U1_month0[3]_lut_out = D1_Date_EN & T1_EO1 & S51_safe_q[3] # !T1_EO1 & S81_safe_q[3] # !D1_Date_EN & S81_safe_q[3];
U1_month0[3] = DFFEAS(U1_month0[3]_lut_out, GLOBAL(F1_f200hz), VCC, , U1L81, , , , );


--H1L92 is disp_data_mux:inst8|Data~416 at LC_X34_Y9_N3
--operation mode is normal

H1L92 = H1L82 & U1_month0[3] # !H1L74 # !H1L82 & U1_month1[3] & H1L74;


--H1L6 is disp_data_mux:inst8|Data~4adv_mux_opt_ptn_443 at LC_X33_Y10_N4
--operation mode is normal

H1L6 = H1L51 & H1L06 & L1L61 # !H1L06 & L1L4 # !H1L51 & H1L06;


--H1L7 is disp_data_mux:inst8|Data~4adv_mux_opt_ptn_444 at LC_X34_Y9_N8
--operation mode is normal

H1L7 = H1L6 & L1L8 # !H1L95 # !H1L6 & H1L92 & H1L95;


--H1L03 is disp_data_mux:inst8|Data~417 at LC_X35_Y8_N2
--operation mode is normal

H1L03 = H1L54 & H1L41 # !H1L54 & H1L41 & L1L42 # !H1L41 & H1L7;


--H1L13 is disp_data_mux:inst8|Data~418 at LC_X35_Y8_N1
--operation mode is normal

H1L13 = H1L03 & L1L02 # !H1L54 # !H1L03 & L1L21 & H1L54;


--H1_Data[3] is disp_data_mux:inst8|Data[3] at LC_X36_Y1_N1
--operation mode is normal

H1_Data[3] = H1L26 & H1L13 # !H1L26 & H1_Data[3];


--H1L47 is disp_data_mux:inst8|disp_select~588 at LC_X33_Y8_N6
--operation mode is normal

H1L47 = G1_time_disp_select[5] & D1_TimeSet_EN # D1_Stopwatch_EN # D1_Timepiece_EN;


--H1L57 is disp_data_mux:inst8|disp_select~589 at LC_X33_Y8_N5
--operation mode is normal

H1L57 = !H1L16 & D1_Alarmclock_EN & J1_alarmclock_disp_select[5] # !D1_Alarmclock_EN & U1_disp_select[5];


--H1_disp_select[5] is disp_data_mux:inst8|disp_select[5] at LC_X33_Y8_N3
--operation mode is normal

H1_disp_select[5] = H1L26 & H1L57 # H1L47 # !H1L26 & H1_disp_select[5];


--H1L67 is disp_data_mux:inst8|disp_select~590 at LC_X34_Y5_N8
--operation mode is normal

H1L67 = G1_time_disp_select[4] & D1_Stopwatch_EN # D1_TimeSet_EN # D1_Timepiece_EN;


--H1L77 is disp_data_mux:inst8|disp_select~591 at LC_X34_Y8_N6
--operation mode is normal

H1L77 = !H1L16 & D1_Alarmclock_EN & J1_alarmclock_disp_select[4] # !D1_Alarmclock_EN & U1_disp_select[4];


--H1_disp_select[4] is disp_data_mux:inst8|disp_select[4] at LC_X34_Y5_N9
--operation mode is normal

H1_disp_select[4] = H1L26 & H1L77 # H1L67 # !H1L26 & H1_disp_select[4];


--H1L87 is disp_data_mux:inst8|disp_select~592 at LC_X34_Y5_N0
--operation mode is normal

H1L87 = G1_time_disp_select[3] & D1_Stopwatch_EN # D1_TimeSet_EN # D1_Timepiece_EN;


--H1L97 is disp_data_mux:inst8|disp_select~593 at LC_X34_Y8_N7
--operation mode is normal

H1L97 = !H1L16 & D1_Alarmclock_EN & J1_alarmclock_disp_select[3] # !D1_Alarmclock_EN & U1_disp_select[3];


--H1_disp_select[3] is disp_data_mux:inst8|disp_select[3] at LC_X34_Y5_N1
--operation mode is normal

H1_disp_select[3] = H1L26 & H1L97 # H1L87 # !H1L26 & H1_disp_select[3];


--H1L08 is disp_data_mux:inst8|disp_select~594 at LC_X34_Y5_N4
--operation mode is normal

H1L08 = G1_time_disp_select[2] & D1_Stopwatch_EN # D1_TimeSet_EN # D1_Timepiece_EN;


--H1L18 is disp_data_mux:inst8|disp_select~595 at LC_X34_Y8_N5
--operation mode is normal

H1L18 = !H1L16 & D1_Alarmclock_EN & J1_alarmclock_disp_select[2] # !D1_Alarmclock_EN & U1_disp_select[2];


--H1_disp_select[2] is disp_data_mux:inst8|disp_select[2] at LC_X34_Y5_N5
--operation mode is normal

H1_disp_select[2] = H1L26 & H1L18 # H1L08 # !H1L26 & H1_disp_select[2];


--H1L28 is disp_data_mux:inst8|disp_select~596 at LC_X34_Y7_N9
--operation mode is normal

H1L28 = J1_alarmclock_disp_select[1] & !H1L16 & D1_Alarmclock_EN;


--H1L38 is disp_data_mux:inst8|disp_select~597 at LC_X34_Y5_N6
--operation mode is normal

H1L38 = G1_time_disp_select[1] & D1_Stopwatch_EN # D1_TimeSet_EN # D1_Timepiece_EN;


--H1_disp_select[1] is disp_data_mux:inst8|disp_select[1] at LC_X34_Y5_N7
--operation mode is normal

H1_disp_select[1] = H1L26 & H1L28 # H1L38 # !H1L26 & H1_disp_select[1];


--H1L48 is disp_data_mux:inst8|disp_select~598 at LC_X34_Y8_N2
--operation mode is normal

H1L48 = J1_alarmclock_disp_select[0] & !H1L16 & D1_Alarmclock_EN;


--H1L58 is disp_data_mux:inst8|disp_select~599 at LC_X34_Y5_N2
--operation mode is normal

H1L58 = G1_time_disp_select[0] & D1_Stopwatch_EN # D1_TimeSet_EN # D1_Timepiece_EN;


--H1_disp_select[0] is disp_data_mux:inst8|disp_select[0] at LC_X34_Y5_N3
--operation mode is normal

H1_disp_select[0] = H1L26 & H1L48 # H1L58 # !H1L26 & H1_disp_select[0];


--W2_safe_q[31] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[31] at LC_X31_Y1_N5
--operation mode is normal

W2_safe_q[31]_carry_eqn = W2L68;
W2_safe_q[31]_lut_out = W2_safe_q[31] $ W2_safe_q[31]_carry_eqn;
W2_safe_q[31] = DFFEAS(W2_safe_q[31]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );


--W2_safe_q[1] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[1] at LC_X31_Y4_N5
--operation mode is arithmetic

W2_safe_q[1]_carry_eqn = W2L2;
W2_safe_q[1]_lut_out = W2_safe_q[1] $ W2_safe_q[1]_carry_eqn;
W2_safe_q[1] = DFFEAS(W2_safe_q[1]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L4 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella1~COUT at LC_X31_Y4_N5
--operation mode is arithmetic

W2L4_cout_0 = !W2L2 # !W2_safe_q[1];
W2L4 = CARRY(W2L4_cout_0);

--W2L5 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella1~COUTCOUT1_1 at LC_X31_Y4_N5
--operation mode is arithmetic

W2L5_cout_1 = !W2L2 # !W2_safe_q[1];
W2L5 = CARRY(W2L5_cout_1);


--W2_safe_q[2] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[2] at LC_X31_Y4_N6
--operation mode is arithmetic

W2_safe_q[2]_carry_eqn = (!W2L2 & W2L4) # (W2L2 & W2L5);
W2_safe_q[2]_lut_out = W2_safe_q[2] $ !W2_safe_q[2]_carry_eqn;
W2_safe_q[2] = DFFEAS(W2_safe_q[2]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L7 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella2~COUT at LC_X31_Y4_N6
--operation mode is arithmetic

W2L7_cout_0 = W2_safe_q[2] & !W2L4;
W2L7 = CARRY(W2L7_cout_0);

--W2L8 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X31_Y4_N6
--operation mode is arithmetic

W2L8_cout_1 = W2_safe_q[2] & !W2L5;
W2L8 = CARRY(W2L8_cout_1);


--W2_safe_q[3] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[3] at LC_X31_Y4_N7
--operation mode is arithmetic

W2_safe_q[3]_carry_eqn = (!W2L2 & W2L7) # (W2L2 & W2L8);
W2_safe_q[3]_lut_out = W2_safe_q[3] $ (W2_safe_q[3]_carry_eqn);
W2_safe_q[3] = DFFEAS(W2_safe_q[3]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L01 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella3~COUT at LC_X31_Y4_N7
--operation mode is arithmetic

W2L01_cout_0 = !W2L7 # !W2_safe_q[3];
W2L01 = CARRY(W2L01_cout_0);

--W2L11 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella3~COUTCOUT1_1 at LC_X31_Y4_N7
--operation mode is arithmetic

W2L11_cout_1 = !W2L8 # !W2_safe_q[3];
W2L11 = CARRY(W2L11_cout_1);


--W2_safe_q[4] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[4] at LC_X31_Y4_N8
--operation mode is arithmetic

W2_safe_q[4]_carry_eqn = (!W2L2 & W2L01) # (W2L2 & W2L11);
W2_safe_q[4]_lut_out = W2_safe_q[4] $ (!W2_safe_q[4]_carry_eqn);
W2_safe_q[4] = DFFEAS(W2_safe_q[4]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L31 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella4~COUT at LC_X31_Y4_N8
--operation mode is arithmetic

W2L31_cout_0 = W2_safe_q[4] & !W2L01;
W2L31 = CARRY(W2L31_cout_0);

--W2L41 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella4~COUTCOUT1_1 at LC_X31_Y4_N8
--operation mode is arithmetic

W2L41_cout_1 = W2_safe_q[4] & !W2L11;
W2L41 = CARRY(W2L41_cout_1);


--W2L021 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]~441 at LC_X31_Y4_N2
--operation mode is normal

W2L021 = !W2_safe_q[4] & !W2_safe_q[1] & !W2_safe_q[3] & !W2_safe_q[2];


--W2_safe_q[5] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[5] at LC_X31_Y4_N9
--operation mode is arithmetic

W2_safe_q[5]_carry_eqn = (!W2L2 & W2L31) # (W2L2 & W2L41);
W2_safe_q[5]_lut_out = W2_safe_q[5] $ W2_safe_q[5]_carry_eqn;
W2_safe_q[5] = DFFEAS(W2_safe_q[5]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L61 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella5~COUT at LC_X31_Y4_N9
--operation mode is arithmetic

W2L61 = CARRY(!W2L41 # !W2_safe_q[5]);


--W2_safe_q[6] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[6] at LC_X31_Y3_N0
--operation mode is arithmetic

W2_safe_q[6]_carry_eqn = W2L61;
W2_safe_q[6]_lut_out = W2_safe_q[6] $ !W2_safe_q[6]_carry_eqn;
W2_safe_q[6] = DFFEAS(W2_safe_q[6]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L81 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella6~COUT at LC_X31_Y3_N0
--operation mode is arithmetic

W2L81_cout_0 = W2_safe_q[6] & !W2L61;
W2L81 = CARRY(W2L81_cout_0);

--W2L91 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella6~COUTCOUT1_1 at LC_X31_Y3_N0
--operation mode is arithmetic

W2L91_cout_1 = W2_safe_q[6] & !W2L61;
W2L91 = CARRY(W2L91_cout_1);


--W2_safe_q[7] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[7] at LC_X31_Y3_N1
--operation mode is arithmetic

W2_safe_q[7]_carry_eqn = (!W2L61 & W2L81) # (W2L61 & W2L91);
W2_safe_q[7]_lut_out = W2_safe_q[7] $ W2_safe_q[7]_carry_eqn;
W2_safe_q[7] = DFFEAS(W2_safe_q[7]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L12 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella7~COUT at LC_X31_Y3_N1
--operation mode is arithmetic

W2L12_cout_0 = !W2L81 # !W2_safe_q[7];
W2L12 = CARRY(W2L12_cout_0);

--W2L22 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella7~COUTCOUT1_1 at LC_X31_Y3_N1
--operation mode is arithmetic

W2L22_cout_1 = !W2L91 # !W2_safe_q[7];
W2L22 = CARRY(W2L22_cout_1);


--W2_safe_q[8] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[8] at LC_X31_Y3_N2
--operation mode is arithmetic

W2_safe_q[8]_carry_eqn = (!W2L61 & W2L12) # (W2L61 & W2L22);
W2_safe_q[8]_lut_out = W2_safe_q[8] $ (!W2_safe_q[8]_carry_eqn);
W2_safe_q[8] = DFFEAS(W2_safe_q[8]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L42 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella8~COUT at LC_X31_Y3_N2
--operation mode is arithmetic

W2L42_cout_0 = W2_safe_q[8] & !W2L12;
W2L42 = CARRY(W2L42_cout_0);

--W2L52 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella8~COUTCOUT1_1 at LC_X31_Y3_N2
--operation mode is arithmetic

W2L52_cout_1 = W2_safe_q[8] & !W2L22;
W2L52 = CARRY(W2L52_cout_1);


--W2L121 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]~442 at LC_X31_Y4_N3
--operation mode is normal

W2L121 = !W2_safe_q[6] & !W2_safe_q[5] & !W2_safe_q[7] & !W2_safe_q[8];


--W2_safe_q[9] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[9] at LC_X31_Y3_N3
--operation mode is arithmetic

W2_safe_q[9]_carry_eqn = (!W2L61 & W2L42) # (W2L61 & W2L52);
W2_safe_q[9]_lut_out = W2_safe_q[9] $ (W2_safe_q[9]_carry_eqn);
W2_safe_q[9] = DFFEAS(W2_safe_q[9]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L72 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella9~COUT at LC_X31_Y3_N3
--operation mode is arithmetic

W2L72_cout_0 = !W2L42 # !W2_safe_q[9];
W2L72 = CARRY(W2L72_cout_0);

--W2L82 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella9~COUTCOUT1_1 at LC_X31_Y3_N3
--operation mode is arithmetic

W2L82_cout_1 = !W2L52 # !W2_safe_q[9];
W2L82 = CARRY(W2L82_cout_1);


--W2_safe_q[10] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[10] at LC_X31_Y3_N4
--operation mode is arithmetic

W2_safe_q[10]_carry_eqn = (!W2L61 & W2L72) # (W2L61 & W2L82);
W2_safe_q[10]_lut_out = W2_safe_q[10] $ (!W2_safe_q[10]_carry_eqn);
W2_safe_q[10] = DFFEAS(W2_safe_q[10]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L03 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella10~COUT at LC_X31_Y3_N4
--operation mode is arithmetic

W2L03 = CARRY(W2_safe_q[10] & !W2L82);


--W2_safe_q[11] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[11] at LC_X31_Y3_N5
--operation mode is arithmetic

W2_safe_q[11]_carry_eqn = W2L03;
W2_safe_q[11]_lut_out = W2_safe_q[11] $ W2_safe_q[11]_carry_eqn;
W2_safe_q[11] = DFFEAS(W2_safe_q[11]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L23 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella11~COUT at LC_X31_Y3_N5
--operation mode is arithmetic

W2L23_cout_0 = !W2L03 # !W2_safe_q[11];
W2L23 = CARRY(W2L23_cout_0);

--W2L33 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella11~COUTCOUT1_1 at LC_X31_Y3_N5
--operation mode is arithmetic

W2L33_cout_1 = !W2L03 # !W2_safe_q[11];
W2L33 = CARRY(W2L33_cout_1);


--W2_safe_q[12] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[12] at LC_X31_Y3_N6
--operation mode is arithmetic

W2_safe_q[12]_carry_eqn = (!W2L03 & W2L23) # (W2L03 & W2L33);
W2_safe_q[12]_lut_out = W2_safe_q[12] $ !W2_safe_q[12]_carry_eqn;
W2_safe_q[12] = DFFEAS(W2_safe_q[12]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L53 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella12~COUT at LC_X31_Y3_N6
--operation mode is arithmetic

W2L53_cout_0 = W2_safe_q[12] & !W2L23;
W2L53 = CARRY(W2L53_cout_0);

--W2L63 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella12~COUTCOUT1_1 at LC_X31_Y3_N6
--operation mode is arithmetic

W2L63_cout_1 = W2_safe_q[12] & !W2L33;
W2L63 = CARRY(W2L63_cout_1);


--W2L221 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]~443 at LC_X32_Y1_N2
--operation mode is normal

W2L221 = !W2_safe_q[9] & !W2_safe_q[11] & !W2_safe_q[10] & !W2_safe_q[12];


--W2_safe_q[13] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[13] at LC_X31_Y3_N7
--operation mode is arithmetic

W2_safe_q[13]_carry_eqn = (!W2L03 & W2L53) # (W2L03 & W2L63);
W2_safe_q[13]_lut_out = W2_safe_q[13] $ (W2_safe_q[13]_carry_eqn);
W2_safe_q[13] = DFFEAS(W2_safe_q[13]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L83 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella13~COUT at LC_X31_Y3_N7
--operation mode is arithmetic

W2L83_cout_0 = !W2L53 # !W2_safe_q[13];
W2L83 = CARRY(W2L83_cout_0);

--W2L93 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella13~COUTCOUT1_1 at LC_X31_Y3_N7
--operation mode is arithmetic

W2L93_cout_1 = !W2L63 # !W2_safe_q[13];
W2L93 = CARRY(W2L93_cout_1);


--W2_safe_q[14] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[14] at LC_X31_Y3_N8
--operation mode is arithmetic

W2_safe_q[14]_carry_eqn = (!W2L03 & W2L83) # (W2L03 & W2L93);
W2_safe_q[14]_lut_out = W2_safe_q[14] $ (!W2_safe_q[14]_carry_eqn);
W2_safe_q[14] = DFFEAS(W2_safe_q[14]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L14 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella14~COUT at LC_X31_Y3_N8
--operation mode is arithmetic

W2L14_cout_0 = W2_safe_q[14] & !W2L83;
W2L14 = CARRY(W2L14_cout_0);

--W2L24 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella14~COUTCOUT1_1 at LC_X31_Y3_N8
--operation mode is arithmetic

W2L24_cout_1 = W2_safe_q[14] & !W2L93;
W2L24 = CARRY(W2L24_cout_1);


--W2_safe_q[15] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[15] at LC_X31_Y3_N9
--operation mode is arithmetic

W2_safe_q[15]_carry_eqn = (!W2L03 & W2L14) # (W2L03 & W2L24);
W2_safe_q[15]_lut_out = W2_safe_q[15] $ W2_safe_q[15]_carry_eqn;
W2_safe_q[15] = DFFEAS(W2_safe_q[15]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L44 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella15~COUT at LC_X31_Y3_N9
--operation mode is arithmetic

W2L44 = CARRY(!W2L24 # !W2_safe_q[15]);


--W2_safe_q[16] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[16] at LC_X31_Y2_N0
--operation mode is arithmetic

W2_safe_q[16]_carry_eqn = W2L44;
W2_safe_q[16]_lut_out = W2_safe_q[16] $ !W2_safe_q[16]_carry_eqn;
W2_safe_q[16] = DFFEAS(W2_safe_q[16]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L64 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella16~COUT at LC_X31_Y2_N0
--operation mode is arithmetic

W2L64_cout_0 = W2_safe_q[16] & !W2L44;
W2L64 = CARRY(W2L64_cout_0);

--W2L74 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella16~COUTCOUT1_1 at LC_X31_Y2_N0
--operation mode is arithmetic

W2L74_cout_1 = W2_safe_q[16] & !W2L44;
W2L74 = CARRY(W2L74_cout_1);


--W2L321 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]~444 at LC_X30_Y3_N2
--operation mode is normal

W2L321 = !W2_safe_q[13] & !W2_safe_q[15] & !W2_safe_q[14] & !W2_safe_q[16];


--W2L421 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]~445 at LC_X31_Y1_N6
--operation mode is normal

W2L421 = W2L321 & W2L121 & W2L021 & W2L221;


--W2_safe_q[18] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[18] at LC_X31_Y2_N2
--operation mode is arithmetic

W2_safe_q[18]_carry_eqn = (!W2L44 & W2L94) # (W2L44 & W2L05);
W2_safe_q[18]_lut_out = W2_safe_q[18] $ (!W2_safe_q[18]_carry_eqn);
W2_safe_q[18] = DFFEAS(W2_safe_q[18]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L25 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella18~COUT at LC_X31_Y2_N2
--operation mode is arithmetic

W2L25_cout_0 = W2_safe_q[18] & !W2L94;
W2L25 = CARRY(W2L25_cout_0);

--W2L35 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella18~COUTCOUT1_1 at LC_X31_Y2_N2
--operation mode is arithmetic

W2L35_cout_1 = W2_safe_q[18] & !W2L05;
W2L35 = CARRY(W2L35_cout_1);


--W2_safe_q[19] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[19] at LC_X31_Y2_N3
--operation mode is arithmetic

W2_safe_q[19]_carry_eqn = (!W2L44 & W2L25) # (W2L44 & W2L35);
W2_safe_q[19]_lut_out = W2_safe_q[19] $ (W2_safe_q[19]_carry_eqn);
W2_safe_q[19] = DFFEAS(W2_safe_q[19]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L55 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella19~COUT at LC_X31_Y2_N3
--operation mode is arithmetic

W2L55_cout_0 = !W2L25 # !W2_safe_q[19];
W2L55 = CARRY(W2L55_cout_0);

--W2L65 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella19~COUTCOUT1_1 at LC_X31_Y2_N3
--operation mode is arithmetic

W2L65_cout_1 = !W2L35 # !W2_safe_q[19];
W2L65 = CARRY(W2L65_cout_1);


--W2_safe_q[29] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[29] at LC_X31_Y1_N3
--operation mode is arithmetic

W2_safe_q[29]_carry_eqn = (!W2L27 & W2L08) # (W2L27 & W2L18);
W2_safe_q[29]_lut_out = W2_safe_q[29] $ (W2_safe_q[29]_carry_eqn);
W2_safe_q[29] = DFFEAS(W2_safe_q[29]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L38 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella29~COUT at LC_X31_Y1_N3
--operation mode is arithmetic

W2L38_cout_0 = !W2L08 # !W2_safe_q[29];
W2L38 = CARRY(W2L38_cout_0);

--W2L48 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella29~COUTCOUT1_1 at LC_X31_Y1_N3
--operation mode is arithmetic

W2L48_cout_1 = !W2L18 # !W2_safe_q[29];
W2L48 = CARRY(W2L48_cout_1);


--W2_safe_q[30] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30] at LC_X31_Y1_N4
--operation mode is arithmetic

W2_safe_q[30]_carry_eqn = (!W2L27 & W2L38) # (W2L27 & W2L48);
W2_safe_q[30]_lut_out = W2_safe_q[30] $ (!W2_safe_q[30]_carry_eqn);
W2_safe_q[30] = DFFEAS(W2_safe_q[30]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L68 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella30~COUT at LC_X31_Y1_N4
--operation mode is arithmetic

W2L68 = CARRY(W2_safe_q[30] & !W2L48);


--F1L3 is fdiv:inst5|LessThan~1040 at LC_X30_Y1_N2
--operation mode is normal

F1L3 = W2_safe_q[18] # W2_safe_q[29] # W2_safe_q[30] # W2_safe_q[19];


--W2_safe_q[17] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[17] at LC_X31_Y2_N1
--operation mode is arithmetic

W2_safe_q[17]_carry_eqn = (!W2L44 & W2L64) # (W2L44 & W2L74);
W2_safe_q[17]_lut_out = W2_safe_q[17] $ W2_safe_q[17]_carry_eqn;
W2_safe_q[17] = DFFEAS(W2_safe_q[17]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L94 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella17~COUT at LC_X31_Y2_N1
--operation mode is arithmetic

W2L94_cout_0 = !W2L64 # !W2_safe_q[17];
W2L94 = CARRY(W2L94_cout_0);

--W2L05 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella17~COUTCOUT1_1 at LC_X31_Y2_N1
--operation mode is arithmetic

W2L05_cout_1 = !W2L74 # !W2_safe_q[17];
W2L05 = CARRY(W2L05_cout_1);


--W2_safe_q[21] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[21] at LC_X31_Y2_N5
--operation mode is arithmetic

W2_safe_q[21]_carry_eqn = W2L85;
W2_safe_q[21]_lut_out = W2_safe_q[21] $ W2_safe_q[21]_carry_eqn;
W2_safe_q[21] = DFFEAS(W2_safe_q[21]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L06 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella21~COUT at LC_X31_Y2_N5
--operation mode is arithmetic

W2L06_cout_0 = !W2L85 # !W2_safe_q[21];
W2L06 = CARRY(W2L06_cout_0);

--W2L16 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella21~COUTCOUT1_1 at LC_X31_Y2_N5
--operation mode is arithmetic

W2L16_cout_1 = !W2L85 # !W2_safe_q[21];
W2L16 = CARRY(W2L16_cout_1);


--W2_safe_q[22] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[22] at LC_X31_Y2_N6
--operation mode is arithmetic

W2_safe_q[22]_carry_eqn = (!W2L85 & W2L06) # (W2L85 & W2L16);
W2_safe_q[22]_lut_out = W2_safe_q[22] $ !W2_safe_q[22]_carry_eqn;
W2_safe_q[22] = DFFEAS(W2_safe_q[22]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L36 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella22~COUT at LC_X31_Y2_N6
--operation mode is arithmetic

W2L36_cout_0 = W2_safe_q[22] & !W2L06;
W2L36 = CARRY(W2L36_cout_0);

--W2L46 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella22~COUTCOUT1_1 at LC_X31_Y2_N6
--operation mode is arithmetic

W2L46_cout_1 = W2_safe_q[22] & !W2L16;
W2L46 = CARRY(W2L46_cout_1);


--W2_safe_q[23] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[23] at LC_X31_Y2_N7
--operation mode is arithmetic

W2_safe_q[23]_carry_eqn = (!W2L85 & W2L36) # (W2L85 & W2L46);
W2_safe_q[23]_lut_out = W2_safe_q[23] $ (W2_safe_q[23]_carry_eqn);
W2_safe_q[23] = DFFEAS(W2_safe_q[23]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L66 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella23~COUT at LC_X31_Y2_N7
--operation mode is arithmetic

W2L66_cout_0 = !W2L36 # !W2_safe_q[23];
W2L66 = CARRY(W2L66_cout_0);

--W2L76 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella23~COUTCOUT1_1 at LC_X31_Y2_N7
--operation mode is arithmetic

W2L76_cout_1 = !W2L46 # !W2_safe_q[23];
W2L76 = CARRY(W2L76_cout_1);


--W2_safe_q[24] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[24] at LC_X31_Y2_N8
--operation mode is arithmetic

W2_safe_q[24]_carry_eqn = (!W2L85 & W2L66) # (W2L85 & W2L76);
W2_safe_q[24]_lut_out = W2_safe_q[24] $ (!W2_safe_q[24]_carry_eqn);
W2_safe_q[24] = DFFEAS(W2_safe_q[24]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L96 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella24~COUT at LC_X31_Y2_N8
--operation mode is arithmetic

W2L96_cout_0 = W2_safe_q[24] & !W2L66;
W2L96 = CARRY(W2L96_cout_0);

--W2L07 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella24~COUTCOUT1_1 at LC_X31_Y2_N8
--operation mode is arithmetic

W2L07_cout_1 = W2_safe_q[24] & !W2L76;
W2L07 = CARRY(W2L07_cout_1);


--W2L521 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]~446 at LC_X32_Y2_N2
--operation mode is normal

W2L521 = !W2_safe_q[21] & !W2_safe_q[22] & !W2_safe_q[23] & !W2_safe_q[24];


--W2_safe_q[20] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[20] at LC_X31_Y2_N4
--operation mode is arithmetic

W2_safe_q[20]_carry_eqn = (!W2L44 & W2L55) # (W2L44 & W2L65);
W2_safe_q[20]_lut_out = W2_safe_q[20] $ (!W2_safe_q[20]_carry_eqn);
W2_safe_q[20] = DFFEAS(W2_safe_q[20]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L85 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella20~COUT at LC_X31_Y2_N4
--operation mode is arithmetic

W2L85 = CARRY(W2_safe_q[20] & !W2L65);


--W2_safe_q[25] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[25] at LC_X31_Y2_N9
--operation mode is arithmetic

W2_safe_q[25]_carry_eqn = (!W2L85 & W2L96) # (W2L85 & W2L07);
W2_safe_q[25]_lut_out = W2_safe_q[25] $ W2_safe_q[25]_carry_eqn;
W2_safe_q[25] = DFFEAS(W2_safe_q[25]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L27 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella25~COUT at LC_X31_Y2_N9
--operation mode is arithmetic

W2L27 = CARRY(!W2L07 # !W2_safe_q[25]);


--W2_safe_q[26] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[26] at LC_X31_Y1_N0
--operation mode is arithmetic

W2_safe_q[26]_carry_eqn = W2L27;
W2_safe_q[26]_lut_out = W2_safe_q[26] $ !W2_safe_q[26]_carry_eqn;
W2_safe_q[26] = DFFEAS(W2_safe_q[26]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L47 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella26~COUT at LC_X31_Y1_N0
--operation mode is arithmetic

W2L47_cout_0 = W2_safe_q[26] & !W2L27;
W2L47 = CARRY(W2L47_cout_0);

--W2L57 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella26~COUTCOUT1_1 at LC_X31_Y1_N0
--operation mode is arithmetic

W2L57_cout_1 = W2_safe_q[26] & !W2L27;
W2L57 = CARRY(W2L57_cout_1);


--W2_safe_q[27] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[27] at LC_X31_Y1_N1
--operation mode is arithmetic

W2_safe_q[27]_carry_eqn = (!W2L27 & W2L47) # (W2L27 & W2L57);
W2_safe_q[27]_lut_out = W2_safe_q[27] $ W2_safe_q[27]_carry_eqn;
W2_safe_q[27] = DFFEAS(W2_safe_q[27]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L77 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella27~COUT at LC_X31_Y1_N1
--operation mode is arithmetic

W2L77_cout_0 = !W2L47 # !W2_safe_q[27];
W2L77 = CARRY(W2L77_cout_0);

--W2L87 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella27~COUTCOUT1_1 at LC_X31_Y1_N1
--operation mode is arithmetic

W2L87_cout_1 = !W2L57 # !W2_safe_q[27];
W2L87 = CARRY(W2L87_cout_1);


--W2_safe_q[28] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[28] at LC_X31_Y1_N2
--operation mode is arithmetic

W2_safe_q[28]_carry_eqn = (!W2L27 & W2L77) # (W2L27 & W2L87);
W2_safe_q[28]_lut_out = W2_safe_q[28] $ (!W2_safe_q[28]_carry_eqn);
W2_safe_q[28] = DFFEAS(W2_safe_q[28]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L08 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella28~COUT at LC_X31_Y1_N2
--operation mode is arithmetic

W2L08_cout_0 = W2_safe_q[28] & !W2L77;
W2L08 = CARRY(W2L08_cout_0);

--W2L18 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella28~COUTCOUT1_1 at LC_X31_Y1_N2
--operation mode is arithmetic

W2L18_cout_1 = W2_safe_q[28] & !W2L87;
W2L18 = CARRY(W2L18_cout_1);


--W2L621 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]~447 at LC_X31_Y1_N9
--operation mode is normal

W2L621 = !W2_safe_q[28] & !W2_safe_q[26] & !W2_safe_q[27] & !W2_safe_q[25];


--F1L4 is fdiv:inst5|LessThan~1046 at LC_X31_Y1_N8
--operation mode is normal

F1L4 = W2L621 & !W2_safe_q[17] & !W2_safe_q[20] & W2L521;


--F1L5 is fdiv:inst5|LessThan~1047 at LC_X31_Y1_N7
--operation mode is normal

F1L5 = !W2_safe_q[31] & F1L3 # !W2L421 # !F1L4;

--F1_f60hz is fdiv:inst5|f60hz at LC_X31_Y1_N7
--operation mode is normal

F1_f60hz = DFFEAS(F1L5, GLOBAL(F1_f200hz), VCC, , , , , , );


--W3_safe_q[31] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[31] at LC_X33_Y3_N5
--operation mode is normal

W3_safe_q[31]_carry_eqn = W3L68;
W3_safe_q[31]_lut_out = W3_safe_q[31] $ W3_safe_q[31]_carry_eqn;
W3_safe_q[31] = DFFEAS(W3_safe_q[31]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );


--W3_safe_q[8] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[8] at LC_X33_Y5_N2
--operation mode is arithmetic

W3_safe_q[8]_carry_eqn = (!W3L61 & W3L12) # (W3L61 & W3L22);
W3_safe_q[8]_lut_out = W3_safe_q[8] $ (!W3_safe_q[8]_carry_eqn);
W3_safe_q[8] = DFFEAS(W3_safe_q[8]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L42 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella8~COUT at LC_X33_Y5_N2
--operation mode is arithmetic

W3L42_cout_0 = W3_safe_q[8] & !W3L12;
W3L42 = CARRY(W3L42_cout_0);

--W3L52 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella8~COUTCOUT1_1 at LC_X33_Y5_N2
--operation mode is arithmetic

W3L52_cout_1 = W3_safe_q[8] & !W3L22;
W3L52 = CARRY(W3L52_cout_1);


--W3_safe_q[9] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[9] at LC_X33_Y5_N3
--operation mode is arithmetic

W3_safe_q[9]_carry_eqn = (!W3L61 & W3L42) # (W3L61 & W3L52);
W3_safe_q[9]_lut_out = W3_safe_q[9] $ (W3_safe_q[9]_carry_eqn);
W3_safe_q[9] = DFFEAS(W3_safe_q[9]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L72 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella9~COUT at LC_X33_Y5_N3
--operation mode is arithmetic

W3L72_cout_0 = !W3L42 # !W3_safe_q[9];
W3L72 = CARRY(W3L72_cout_0);

--W3L82 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella9~COUTCOUT1_1 at LC_X33_Y5_N3
--operation mode is arithmetic

W3L82_cout_1 = !W3L52 # !W3_safe_q[9];
W3L82 = CARRY(W3L82_cout_1);


--W3_safe_q[10] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[10] at LC_X33_Y5_N4
--operation mode is arithmetic

W3_safe_q[10]_carry_eqn = (!W3L61 & W3L72) # (W3L61 & W3L82);
W3_safe_q[10]_lut_out = W3_safe_q[10] $ (!W3_safe_q[10]_carry_eqn);
W3_safe_q[10] = DFFEAS(W3_safe_q[10]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L03 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella10~COUT at LC_X33_Y5_N4
--operation mode is arithmetic

W3L03 = CARRY(W3_safe_q[10] & !W3L82);


--W3_safe_q[11] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[11] at LC_X33_Y5_N5
--operation mode is arithmetic

W3_safe_q[11]_carry_eqn = W3L03;
W3_safe_q[11]_lut_out = W3_safe_q[11] $ W3_safe_q[11]_carry_eqn;
W3_safe_q[11] = DFFEAS(W3_safe_q[11]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L23 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella11~COUT at LC_X33_Y5_N5
--operation mode is arithmetic

W3L23_cout_0 = !W3L03 # !W3_safe_q[11];
W3L23 = CARRY(W3L23_cout_0);

--W3L33 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella11~COUTCOUT1_1 at LC_X33_Y5_N5
--operation mode is arithmetic

W3L33_cout_1 = !W3L03 # !W3_safe_q[11];
W3L33 = CARRY(W3L33_cout_1);


--F1L6 is fdiv:inst5|LessThan~1048 at LC_X32_Y5_N2
--operation mode is normal

F1L6 = !W3_safe_q[11] & !W3_safe_q[9] & !W3_safe_q[10] & !W3_safe_q[8];


--W3_safe_q[0] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[0] at LC_X33_Y6_N4
--operation mode is arithmetic

W3_safe_q[0]_lut_out = !W3_safe_q[0];
W3_safe_q[0] = DFFEAS(W3_safe_q[0]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L2 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella0~COUT at LC_X33_Y6_N4
--operation mode is arithmetic

W3L2 = CARRY(W3_safe_q[0]);


--W3_safe_q[1] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[1] at LC_X33_Y6_N5
--operation mode is arithmetic

W3_safe_q[1]_carry_eqn = W3L2;
W3_safe_q[1]_lut_out = W3_safe_q[1] $ W3_safe_q[1]_carry_eqn;
W3_safe_q[1] = DFFEAS(W3_safe_q[1]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L4 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella1~COUT at LC_X33_Y6_N5
--operation mode is arithmetic

W3L4_cout_0 = !W3L2 # !W3_safe_q[1];
W3L4 = CARRY(W3L4_cout_0);

--W3L5 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella1~COUTCOUT1_1 at LC_X33_Y6_N5
--operation mode is arithmetic

W3L5_cout_1 = !W3L2 # !W3_safe_q[1];
W3L5 = CARRY(W3L5_cout_1);


--W3_safe_q[2] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[2] at LC_X33_Y6_N6
--operation mode is arithmetic

W3_safe_q[2]_carry_eqn = (!W3L2 & W3L4) # (W3L2 & W3L5);
W3_safe_q[2]_lut_out = W3_safe_q[2] $ !W3_safe_q[2]_carry_eqn;
W3_safe_q[2] = DFFEAS(W3_safe_q[2]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L7 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella2~COUT at LC_X33_Y6_N6
--operation mode is arithmetic

W3L7_cout_0 = W3_safe_q[2] & !W3L4;
W3L7 = CARRY(W3L7_cout_0);

--W3L8 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X33_Y6_N6
--operation mode is arithmetic

W3L8_cout_1 = W3_safe_q[2] & !W3L5;
W3L8 = CARRY(W3L8_cout_1);


--F1L7 is fdiv:inst5|LessThan~1049 at LC_X33_Y6_N2
--operation mode is normal

F1L7 = !W3_safe_q[2] # !W3_safe_q[1] # !W3_safe_q[0];


--W3_safe_q[3] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[3] at LC_X33_Y6_N7
--operation mode is arithmetic

W3_safe_q[3]_carry_eqn = (!W3L2 & W3L7) # (W3L2 & W3L8);
W3_safe_q[3]_lut_out = W3_safe_q[3] $ (W3_safe_q[3]_carry_eqn);
W3_safe_q[3] = DFFEAS(W3_safe_q[3]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L01 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella3~COUT at LC_X33_Y6_N7
--operation mode is arithmetic

W3L01_cout_0 = !W3L7 # !W3_safe_q[3];
W3L01 = CARRY(W3L01_cout_0);

--W3L11 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella3~COUTCOUT1_1 at LC_X33_Y6_N7
--operation mode is arithmetic

W3L11_cout_1 = !W3L8 # !W3_safe_q[3];
W3L11 = CARRY(W3L11_cout_1);


--W3_safe_q[4] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[4] at LC_X33_Y6_N8
--operation mode is arithmetic

W3_safe_q[4]_carry_eqn = (!W3L2 & W3L01) # (W3L2 & W3L11);
W3_safe_q[4]_lut_out = W3_safe_q[4] $ (!W3_safe_q[4]_carry_eqn);
W3_safe_q[4] = DFFEAS(W3_safe_q[4]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L31 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella4~COUT at LC_X33_Y6_N8
--operation mode is arithmetic

W3L31_cout_0 = W3_safe_q[4] & !W3L01;
W3L31 = CARRY(W3L31_cout_0);

--W3L41 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella4~COUTCOUT1_1 at LC_X33_Y6_N8
--operation mode is arithmetic

W3L41_cout_1 = W3_safe_q[4] & !W3L11;
W3L41 = CARRY(W3L41_cout_1);


--W3_safe_q[5] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[5] at LC_X33_Y6_N9
--operation mode is arithmetic

W3_safe_q[5]_carry_eqn = (!W3L2 & W3L31) # (W3L2 & W3L41);
W3_safe_q[5]_lut_out = W3_safe_q[5] $ W3_safe_q[5]_carry_eqn;
W3_safe_q[5] = DFFEAS(W3_safe_q[5]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L61 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella5~COUT at LC_X33_Y6_N9
--operation mode is arithmetic

W3L61 = CARRY(!W3L41 # !W3_safe_q[5]);


--F1L8 is fdiv:inst5|LessThan~1050 at LC_X32_Y5_N4
--operation mode is normal

F1L8 = !W3_safe_q[5] & !W3_safe_q[4] & !W3_safe_q[3] & F1L7;


--W3_safe_q[6] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[6] at LC_X33_Y5_N0
--operation mode is arithmetic

W3_safe_q[6]_carry_eqn = W3L61;
W3_safe_q[6]_lut_out = W3_safe_q[6] $ !W3_safe_q[6]_carry_eqn;
W3_safe_q[6] = DFFEAS(W3_safe_q[6]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L81 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella6~COUT at LC_X33_Y5_N0
--operation mode is arithmetic

W3L81_cout_0 = W3_safe_q[6] & !W3L61;
W3L81 = CARRY(W3L81_cout_0);

--W3L91 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella6~COUTCOUT1_1 at LC_X33_Y5_N0
--operation mode is arithmetic

W3L91_cout_1 = W3_safe_q[6] & !W3L61;
W3L91 = CARRY(W3L91_cout_1);


--W3_safe_q[7] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[7] at LC_X33_Y5_N1
--operation mode is arithmetic

W3_safe_q[7]_carry_eqn = (!W3L61 & W3L81) # (W3L61 & W3L91);
W3_safe_q[7]_lut_out = W3_safe_q[7] $ W3_safe_q[7]_carry_eqn;
W3_safe_q[7] = DFFEAS(W3_safe_q[7]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L12 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella7~COUT at LC_X33_Y5_N1
--operation mode is arithmetic

W3L12_cout_0 = !W3L81 # !W3_safe_q[7];
W3L12 = CARRY(W3L12_cout_0);

--W3L22 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella7~COUTCOUT1_1 at LC_X33_Y5_N1
--operation mode is arithmetic

W3L22_cout_1 = !W3L91 # !W3_safe_q[7];
W3L22 = CARRY(W3L22_cout_1);


--F1L9 is fdiv:inst5|LessThan~1051 at LC_X32_Y5_N8
--operation mode is normal

F1L9 = F1L6 & F1L8 # !W3_safe_q[6] # !W3_safe_q[7];


--W3_safe_q[12] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[12] at LC_X33_Y5_N6
--operation mode is arithmetic

W3_safe_q[12]_carry_eqn = (!W3L03 & W3L23) # (W3L03 & W3L33);
W3_safe_q[12]_lut_out = W3_safe_q[12] $ !W3_safe_q[12]_carry_eqn;
W3_safe_q[12] = DFFEAS(W3_safe_q[12]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L53 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella12~COUT at LC_X33_Y5_N6
--operation mode is arithmetic

W3L53_cout_0 = W3_safe_q[12] & !W3L23;
W3L53 = CARRY(W3L53_cout_0);

--W3L63 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella12~COUTCOUT1_1 at LC_X33_Y5_N6
--operation mode is arithmetic

W3L63_cout_1 = W3_safe_q[12] & !W3L33;
W3L63 = CARRY(W3L63_cout_1);


--W3_safe_q[13] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[13] at LC_X33_Y5_N7
--operation mode is arithmetic

W3_safe_q[13]_carry_eqn = (!W3L03 & W3L53) # (W3L03 & W3L63);
W3_safe_q[13]_lut_out = W3_safe_q[13] $ (W3_safe_q[13]_carry_eqn);
W3_safe_q[13] = DFFEAS(W3_safe_q[13]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L83 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella13~COUT at LC_X33_Y5_N7
--operation mode is arithmetic

W3L83_cout_0 = !W3L53 # !W3_safe_q[13];
W3L83 = CARRY(W3L83_cout_0);

--W3L93 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella13~COUTCOUT1_1 at LC_X33_Y5_N7
--operation mode is arithmetic

W3L93_cout_1 = !W3L63 # !W3_safe_q[13];
W3L93 = CARRY(W3L93_cout_1);


--W3_safe_q[14] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[14] at LC_X33_Y5_N8
--operation mode is arithmetic

W3_safe_q[14]_carry_eqn = (!W3L03 & W3L83) # (W3L03 & W3L93);
W3_safe_q[14]_lut_out = W3_safe_q[14] $ (!W3_safe_q[14]_carry_eqn);
W3_safe_q[14] = DFFEAS(W3_safe_q[14]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L14 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella14~COUT at LC_X33_Y5_N8
--operation mode is arithmetic

W3L14_cout_0 = W3_safe_q[14] & !W3L83;
W3L14 = CARRY(W3L14_cout_0);

--W3L24 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella14~COUTCOUT1_1 at LC_X33_Y5_N8
--operation mode is arithmetic

W3L24_cout_1 = W3_safe_q[14] & !W3L93;
W3L24 = CARRY(W3L24_cout_1);


--W3_safe_q[15] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[15] at LC_X33_Y5_N9
--operation mode is arithmetic

W3_safe_q[15]_carry_eqn = (!W3L03 & W3L14) # (W3L03 & W3L24);
W3_safe_q[15]_lut_out = W3_safe_q[15] $ W3_safe_q[15]_carry_eqn;
W3_safe_q[15] = DFFEAS(W3_safe_q[15]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L44 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella15~COUT at LC_X33_Y5_N9
--operation mode is arithmetic

W3L44 = CARRY(!W3L24 # !W3_safe_q[15]);


--F1L01 is fdiv:inst5|LessThan~1052 at LC_X31_Y5_N7
--operation mode is normal

F1L01 = !W3_safe_q[12] & !W3_safe_q[14] & !W3_safe_q[13] & !W3_safe_q[15];


--W3_safe_q[16] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[16] at LC_X33_Y4_N0
--operation mode is arithmetic

W3_safe_q[16]_carry_eqn = W3L44;
W3_safe_q[16]_lut_out = W3_safe_q[16] $ !W3_safe_q[16]_carry_eqn;
W3_safe_q[16] = DFFEAS(W3_safe_q[16]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L64 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella16~COUT at LC_X33_Y4_N0
--operation mode is arithmetic

W3L64_cout_0 = W3_safe_q[16] & !W3L44;
W3L64 = CARRY(W3L64_cout_0);

--W3L74 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella16~COUTCOUT1_1 at LC_X33_Y4_N0
--operation mode is arithmetic

W3L74_cout_1 = W3_safe_q[16] & !W3L44;
W3L74 = CARRY(W3L74_cout_1);


--W3_safe_q[17] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[17] at LC_X33_Y4_N1
--operation mode is arithmetic

W3_safe_q[17]_carry_eqn = (!W3L44 & W3L64) # (W3L44 & W3L74);
W3_safe_q[17]_lut_out = W3_safe_q[17] $ W3_safe_q[17]_carry_eqn;
W3_safe_q[17] = DFFEAS(W3_safe_q[17]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L94 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella17~COUT at LC_X33_Y4_N1
--operation mode is arithmetic

W3L94_cout_0 = !W3L64 # !W3_safe_q[17];
W3L94 = CARRY(W3L94_cout_0);

--W3L05 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella17~COUTCOUT1_1 at LC_X33_Y4_N1
--operation mode is arithmetic

W3L05_cout_1 = !W3L74 # !W3_safe_q[17];
W3L05 = CARRY(W3L05_cout_1);


--W3_safe_q[18] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[18] at LC_X33_Y4_N2
--operation mode is arithmetic

W3_safe_q[18]_carry_eqn = (!W3L44 & W3L94) # (W3L44 & W3L05);
W3_safe_q[18]_lut_out = W3_safe_q[18] $ (!W3_safe_q[18]_carry_eqn);
W3_safe_q[18] = DFFEAS(W3_safe_q[18]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L25 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella18~COUT at LC_X33_Y4_N2
--operation mode is arithmetic

W3L25_cout_0 = W3_safe_q[18] & !W3L94;
W3L25 = CARRY(W3L25_cout_0);

--W3L35 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella18~COUTCOUT1_1 at LC_X33_Y4_N2
--operation mode is arithmetic

W3L35_cout_1 = W3_safe_q[18] & !W3L05;
W3L35 = CARRY(W3L35_cout_1);


--W3_safe_q[19] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[19] at LC_X33_Y4_N3
--operation mode is arithmetic

W3_safe_q[19]_carry_eqn = (!W3L44 & W3L25) # (W3L44 & W3L35);
W3_safe_q[19]_lut_out = W3_safe_q[19] $ (W3_safe_q[19]_carry_eqn);
W3_safe_q[19] = DFFEAS(W3_safe_q[19]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L55 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella19~COUT at LC_X33_Y4_N3
--operation mode is arithmetic

W3L55_cout_0 = !W3L25 # !W3_safe_q[19];
W3L55 = CARRY(W3L55_cout_0);

--W3L65 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella19~COUTCOUT1_1 at LC_X33_Y4_N3
--operation mode is arithmetic

W3L65_cout_1 = !W3L35 # !W3_safe_q[19];
W3L65 = CARRY(W3L65_cout_1);


--F1L11 is fdiv:inst5|LessThan~1053 at LC_X32_Y3_N2
--operation mode is normal

F1L11 = !W3_safe_q[16] & !W3_safe_q[17] & !W3_safe_q[18] & !W3_safe_q[19];


--W3_safe_q[20] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[20] at LC_X33_Y4_N4
--operation mode is arithmetic

W3_safe_q[20]_carry_eqn = (!W3L44 & W3L55) # (W3L44 & W3L65);
W3_safe_q[20]_lut_out = W3_safe_q[20] $ (!W3_safe_q[20]_carry_eqn);
W3_safe_q[20] = DFFEAS(W3_safe_q[20]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L85 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella20~COUT at LC_X33_Y4_N4
--operation mode is arithmetic

W3L85 = CARRY(W3_safe_q[20] & !W3L65);


--W3_safe_q[21] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[21] at LC_X33_Y4_N5
--operation mode is arithmetic

W3_safe_q[21]_carry_eqn = W3L85;
W3_safe_q[21]_lut_out = W3_safe_q[21] $ W3_safe_q[21]_carry_eqn;
W3_safe_q[21] = DFFEAS(W3_safe_q[21]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L06 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella21~COUT at LC_X33_Y4_N5
--operation mode is arithmetic

W3L06_cout_0 = !W3L85 # !W3_safe_q[21];
W3L06 = CARRY(W3L06_cout_0);

--W3L16 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella21~COUTCOUT1_1 at LC_X33_Y4_N5
--operation mode is arithmetic

W3L16_cout_1 = !W3L85 # !W3_safe_q[21];
W3L16 = CARRY(W3L16_cout_1);


--W3_safe_q[22] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[22] at LC_X33_Y4_N6
--operation mode is arithmetic

W3_safe_q[22]_carry_eqn = (!W3L85 & W3L06) # (W3L85 & W3L16);
W3_safe_q[22]_lut_out = W3_safe_q[22] $ !W3_safe_q[22]_carry_eqn;
W3_safe_q[22] = DFFEAS(W3_safe_q[22]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L36 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella22~COUT at LC_X33_Y4_N6
--operation mode is arithmetic

W3L36_cout_0 = W3_safe_q[22] & !W3L06;
W3L36 = CARRY(W3L36_cout_0);

--W3L46 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella22~COUTCOUT1_1 at LC_X33_Y4_N6
--operation mode is arithmetic

W3L46_cout_1 = W3_safe_q[22] & !W3L16;
W3L46 = CARRY(W3L46_cout_1);


--W3_safe_q[23] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[23] at LC_X33_Y4_N7
--operation mode is arithmetic

W3_safe_q[23]_carry_eqn = (!W3L85 & W3L36) # (W3L85 & W3L46);
W3_safe_q[23]_lut_out = W3_safe_q[23] $ (W3_safe_q[23]_carry_eqn);
W3_safe_q[23] = DFFEAS(W3_safe_q[23]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L66 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella23~COUT at LC_X33_Y4_N7
--operation mode is arithmetic

W3L66_cout_0 = !W3L36 # !W3_safe_q[23];
W3L66 = CARRY(W3L66_cout_0);

--W3L76 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella23~COUTCOUT1_1 at LC_X33_Y4_N7
--operation mode is arithmetic

W3L76_cout_1 = !W3L46 # !W3_safe_q[23];
W3L76 = CARRY(W3L76_cout_1);


--F1L21 is fdiv:inst5|LessThan~1054 at LC_X32_Y4_N2
--operation mode is normal

F1L21 = !W3_safe_q[23] & !W3_safe_q[22] & !W3_safe_q[20] & !W3_safe_q[21];


--W3_safe_q[24] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[24] at LC_X33_Y4_N8
--operation mode is arithmetic

W3_safe_q[24]_carry_eqn = (!W3L85 & W3L66) # (W3L85 & W3L76);
W3_safe_q[24]_lut_out = W3_safe_q[24] $ (!W3_safe_q[24]_carry_eqn);
W3_safe_q[24] = DFFEAS(W3_safe_q[24]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L96 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella24~COUT at LC_X33_Y4_N8
--operation mode is arithmetic

W3L96_cout_0 = W3_safe_q[24] & !W3L66;
W3L96 = CARRY(W3L96_cout_0);

--W3L07 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella24~COUTCOUT1_1 at LC_X33_Y4_N8
--operation mode is arithmetic

W3L07_cout_1 = W3_safe_q[24] & !W3L76;
W3L07 = CARRY(W3L07_cout_1);


--W3_safe_q[25] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[25] at LC_X33_Y4_N9
--operation mode is arithmetic

W3_safe_q[25]_carry_eqn = (!W3L85 & W3L96) # (W3L85 & W3L07);
W3_safe_q[25]_lut_out = W3_safe_q[25] $ W3_safe_q[25]_carry_eqn;
W3_safe_q[25] = DFFEAS(W3_safe_q[25]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L27 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella25~COUT at LC_X33_Y4_N9
--operation mode is arithmetic

W3L27 = CARRY(!W3L07 # !W3_safe_q[25]);


--W3_safe_q[26] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[26] at LC_X33_Y3_N0
--operation mode is arithmetic

W3_safe_q[26]_carry_eqn = W3L27;
W3_safe_q[26]_lut_out = W3_safe_q[26] $ !W3_safe_q[26]_carry_eqn;
W3_safe_q[26] = DFFEAS(W3_safe_q[26]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L47 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella26~COUT at LC_X33_Y3_N0
--operation mode is arithmetic

W3L47_cout_0 = W3_safe_q[26] & !W3L27;
W3L47 = CARRY(W3L47_cout_0);

--W3L57 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella26~COUTCOUT1_1 at LC_X33_Y3_N0
--operation mode is arithmetic

W3L57_cout_1 = W3_safe_q[26] & !W3L27;
W3L57 = CARRY(W3L57_cout_1);


--W3_safe_q[27] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[27] at LC_X33_Y3_N1
--operation mode is arithmetic

W3_safe_q[27]_carry_eqn = (!W3L27 & W3L47) # (W3L27 & W3L57);
W3_safe_q[27]_lut_out = W3_safe_q[27] $ W3_safe_q[27]_carry_eqn;
W3_safe_q[27] = DFFEAS(W3_safe_q[27]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L77 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella27~COUT at LC_X33_Y3_N1
--operation mode is arithmetic

W3L77_cout_0 = !W3L47 # !W3_safe_q[27];
W3L77 = CARRY(W3L77_cout_0);

--W3L87 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella27~COUTCOUT1_1 at LC_X33_Y3_N1
--operation mode is arithmetic

W3L87_cout_1 = !W3L57 # !W3_safe_q[27];
W3L87 = CARRY(W3L87_cout_1);


--F1L31 is fdiv:inst5|LessThan~1055 at LC_X32_Y5_N5
--operation mode is normal

F1L31 = !W3_safe_q[24] & !W3_safe_q[25] & !W3_safe_q[27] & !W3_safe_q[26];


--F1L41 is fdiv:inst5|LessThan~1056 at LC_X32_Y5_N6
--operation mode is normal

F1L41 = F1L01 & F1L11 & F1L21 & F1L31;


--W3_safe_q[28] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[28] at LC_X33_Y3_N2
--operation mode is arithmetic

W3_safe_q[28]_carry_eqn = (!W3L27 & W3L77) # (W3L27 & W3L87);
W3_safe_q[28]_lut_out = W3_safe_q[28] $ (!W3_safe_q[28]_carry_eqn);
W3_safe_q[28] = DFFEAS(W3_safe_q[28]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L08 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella28~COUT at LC_X33_Y3_N2
--operation mode is arithmetic

W3L08_cout_0 = W3_safe_q[28] & !W3L77;
W3L08 = CARRY(W3L08_cout_0);

--W3L18 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella28~COUTCOUT1_1 at LC_X33_Y3_N2
--operation mode is arithmetic

W3L18_cout_1 = W3_safe_q[28] & !W3L87;
W3L18 = CARRY(W3L18_cout_1);


--W3_safe_q[29] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[29] at LC_X33_Y3_N3
--operation mode is arithmetic

W3_safe_q[29]_carry_eqn = (!W3L27 & W3L08) # (W3L27 & W3L18);
W3_safe_q[29]_lut_out = W3_safe_q[29] $ (W3_safe_q[29]_carry_eqn);
W3_safe_q[29] = DFFEAS(W3_safe_q[29]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L38 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella29~COUT at LC_X33_Y3_N3
--operation mode is arithmetic

W3L38_cout_0 = !W3L08 # !W3_safe_q[29];
W3L38 = CARRY(W3L38_cout_0);

--W3L48 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella29~COUTCOUT1_1 at LC_X33_Y3_N3
--operation mode is arithmetic

W3L48_cout_1 = !W3L18 # !W3_safe_q[29];
W3L48 = CARRY(W3L48_cout_1);


--W3_safe_q[30] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[30] at LC_X33_Y3_N4
--operation mode is arithmetic

W3_safe_q[30]_carry_eqn = (!W3L27 & W3L38) # (W3L27 & W3L48);
W3_safe_q[30]_lut_out = W3_safe_q[30] $ (!W3_safe_q[30]_carry_eqn);
W3_safe_q[30] = DFFEAS(W3_safe_q[30]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L1, );

--W3L68 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella30~COUT at LC_X33_Y3_N4
--operation mode is arithmetic

W3L68 = CARRY(W3_safe_q[30] & !W3L48);


--F1L51 is fdiv:inst5|LessThan~1057 at LC_X33_Y3_N9
--operation mode is normal

F1L51 = !W3_safe_q[28] & !W3_safe_q[29] & !W3_safe_q[30];


--F1L1 is fdiv:inst5|LessThan~518 at LC_X32_Y5_N7
--operation mode is normal

F1L1 = !W3_safe_q[31] & !F1L41 # !F1L51 # !F1L9;

--F1_f1hz is fdiv:inst5|f1hz at LC_X32_Y5_N7
--operation mode is normal

F1_f1hz = DFFEAS(F1L1, GLOBAL(F1_f200hz), VCC, , , , , , );


--S31_safe_q[0] is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|safe_q[0] at LC_X35_Y12_N5
--operation mode is arithmetic

S31_safe_q[0]_lut_out = !S31_safe_q[0];
S31_safe_q[0] = DFFEAS(S31_safe_q[0]_lut_out, GLOBAL(N1_EO), VCC, , T1L51, , , T1L81, );

--S31L2 is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|counter_cella0~COUT at LC_X35_Y12_N5
--operation mode is arithmetic

S31L2_cout_0 = S31_safe_q[0];
S31L2 = CARRY(S31L2_cout_0);

--S31L3 is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X35_Y12_N5
--operation mode is arithmetic

S31L3_cout_1 = S31_safe_q[0];
S31L3 = CARRY(S31L3_cout_1);


--S61_safe_q[0] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|safe_q[0] at LC_X34_Y14_N6
--operation mode is arithmetic

S61_safe_q[0]_lut_out = !S61_safe_q[0];
S61_safe_q[0] = DFFEAS(S61_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , U1L4, , , V1L2, );

--S61L2 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|counter_cella0~COUT at LC_X34_Y14_N6
--operation mode is arithmetic

S61L2_cout_0 = S61_safe_q[0];
S61L2 = CARRY(S61L2_cout_0);

--S61L3 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X34_Y14_N6
--operation mode is arithmetic

S61L3_cout_1 = S61_safe_q[0];
S61L3 = CARRY(S61L3_cout_1);


--T1_EO1 is date_main:inst4|autodate:b2v_inst|EO1 at LC_X35_Y14_N2
--operation mode is normal

T1_EO1_lut_out = !D1_DateSet_EN;
T1_EO1 = DFFEAS(T1_EO1_lut_out, GLOBAL(N1_EO), VCC, , , , , , );


--U1L81 is date_main:inst4|datecontrol:b2v_inst1|disp_select[3]~43 at LC_X35_Y14_N3
--operation mode is normal

U1L81 = D1_DateSet_EN # D1_Date_EN & T1_EO1;


--V1_disp_drive[0] is date_main:inst4|setdate:b2v_inst2|disp_drive[0] at LC_X34_Y14_N4
--operation mode is normal

V1_disp_drive[0]_lut_out = !V1_disp_drive[0];
V1_disp_drive[0] = DFFEAS(V1_disp_drive[0]_lut_out, GLOBAL(SW1), VCC, , D1_DateSet_EN, , , , );


--V1_disp_drive[1] is date_main:inst4|setdate:b2v_inst2|disp_drive[1] at LC_X34_Y14_N1
--operation mode is normal

V1_disp_drive[1]_lut_out = V1_disp_drive[0] $ (V1_disp_drive[1]);
V1_disp_drive[1] = DFFEAS(V1_disp_drive[1]_lut_out, GLOBAL(SW1), VCC, , D1_DateSet_EN, , , , );


--T1_month1[0] is date_main:inst4|autodate:b2v_inst|month1[0] at LC_X34_Y13_N0
--operation mode is normal

T1_month1[0]_lut_out = !T1_month1[0];
T1_month1[0] = DFFEAS(T1_month1[0]_lut_out, GLOBAL(N1_EO), VCC, , T1L03, , , , );


--S91_safe_q[0] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|safe_q[0] at LC_X34_Y12_N5
--operation mode is arithmetic

S91_safe_q[0]_lut_out = !S91_safe_q[0];
S91_safe_q[0] = DFFEAS(S91_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , U1L1, , , V1L3, );

--S91L2 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|counter_cella0~COUT at LC_X34_Y12_N5
--operation mode is arithmetic

S91L2_cout_0 = S91_safe_q[0];
S91L2 = CARRY(S91L2_cout_0);

--S91L3 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X34_Y12_N5
--operation mode is arithmetic

S91L3_cout_1 = S91_safe_q[0];
S91L3 = CARRY(S91L3_cout_1);


--S41_safe_q[0] is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|safe_q[0] at LC_X36_Y13_N0
--operation mode is arithmetic

S41_safe_q[0]_lut_out = !S41_safe_q[0];
S41_safe_q[0] = DFFEAS(S41_safe_q[0]_lut_out, GLOBAL(N1_EO), VCC, , T1L12, , , T1L22, );

--S41L2 is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|counter_cella0~COUT at LC_X36_Y13_N0
--operation mode is arithmetic

S41L2_cout_0 = S41_safe_q[0];
S41L2 = CARRY(S41L2_cout_0);

--S41L3 is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X36_Y13_N0
--operation mode is arithmetic

S41L3_cout_1 = S41_safe_q[0];
S41L3 = CARRY(S41L3_cout_1);


--S71_safe_q[0] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|safe_q[0] at LC_X36_Y14_N0
--operation mode is arithmetic

S71_safe_q[0]_lut_out = !S71_safe_q[0];
S71_safe_q[0] = DFFEAS(S71_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , U1L3, , , V1L4, );

--S71L2 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|counter_cella0~COUT at LC_X36_Y14_N0
--operation mode is arithmetic

S71L2_cout_0 = S71_safe_q[0];
S71L2 = CARRY(S71L2_cout_0);

--S71L3 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X36_Y14_N0
--operation mode is arithmetic

S71L3_cout_1 = S71_safe_q[0];
S71L3 = CARRY(S71L3_cout_1);


--S51_safe_q[0] is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|safe_q[0] at LC_X35_Y13_N0
--operation mode is arithmetic

S51_safe_q[0]_lut_out = !S51_safe_q[0];
S51_safe_q[0] = DFFEAS(S51_safe_q[0]_lut_out, GLOBAL(N1_EO), VCC, , T1L42, , , T1L62, );

--S51L2 is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|counter_cella0~COUT at LC_X35_Y13_N0
--operation mode is arithmetic

S51L2_cout_0 = S51_safe_q[0];
S51L2 = CARRY(S51L2_cout_0);

--S51L3 is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X35_Y13_N0
--operation mode is arithmetic

S51L3_cout_1 = S51_safe_q[0];
S51L3 = CARRY(S51L3_cout_1);


--S81_safe_q[0] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|safe_q[0] at LC_X35_Y15_N1
--operation mode is arithmetic

S81_safe_q[0]_lut_out = !S81_safe_q[0];
S81_safe_q[0] = DFFEAS(S81_safe_q[0]_lut_out, GLOBAL(SW2), VCC, , U1L2, , , V1L1, );

--S81L2 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|counter_cella0~COUT at LC_X35_Y15_N1
--operation mode is arithmetic

S81L2_cout_0 = S81_safe_q[0];
S81L2 = CARRY(S81L2_cout_0);

--S81L3 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X35_Y15_N1
--operation mode is arithmetic

S81L3_cout_1 = S81_safe_q[0];
S81L3 = CARRY(S81L3_cout_1);


--S91_safe_q[1] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|safe_q[1] at LC_X34_Y12_N6
--operation mode is arithmetic

S91_safe_q[1]_lut_out = S91_safe_q[1] $ S91L2;
S91_safe_q[1] = DFFEAS(S91_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , U1L1, , , V1L3, );

--S91L5 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|counter_cella1~COUT at LC_X34_Y12_N6
--operation mode is arithmetic

S91L5_cout_0 = !S91L2 # !S91_safe_q[1];
S91L5 = CARRY(S91L5_cout_0);

--S91L6 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X34_Y12_N6
--operation mode is arithmetic

S91L6_cout_1 = !S91L3 # !S91_safe_q[1];
S91L6 = CARRY(S91L6_cout_1);


--S31_safe_q[1] is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|safe_q[1] at LC_X35_Y12_N6
--operation mode is arithmetic

S31_safe_q[1]_lut_out = S31_safe_q[1] $ S31L2;
S31_safe_q[1] = DFFEAS(S31_safe_q[1]_lut_out, GLOBAL(N1_EO), VCC, , T1L51, , , T1L81, );

--S31L5 is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|counter_cella1~COUT at LC_X35_Y12_N6
--operation mode is arithmetic

S31L5_cout_0 = !S31L2 # !S31_safe_q[1];
S31L5 = CARRY(S31L5_cout_0);

--S31L6 is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X35_Y12_N6
--operation mode is arithmetic

S31L6_cout_1 = !S31L3 # !S31_safe_q[1];
S31L6 = CARRY(S31L6_cout_1);


--S61_safe_q[1] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|safe_q[1] at LC_X34_Y14_N7
--operation mode is arithmetic

S61_safe_q[1]_lut_out = S61_safe_q[1] $ (S61L2);
S61_safe_q[1] = DFFEAS(S61_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , U1L4, , , V1L2, );

--S61L5 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|counter_cella1~COUT at LC_X34_Y14_N7
--operation mode is arithmetic

S61L5_cout_0 = !S61L2 # !S61_safe_q[1];
S61L5 = CARRY(S61L5_cout_0);

--S61L6 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X34_Y14_N7
--operation mode is arithmetic

S61L6_cout_1 = !S61L3 # !S61_safe_q[1];
S61L6 = CARRY(S61L6_cout_1);


--S41_safe_q[1] is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|safe_q[1] at LC_X36_Y13_N1
--operation mode is arithmetic

S41_safe_q[1]_lut_out = S41_safe_q[1] $ S41L2;
S41_safe_q[1] = DFFEAS(S41_safe_q[1]_lut_out, GLOBAL(N1_EO), VCC, , T1L12, , , T1L22, );

--S41L5 is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|counter_cella1~COUT at LC_X36_Y13_N1
--operation mode is arithmetic

S41L5_cout_0 = !S41L2 # !S41_safe_q[1];
S41L5 = CARRY(S41L5_cout_0);

--S41L6 is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X36_Y13_N1
--operation mode is arithmetic

S41L6_cout_1 = !S41L3 # !S41_safe_q[1];
S41L6 = CARRY(S41L6_cout_1);


--S71_safe_q[1] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|safe_q[1] at LC_X36_Y14_N1
--operation mode is arithmetic

S71_safe_q[1]_lut_out = S71_safe_q[1] $ S71L2;
S71_safe_q[1] = DFFEAS(S71_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , U1L3, , , V1L4, );

--S71L5 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|counter_cella1~COUT at LC_X36_Y14_N1
--operation mode is arithmetic

S71L5_cout_0 = !S71L2 # !S71_safe_q[1];
S71L5 = CARRY(S71L5_cout_0);

--S71L6 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X36_Y14_N1
--operation mode is arithmetic

S71L6_cout_1 = !S71L3 # !S71_safe_q[1];
S71L6 = CARRY(S71L6_cout_1);


--S51_safe_q[1] is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|safe_q[1] at LC_X35_Y13_N1
--operation mode is arithmetic

S51_safe_q[1]_lut_out = S51_safe_q[1] $ S51L2;
S51_safe_q[1] = DFFEAS(S51_safe_q[1]_lut_out, GLOBAL(N1_EO), VCC, , T1L42, , , T1L62, );

--S51L5 is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|counter_cella1~COUT at LC_X35_Y13_N1
--operation mode is arithmetic

S51L5_cout_0 = !S51L2 # !S51_safe_q[1];
S51L5 = CARRY(S51L5_cout_0);

--S51L6 is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X35_Y13_N1
--operation mode is arithmetic

S51L6_cout_1 = !S51L3 # !S51_safe_q[1];
S51L6 = CARRY(S51L6_cout_1);


--S81_safe_q[1] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|safe_q[1] at LC_X35_Y15_N2
--operation mode is arithmetic

S81_safe_q[1]_lut_out = S81_safe_q[1] $ (S81L2);
S81_safe_q[1] = DFFEAS(S81_safe_q[1]_lut_out, GLOBAL(SW2), VCC, , U1L2, , , V1L1, );

--S81L5 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|counter_cella1~COUT at LC_X35_Y15_N2
--operation mode is arithmetic

S81L5_cout_0 = !S81L2 # !S81_safe_q[1];
S81L5 = CARRY(S81L5_cout_0);

--S81L6 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|counter_cella1~COUTCOUT1 at LC_X35_Y15_N2
--operation mode is arithmetic

S81L6_cout_1 = !S81L3 # !S81_safe_q[1];
S81L6 = CARRY(S81L6_cout_1);


--S31_safe_q[2] is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|safe_q[2] at LC_X35_Y12_N7
--operation mode is arithmetic

S31_safe_q[2]_lut_out = S31_safe_q[2] $ (!S31L5);
S31_safe_q[2] = DFFEAS(S31_safe_q[2]_lut_out, GLOBAL(N1_EO), VCC, , T1L51, , , T1L81, );

--S31L8 is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|counter_cella2~COUT at LC_X35_Y12_N7
--operation mode is arithmetic

S31L8_cout_0 = S31_safe_q[2] & !S31L5;
S31L8 = CARRY(S31L8_cout_0);

--S31L9 is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X35_Y12_N7
--operation mode is arithmetic

S31L9_cout_1 = S31_safe_q[2] & !S31L6;
S31L9 = CARRY(S31L9_cout_1);


--S61_safe_q[2] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|safe_q[2] at LC_X34_Y14_N8
--operation mode is arithmetic

S61_safe_q[2]_lut_out = S61_safe_q[2] $ (!S61L5);
S61_safe_q[2] = DFFEAS(S61_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , U1L4, , , V1L2, );

--S61L8 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|counter_cella2~COUT at LC_X34_Y14_N8
--operation mode is arithmetic

S61L8_cout_0 = S61_safe_q[2] & !S61L5;
S61L8 = CARRY(S61L8_cout_0);

--S61L9 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X34_Y14_N8
--operation mode is arithmetic

S61L9_cout_1 = S61_safe_q[2] & !S61L6;
S61L9 = CARRY(S61L9_cout_1);


--S91_safe_q[2] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|safe_q[2] at LC_X34_Y12_N7
--operation mode is arithmetic

S91_safe_q[2]_lut_out = S91_safe_q[2] $ (!S91L5);
S91_safe_q[2] = DFFEAS(S91_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , U1L1, , , V1L3, );

--S91L8 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|counter_cella2~COUT at LC_X34_Y12_N7
--operation mode is arithmetic

S91L8_cout_0 = S91_safe_q[2] & !S91L5;
S91L8 = CARRY(S91L8_cout_0);

--S91L9 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X34_Y12_N7
--operation mode is arithmetic

S91L9_cout_1 = S91_safe_q[2] & !S91L6;
S91L9 = CARRY(S91L9_cout_1);


--S41_safe_q[2] is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|safe_q[2] at LC_X36_Y13_N2
--operation mode is arithmetic

S41_safe_q[2]_lut_out = S41_safe_q[2] $ (!S41L5);
S41_safe_q[2] = DFFEAS(S41_safe_q[2]_lut_out, GLOBAL(N1_EO), VCC, , T1L12, , , T1L22, );

--S41L8 is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|counter_cella2~COUT at LC_X36_Y13_N2
--operation mode is arithmetic

S41L8_cout_0 = S41_safe_q[2] & !S41L5;
S41L8 = CARRY(S41L8_cout_0);

--S41L9 is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X36_Y13_N2
--operation mode is arithmetic

S41L9_cout_1 = S41_safe_q[2] & !S41L6;
S41L9 = CARRY(S41L9_cout_1);


--S71_safe_q[2] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|safe_q[2] at LC_X36_Y14_N2
--operation mode is arithmetic

S71_safe_q[2]_lut_out = S71_safe_q[2] $ (!S71L5);
S71_safe_q[2] = DFFEAS(S71_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , U1L3, , , V1L4, );

--S71L8 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|counter_cella2~COUT at LC_X36_Y14_N2
--operation mode is arithmetic

S71L8_cout_0 = S71_safe_q[2] & !S71L5;
S71L8 = CARRY(S71L8_cout_0);

--S71L9 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X36_Y14_N2
--operation mode is arithmetic

S71L9_cout_1 = S71_safe_q[2] & !S71L6;
S71L9 = CARRY(S71L9_cout_1);


--S51_safe_q[2] is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|safe_q[2] at LC_X35_Y13_N2
--operation mode is arithmetic

S51_safe_q[2]_lut_out = S51_safe_q[2] $ (!S51L5);
S51_safe_q[2] = DFFEAS(S51_safe_q[2]_lut_out, GLOBAL(N1_EO), VCC, , T1L42, , , T1L62, );

--S51L8 is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|counter_cella2~COUT at LC_X35_Y13_N2
--operation mode is arithmetic

S51L8_cout_0 = S51_safe_q[2] & !S51L5;
S51L8 = CARRY(S51L8_cout_0);

--S51L9 is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X35_Y13_N2
--operation mode is arithmetic

S51L9_cout_1 = S51_safe_q[2] & !S51L6;
S51L9 = CARRY(S51L9_cout_1);


--S81_safe_q[2] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|safe_q[2] at LC_X35_Y15_N3
--operation mode is arithmetic

S81_safe_q[2]_lut_out = S81_safe_q[2] $ (!S81L5);
S81_safe_q[2] = DFFEAS(S81_safe_q[2]_lut_out, GLOBAL(SW2), VCC, , U1L2, , , V1L1, );

--S81L8 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|counter_cella2~COUT at LC_X35_Y15_N3
--operation mode is arithmetic

S81L8_cout_0 = S81_safe_q[2] & !S81L5;
S81L8 = CARRY(S81L8_cout_0);

--S81L9 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X35_Y15_N3
--operation mode is arithmetic

S81L9_cout_1 = S81_safe_q[2] & !S81L6;
S81L9 = CARRY(S81L9_cout_1);


--S91_safe_q[3] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|safe_q[3] at LC_X34_Y12_N8
--operation mode is normal

S91_safe_q[3]_lut_out = S91L8 $ S91_safe_q[3];
S91_safe_q[3] = DFFEAS(S91_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , U1L1, , , V1L3, );


--S31_safe_q[3] is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|safe_q[3] at LC_X35_Y12_N8
--operation mode is normal

S31_safe_q[3]_lut_out = S31L8 $ S31_safe_q[3];
S31_safe_q[3] = DFFEAS(S31_safe_q[3]_lut_out, GLOBAL(N1_EO), VCC, , T1L51, , , T1L81, );


--S61_safe_q[3] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|safe_q[3] at LC_X34_Y14_N9
--operation mode is normal

S61_safe_q[3]_lut_out = S61L8 $ S61_safe_q[3];
S61_safe_q[3] = DFFEAS(S61_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , U1L4, , , V1L2, );


--S41_safe_q[3] is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|safe_q[3] at LC_X36_Y13_N3
--operation mode is normal

S41_safe_q[3]_lut_out = S41_safe_q[3] $ (S41L8);
S41_safe_q[3] = DFFEAS(S41_safe_q[3]_lut_out, GLOBAL(N1_EO), VCC, , T1L12, , , T1L22, );


--S71_safe_q[3] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|safe_q[3] at LC_X36_Y14_N3
--operation mode is normal

S71_safe_q[3]_lut_out = S71_safe_q[3] $ (S71L8);
S71_safe_q[3] = DFFEAS(S71_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , U1L3, , , V1L4, );


--S51_safe_q[3] is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|safe_q[3] at LC_X35_Y13_N3
--operation mode is normal

S51_safe_q[3]_lut_out = S51_safe_q[3] $ (S51L8);
S51_safe_q[3] = DFFEAS(S51_safe_q[3]_lut_out, GLOBAL(N1_EO), VCC, , T1L42, , , T1L62, );


--S81_safe_q[3] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|safe_q[3] at LC_X35_Y15_N4
--operation mode is normal

S81_safe_q[3]_lut_out = S81L8 $ S81_safe_q[3];
S81_safe_q[3] = DFFEAS(S81_safe_q[3]_lut_out, GLOBAL(SW2), VCC, , U1L2, , , V1L1, );


--W2_safe_q[0] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[0] at LC_X31_Y4_N4
--operation mode is arithmetic

W2_safe_q[0]_lut_out = !W2_safe_q[0];
W2_safe_q[0] = DFFEAS(W2_safe_q[0]_lut_out, GLOBAL(F1_f200hz), VCC, , , , , F1L5, );

--W2L2 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella0~COUT at LC_X31_Y4_N4
--operation mode is arithmetic

W2L2 = CARRY(W2_safe_q[0]);


--W1_safe_q[31] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[31] at LC_X28_Y1_N5
--operation mode is normal

W1_safe_q[31]_carry_eqn = W1L68;
W1_safe_q[31]_lut_out = W1_safe_q[31] $ W1_safe_q[31]_carry_eqn;
W1_safe_q[31] = DFFEAS(W1_safe_q[31]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );


--W1_safe_q[2] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[2] at LC_X28_Y4_N6
--operation mode is arithmetic

W1_safe_q[2]_carry_eqn = (!W1L2 & W1L4) # (W1L2 & W1L5);
W1_safe_q[2]_lut_out = W1_safe_q[2] $ !W1_safe_q[2]_carry_eqn;
W1_safe_q[2] = DFFEAS(W1_safe_q[2]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L7 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella2~COUT at LC_X28_Y4_N6
--operation mode is arithmetic

W1L7_cout_0 = W1_safe_q[2] & !W1L4;
W1L7 = CARRY(W1L7_cout_0);

--W1L8 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X28_Y4_N6
--operation mode is arithmetic

W1L8_cout_1 = W1_safe_q[2] & !W1L5;
W1L8 = CARRY(W1L8_cout_1);


--W1_safe_q[3] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[3] at LC_X28_Y4_N7
--operation mode is arithmetic

W1_safe_q[3]_carry_eqn = (!W1L2 & W1L7) # (W1L2 & W1L8);
W1_safe_q[3]_lut_out = W1_safe_q[3] $ (W1_safe_q[3]_carry_eqn);
W1_safe_q[3] = DFFEAS(W1_safe_q[3]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L01 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella3~COUT at LC_X28_Y4_N7
--operation mode is arithmetic

W1L01_cout_0 = !W1L7 # !W1_safe_q[3];
W1L01 = CARRY(W1L01_cout_0);

--W1L11 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella3~COUTCOUT1_1 at LC_X28_Y4_N7
--operation mode is arithmetic

W1L11_cout_1 = !W1L8 # !W1_safe_q[3];
W1L11 = CARRY(W1L11_cout_1);


--W1_safe_q[4] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[4] at LC_X28_Y4_N8
--operation mode is arithmetic

W1_safe_q[4]_carry_eqn = (!W1L2 & W1L01) # (W1L2 & W1L11);
W1_safe_q[4]_lut_out = W1_safe_q[4] $ (!W1_safe_q[4]_carry_eqn);
W1_safe_q[4] = DFFEAS(W1_safe_q[4]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L31 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella4~COUT at LC_X28_Y4_N8
--operation mode is arithmetic

W1L31_cout_0 = W1_safe_q[4] & !W1L01;
W1L31 = CARRY(W1L31_cout_0);

--W1L41 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella4~COUTCOUT1_1 at LC_X28_Y4_N8
--operation mode is arithmetic

W1L41_cout_1 = W1_safe_q[4] & !W1L11;
W1L41 = CARRY(W1L41_cout_1);


--W1_safe_q[5] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[5] at LC_X28_Y4_N9
--operation mode is arithmetic

W1_safe_q[5]_carry_eqn = (!W1L2 & W1L31) # (W1L2 & W1L41);
W1_safe_q[5]_lut_out = W1_safe_q[5] $ W1_safe_q[5]_carry_eqn;
W1_safe_q[5] = DFFEAS(W1_safe_q[5]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L61 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella5~COUT at LC_X28_Y4_N9
--operation mode is arithmetic

W1L61 = CARRY(!W1L41 # !W1_safe_q[5]);


--W1L021 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~424 at LC_X28_Y4_N2
--operation mode is normal

W1L021 = !W1_safe_q[4] & !W1_safe_q[2] & !W1_safe_q[3] & !W1_safe_q[5];


--W1_safe_q[6] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[6] at LC_X28_Y3_N0
--operation mode is arithmetic

W1_safe_q[6]_carry_eqn = W1L61;
W1_safe_q[6]_lut_out = W1_safe_q[6] $ !W1_safe_q[6]_carry_eqn;
W1_safe_q[6] = DFFEAS(W1_safe_q[6]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L81 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella6~COUT at LC_X28_Y3_N0
--operation mode is arithmetic

W1L81_cout_0 = W1_safe_q[6] & !W1L61;
W1L81 = CARRY(W1L81_cout_0);

--W1L91 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella6~COUTCOUT1_1 at LC_X28_Y3_N0
--operation mode is arithmetic

W1L91_cout_1 = W1_safe_q[6] & !W1L61;
W1L91 = CARRY(W1L91_cout_1);


--W1_safe_q[7] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[7] at LC_X28_Y3_N1
--operation mode is arithmetic

W1_safe_q[7]_carry_eqn = (!W1L61 & W1L81) # (W1L61 & W1L91);
W1_safe_q[7]_lut_out = W1_safe_q[7] $ W1_safe_q[7]_carry_eqn;
W1_safe_q[7] = DFFEAS(W1_safe_q[7]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L12 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella7~COUT at LC_X28_Y3_N1
--operation mode is arithmetic

W1L12_cout_0 = !W1L81 # !W1_safe_q[7];
W1L12 = CARRY(W1L12_cout_0);

--W1L22 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella7~COUTCOUT1_1 at LC_X28_Y3_N1
--operation mode is arithmetic

W1L22_cout_1 = !W1L91 # !W1_safe_q[7];
W1L22 = CARRY(W1L22_cout_1);


--W1_safe_q[8] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[8] at LC_X28_Y3_N2
--operation mode is arithmetic

W1_safe_q[8]_carry_eqn = (!W1L61 & W1L12) # (W1L61 & W1L22);
W1_safe_q[8]_lut_out = W1_safe_q[8] $ (!W1_safe_q[8]_carry_eqn);
W1_safe_q[8] = DFFEAS(W1_safe_q[8]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L42 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella8~COUT at LC_X28_Y3_N2
--operation mode is arithmetic

W1L42_cout_0 = W1_safe_q[8] & !W1L12;
W1L42 = CARRY(W1L42_cout_0);

--W1L52 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella8~COUTCOUT1_1 at LC_X28_Y3_N2
--operation mode is arithmetic

W1L52_cout_1 = W1_safe_q[8] & !W1L22;
W1L52 = CARRY(W1L52_cout_1);


--W1_safe_q[9] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[9] at LC_X28_Y3_N3
--operation mode is arithmetic

W1_safe_q[9]_carry_eqn = (!W1L61 & W1L42) # (W1L61 & W1L52);
W1_safe_q[9]_lut_out = W1_safe_q[9] $ (W1_safe_q[9]_carry_eqn);
W1_safe_q[9] = DFFEAS(W1_safe_q[9]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L72 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella9~COUT at LC_X28_Y3_N3
--operation mode is arithmetic

W1L72_cout_0 = !W1L42 # !W1_safe_q[9];
W1L72 = CARRY(W1L72_cout_0);

--W1L82 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella9~COUTCOUT1_1 at LC_X28_Y3_N3
--operation mode is arithmetic

W1L82_cout_1 = !W1L52 # !W1_safe_q[9];
W1L82 = CARRY(W1L82_cout_1);


--W1L121 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~425 at LC_X27_Y3_N2
--operation mode is normal

W1L121 = !W1_safe_q[7] & !W1_safe_q[8] & !W1_safe_q[6] & !W1_safe_q[9];


--W1_safe_q[10] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[10] at LC_X28_Y3_N4
--operation mode is arithmetic

W1_safe_q[10]_carry_eqn = (!W1L61 & W1L72) # (W1L61 & W1L82);
W1_safe_q[10]_lut_out = W1_safe_q[10] $ (!W1_safe_q[10]_carry_eqn);
W1_safe_q[10] = DFFEAS(W1_safe_q[10]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L03 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella10~COUT at LC_X28_Y3_N4
--operation mode is arithmetic

W1L03 = CARRY(W1_safe_q[10] & !W1L82);


--W1_safe_q[11] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[11] at LC_X28_Y3_N5
--operation mode is arithmetic

W1_safe_q[11]_carry_eqn = W1L03;
W1_safe_q[11]_lut_out = W1_safe_q[11] $ W1_safe_q[11]_carry_eqn;
W1_safe_q[11] = DFFEAS(W1_safe_q[11]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L23 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella11~COUT at LC_X28_Y3_N5
--operation mode is arithmetic

W1L23_cout_0 = !W1L03 # !W1_safe_q[11];
W1L23 = CARRY(W1L23_cout_0);

--W1L33 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella11~COUTCOUT1_1 at LC_X28_Y3_N5
--operation mode is arithmetic

W1L33_cout_1 = !W1L03 # !W1_safe_q[11];
W1L33 = CARRY(W1L33_cout_1);


--W1_safe_q[12] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[12] at LC_X28_Y3_N6
--operation mode is arithmetic

W1_safe_q[12]_carry_eqn = (!W1L03 & W1L23) # (W1L03 & W1L33);
W1_safe_q[12]_lut_out = W1_safe_q[12] $ !W1_safe_q[12]_carry_eqn;
W1_safe_q[12] = DFFEAS(W1_safe_q[12]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L53 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella12~COUT at LC_X28_Y3_N6
--operation mode is arithmetic

W1L53_cout_0 = W1_safe_q[12] & !W1L23;
W1L53 = CARRY(W1L53_cout_0);

--W1L63 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella12~COUTCOUT1_1 at LC_X28_Y3_N6
--operation mode is arithmetic

W1L63_cout_1 = W1_safe_q[12] & !W1L33;
W1L63 = CARRY(W1L63_cout_1);


--W1_safe_q[13] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[13] at LC_X28_Y3_N7
--operation mode is arithmetic

W1_safe_q[13]_carry_eqn = (!W1L03 & W1L53) # (W1L03 & W1L63);
W1_safe_q[13]_lut_out = W1_safe_q[13] $ (W1_safe_q[13]_carry_eqn);
W1_safe_q[13] = DFFEAS(W1_safe_q[13]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L83 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella13~COUT at LC_X28_Y3_N7
--operation mode is arithmetic

W1L83_cout_0 = !W1L53 # !W1_safe_q[13];
W1L83 = CARRY(W1L83_cout_0);

--W1L93 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella13~COUTCOUT1_1 at LC_X28_Y3_N7
--operation mode is arithmetic

W1L93_cout_1 = !W1L63 # !W1_safe_q[13];
W1L93 = CARRY(W1L93_cout_1);


--W1L221 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~426 at LC_X29_Y3_N2
--operation mode is normal

W1L221 = !W1_safe_q[11] & !W1_safe_q[10] & !W1_safe_q[12] & !W1_safe_q[13];


--W1_safe_q[14] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[14] at LC_X28_Y3_N8
--operation mode is arithmetic

W1_safe_q[14]_carry_eqn = (!W1L03 & W1L83) # (W1L03 & W1L93);
W1_safe_q[14]_lut_out = W1_safe_q[14] $ (!W1_safe_q[14]_carry_eqn);
W1_safe_q[14] = DFFEAS(W1_safe_q[14]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L14 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella14~COUT at LC_X28_Y3_N8
--operation mode is arithmetic

W1L14_cout_0 = W1_safe_q[14] & !W1L83;
W1L14 = CARRY(W1L14_cout_0);

--W1L24 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella14~COUTCOUT1_1 at LC_X28_Y3_N8
--operation mode is arithmetic

W1L24_cout_1 = W1_safe_q[14] & !W1L93;
W1L24 = CARRY(W1L24_cout_1);


--W1_safe_q[15] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[15] at LC_X28_Y3_N9
--operation mode is arithmetic

W1_safe_q[15]_carry_eqn = (!W1L03 & W1L14) # (W1L03 & W1L24);
W1_safe_q[15]_lut_out = W1_safe_q[15] $ W1_safe_q[15]_carry_eqn;
W1_safe_q[15] = DFFEAS(W1_safe_q[15]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L44 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella15~COUT at LC_X28_Y3_N9
--operation mode is arithmetic

W1L44 = CARRY(!W1L24 # !W1_safe_q[15]);


--W1_safe_q[16] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[16] at LC_X28_Y2_N0
--operation mode is arithmetic

W1_safe_q[16]_carry_eqn = W1L44;
W1_safe_q[16]_lut_out = W1_safe_q[16] $ !W1_safe_q[16]_carry_eqn;
W1_safe_q[16] = DFFEAS(W1_safe_q[16]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L64 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella16~COUT at LC_X28_Y2_N0
--operation mode is arithmetic

W1L64_cout_0 = W1_safe_q[16] & !W1L44;
W1L64 = CARRY(W1L64_cout_0);

--W1L74 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella16~COUTCOUT1_1 at LC_X28_Y2_N0
--operation mode is arithmetic

W1L74_cout_1 = W1_safe_q[16] & !W1L44;
W1L74 = CARRY(W1L74_cout_1);


--W1_safe_q[17] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[17] at LC_X28_Y2_N1
--operation mode is arithmetic

W1_safe_q[17]_carry_eqn = (!W1L44 & W1L64) # (W1L44 & W1L74);
W1_safe_q[17]_lut_out = W1_safe_q[17] $ W1_safe_q[17]_carry_eqn;
W1_safe_q[17] = DFFEAS(W1_safe_q[17]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L94 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella17~COUT at LC_X28_Y2_N1
--operation mode is arithmetic

W1L94_cout_0 = !W1L64 # !W1_safe_q[17];
W1L94 = CARRY(W1L94_cout_0);

--W1L05 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella17~COUTCOUT1_1 at LC_X28_Y2_N1
--operation mode is arithmetic

W1L05_cout_1 = !W1L74 # !W1_safe_q[17];
W1L05 = CARRY(W1L05_cout_1);


--W1L321 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~427 at LC_X29_Y2_N2
--operation mode is normal

W1L321 = !W1_safe_q[16] & !W1_safe_q[15] & !W1_safe_q[14] & !W1_safe_q[17];


--W1L421 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~428 at LC_X28_Y1_N9
--operation mode is normal

W1L421 = W1L021 & W1L121 & W1L221 & W1L321;


--W1_safe_q[18] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[18] at LC_X28_Y2_N2
--operation mode is arithmetic

W1_safe_q[18]_carry_eqn = (!W1L44 & W1L94) # (W1L44 & W1L05);
W1_safe_q[18]_lut_out = W1_safe_q[18] $ (!W1_safe_q[18]_carry_eqn);
W1_safe_q[18] = DFFEAS(W1_safe_q[18]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L25 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella18~COUT at LC_X28_Y2_N2
--operation mode is arithmetic

W1L25_cout_0 = W1_safe_q[18] & !W1L94;
W1L25 = CARRY(W1L25_cout_0);

--W1L35 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella18~COUTCOUT1_1 at LC_X28_Y2_N2
--operation mode is arithmetic

W1L35_cout_1 = W1_safe_q[18] & !W1L05;
W1L35 = CARRY(W1L35_cout_1);


--W1_safe_q[19] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[19] at LC_X28_Y2_N3
--operation mode is arithmetic

W1_safe_q[19]_carry_eqn = (!W1L44 & W1L25) # (W1L44 & W1L35);
W1_safe_q[19]_lut_out = W1_safe_q[19] $ (W1_safe_q[19]_carry_eqn);
W1_safe_q[19] = DFFEAS(W1_safe_q[19]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L55 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella19~COUT at LC_X28_Y2_N3
--operation mode is arithmetic

W1L55_cout_0 = !W1L25 # !W1_safe_q[19];
W1L55 = CARRY(W1L55_cout_0);

--W1L65 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella19~COUTCOUT1_1 at LC_X28_Y2_N3
--operation mode is arithmetic

W1L65_cout_1 = !W1L35 # !W1_safe_q[19];
W1L65 = CARRY(W1L65_cout_1);


--W1_safe_q[20] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[20] at LC_X28_Y2_N4
--operation mode is arithmetic

W1_safe_q[20]_carry_eqn = (!W1L44 & W1L55) # (W1L44 & W1L65);
W1_safe_q[20]_lut_out = W1_safe_q[20] $ (!W1_safe_q[20]_carry_eqn);
W1_safe_q[20] = DFFEAS(W1_safe_q[20]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L85 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella20~COUT at LC_X28_Y2_N4
--operation mode is arithmetic

W1L85 = CARRY(W1_safe_q[20] & !W1L65);


--W1_safe_q[21] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[21] at LC_X28_Y2_N5
--operation mode is arithmetic

W1_safe_q[21]_carry_eqn = W1L85;
W1_safe_q[21]_lut_out = W1_safe_q[21] $ W1_safe_q[21]_carry_eqn;
W1_safe_q[21] = DFFEAS(W1_safe_q[21]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L06 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella21~COUT at LC_X28_Y2_N5
--operation mode is arithmetic

W1L06_cout_0 = !W1L85 # !W1_safe_q[21];
W1L06 = CARRY(W1L06_cout_0);

--W1L16 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella21~COUTCOUT1_1 at LC_X28_Y2_N5
--operation mode is arithmetic

W1L16_cout_1 = !W1L85 # !W1_safe_q[21];
W1L16 = CARRY(W1L16_cout_1);


--W1L521 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~429 at LC_X27_Y1_N2
--operation mode is normal

W1L521 = !W1_safe_q[20] & !W1_safe_q[19] & !W1_safe_q[18] & !W1_safe_q[21];


--W1_safe_q[22] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[22] at LC_X28_Y2_N6
--operation mode is arithmetic

W1_safe_q[22]_carry_eqn = (!W1L85 & W1L06) # (W1L85 & W1L16);
W1_safe_q[22]_lut_out = W1_safe_q[22] $ !W1_safe_q[22]_carry_eqn;
W1_safe_q[22] = DFFEAS(W1_safe_q[22]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L36 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella22~COUT at LC_X28_Y2_N6
--operation mode is arithmetic

W1L36_cout_0 = W1_safe_q[22] & !W1L06;
W1L36 = CARRY(W1L36_cout_0);

--W1L46 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella22~COUTCOUT1_1 at LC_X28_Y2_N6
--operation mode is arithmetic

W1L46_cout_1 = W1_safe_q[22] & !W1L16;
W1L46 = CARRY(W1L46_cout_1);


--W1_safe_q[23] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[23] at LC_X28_Y2_N7
--operation mode is arithmetic

W1_safe_q[23]_carry_eqn = (!W1L85 & W1L36) # (W1L85 & W1L46);
W1_safe_q[23]_lut_out = W1_safe_q[23] $ (W1_safe_q[23]_carry_eqn);
W1_safe_q[23] = DFFEAS(W1_safe_q[23]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L66 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella23~COUT at LC_X28_Y2_N7
--operation mode is arithmetic

W1L66_cout_0 = !W1L36 # !W1_safe_q[23];
W1L66 = CARRY(W1L66_cout_0);

--W1L76 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella23~COUTCOUT1_1 at LC_X28_Y2_N7
--operation mode is arithmetic

W1L76_cout_1 = !W1L46 # !W1_safe_q[23];
W1L76 = CARRY(W1L76_cout_1);


--W1_safe_q[24] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[24] at LC_X28_Y2_N8
--operation mode is arithmetic

W1_safe_q[24]_carry_eqn = (!W1L85 & W1L66) # (W1L85 & W1L76);
W1_safe_q[24]_lut_out = W1_safe_q[24] $ (!W1_safe_q[24]_carry_eqn);
W1_safe_q[24] = DFFEAS(W1_safe_q[24]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L96 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella24~COUT at LC_X28_Y2_N8
--operation mode is arithmetic

W1L96_cout_0 = W1_safe_q[24] & !W1L66;
W1L96 = CARRY(W1L96_cout_0);

--W1L07 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella24~COUTCOUT1_1 at LC_X28_Y2_N8
--operation mode is arithmetic

W1L07_cout_1 = W1_safe_q[24] & !W1L76;
W1L07 = CARRY(W1L07_cout_1);


--W1_safe_q[25] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[25] at LC_X28_Y2_N9
--operation mode is arithmetic

W1_safe_q[25]_carry_eqn = (!W1L85 & W1L96) # (W1L85 & W1L07);
W1_safe_q[25]_lut_out = W1_safe_q[25] $ W1_safe_q[25]_carry_eqn;
W1_safe_q[25] = DFFEAS(W1_safe_q[25]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L27 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella25~COUT at LC_X28_Y2_N9
--operation mode is arithmetic

W1L27 = CARRY(!W1L07 # !W1_safe_q[25]);


--W1L621 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~430 at LC_X29_Y1_N2
--operation mode is normal

W1L621 = !W1_safe_q[22] & !W1_safe_q[25] & !W1_safe_q[23] & !W1_safe_q[24];


--W1_safe_q[26] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[26] at LC_X28_Y1_N0
--operation mode is arithmetic

W1_safe_q[26]_carry_eqn = W1L27;
W1_safe_q[26]_lut_out = W1_safe_q[26] $ !W1_safe_q[26]_carry_eqn;
W1_safe_q[26] = DFFEAS(W1_safe_q[26]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L47 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella26~COUT at LC_X28_Y1_N0
--operation mode is arithmetic

W1L47_cout_0 = W1_safe_q[26] & !W1L27;
W1L47 = CARRY(W1L47_cout_0);

--W1L57 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella26~COUTCOUT1_1 at LC_X28_Y1_N0
--operation mode is arithmetic

W1L57_cout_1 = W1_safe_q[26] & !W1L27;
W1L57 = CARRY(W1L57_cout_1);


--W1_safe_q[27] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[27] at LC_X28_Y1_N1
--operation mode is arithmetic

W1_safe_q[27]_carry_eqn = (!W1L27 & W1L47) # (W1L27 & W1L57);
W1_safe_q[27]_lut_out = W1_safe_q[27] $ W1_safe_q[27]_carry_eqn;
W1_safe_q[27] = DFFEAS(W1_safe_q[27]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L77 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella27~COUT at LC_X28_Y1_N1
--operation mode is arithmetic

W1L77_cout_0 = !W1L47 # !W1_safe_q[27];
W1L77 = CARRY(W1L77_cout_0);

--W1L87 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella27~COUTCOUT1_1 at LC_X28_Y1_N1
--operation mode is arithmetic

W1L87_cout_1 = !W1L57 # !W1_safe_q[27];
W1L87 = CARRY(W1L87_cout_1);


--W1_safe_q[28] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[28] at LC_X28_Y1_N2
--operation mode is arithmetic

W1_safe_q[28]_carry_eqn = (!W1L27 & W1L77) # (W1L27 & W1L87);
W1_safe_q[28]_lut_out = W1_safe_q[28] $ (!W1_safe_q[28]_carry_eqn);
W1_safe_q[28] = DFFEAS(W1_safe_q[28]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L08 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella28~COUT at LC_X28_Y1_N2
--operation mode is arithmetic

W1L08_cout_0 = W1_safe_q[28] & !W1L77;
W1L08 = CARRY(W1L08_cout_0);

--W1L18 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella28~COUTCOUT1_1 at LC_X28_Y1_N2
--operation mode is arithmetic

W1L18_cout_1 = W1_safe_q[28] & !W1L87;
W1L18 = CARRY(W1L18_cout_1);


--W1_safe_q[29] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[29] at LC_X28_Y1_N3
--operation mode is arithmetic

W1_safe_q[29]_carry_eqn = (!W1L27 & W1L08) # (W1L27 & W1L18);
W1_safe_q[29]_lut_out = W1_safe_q[29] $ (W1_safe_q[29]_carry_eqn);
W1_safe_q[29] = DFFEAS(W1_safe_q[29]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L38 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella29~COUT at LC_X28_Y1_N3
--operation mode is arithmetic

W1L38_cout_0 = !W1L08 # !W1_safe_q[29];
W1L38 = CARRY(W1L38_cout_0);

--W1L48 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella29~COUTCOUT1_1 at LC_X28_Y1_N3
--operation mode is arithmetic

W1L48_cout_1 = !W1L18 # !W1_safe_q[29];
W1L48 = CARRY(W1L48_cout_1);


--W1L721 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~431 at LC_X28_Y1_N6
--operation mode is normal

W1L721 = !W1_safe_q[28] & !W1_safe_q[27] & !W1_safe_q[29] & !W1_safe_q[26];


--W1_safe_q[30] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30] at LC_X28_Y1_N4
--operation mode is arithmetic

W1_safe_q[30]_carry_eqn = (!W1L27 & W1L38) # (W1L27 & W1L48);
W1_safe_q[30]_lut_out = W1_safe_q[30] $ (!W1_safe_q[30]_carry_eqn);
W1_safe_q[30] = DFFEAS(W1_safe_q[30]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L68 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella30~COUT at LC_X28_Y1_N4
--operation mode is arithmetic

W1L68 = CARRY(W1_safe_q[30] & !W1L48);


--W1L821 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~432 at LC_X28_Y1_N7
--operation mode is normal

W1L821 = !W1_safe_q[30] & W1L521 & W1L721 & W1L621;


--F1L2 is fdiv:inst5|LessThan~774 at LC_X28_Y1_N8
--operation mode is normal

F1L2 = !W1_safe_q[31] & !W1L821 # !W1L421;

--F1_f200hz is fdiv:inst5|f200hz at LC_X28_Y1_N8
--operation mode is normal

F1_f200hz = DFFEAS(F1L2, GLOBAL(Clock), VCC, , , , , , );


--G1L31 is time_disp_select:inst6|disp_drive~63 at LC_X36_Y6_N2
--operation mode is normal

G1L31 = M1_disp_drive[0] & !D1_Timepiece_EN;


--G1_auto_disp_drive[0] is time_disp_select:inst6|auto_disp_drive[0] at LC_X36_Y5_N5
--operation mode is normal

G1_auto_disp_drive[0]_lut_out = !G1_auto_disp_drive[0] & !G1_auto_disp_drive[1] # !G1_auto_disp_drive[2];
G1_auto_disp_drive[0] = DFFEAS(G1_auto_disp_drive[0]_lut_out, GLOBAL(Clock), VCC, , , , , , );


--G1L41 is time_disp_select:inst6|disp_drive~64 at LC_X36_Y6_N5
--operation mode is normal

G1L41 = G1_auto_disp_drive[0] & D1_Timepiece_EN;


--G1L1 is time_disp_select:inst6|always1~2 at LC_X36_Y6_N0
--operation mode is normal

G1L1 = !D1_TimeSet_EN & !D1_Timepiece_EN;


--G1_disp_drive[0] is time_disp_select:inst6|disp_drive[0] at LC_X35_Y6_N7
--operation mode is normal

G1_disp_drive[0] = G1L1 & G1_disp_drive[0] # !G1L1 & G1L41 # G1L31;


--G1L51 is time_disp_select:inst6|disp_drive~65 at LC_X36_Y6_N4
--operation mode is normal

G1L51 = !D1_Timepiece_EN & M1_disp_drive[2];


--G1_auto_disp_drive[2] is time_disp_select:inst6|auto_disp_drive[2] at LC_X36_Y5_N4
--operation mode is normal

G1_auto_disp_drive[2]_lut_out = G1_auto_disp_drive[2] & !G1_auto_disp_drive[0] & !G1_auto_disp_drive[1] # !G1_auto_disp_drive[2] & G1_auto_disp_drive[0] & G1_auto_disp_drive[1];
G1_auto_disp_drive[2] = DFFEAS(G1_auto_disp_drive[2]_lut_out, GLOBAL(Clock), VCC, , , , , , );


--G1L61 is time_disp_select:inst6|disp_drive~66 at LC_X36_Y6_N3
--operation mode is normal

G1L61 = D1_Timepiece_EN & G1_auto_disp_drive[2];


--G1_disp_drive[2] is time_disp_select:inst6|disp_drive[2] at LC_X35_Y6_N1
--operation mode is normal

G1_disp_drive[2] = G1L1 & G1_disp_drive[2] # !G1L1 & G1L61 # G1L51;


--G1L71 is time_disp_select:inst6|disp_drive~67 at LC_X36_Y6_N8
--operation mode is normal

G1L71 = !D1_Timepiece_EN & M1_disp_drive[1];


--G1_auto_disp_drive[1] is time_disp_select:inst6|auto_disp_drive[1] at LC_X36_Y5_N2
--operation mode is normal

G1_auto_disp_drive[1]_lut_out = !G1_auto_disp_drive[2] & G1_auto_disp_drive[0] $ G1_auto_disp_drive[1];
G1_auto_disp_drive[1] = DFFEAS(G1_auto_disp_drive[1]_lut_out, GLOBAL(Clock), VCC, , , , , , );


--G1L81 is time_disp_select:inst6|disp_drive~68 at LC_X36_Y6_N7
--operation mode is normal

G1L81 = D1_Timepiece_EN & G1_auto_disp_drive[1];


--G1_disp_drive[1] is time_disp_select:inst6|disp_drive[1] at LC_X35_Y6_N0
--operation mode is normal

G1_disp_drive[1] = G1L1 & G1_disp_drive[1] # !G1L1 & G1L71 # G1L81;


--G1L7 is time_disp_select:inst6|clk~21 at LC_X35_Y6_N2
--operation mode is normal

G1L7 = F1_f200hz & !D1_Timepiece_EN;


--G1L8 is time_disp_select:inst6|clk~22 at LC_X35_Y6_N5
--operation mode is normal

G1L8 = D1_Timepiece_EN & Clock;


--G1_clk is time_disp_select:inst6|clk at LC_X35_Y6_N3
--operation mode is normal

G1_clk = G1L1 & G1_clk # !G1L1 & G1L8 # G1L7;


--T1L5 is date_main:inst4|autodate:b2v_inst|always0~575 at LC_X36_Y12_N6
--operation mode is normal

T1L5 = !S41_safe_q[3] & !S41_safe_q[2];


--T1L6 is date_main:inst4|autodate:b2v_inst|always0~576 at LC_X35_Y12_N3
--operation mode is normal

T1L6 = !S31_safe_q[3] & !S31_safe_q[0] & !S31_safe_q[2] & !S31_safe_q[1];


--T1L7 is date_main:inst4|autodate:b2v_inst|always0~577 at LC_X35_Y12_N4
--operation mode is normal

T1L7 = T1L5 & S41_safe_q[1] & S41_safe_q[0] & T1L6;


--T1L8 is date_main:inst4|autodate:b2v_inst|always0~578 at LC_X34_Y13_N3
--operation mode is normal

T1L8 = S51_safe_q[2] # !T1_month1[0] & S51_safe_q[1];


--T1L9 is date_main:inst4|autodate:b2v_inst|always0~579 at LC_X34_Y13_N8
--operation mode is normal

T1L9 = S51_safe_q[0] & T1_month1[0] # S51_safe_q[3] # !S51_safe_q[0] & T1L8 # T1_month1[0] & S51_safe_q[3];


--T1L61 is date_main:inst4|autodate:b2v_inst|day0[2]~462 at LC_X35_Y12_N1
--operation mode is normal

T1L61 = !T1L9 & T1L7;


--T1L01 is date_main:inst4|autodate:b2v_inst|always0~580 at LC_X36_Y12_N8
--operation mode is normal

T1L01 = !S41_safe_q[3] & !S41_safe_q[1] & !S41_safe_q[2];


--T1L11 is date_main:inst4|autodate:b2v_inst|always0~581 at LC_X36_Y12_N5
--operation mode is normal

T1L11 = !S31_safe_q[0] & !S31_safe_q[1] & !S31_safe_q[2];


--T1L2 is date_main:inst4|autodate:b2v_inst|LessThan~216 at LC_X36_Y13_N4
--operation mode is normal

T1L2 = S41_safe_q[3] # S41_safe_q[2] # S41_safe_q[0] & S41_safe_q[1];


--T1L21 is date_main:inst4|autodate:b2v_inst|always0~582 at LC_X36_Y12_N2
--operation mode is normal

T1L21 = T1L01 & T1L11 # !S31_safe_q[3] # !T1L01 & !T1L2 & !S31_safe_q[3];


--T1L31 is date_main:inst4|autodate:b2v_inst|always0~583 at LC_X35_Y13_N8
--operation mode is normal

T1L31 = !S51_safe_q[1] & !S51_safe_q[2] & T1_month1[0] $ S51_safe_q[3];


--T1L13 is date_main:inst4|autodate:b2v_inst|month1[2]~198 at LC_X35_Y13_N6
--operation mode is normal

T1L13 = !S51_safe_q[3] & !T1_month1[0];


--T1L4 is date_main:inst4|autodate:b2v_inst|always0~118 at LC_X35_Y13_N7
--operation mode is normal

T1L4 = S51_safe_q[0] & T1L31 # !S51_safe_q[0] & S51_safe_q[2] & T1L13;


--T1L71 is date_main:inst4|autodate:b2v_inst|day0[2]~463 at LC_X36_Y13_N9
--operation mode is normal

T1L71 = T1L9 & !T1L4;


--T1L41 is date_main:inst4|autodate:b2v_inst|always0~584 at LC_X36_Y12_N9
--operation mode is normal

T1L41 = T1L2 # !T1L11 & S31_safe_q[3];


--T1L81 is date_main:inst4|autodate:b2v_inst|day0[2]~464 at LC_X35_Y12_N0
--operation mode is normal

T1L81 = !T1L61 & T1L71 & !T1L21 # !T1L71 & T1L41;


--T1L3 is date_main:inst4|autodate:b2v_inst|always0~24 at LC_X36_Y12_N7
--operation mode is normal

T1L3 = S51_safe_q[2] # S51_safe_q[0] # !T1L13 # !S51_safe_q[1];


--T1L51 is date_main:inst4|autodate:b2v_inst|day0[0]~adv_mux_opt_ce_267 at LC_X35_Y12_N9
--operation mode is normal

T1L51 = !D1_DateSet_EN & T1L4 # !T1L3 # !T1L9;


--V1L2 is date_main:inst4|setdate:b2v_inst2|LessThan~146 at LC_X34_Y14_N0
--operation mode is normal

V1L2 = S61_safe_q[3] & S61_safe_q[2] # S61_safe_q[0] # S61_safe_q[1];


--U1L4 is date_main:inst4|datecontrol:b2v_inst1|Decoder~17 at LC_X34_Y14_N5
--operation mode is normal

U1L4 = V1_disp_drive[0] & V1_disp_drive[1];


--T1L52 is date_main:inst4|autodate:b2v_inst|month0[3]~522 at LC_X34_Y13_N2
--operation mode is normal

T1L52 = S51_safe_q[1] # S51_safe_q[3] & T1_month1[0] # S51_safe_q[0];


--T1L62 is date_main:inst4|autodate:b2v_inst|month0[3]~523 at LC_X34_Y13_N4
--operation mode is normal

T1L62 = !T1L13 & !T1L71 & T1L52 # S51_safe_q[2];


--T1L92 is date_main:inst4|autodate:b2v_inst|month1[0]~199 at LC_X34_Y13_N1
--operation mode is normal

T1L92 = !D1_DateSet_EN & T1L9 # !T1L7;


--T1L03 is date_main:inst4|autodate:b2v_inst|month1[0]~adv_mux_opt_ce_287 at LC_X34_Y13_N5
--operation mode is normal

T1L03 = T1L62 & T1L92 & T1L2;


--V1L3 is date_main:inst4|setdate:b2v_inst2|LessThan~199 at LC_X34_Y12_N0
--operation mode is normal

V1L3 = S91_safe_q[1] # S91_safe_q[2] # S91_safe_q[3];


--U1L1 is date_main:inst4|datecontrol:b2v_inst1|Decoder~14 at LC_X34_Y14_N2
--operation mode is normal

U1L1 = !V1_disp_drive[0] & !V1_disp_drive[1];


--T1L22 is date_main:inst4|autodate:b2v_inst|day1[1]~703 at LC_X36_Y13_N6
--operation mode is normal

T1L22 = S41_safe_q[1] & T1L71 # S41_safe_q[0] # !T1L5;


--T1L91 is date_main:inst4|autodate:b2v_inst|day1[0]~704 at LC_X36_Y13_N7
--operation mode is normal

T1L91 = T1L9 & !T1L41 & T1L4 # !T1L9 & T1L7 # !T1L41;


--T1L02 is date_main:inst4|autodate:b2v_inst|day1[0]~705 at LC_X36_Y12_N4
--operation mode is normal

T1L02 = T1L3 # T1L21;


--T1L12 is date_main:inst4|autodate:b2v_inst|day1[0]~706 at LC_X36_Y13_N8
--operation mode is normal

T1L12 = !D1_DateSet_EN & !T1L91 & !T1L02 # !T1L71;


--V1L4 is date_main:inst4|setdate:b2v_inst2|LessThan~200 at LC_X36_Y14_N8
--operation mode is normal

V1L4 = S71_safe_q[3] # S71_safe_q[2] # S71_safe_q[0] & S71_safe_q[1];


--U1L3 is date_main:inst4|datecontrol:b2v_inst1|Decoder~16 at LC_X36_Y14_N7
--operation mode is normal

U1L3 = !V1_disp_drive[0] & V1_disp_drive[1];


--T1L32 is date_main:inst4|autodate:b2v_inst|month0[0]~524 at LC_X35_Y13_N9
--operation mode is normal

T1L32 = T1L71 & T1L01 # T1L3 # !T1L92;


--T1L42 is date_main:inst4|autodate:b2v_inst|month0[0]~525 at LC_X35_Y13_N4
--operation mode is normal

T1L42 = !T1L32 & T1L2 # T1L71 & S31_safe_q[3];


--V1L1 is date_main:inst4|setdate:b2v_inst2|LessThan~114 at LC_X35_Y15_N6
--operation mode is normal

V1L1 = S81_safe_q[3] & S81_safe_q[1] # S81_safe_q[0] # S81_safe_q[2];


--U1L2 is date_main:inst4|datecontrol:b2v_inst1|Decoder~15 at LC_X34_Y14_N3
--operation mode is normal

U1L2 = V1_disp_drive[0] & !V1_disp_drive[1];


--W1_safe_q[1] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[1] at LC_X28_Y4_N5
--operation mode is arithmetic

W1_safe_q[1]_carry_eqn = W1L2;
W1_safe_q[1]_lut_out = W1_safe_q[1] $ W1_safe_q[1]_carry_eqn;
W1_safe_q[1] = DFFEAS(W1_safe_q[1]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L4 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella1~COUT at LC_X28_Y4_N5
--operation mode is arithmetic

W1L4_cout_0 = !W1L2 # !W1_safe_q[1];
W1L4 = CARRY(W1L4_cout_0);

--W1L5 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella1~COUTCOUT1_1 at LC_X28_Y4_N5
--operation mode is arithmetic

W1L5_cout_1 = !W1L2 # !W1_safe_q[1];
W1L5 = CARRY(W1L5_cout_1);


--W1_safe_q[0] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[0] at LC_X28_Y4_N4
--operation mode is arithmetic

W1_safe_q[0]_lut_out = !W1_safe_q[0];
W1_safe_q[0] = DFFEAS(W1_safe_q[0]_lut_out, GLOBAL(Clock), VCC, , , , , F1L2, );

--W1L2 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella0~COUT at LC_X28_Y4_N4
--operation mode is arithmetic

W1L2 = CARRY(W1_safe_q[0]);


--SW2 is SW2 at PIN_L2
--operation mode is input

SW2 = INPUT();


--SW3 is SW3 at PIN_M2
--operation mode is input

SW3 = INPUT();


--SW1 is SW1 at PIN_M3
--operation mode is input

SW1 = INPUT();


--Clock is Clock at PIN_L3
--operation mode is input

Clock = INPUT();


--alarm is alarm at PIN_P8
--operation mode is output

alarm = OUTPUT(!J1_alarm);


--disp_data[6] is disp_data[6] at PIN_W9
--operation mode is output

disp_data[6] = OUTPUT(!H1L68);


--disp_data[5] is disp_data[5] at PIN_T8
--operation mode is output

disp_data[5] = OUTPUT(!H1L78);


--disp_data[4] is disp_data[4] at PIN_AA8
--operation mode is output

disp_data[4] = OUTPUT(!H1L88);


--disp_data[3] is disp_data[3] at PIN_U9
--operation mode is output

disp_data[3] = OUTPUT(!H1L66);


--disp_data[2] is disp_data[2] at PIN_Y8
--operation mode is output

disp_data[2] = OUTPUT(!H1L56);


--disp_data[1] is disp_data[1] at PIN_Y9
--operation mode is output

disp_data[1] = OUTPUT(!H1L46);


--disp_data[0] is disp_data[0] at PIN_V9
--operation mode is output

disp_data[0] = OUTPUT(H1L36);


--disp_select[5] is disp_select[5] at PIN_T9
--operation mode is output

disp_select[5] = OUTPUT(H1_disp_select[5]);


--disp_select[4] is disp_select[4] at PIN_T10
--operation mode is output

disp_select[4] = OUTPUT(H1_disp_select[4]);


--disp_select[3] is disp_select[3] at PIN_P10
--operation mode is output

disp_select[3] = OUTPUT(H1_disp_select[3]);


--disp_select[2] is disp_select[2] at PIN_M8
--operation mode is output

disp_select[2] = OUTPUT(H1_disp_select[2]);


--disp_select[1] is disp_select[1] at PIN_N8
--operation mode is output

disp_select[1] = OUTPUT(H1_disp_select[1]);


--disp_select[0] is disp_select[0] at PIN_P9
--operation mode is output

disp_select[0] = OUTPUT(H1_disp_select[0]);



