--A1L53 is always1~187 at LC1
A1L53_p1_out = dp_s10hz & disp_select[1] & !disp_select[2] & disp_select[0];
A1L53_p2_out = !disp_select[1] & disp_select[2] & disp_select[0] & dp_s1hz;
A1L53_p3_out = !disp_select[1] & !disp_select[2] & disp_select[0] & dp_s100hz;
A1L53_or_out = A1L53_p1_out # A1L53_p2_out # A1L53_p3_out;
A1L53 = A1L53_or_out;


--A1L97 is reduce_or~1056 at LC9
A1L97_p1_out = data_in[2] & !data_in[1] & !data_in[3];
A1L97_p2_out = data_in[2] & !data_in[3] & !data_in[0];
A1L97_p3_out = !data_in[2] & data_in[1] & !data_in[3];
A1L97_p4_out = !data_in[2] & !data_in[1] & data_in[3];
A1L97_or_out = A1L97_p1_out # A1L97_p2_out # A1L97_p3_out # A1L97_p4_out;
A1L97 = A1L97_or_out;


--A1L56 is hide~363 at LC34
A1L56_p0_out = !disp_select[1] & !disp_select[0] & !counter_out & !Q5[3] & !Q5[2] & !Q5[1] & !Q5[0] & !dp_s100hz & !Q4[3] & !Q4[2] & !Q4[1] & !Q4[0] & !Q3[3] & !Q3[2] & !Q3[1] & !Q3[0] & !dp_s10hz & !Q2[0] & !Q2[1] & !Q2[2] & !Q2[3] & !Q1[3] & !Q1[2] & !Q1[1] & !Q1[0];
A1L56_p1_out = !disp_select[2] & !disp_select[1] & !disp_select[0] & !counter_out & !Q5[3] & !Q5[2] & !Q5[1] & !Q5[0];
A1L56_p2_out = !disp_select[2] & !disp_select[1] & !counter_out & !Q5[3] & !Q5[2] & !Q5[1] & !Q5[0] & !dp_s100hz & !Q4[3] & !Q4[2] & !Q4[1] & !Q4[0];
A1L56_p3_out = !disp_select[2] & !disp_select[0] & !counter_out & !Q5[3] & !Q5[2] & !Q5[1] & !Q5[0] & !dp_s100hz & !Q4[3] & !Q4[2] & !Q4[1] & !Q4[0] & !Q3[3] & !Q3[2] & !Q3[1] & !Q3[0];
A1L56_p4_out = !disp_select[2] & !counter_out & !Q5[3] & !Q5[2] & !Q5[1] & !Q5[0] & !dp_s100hz & !Q4[3] & !Q4[2] & !Q4[1] & !Q4[0] & !Q3[3] & !Q3[2] & !Q3[1] & !Q3[0] & !dp_s10hz & !Q2[0] & !Q2[1] & !Q2[2] & !Q2[3];
A1L56_or_out = A1L56_p0_out # A1L56_p1_out # A1L56_p2_out # A1L56_p3_out # A1L56_p4_out;
A1L56 = A1L56_or_out;


--A1L65 is data_out[6]$latch~10 at LC2
A1L65_p1_out = !A1L56 & A1L47 & A1L07 & A1L66 & A1L76;
A1L65_p2_out = A1L56 & A1L65;
A1L65_p3_out = A1L65 & A1L47 & A1L07 & A1L66 & A1L76;
A1L65_or_out = A1L65_p1_out # A1L65_p2_out # A1L65_p3_out;
A1L65 = A1L65_or_out;


--A1L45 is data_out[5]$latch~10 at LC3
A1L45_p1_out = !A1L56 & A1L47 & A1L07 & A1L86 & A1L96;
A1L45_p2_out = A1L56 & A1L45;
A1L45_p3_out = A1L45 & A1L47 & A1L07 & A1L86 & A1L96;
A1L45_or_out = A1L45_p1_out # A1L45_p2_out # A1L45_p3_out;
A1L45 = A1L45_or_out;


--A1L25 is data_out[4]$latch~10 at LC17
A1L25_p1_out = !A1L56 & A1L08 & A1L18 & A1L17;
A1L25_p2_out = A1L56 & A1L25;
A1L25_p3_out = A1L25 & A1L08 & A1L18 & A1L17;
A1L25_or_out = A1L25_p1_out # A1L25_p2_out # A1L25_p3_out;
A1L25 = A1L25_or_out;


--A1L05 is data_out[3]$latch~10 at LC18
A1L05_p1_out = !A1L56 & A1L08 & A1L27 & A1L28 & A1L18 & A1L37;
A1L05_p2_out = A1L56 & A1L05;
A1L05_p3_out = A1L05 & A1L08 & A1L27 & A1L28 & A1L18 & A1L37;
A1L05_or_out = A1L05_p1_out # A1L05_p2_out # A1L05_p3_out;
A1L05 = A1L05_or_out;


--A1L84 is data_out[2]$latch~10 at LC19
A1L84_p1_out = !A1L56 & A1L08 & A1L57 & !data_in[0];
A1L84_p2_out = A1L56 & A1L84;
A1L84_p3_out = A1L84 & A1L08 & A1L57 & !data_in[0];
A1L84_or_out = A1L84_p1_out # A1L84_p2_out # A1L84_p3_out;
A1L84 = A1L84_or_out;


--A1L64 is data_out[1]$latch~10 at LC20
A1L64_p1_out = !A1L56 & A1L67 & A1L18 & A1L77 & A1L87;
A1L64_p2_out = A1L56 & A1L64;
A1L64_p3_out = A1L64 & A1L67 & A1L18 & A1L77 & A1L87;
A1L64_or_out = A1L64_p1_out # A1L64_p2_out # A1L64_p3_out;
A1L64 = A1L64_or_out;


--A1L44 is data_out[0]$latch~10 at LC4
A1L44_p1_out = A1L97 & !A1L56;
A1L44_p2_out = A1L56 & A1L44;
A1L44_p3_out = A1L97 & A1L44;
A1L44_or_out = A1L44_p1_out # A1L44_p2_out # A1L44_p3_out;
A1L44 = A1L44_or_out;


--A1L47 is reduce_or~1054sexp2 at SEXP2
A1L47 = EXP(data_in[3] & data_in[1]);


--A1L57 is reduce_or~1054sexp3 at SEXP20
A1L57 = EXP(!data_in[1] & data_in[2]);


--A1L07 is reduce_or~1052sexp2 at SEXP1
A1L07 = EXP(data_in[3] & data_in[2]);


--A1L17 is reduce_or~1052sexp3 at SEXP19
A1L17 = EXP(!data_in[2] & data_in[1] & !data_in[0]);


--A1L67 is reduce_or~1055sexp1 at SEXP18
A1L67 = EXP(!data_in[3] & !data_in[2] & data_in[0]);


--A1L77 is reduce_or~1055sexp3 at SEXP17
A1L77 = EXP(!data_in[2] & data_in[1]);


--A1L87 is reduce_or~1055sexp4 at SEXP24
A1L87 = EXP(data_in[1] & data_in[0]);


--A1L66 is reduce_or~1050sexp3 at SEXP3
A1L66 = EXP(!data_in[3] & !data_in[1] & !data_in[2] & data_in[0]);


--A1L76 is reduce_or~1050sexp4 at SEXP4
A1L76 = EXP(!data_in[1] & data_in[2] & !data_in[0]);


--A1L86 is reduce_or~1051sexp3 at SEXP9
A1L86 = EXP(data_in[2] & !data_in[1] & data_in[0]);


--A1L96 is reduce_or~1051sexp4 at SEXP5
A1L96 = EXP(data_in[2] & data_in[1] & !data_in[0]);


--A1L27 is reduce_or~1053sexp2 at SEXP25
A1L27 = EXP(!data_in[2] & !data_in[1] & data_in[0]);


--A1L37 is reduce_or~1053sexp5 at SEXP26
A1L37 = EXP(data_in[2] & data_in[1] & data_in[0]);


--data_in[3] is data_in[3] at PIN_60
--operation mode is input

data_in[3] = INPUT();


--data_in[2] is data_in[2] at PIN_93
--operation mode is input

data_in[2] = INPUT();


--data_in[1] is data_in[1] at PIN_16
--operation mode is input

data_in[1] = INPUT();


--data_in[0] is data_in[0] at PIN_61
--operation mode is input

data_in[0] = INPUT();


--disp_select[2] is disp_select[2] at PIN_84
--operation mode is input

disp_select[2] = INPUT();


--disp_select[1] is disp_select[1] at PIN_92
--operation mode is input

disp_select[1] = INPUT();


--disp_select[0] is disp_select[0] at PIN_85
--operation mode is input

disp_select[0] = INPUT();


--dp_s1hz is dp_s1hz at PIN_69
--operation mode is input

dp_s1hz = INPUT();


--dp_s10hz is dp_s10hz at PIN_29
--operation mode is input

dp_s10hz = INPUT();


--dp_s100hz is dp_s100hz at PIN_94
--operation mode is input

dp_s100hz = INPUT();


--Q5[3] is Q5[3] at PIN_52
--operation mode is input

Q5[3] = INPUT();


--Q5[2] is Q5[2] at PIN_99
--operation mode is input

Q5[2] = INPUT();


--Q5[1] is Q5[1] at PIN_97
--operation mode is input

Q5[1] = INPUT();


--Q5[0] is Q5[0] at PIN_57
--operation mode is input

Q5[0] = INPUT();


--Q4[3] is Q4[3] at PIN_96
--operation mode is input

Q4[3] = INPUT();


--Q4[2] is Q4[2] at PIN_81
--operation mode is input

Q4[2] = INPUT();


--Q4[1] is Q4[1] at PIN_58
--operation mode is input

Q4[1] = INPUT();


--Q4[0] is Q4[0] at PIN_83
--operation mode is input

Q4[0] = INPUT();


--Q3[3] is Q3[3] at PIN_17
--operation mode is input

Q3[3] = INPUT();


--Q3[2] is Q3[2] at PIN_71
--operation mode is input

Q3[2] = INPUT();


--Q3[1] is Q3[1] at PIN_19
--operation mode is input

Q3[1] = INPUT();


--Q3[0] is Q3[0] at PIN_48
--operation mode is input

Q3[0] = INPUT();


--Q2[3] is Q2[3] at PIN_6
--operation mode is input

Q2[3] = INPUT();


--Q2[2] is Q2[2] at PIN_47
--operation mode is input

Q2[2] = INPUT();


--Q2[1] is Q2[1] at PIN_30
--operation mode is input

Q2[1] = INPUT();


--Q2[0] is Q2[0] at PIN_46
--operation mode is input

Q2[0] = INPUT();


--Q1[3] is Q1[3] at PIN_8
--operation mode is input

Q1[3] = INPUT();


--Q1[2] is Q1[2] at PIN_31
--operation mode is input

Q1[2] = INPUT();


--Q1[1] is Q1[1] at PIN_68
--operation mode is input

Q1[1] = INPUT();


--Q1[0] is Q1[0] at PIN_9
--operation mode is input

Q1[0] = INPUT();


--Q0[3] is Q0[3] at PIN_21
--operation mode is input

Q0[3] = INPUT();


--Q0[2] is Q0[2] at PIN_56
--operation mode is input

Q0[2] = INPUT();


--Q0[1] is Q0[1] at PIN_80
--operation mode is input

Q0[1] = INPUT();


--Q0[0] is Q0[0] at PIN_20
--operation mode is input

Q0[0] = INPUT();


--counter_out is counter_out at PIN_45
--operation mode is input

counter_out = INPUT();


--dp is dp at PIN_14
--operation mode is output

dp = OUTPUT(A1L53);


--data_out[6] is data_out[6] at PIN_13
--operation mode is output

data_out[6] = OUTPUT(A1L65);


--data_out[5] is data_out[5] at PIN_12
--operation mode is output

data_out[5] = OUTPUT(A1L45);


--data_out[4] is data_out[4] at PIN_37
--operation mode is output

data_out[4] = OUTPUT(A1L25);


--data_out[3] is data_out[3] at PIN_36
--operation mode is output

data_out[3] = OUTPUT(A1L05);


--data_out[2] is data_out[2] at PIN_35
--operation mode is output

data_out[2] = OUTPUT(A1L84);


--data_out[1] is data_out[1] at PIN_33
--operation mode is output

data_out[1] = OUTPUT(A1L64);


--data_out[0] is data_out[0] at PIN_10
--operation mode is output

data_out[0] = OUTPUT(A1L44);






--A1L08 is reduce_or~1091 at SEXP21
A1L08 = EXP(data_in[3] & data_in[1]);


--A1L18 is reduce_or~1092 at SEXP22
A1L18 = EXP(data_in[3] & data_in[2]);


--A1L28 is reduce_or~1093 at SEXP23
A1L28 = EXP(!data_in[1] & data_in[2] & !data_in[0]);


