--Data[15] is Data[15] at LC4_B2
--operation mode is normal

Data[15]_lut_out = Adc_Sdata;
Data[15] = DFFEA(Data[15]_lut_out, !GLOBAL(Adc_SCL), , , A1L04, , );


--Data[14] is Data[14] at LC1_B2
--operation mode is normal

Data[14]_lut_out = Adc_Sdata;
Data[14] = DFFEA(Data[14]_lut_out, !GLOBAL(Adc_SCL), , , A1L93, , );


--Data[13] is Data[13] at LC5_B1
--operation mode is normal

Data[13]_lut_out = Adc_Sdata;
Data[13] = DFFEA(Data[13]_lut_out, !GLOBAL(Adc_SCL), , , A1L83, , );


--Data[12] is Data[12] at LC2_B1
--operation mode is normal

Data[12]_lut_out = Adc_Sdata;
Data[12] = DFFEA(Data[12]_lut_out, !GLOBAL(Adc_SCL), , , A1L73, , );


--Data[11] is Data[11] at LC4_B1
--operation mode is normal

Data[11]_lut_out = Adc_Sdata;
Data[11] = DFFEA(Data[11]_lut_out, !GLOBAL(Adc_SCL), , , A1L63, , );


--Data[10] is Data[10] at LC3_B1
--operation mode is normal

Data[10]_lut_out = Adc_Sdata;
Data[10] = DFFEA(Data[10]_lut_out, !GLOBAL(Adc_SCL), , , A1L53, , );


--Data[9] is Data[9] at LC8_B4
--operation mode is normal

Data[9]_lut_out = Adc_Sdata;
Data[9] = DFFEA(Data[9]_lut_out, !GLOBAL(Adc_SCL), , , A1L43, , );


--Data[8] is Data[8] at LC6_B2
--operation mode is normal

Data[8]_lut_out = Adc_Sdata;
Data[8] = DFFEA(Data[8]_lut_out, !GLOBAL(Adc_SCL), , , A1L33, , );


--Data[7] is Data[7] at LC5_B2
--operation mode is normal

Data[7]_lut_out = Adc_Sdata;
Data[7] = DFFEA(Data[7]_lut_out, !GLOBAL(Adc_SCL), , , A1L23, , );


--Data[6] is Data[6] at LC4_B4
--operation mode is normal

Data[6]_lut_out = Adc_Sdata;
Data[6] = DFFEA(Data[6]_lut_out, !GLOBAL(Adc_SCL), , , A1L13, , );


--Data[5] is Data[5] at LC5_B4
--operation mode is normal

Data[5]_lut_out = Adc_Sdata;
Data[5] = DFFEA(Data[5]_lut_out, !GLOBAL(Adc_SCL), , , A1L03, , );


--Data[4] is Data[4] at LC3_B2
--operation mode is normal

Data[4]_lut_out = Adc_Sdata;
Data[4] = DFFEA(Data[4]_lut_out, !GLOBAL(Adc_SCL), , , A1L92, , );


--C1_q[0] is lpm_counter:cnt_rtl_0|alt_counter_f10ke:wysi_counter|q[0] at LC4_B3
--operation mode is up_dn_cntr

C1_q[0]_lut_out = !C1_q[0];
C1_q[0] = DFFEA(C1_q[0]_lut_out, !GLOBAL(Adc_SCL), , , , , );

--C1L3 is lpm_counter:cnt_rtl_0|alt_counter_f10ke:wysi_counter|counter_cell[0]~COUT at LC4_B3
--operation mode is up_dn_cntr

C1L3 = CARRY(C1_q[0]);


--C1_q[1] is lpm_counter:cnt_rtl_0|alt_counter_f10ke:wysi_counter|q[1] at LC5_B3
--operation mode is up_dn_cntr

C1_q[1]_lut_out = C1_q[1] $ C1L3;
C1_q[1] = DFFEA(C1_q[1]_lut_out, !GLOBAL(Adc_SCL), , , , , );

--C1L5 is lpm_counter:cnt_rtl_0|alt_counter_f10ke:wysi_counter|counter_cell[1]~COUT at LC5_B3
--operation mode is up_dn_cntr

C1L5 = CARRY(C1_q[1] & C1L3);


--C1_q[2] is lpm_counter:cnt_rtl_0|alt_counter_f10ke:wysi_counter|q[2] at LC6_B3
--operation mode is up_dn_cntr

C1_q[2]_lut_out = C1_q[2] $ C1L5;
C1_q[2] = DFFEA(C1_q[2]_lut_out, !GLOBAL(Adc_SCL), , , , , );

--C1L7 is lpm_counter:cnt_rtl_0|alt_counter_f10ke:wysi_counter|counter_cell[2]~COUT at LC6_B3
--operation mode is up_dn_cntr

C1L7 = CARRY(C1_q[2] & C1L5);


--C1_q[3] is lpm_counter:cnt_rtl_0|alt_counter_f10ke:wysi_counter|q[3] at LC7_B3
--operation mode is up_dn_cntr

C1_q[3]_lut_out = C1_q[3] $ C1L7;
C1_q[3] = DFFEA(C1_q[3]_lut_out, !GLOBAL(Adc_SCL), , , , , );


--A1L04 is Decoder~32 at LC2_B2
--operation mode is normal

A1L04 = C1_q[0] & C1_q[1] & C1_q[2] & C1_q[3];


--A1L93 is Decoder~31 at LC7_B2
--operation mode is normal

A1L93 = !C1_q[0] & C1_q[1] & C1_q[2] & C1_q[3];


--A1L83 is Decoder~30 at LC1_B1
--operation mode is normal

A1L83 = C1_q[0] & !C1_q[1] & C1_q[2] & C1_q[3];


--A1L73 is Decoder~29 at LC6_B1
--operation mode is normal

A1L73 = !C1_q[0] & !C1_q[1] & C1_q[2] & C1_q[3];


--A1L63 is Decoder~28 at LC7_B1
--operation mode is normal

A1L63 = C1_q[0] & C1_q[1] & !C1_q[2] & C1_q[3];


--A1L53 is Decoder~27 at LC8_B1
--operation mode is normal

A1L53 = !C1_q[0] & C1_q[1] & !C1_q[2] & C1_q[3];


--A1L43 is Decoder~26 at LC2_B3
--operation mode is normal

A1L43 = C1_q[0] & !C1_q[1] & !C1_q[2] & C1_q[3];


--A1L33 is Decoder~25 at LC3_B3
--operation mode is normal

A1L33 = !C1_q[0] & !C1_q[1] & !C1_q[2] & C1_q[3];


--A1L23 is Decoder~24 at LC8_B2
--operation mode is normal

A1L23 = C1_q[0] & C1_q[1] & C1_q[2] & !C1_q[3];


--A1L13 is Decoder~23 at LC1_B3
--operation mode is normal

A1L13 = !C1_q[0] & C1_q[1] & C1_q[2] & !C1_q[3];


--A1L03 is Decoder~22 at LC1_B4
--operation mode is normal

A1L03 = C1_q[0] & !C1_q[1] & C1_q[2] & !C1_q[3];


--A1L92 is Decoder~21 at LC8_B3
--operation mode is normal

A1L92 = !C1_q[0] & !C1_q[1] & C1_q[2] & !C1_q[3];


--En is En at PIN_38
--operation mode is input

En = INPUT();


--Reset is Reset at PIN_89
--operation mode is input

Reset = INPUT();


--Adc_Sdata is Adc_Sdata at PIN_91
--operation mode is input

Adc_Sdata = INPUT();


--Adc_SCL is Adc_SCL at PIN_39
--operation mode is input

Adc_SCL = INPUT();


--Current_Data[11] is Current_Data[11] at PIN_77
--operation mode is output

Current_Data[11] = OUTPUT(Data[15]);


--Current_Data[10] is Current_Data[10] at PIN_65
--operation mode is output

Current_Data[10] = OUTPUT(Data[14]);


--Current_Data[9] is Current_Data[9] at PIN_15
--operation mode is output

Current_Data[9] = OUTPUT(Data[13]);


--Current_Data[8] is Current_Data[8] at PIN_64
--operation mode is output

Current_Data[8] = OUTPUT(Data[12]);


--Current_Data[7] is Current_Data[7] at PIN_50
--operation mode is output

Current_Data[7] = OUTPUT(Data[11]);


--Current_Data[6] is Current_Data[6] at PIN_14
--operation mode is output

Current_Data[6] = OUTPUT(Data[10]);


--Current_Data[5] is Current_Data[5] at PIN_61
--operation mode is output

Current_Data[5] = OUTPUT(Data[9]);


--Current_Data[4] is Current_Data[4] at PIN_16
--operation mode is output

Current_Data[4] = OUTPUT(Data[8]);


--Current_Data[3] is Current_Data[3] at PIN_62
--operation mode is output

Current_Data[3] = OUTPUT(Data[7]);


--Current_Data[2] is Current_Data[2] at PIN_81
--operation mode is output

Current_Data[2] = OUTPUT(Data[6]);


--Current_Data[1] is Current_Data[1] at PIN_80
--operation mode is output

Current_Data[1] = OUTPUT(Data[5]);


--Current_Data[0] is Current_Data[0] at PIN_63
--operation mode is output

Current_Data[0] = OUTPUT(Data[4]);


