--A1L04 is pulse_16_out~232 at LC17
A1L04_p1_out = !Reset & counter_data[0];
A1L04_or_out = A1L04_p1_out;
A1L04 = A1L04_or_out;


--A1L14 is pulse_16_out~234 at LC7
A1L14_p1_out = counter_data[1] & !Reset & !counter_data[0];
A1L14_or_out = A1L14_p1_out;
A1L14 = A1L14_or_out;


--A1L24 is pulse_16_out~236 at LC9
A1L24_p1_out = counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L24_or_out = A1L24_p1_out;
A1L24 = A1L24_or_out;


--A1L34 is pulse_16_out~238 at LC10
A1L34_p1_out = counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L34_or_out = A1L34_p1_out;
A1L34 = A1L34_or_out;


--A1L44 is pulse_16_out~240 at LC11
A1L44_p1_out = counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L44_or_out = A1L44_p1_out;
A1L44 = A1L44_or_out;


--A1L54 is pulse_16_out~242 at LC16
A1L54_p1_out = counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L54_or_out = A1L54_p1_out;
A1L54 = A1L54_or_out;


--A1L64 is pulse_16_out~244 at LC15
A1L64_p1_out = counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L64_or_out = A1L64_p1_out;
A1L64 = A1L64_or_out;


--A1L74 is pulse_16_out~246 at LC14
A1L74_p1_out = counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L74_or_out = A1L74_p1_out;
A1L74 = A1L74_or_out;


--A1L84 is pulse_16_out~248 at LC13
A1L84_p1_out = counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L84_or_out = A1L84_p1_out;
A1L84 = A1L84_or_out;


--A1L94 is pulse_16_out~250 at LC12
A1L94_p1_out = counter_data[9] & !counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L94_or_out = A1L94_p1_out;
A1L94 = A1L94_or_out;


--A1L05 is pulse_16_out~252 at LC6
A1L05_p1_out = counter_data[10] & !counter_data[9] & !counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L05_or_out = A1L05_p1_out;
A1L05 = A1L05_or_out;


--A1L15 is pulse_16_out~254 at LC5
A1L15_p1_out = counter_data[11] & !counter_data[10] & !counter_data[9] & !counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L15_or_out = A1L15_p1_out;
A1L15 = A1L15_or_out;


--A1L25 is pulse_16_out~256 at LC4
A1L25_p1_out = counter_data[12] & !counter_data[11] & !counter_data[10] & !counter_data[9] & !counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L25_or_out = A1L25_p1_out;
A1L25 = A1L25_or_out;


--A1L35 is pulse_16_out~258 at LC3
A1L35_p1_out = counter_data[13] & !counter_data[12] & !counter_data[11] & !counter_data[10] & !counter_data[9] & !counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L35_or_out = A1L35_p1_out;
A1L35 = A1L35_or_out;


--A1L45 is pulse_16_out~260 at LC2
A1L45_p1_out = counter_data[14] & !counter_data[13] & !counter_data[12] & !counter_data[11] & !counter_data[10] & !counter_data[9] & !counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0];
A1L45_or_out = A1L45_p1_out;
A1L45 = A1L45_or_out;


--A1L55 is pulse_16_out~262 at LC1
A1L55_p1_out = !counter_data[14] & !counter_data[13] & !counter_data[12] & !counter_data[11] & !counter_data[10] & !counter_data[9] & !counter_data[8] & !counter_data[7] & !counter_data[6] & !counter_data[5] & !counter_data[4] & !counter_data[3] & !counter_data[2] & !counter_data[1] & !Reset & !counter_data[0] & counter_data[15];
A1L55_or_out = A1L55_p1_out;
A1L55 = A1L55_or_out;


--Reset is Reset at PIN_84
--operation mode is input

Reset = INPUT();


--counter_data[15] is counter_data[15] at PIN_58
--operation mode is input

counter_data[15] = INPUT();


--counter_data[14] is counter_data[14] at PIN_57
--operation mode is input

counter_data[14] = INPUT();


--counter_data[13] is counter_data[13] at PIN_60
--operation mode is input

counter_data[13] = INPUT();


--counter_data[12] is counter_data[12] at PIN_20
--operation mode is input

counter_data[12] = INPUT();


--counter_data[11] is counter_data[11] at PIN_29
--operation mode is input

counter_data[11] = INPUT();


--counter_data[10] is counter_data[10] at PIN_46
--operation mode is input

counter_data[10] = INPUT();


--counter_data[9] is counter_data[9] at PIN_16
--operation mode is input

counter_data[9] = INPUT();


--counter_data[8] is counter_data[8] at PIN_61
--operation mode is input

counter_data[8] = INPUT();


--counter_data[7] is counter_data[7] at PIN_17
--operation mode is input

counter_data[7] = INPUT();


--counter_data[6] is counter_data[6] at PIN_83
--operation mode is input

counter_data[6] = INPUT();


--counter_data[5] is counter_data[5] at PIN_19
--operation mode is input

counter_data[5] = INPUT();


--counter_data[4] is counter_data[4] at PIN_56
--operation mode is input

counter_data[4] = INPUT();


--counter_data[3] is counter_data[3] at PIN_23
--operation mode is input

counter_data[3] = INPUT();


--counter_data[2] is counter_data[2] at PIN_54
--operation mode is input

counter_data[2] = INPUT();


--counter_data[1] is counter_data[1] at PIN_48
--operation mode is input

counter_data[1] = INPUT();


--counter_data[0] is counter_data[0] at PIN_85
--operation mode is input

counter_data[0] = INPUT();


--pulse_16_out[15] is pulse_16_out[15] at PIN_37
--operation mode is output

pulse_16_out[15] = OUTPUT(A1L04);


--pulse_16_out[14] is pulse_16_out[14] at PIN_6
--operation mode is output

pulse_16_out[14] = OUTPUT(A1L14);


--pulse_16_out[13] is pulse_16_out[13] at PIN_100
--operation mode is output

pulse_16_out[13] = OUTPUT(A1L24);


--pulse_16_out[12] is pulse_16_out[12] at PIN_99
--operation mode is output

pulse_16_out[12] = OUTPUT(A1L34);


--pulse_16_out[11] is pulse_16_out[11] at PIN_98
--operation mode is output

pulse_16_out[11] = OUTPUT(A1L44);


--pulse_16_out[10] is pulse_16_out[10] at PIN_92
--operation mode is output

pulse_16_out[10] = OUTPUT(A1L54);


--pulse_16_out[9] is pulse_16_out[9] at PIN_93
--operation mode is output

pulse_16_out[9] = OUTPUT(A1L64);


--pulse_16_out[8] is pulse_16_out[8] at PIN_94
--operation mode is output

pulse_16_out[8] = OUTPUT(A1L74);


--pulse_16_out[7] is pulse_16_out[7] at PIN_96
--operation mode is output

pulse_16_out[7] = OUTPUT(A1L84);


--pulse_16_out[6] is pulse_16_out[6] at PIN_97
--operation mode is output

pulse_16_out[6] = OUTPUT(A1L94);


--pulse_16_out[5] is pulse_16_out[5] at PIN_8
--operation mode is output

pulse_16_out[5] = OUTPUT(A1L05);


--pulse_16_out[4] is pulse_16_out[4] at PIN_9
--operation mode is output

pulse_16_out[4] = OUTPUT(A1L15);


--pulse_16_out[3] is pulse_16_out[3] at PIN_10
--operation mode is output

pulse_16_out[3] = OUTPUT(A1L25);


--pulse_16_out[2] is pulse_16_out[2] at PIN_12
--operation mode is output

pulse_16_out[2] = OUTPUT(A1L35);


--pulse_16_out[1] is pulse_16_out[1] at PIN_13
--operation mode is output

pulse_16_out[1] = OUTPUT(A1L45);


--pulse_16_out[0] is pulse_16_out[0] at PIN_14
--operation mode is output

pulse_16_out[0] = OUTPUT(A1L55);






