--B1_sdata[1] is scan:inst|sdata[1] at LC_X20_Y7_N0
--operation mode is normal

B1_sdata[1]_lut_out = !B1_sdata[1];
B1_sdata[1] = DFFEAS(B1_sdata[1]_lut_out, GLOBAL(B1_EN_in), VCC, , B1_sdata[0], , , , );


--M1L3 is control:inst14|Red1~14 at LC_X19_Y6_N8
--operation mode is normal

M1L3 = B1_sdata[1] & Reset & SW;


--M1L4 is control:inst14|Yellow1~11 at LC_X20_Y7_N9
--operation mode is normal

M1L4 = SW & Reset & !B1_sdata[1];


--B1_sdata[0] is scan:inst|sdata[0] at LC_X19_Y6_N3
--operation mode is normal

B1_sdata[0]_lut_out = !B1_sdata[0];
B1_sdata[0] = DFFEAS(B1_sdata[0]_lut_out, GLOBAL(B1_EN_in), VCC, , , , , , );


--M1L5 is control:inst14|Yellow1~12 at LC_X19_Y6_N1
--operation mode is normal

M1L5 = SW & !B1_sdata[1] & Reset & B1_sdata[0];


--M1L6 is control:inst14|Yellow2~10 at LC_X19_Y6_N0
--operation mode is normal

M1L6 = SW & B1_sdata[1] & Reset & B1_sdata[0];


--M1L1 is control:inst14|Green1~1 at LC_X19_Y6_N4
--operation mode is normal

M1L1 = B1_sdata[1] # B1_sdata[0] # !Reset # !SW;


--M1L2 is control:inst14|Green2~10 at LC_X19_Y6_N6
--operation mode is normal

M1L2 = SW & B1_sdata[1] & Reset & !B1_sdata[0];


--J1_D_OUT[0] is dispselect:inst9|D_OUT[0] at LC_X21_Y9_N0
--operation mode is normal

J1_D_OUT[0]_lut_out = !J1_D_OUT[0];
J1_D_OUT[0] = DFFEAS(J1_D_OUT[0]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , , );


--P2_safe_q[0] is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|safe_q[0] at LC_X20_Y8_N5
--operation mode is arithmetic

P2_safe_q[0]_lut_out = !P2_safe_q[0];
P2_safe_q[0] = DFFEAS(P2_safe_q[0]_lut_out, GLOBAL(K1_clk_out), VCC, , , , , D1L1, );

--P2L2 is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|counter_cella0~COUT at LC_X20_Y8_N5
--operation mode is arithmetic

P2L2_cout_0 = P2_safe_q[0];
P2L2 = CARRY(P2L2_cout_0);

--P2L3 is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X20_Y8_N5
--operation mode is arithmetic

P2L3_cout_1 = P2_safe_q[0];
P2L3 = CARRY(P2L3_cout_1);


--P1_safe_q[0] is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|safe_q[0] at LC_X21_Y8_N1
--operation mode is arithmetic

P1_safe_q[0]_lut_out = !P1_safe_q[0];
P1_safe_q[0] = DFFEAS(P1_safe_q[0]_lut_out, GLOBAL(K1_clk_out), VCC, , , , , C1L1, );

--P1L2 is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|counter_cella0~COUT at LC_X21_Y8_N1
--operation mode is arithmetic

P1L2_cout_0 = P1_safe_q[0];
P1L2 = CARRY(P1L2_cout_0);

--P1L3 is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X21_Y8_N1
--operation mode is arithmetic

P1L3_cout_1 = P1_safe_q[0];
P1L3 = CARRY(P1L3_cout_1);


--P1_safe_q[3] is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|safe_q[3] at LC_X21_Y8_N4
--operation mode is normal

P1_safe_q[3]_lut_out = P1_safe_q[3] $ P1L8;
P1_safe_q[3] = DFFEAS(P1_safe_q[3]_lut_out, GLOBAL(K1_clk_out), VCC, , , , , C1L1, );


--P1_safe_q[1] is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|safe_q[1] at LC_X21_Y8_N2
--operation mode is arithmetic

P1_safe_q[1]_lut_out = P1_safe_q[1] $ (P1L2);
P1_safe_q[1] = DFFEAS(P1_safe_q[1]_lut_out, GLOBAL(K1_clk_out), VCC, , , , , C1L1, );

--P1L5 is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|counter_cella1~COUT at LC_X21_Y8_N2
--operation mode is arithmetic

P1L5_cout_0 = !P1L2 # !P1_safe_q[1];
P1L5 = CARRY(P1L5_cout_0);

--P1L6 is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|counter_cella1~COUTCOUT1 at LC_X21_Y8_N2
--operation mode is arithmetic

P1L6_cout_1 = !P1L3 # !P1_safe_q[1];
P1L6 = CARRY(P1L6_cout_1);


--P1_safe_q[2] is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|safe_q[2] at LC_X21_Y8_N3
--operation mode is arithmetic

P1_safe_q[2]_lut_out = P1_safe_q[2] $ !P1L5;
P1_safe_q[2] = DFFEAS(P1_safe_q[2]_lut_out, GLOBAL(K1_clk_out), VCC, , , , , C1L1, );

--P1L8 is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|counter_cella2~COUT at LC_X21_Y8_N3
--operation mode is arithmetic

P1L8_cout_0 = P1_safe_q[2] & !P1L5;
P1L8 = CARRY(P1L8_cout_0);

--P1L9 is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X21_Y8_N3
--operation mode is arithmetic

P1L9_cout_1 = P1_safe_q[2] & !P1L6;
P1L9 = CARRY(P1L9_cout_1);


--F1L1 is datamux:inst6|D_OUT0[0]~112 at LC_X20_Y8_N1
--operation mode is normal

F1L1 = P1_safe_q[0] # P1_safe_q[3] # P1_safe_q[1] & P1_safe_q[2];


--H1L1 is dispmux:inst8|D_OUT[0]~737 at LC_X20_Y8_N2
--operation mode is normal

H1L1 = J1_D_OUT[0] & B1_sdata[0] & !F1L1 # !B1_sdata[0] & !P2_safe_q[0];


--D1L51 is counter55:inst2|add~161 at LC_X20_Y7_N4
--operation mode is arithmetic

D1L51 = Q1_safe_q[0] $ D1L31;

--D1L61 is counter55:inst2|add~161COUT at LC_X20_Y7_N4
--operation mode is arithmetic

D1L61 = D1L71;


--D1L52 is counter55:inst2|add~164 at LC_X20_Y7_N7
--operation mode is normal

D1L52_carry_eqn = (!D1L61 & D1L32) # (D1L61 & D1L42);
D1L52 = D1L52_carry_eqn $ Q1_safe_q[3];


--H1L5 is dispmux:inst8|D_OUT[1]~738 at LC_X20_Y7_N8
--operation mode is normal

H1L5 = !B1_sdata[0] & !D1L52 & !J1_D_OUT[0];


--D1L91 is counter55:inst2|add~162 at LC_X20_Y7_N5
--operation mode is arithmetic

D1L91_carry_eqn = (!D1L61 & GND) # (D1L61 & VCC);
D1L91 = Q1_safe_q[1] $ D1L91_carry_eqn;

--D1L02 is counter55:inst2|add~162COUT at LC_X20_Y7_N5
--operation mode is arithmetic

D1L02_cout_0 = !Q1_safe_q[1] & !D1L61;
D1L02 = CARRY(D1L02_cout_0);

--D1L12 is counter55:inst2|add~162COUTCOUT1_194 at LC_X20_Y7_N5
--operation mode is arithmetic

D1L12_cout_1 = !Q1_safe_q[1] & !D1L61;
D1L12 = CARRY(D1L12_cout_1);


--D1L22 is counter55:inst2|add~163 at LC_X20_Y7_N6
--operation mode is arithmetic

D1L22_carry_eqn = (!D1L61 & D1L02) # (D1L61 & D1L12);
D1L22 = Q1_safe_q[2] $ (D1L22_carry_eqn);

--D1L32 is counter55:inst2|add~163COUT at LC_X20_Y7_N6
--operation mode is arithmetic

D1L32_cout_0 = Q1_safe_q[2] & !D1L02;
D1L32 = CARRY(D1L32_cout_0);

--D1L42 is counter55:inst2|add~163COUTCOUT1_195 at LC_X20_Y7_N6
--operation mode is arithmetic

D1L42_cout_1 = Q1_safe_q[2] & !D1L12;
D1L42 = CARRY(D1L42_cout_1);


--H1L7 is dispmux:inst8|D_OUT[2]~739 at LC_X20_Y9_N2
--operation mode is normal

H1L7 = H1L5 & !D1L22 # !D1L91;


--H1L2 is dispmux:inst8|D_OUT[0]~740 at LC_X20_Y8_N4
--operation mode is normal

H1L2 = H1L1 # D1L51 & H1L7;


--H1L6 is dispmux:inst8|D_OUT[1]~741 at LC_X20_Y9_N4
--operation mode is normal

H1L6 = D1L91 & !D1L22 & H1L5;


--D1L21 is counter55:inst2|add~160 at LC_X20_Y7_N3
--operation mode is arithmetic

D1L21 = P2_safe_q[3] $ (D1L01);

--D1L31 is counter55:inst2|add~160COUT at LC_X20_Y7_N3
--operation mode is arithmetic

D1L31_cout_0 = !P2_safe_q[3] & !D1L01;
D1L31 = CARRY(D1L31_cout_0);

--D1L41 is counter55:inst2|add~160COUTCOUT1 at LC_X20_Y7_N3
--operation mode is arithmetic

D1L41_cout_1 = !P2_safe_q[3] & !D1L11;
D1L41 = CARRY(D1L41_cout_1);


--D1L9 is counter55:inst2|add~159 at LC_X20_Y7_N2
--operation mode is arithmetic

D1L9 = P2_safe_q[2] $ (D1L6);

--D1L01 is counter55:inst2|add~159COUT at LC_X20_Y7_N2
--operation mode is arithmetic

D1L01_cout_0 = P2_safe_q[2] & !D1L6;
D1L01 = CARRY(D1L01_cout_0);

--D1L11 is counter55:inst2|add~159COUTCOUT1_193 at LC_X20_Y7_N2
--operation mode is arithmetic

D1L11_cout_1 = P2_safe_q[2] & !D1L8;
D1L11 = CARRY(D1L11_cout_1);


--P2_safe_q[1] is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|safe_q[1] at LC_X20_Y8_N6
--operation mode is arithmetic

P2_safe_q[1]_lut_out = P2_safe_q[1] $ (P2L2);
P2_safe_q[1] = DFFEAS(P2_safe_q[1]_lut_out, GLOBAL(K1_clk_out), VCC, , , , , D1L1, );

--P2L5 is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|counter_cella1~COUT at LC_X20_Y8_N6
--operation mode is arithmetic

P2L5_cout_0 = !P2L2 # !P2_safe_q[1];
P2L5 = CARRY(P2L5_cout_0);

--P2L6 is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|counter_cella1~COUTCOUT1 at LC_X20_Y8_N6
--operation mode is arithmetic

P2L6_cout_1 = !P2L3 # !P2_safe_q[1];
P2L6 = CARRY(P2L6_cout_1);


--D1L5 is counter55:inst2|LessThan~93 at LC_X21_Y9_N6
--operation mode is normal

D1L5 = D1L9 # P2_safe_q[1];


--H1L51 is dispmux:inst8|D_OUT[3]~742 at LC_X21_Y9_N5
--operation mode is normal

H1L51 = J1_D_OUT[0] & B1_sdata[0] # D1L21 & D1L5;


--H1L21 is dispmux:inst8|D_OUT[3]~65 at LC_X21_Y8_N5
--operation mode is normal

H1L21 = P1_safe_q[3] # P1_safe_q[1] & P1_safe_q[2] # !J1_D_OUT[0];


--H1L8 is dispmux:inst8|D_OUT[2]~743 at LC_X21_Y9_N1
--operation mode is normal

H1L8 = J1_D_OUT[0] & !B1_sdata[0];


--H1L4 is dispmux:inst8|D_OUT[1]~23adv_mux_opt_ptn_119 at LC_X21_Y8_N6
--operation mode is normal

H1L4 = H1L51 & P1_safe_q[1] & H1L61 # !H1L51 & H1L6 # !H1L61;


--H1L3 is dispmux:inst8|D_OUT[1]~23 at LC_X21_Y8_N7
--operation mode is normal

H1L3 = H1L4 $ (!P2_safe_q[1] & !B1_sdata[0] & J1_D_OUT[0]);


--H1L9 is dispmux:inst8|D_OUT[2]~744 at LC_X21_Y8_N0
--operation mode is normal

H1L9 = B1_sdata[0] & J1_D_OUT[0] & P1_safe_q[1] $ !P1_safe_q[2];


--H1L01 is dispmux:inst8|D_OUT[2]~745 at LC_X21_Y9_N7
--operation mode is normal

H1L01 = H1L8 & D1L9 $ (D1L21 & P2_safe_q[1]);


--H1L11 is dispmux:inst8|D_OUT[2]~746 at LC_X21_Y8_N9
--operation mode is normal

H1L11 = H1L01 # H1L9 # D1L22 & H1L7;


--H1L31 is dispmux:inst8|D_OUT[3]~729 at LC_X21_Y9_N8
--operation mode is normal

H1L31 = H1L51 & !H1L8 # !D1L9 # !P2_safe_q[1];


--G1L5 is dispdecoder:inst7|reduce_or~38 at LC_X21_Y9_N3
--operation mode is normal

G1L5 = H1L3 & H1L41 # !H1L3 & H1L11 $ (H1L2 & !H1L41);


--G1L6 is dispdecoder:inst7|reduce_or~40 at LC_X21_Y9_N2
--operation mode is normal

G1L6 = H1L41 & H1L3 # H1L11 # !H1L41 & H1L11 & H1L3 $ H1L2;


--G1L7 is dispdecoder:inst7|reduce_or~42 at LC_X21_Y9_N4
--operation mode is normal

G1L7 = H1L11 & H1L41 # !H1L11 & H1L3 & H1L41 # !H1L2;


--G1L4 is dispdecoder:inst7|data_out[4]~31 at LC_X22_Y9_N1
--operation mode is normal

G1L4 = H1L2 & H1L41 # H1L3 $ !H1L11 # !H1L2 & H1L3 & H1L41 # !H1L3 & H1L11;


--G1L3 is dispdecoder:inst7|data_out[3]~33 at LC_X22_Y9_N6
--operation mode is normal

G1L3 = H1L2 # H1L3 & H1L41 # !H1L3 & H1L11;


--G1L2 is dispdecoder:inst7|data_out[2]~35 at LC_X22_Y9_N4
--operation mode is normal

G1L2 = H1L2 & H1L3 # H1L41 $ !H1L11 # !H1L2 & H1L11 & H1L41 # !H1L11 & H1L3;


--G1L1 is dispdecoder:inst7|data_out[1]~37 at LC_X22_Y9_N2
--operation mode is normal

G1L1 = H1L3 & !H1L41 & !H1L11 # !H1L2 # !H1L3 & H1L41 $ H1L11;


--C1_C_out is counter05:inst1|C_out at LC_X19_Y6_N7
--operation mode is normal

C1_C_out_lut_out = B1_sdata[0] & Reset & C1L3;
C1_C_out = DFFEAS(C1_C_out_lut_out, GLOBAL(K1_clk_out), VCC, , , , , , );


--D1_C_out is counter55:inst2|C_out at LC_X19_Y6_N5
--operation mode is normal

D1_C_out_lut_out = D1L2 & D1L62 $ (!Q1L51 # !D1L92);
D1_C_out = DFFEAS(D1_C_out_lut_out, GLOBAL(K1_clk_out), VCC, , , , , , );


--B1_EN_in is scan:inst|EN_in at LC_X19_Y6_N9
--operation mode is normal

B1_EN_in = C1_C_out # D1_C_out;


--Q1_safe_q[3] is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|safe_q[3] at LC_X19_Y8_N8
--operation mode is normal

Q1_safe_q[3]_lut_out = Q1_safe_q[3] $ Q1L8;
Q1_safe_q[3] = DFFEAS(Q1_safe_q[3]_lut_out, GLOBAL(K1_clk_out), VCC, , D1L1, , , D1L3, );


--Q1_safe_q[1] is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|safe_q[1] at LC_X19_Y8_N6
--operation mode is arithmetic

Q1_safe_q[1]_lut_out = Q1_safe_q[1] $ (Q1L2);
Q1_safe_q[1] = DFFEAS(Q1_safe_q[1]_lut_out, GLOBAL(K1_clk_out), VCC, , D1L1, , , D1L3, );

--Q1L5 is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|counter_cella1~COUT at LC_X19_Y8_N6
--operation mode is arithmetic

Q1L5_cout_0 = !Q1L2 # !Q1_safe_q[1];
Q1L5 = CARRY(Q1L5_cout_0);

--Q1L6 is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|counter_cella1~COUTCOUT1 at LC_X19_Y8_N6
--operation mode is arithmetic

Q1L6_cout_1 = !Q1L3 # !Q1_safe_q[1];
Q1L6 = CARRY(Q1L6_cout_1);


--P2_safe_q[3] is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|safe_q[3] at LC_X20_Y8_N8
--operation mode is normal

P2_safe_q[3]_lut_out = P2_safe_q[3] $ P2L8;
P2_safe_q[3] = DFFEAS(P2_safe_q[3]_lut_out, GLOBAL(K1_clk_out), VCC, , , , , D1L1, );


--Q1_safe_q[0] is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|safe_q[0] at LC_X19_Y8_N5
--operation mode is arithmetic

Q1_safe_q[0]_lut_out = !Q1_safe_q[0];
Q1_safe_q[0] = DFFEAS(Q1_safe_q[0]_lut_out, GLOBAL(K1_clk_out), VCC, , D1L1, , , D1L3, );

--Q1L2 is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|counter_cella0~COUT at LC_X19_Y8_N5
--operation mode is arithmetic

Q1L2_cout_0 = Q1_safe_q[0];
Q1L2 = CARRY(Q1L2_cout_0);

--Q1L3 is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|counter_cella0~COUTCOUT1_1 at LC_X19_Y8_N5
--operation mode is arithmetic

Q1L3_cout_1 = Q1_safe_q[0];
Q1L3 = CARRY(Q1L3_cout_1);


--P2_safe_q[2] is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|safe_q[2] at LC_X20_Y8_N7
--operation mode is arithmetic

P2_safe_q[2]_lut_out = P2_safe_q[2] $ (!P2L5);
P2_safe_q[2] = DFFEAS(P2_safe_q[2]_lut_out, GLOBAL(K1_clk_out), VCC, , , , , D1L1, );

--P2L8 is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|counter_cella2~COUT at LC_X20_Y8_N7
--operation mode is arithmetic

P2L8_cout_0 = P2_safe_q[2] & !P2L5;
P2L8 = CARRY(P2L8_cout_0);

--P2L9 is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X20_Y8_N7
--operation mode is arithmetic

P2L9_cout_1 = P2_safe_q[2] & !P2L6;
P2L9 = CARRY(P2L9_cout_1);


--D1L72 is counter55:inst2|always0~42 at LC_X19_Y8_N2
--operation mode is normal

D1L72 = P2_safe_q[3] # Q1_safe_q[1] # !P2_safe_q[2] # !Q1_safe_q[0];


--Q1_safe_q[2] is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|safe_q[2] at LC_X19_Y8_N7
--operation mode is arithmetic

Q1_safe_q[2]_lut_out = Q1_safe_q[2] $ (!Q1L5);
Q1_safe_q[2] = DFFEAS(Q1_safe_q[2]_lut_out, GLOBAL(K1_clk_out), VCC, , D1L1, , , D1L3, );

--Q1L8 is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|counter_cella2~COUT at LC_X19_Y8_N7
--operation mode is arithmetic

Q1L8_cout_0 = Q1_safe_q[2] & !Q1L5;
Q1L8 = CARRY(Q1L8_cout_0);

--Q1L9 is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X19_Y8_N7
--operation mode is arithmetic

Q1L9_cout_1 = Q1_safe_q[2] & !Q1L6;
Q1L9 = CARRY(Q1L9_cout_1);


--D1L82 is counter55:inst2|always0~43 at LC_X20_Y8_N9
--operation mode is normal

D1L82 = !P2_safe_q[1] & P2_safe_q[0];


--D1L62 is counter55:inst2|always0~1 at LC_X19_Y8_N3
--operation mode is normal

D1L62 = Q1_safe_q[3] # D1L72 # !D1L82 # !Q1_safe_q[2];


--D1L92 is counter55:inst2|reduce_or~31 at LC_X19_Y8_N9
--operation mode is normal

D1L92 = !P2_safe_q[1] & P2_safe_q[0] & !P2_safe_q[2] & P2_safe_q[3];


--D1L2 is counter55:inst2|CData0[0]~64 at LC_X19_Y6_N2
--operation mode is normal

D1L2 = Reset & !B1_sdata[0];


--C1L3 is counter05:inst1|reduce_or~28 at LC_X20_Y8_N3
--operation mode is normal

C1L3 = P1_safe_q[0] & !P1_safe_q[3] & !P1_safe_q[1] & P1_safe_q[2];


--C1L1 is counter05:inst1|CData0[0]~16 at LC_X20_Y8_N0
--operation mode is normal

C1L1 = C1L3 # !Reset # !B1_sdata[0];


--D1L6 is counter55:inst2|add~158 at LC_X20_Y7_N1
--operation mode is arithmetic

D1L6_cout_0 = !P2_safe_q[1];
D1L6 = CARRY(D1L6_cout_0);

--D1L8 is counter55:inst2|add~158COUT1_192 at LC_X20_Y7_N1
--operation mode is arithmetic

D1L8_cout_1 = !P2_safe_q[1];
D1L8 = CARRY(D1L8_cout_1);


--Q1L51 is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|safe_q[2]~88 at LC_X19_Y8_N0
--operation mode is normal

Q1L51 = Q1_safe_q[2] & !Q1_safe_q[0] & !Q1_safe_q[3] & Q1_safe_q[1];


--R2_safe_q[31] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[31] at LC_X7_Y10_N5
--operation mode is normal

R2_safe_q[31]_carry_eqn = R2L68;
R2_safe_q[31]_lut_out = R2_safe_q[31]_carry_eqn $ R2_safe_q[31];
R2_safe_q[31] = DFFEAS(R2_safe_q[31]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );


--R2_safe_q[9] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[9] at LC_X7_Y12_N3
--operation mode is arithmetic

R2_safe_q[9]_carry_eqn = (!R2L61 & R2L42) # (R2L61 & R2L52);
R2_safe_q[9]_lut_out = R2_safe_q[9] $ R2_safe_q[9]_carry_eqn;
R2_safe_q[9] = DFFEAS(R2_safe_q[9]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L72 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella9~COUT at LC_X7_Y12_N3
--operation mode is arithmetic

R2L72_cout_0 = !R2L42 # !R2_safe_q[9];
R2L72 = CARRY(R2L72_cout_0);

--R2L82 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella9~COUTCOUT1_1 at LC_X7_Y12_N3
--operation mode is arithmetic

R2L82_cout_1 = !R2L52 # !R2_safe_q[9];
R2L82 = CARRY(R2L82_cout_1);


--R2_safe_q[10] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[10] at LC_X7_Y12_N4
--operation mode is arithmetic

R2_safe_q[10]_carry_eqn = (!R2L61 & R2L72) # (R2L61 & R2L82);
R2_safe_q[10]_lut_out = R2_safe_q[10] $ !R2_safe_q[10]_carry_eqn;
R2_safe_q[10] = DFFEAS(R2_safe_q[10]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L03 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella10~COUT at LC_X7_Y12_N4
--operation mode is arithmetic

R2L03 = CARRY(R2_safe_q[10] & !R2L82);


--L1L2 is fdiv1khz:inst12|LessThan~471 at LC_X6_Y10_N2
--operation mode is normal

L1L2 = !R2_safe_q[10] # !R2_safe_q[9];


--R2_safe_q[0] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[0] at LC_X7_Y13_N4
--operation mode is arithmetic

R2_safe_q[0]_lut_out = !R2_safe_q[0];
R2_safe_q[0] = DFFEAS(R2_safe_q[0]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L2 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella0~COUT at LC_X7_Y13_N4
--operation mode is arithmetic

R2L2 = CARRY(R2_safe_q[0]);


--R2_safe_q[1] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[1] at LC_X7_Y13_N5
--operation mode is arithmetic

R2_safe_q[1]_carry_eqn = R2L2;
R2_safe_q[1]_lut_out = R2_safe_q[1] $ R2_safe_q[1]_carry_eqn;
R2_safe_q[1] = DFFEAS(R2_safe_q[1]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L4 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella1~COUT at LC_X7_Y13_N5
--operation mode is arithmetic

R2L4_cout_0 = !R2L2 # !R2_safe_q[1];
R2L4 = CARRY(R2L4_cout_0);

--R2L5 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella1~COUTCOUT1_1 at LC_X7_Y13_N5
--operation mode is arithmetic

R2L5_cout_1 = !R2L2 # !R2_safe_q[1];
R2L5 = CARRY(R2L5_cout_1);


--R2_safe_q[2] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[2] at LC_X7_Y13_N6
--operation mode is arithmetic

R2_safe_q[2]_carry_eqn = (!R2L2 & R2L4) # (R2L2 & R2L5);
R2_safe_q[2]_lut_out = R2_safe_q[2] $ (!R2_safe_q[2]_carry_eqn);
R2_safe_q[2] = DFFEAS(R2_safe_q[2]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L7 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella2~COUT at LC_X7_Y13_N6
--operation mode is arithmetic

R2L7_cout_0 = R2_safe_q[2] & !R2L4;
R2L7 = CARRY(R2L7_cout_0);

--R2L8 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X7_Y13_N6
--operation mode is arithmetic

R2L8_cout_1 = R2_safe_q[2] & !R2L5;
R2L8 = CARRY(R2L8_cout_1);


--R2_safe_q[3] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[3] at LC_X7_Y13_N7
--operation mode is arithmetic

R2_safe_q[3]_carry_eqn = (!R2L2 & R2L7) # (R2L2 & R2L8);
R2_safe_q[3]_lut_out = R2_safe_q[3] $ (R2_safe_q[3]_carry_eqn);
R2_safe_q[3] = DFFEAS(R2_safe_q[3]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L01 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella3~COUT at LC_X7_Y13_N7
--operation mode is arithmetic

R2L01_cout_0 = !R2L7 # !R2_safe_q[3];
R2L01 = CARRY(R2L01_cout_0);

--R2L11 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella3~COUTCOUT1_1 at LC_X7_Y13_N7
--operation mode is arithmetic

R2L11_cout_1 = !R2L8 # !R2_safe_q[3];
R2L11 = CARRY(R2L11_cout_1);


--L1L3 is fdiv1khz:inst12|LessThan~472 at LC_X7_Y13_N3
--operation mode is normal

L1L3 = !R2_safe_q[1] # !R2_safe_q[3] # !R2_safe_q[0] # !R2_safe_q[2];


--R2_safe_q[4] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[4] at LC_X7_Y13_N8
--operation mode is arithmetic

R2_safe_q[4]_carry_eqn = (!R2L2 & R2L01) # (R2L2 & R2L11);
R2_safe_q[4]_lut_out = R2_safe_q[4] $ !R2_safe_q[4]_carry_eqn;
R2_safe_q[4] = DFFEAS(R2_safe_q[4]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L31 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella4~COUT at LC_X7_Y13_N8
--operation mode is arithmetic

R2L31_cout_0 = R2_safe_q[4] & !R2L01;
R2L31 = CARRY(R2L31_cout_0);

--R2L41 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella4~COUTCOUT1_1 at LC_X7_Y13_N8
--operation mode is arithmetic

R2L41_cout_1 = R2_safe_q[4] & !R2L11;
R2L41 = CARRY(R2L41_cout_1);


--R2_safe_q[5] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[5] at LC_X7_Y13_N9
--operation mode is arithmetic

R2_safe_q[5]_carry_eqn = (!R2L2 & R2L31) # (R2L2 & R2L41);
R2_safe_q[5]_lut_out = R2_safe_q[5] $ (R2_safe_q[5]_carry_eqn);
R2_safe_q[5] = DFFEAS(R2_safe_q[5]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L61 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella5~COUT at LC_X7_Y13_N9
--operation mode is arithmetic

R2L61 = CARRY(!R2L41 # !R2_safe_q[5]);


--R2_safe_q[6] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[6] at LC_X7_Y12_N0
--operation mode is arithmetic

R2_safe_q[6]_carry_eqn = R2L61;
R2_safe_q[6]_lut_out = R2_safe_q[6] $ !R2_safe_q[6]_carry_eqn;
R2_safe_q[6] = DFFEAS(R2_safe_q[6]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L81 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella6~COUT at LC_X7_Y12_N0
--operation mode is arithmetic

R2L81_cout_0 = R2_safe_q[6] & !R2L61;
R2L81 = CARRY(R2L81_cout_0);

--R2L91 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella6~COUTCOUT1_1 at LC_X7_Y12_N0
--operation mode is arithmetic

R2L91_cout_1 = R2_safe_q[6] & !R2L61;
R2L91 = CARRY(R2L91_cout_1);


--R2_safe_q[7] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[7] at LC_X7_Y12_N1
--operation mode is arithmetic

R2_safe_q[7]_carry_eqn = (!R2L61 & R2L81) # (R2L61 & R2L91);
R2_safe_q[7]_lut_out = R2_safe_q[7] $ (R2_safe_q[7]_carry_eqn);
R2_safe_q[7] = DFFEAS(R2_safe_q[7]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L12 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella7~COUT at LC_X7_Y12_N1
--operation mode is arithmetic

R2L12_cout_0 = !R2L81 # !R2_safe_q[7];
R2L12 = CARRY(R2L12_cout_0);

--R2L22 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella7~COUTCOUT1_1 at LC_X7_Y12_N1
--operation mode is arithmetic

R2L22_cout_1 = !R2L91 # !R2_safe_q[7];
R2L22 = CARRY(R2L22_cout_1);


--L1L4 is fdiv1khz:inst12|LessThan~473 at LC_X7_Y13_N2
--operation mode is normal

L1L4 = !R2_safe_q[6] & !R2_safe_q[4] & !R2_safe_q[5] & !R2_safe_q[7];


--R2_safe_q[8] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[8] at LC_X7_Y12_N2
--operation mode is arithmetic

R2_safe_q[8]_carry_eqn = (!R2L61 & R2L12) # (R2L61 & R2L22);
R2_safe_q[8]_lut_out = R2_safe_q[8] $ (!R2_safe_q[8]_carry_eqn);
R2_safe_q[8] = DFFEAS(R2_safe_q[8]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L42 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella8~COUT at LC_X7_Y12_N2
--operation mode is arithmetic

R2L42_cout_0 = R2_safe_q[8] & !R2L12;
R2L42 = CARRY(R2L42_cout_0);

--R2L52 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella8~COUTCOUT1_1 at LC_X7_Y12_N2
--operation mode is arithmetic

R2L52_cout_1 = R2_safe_q[8] & !R2L22;
R2L52 = CARRY(R2L52_cout_1);


--L1L5 is fdiv1khz:inst12|LessThan~474 at LC_X7_Y10_N7
--operation mode is normal

L1L5 = L1L2 # L1L3 & L1L4 # !R2_safe_q[8];


--R2_safe_q[11] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[11] at LC_X7_Y12_N5
--operation mode is arithmetic

R2_safe_q[11]_carry_eqn = R2L03;
R2_safe_q[11]_lut_out = R2_safe_q[11] $ R2_safe_q[11]_carry_eqn;
R2_safe_q[11] = DFFEAS(R2_safe_q[11]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L23 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella11~COUT at LC_X7_Y12_N5
--operation mode is arithmetic

R2L23_cout_0 = !R2L03 # !R2_safe_q[11];
R2L23 = CARRY(R2L23_cout_0);

--R2L33 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella11~COUTCOUT1_1 at LC_X7_Y12_N5
--operation mode is arithmetic

R2L33_cout_1 = !R2L03 # !R2_safe_q[11];
R2L33 = CARRY(R2L33_cout_1);


--R2_safe_q[12] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[12] at LC_X7_Y12_N6
--operation mode is arithmetic

R2_safe_q[12]_carry_eqn = (!R2L03 & R2L23) # (R2L03 & R2L33);
R2_safe_q[12]_lut_out = R2_safe_q[12] $ (!R2_safe_q[12]_carry_eqn);
R2_safe_q[12] = DFFEAS(R2_safe_q[12]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L53 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella12~COUT at LC_X7_Y12_N6
--operation mode is arithmetic

R2L53_cout_0 = R2_safe_q[12] & !R2L23;
R2L53 = CARRY(R2L53_cout_0);

--R2L63 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella12~COUTCOUT1_1 at LC_X7_Y12_N6
--operation mode is arithmetic

R2L63_cout_1 = R2_safe_q[12] & !R2L33;
R2L63 = CARRY(R2L63_cout_1);


--R2_safe_q[13] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[13] at LC_X7_Y12_N7
--operation mode is arithmetic

R2_safe_q[13]_carry_eqn = (!R2L03 & R2L53) # (R2L03 & R2L63);
R2_safe_q[13]_lut_out = R2_safe_q[13] $ (R2_safe_q[13]_carry_eqn);
R2_safe_q[13] = DFFEAS(R2_safe_q[13]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L83 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella13~COUT at LC_X7_Y12_N7
--operation mode is arithmetic

R2L83_cout_0 = !R2L53 # !R2_safe_q[13];
R2L83 = CARRY(R2L83_cout_0);

--R2L93 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella13~COUTCOUT1_1 at LC_X7_Y12_N7
--operation mode is arithmetic

R2L93_cout_1 = !R2L63 # !R2_safe_q[13];
R2L93 = CARRY(R2L93_cout_1);


--L1L6 is fdiv1khz:inst12|LessThan~475 at LC_X7_Y10_N8
--operation mode is normal

L1L6 = L1L5 & !R2_safe_q[12] & !R2_safe_q[11] # !R2_safe_q[13];


--R2_safe_q[14] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[14] at LC_X7_Y12_N8
--operation mode is arithmetic

R2_safe_q[14]_carry_eqn = (!R2L03 & R2L83) # (R2L03 & R2L93);
R2_safe_q[14]_lut_out = R2_safe_q[14] $ !R2_safe_q[14]_carry_eqn;
R2_safe_q[14] = DFFEAS(R2_safe_q[14]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L14 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella14~COUT at LC_X7_Y12_N8
--operation mode is arithmetic

R2L14_cout_0 = R2_safe_q[14] & !R2L83;
R2L14 = CARRY(R2L14_cout_0);

--R2L24 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella14~COUTCOUT1_1 at LC_X7_Y12_N8
--operation mode is arithmetic

R2L24_cout_1 = R2_safe_q[14] & !R2L93;
R2L24 = CARRY(R2L24_cout_1);


--R2_safe_q[15] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[15] at LC_X7_Y12_N9
--operation mode is arithmetic

R2_safe_q[15]_carry_eqn = (!R2L03 & R2L14) # (R2L03 & R2L24);
R2_safe_q[15]_lut_out = R2_safe_q[15] $ (R2_safe_q[15]_carry_eqn);
R2_safe_q[15] = DFFEAS(R2_safe_q[15]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L44 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella15~COUT at LC_X7_Y12_N9
--operation mode is arithmetic

R2L44 = CARRY(!R2L24 # !R2_safe_q[15]);


--R2_safe_q[16] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[16] at LC_X7_Y11_N0
--operation mode is arithmetic

R2_safe_q[16]_carry_eqn = R2L44;
R2_safe_q[16]_lut_out = R2_safe_q[16] $ !R2_safe_q[16]_carry_eqn;
R2_safe_q[16] = DFFEAS(R2_safe_q[16]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L64 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella16~COUT at LC_X7_Y11_N0
--operation mode is arithmetic

R2L64_cout_0 = R2_safe_q[16] & !R2L44;
R2L64 = CARRY(R2L64_cout_0);

--R2L74 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella16~COUTCOUT1_1 at LC_X7_Y11_N0
--operation mode is arithmetic

R2L74_cout_1 = R2_safe_q[16] & !R2L44;
R2L74 = CARRY(R2L74_cout_1);


--R2_safe_q[17] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[17] at LC_X7_Y11_N1
--operation mode is arithmetic

R2_safe_q[17]_carry_eqn = (!R2L44 & R2L64) # (R2L44 & R2L74);
R2_safe_q[17]_lut_out = R2_safe_q[17] $ (R2_safe_q[17]_carry_eqn);
R2_safe_q[17] = DFFEAS(R2_safe_q[17]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L94 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella17~COUT at LC_X7_Y11_N1
--operation mode is arithmetic

R2L94_cout_0 = !R2L64 # !R2_safe_q[17];
R2L94 = CARRY(R2L94_cout_0);

--R2L05 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella17~COUTCOUT1_1 at LC_X7_Y11_N1
--operation mode is arithmetic

R2L05_cout_1 = !R2L74 # !R2_safe_q[17];
R2L05 = CARRY(R2L05_cout_1);


--L1L7 is fdiv1khz:inst12|LessThan~476 at LC_X6_Y12_N2
--operation mode is normal

L1L7 = !R2_safe_q[14] & !R2_safe_q[15] & !R2_safe_q[17] & !R2_safe_q[16];


--R2_safe_q[18] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[18] at LC_X7_Y11_N2
--operation mode is arithmetic

R2_safe_q[18]_carry_eqn = (!R2L44 & R2L94) # (R2L44 & R2L05);
R2_safe_q[18]_lut_out = R2_safe_q[18] $ (!R2_safe_q[18]_carry_eqn);
R2_safe_q[18] = DFFEAS(R2_safe_q[18]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L25 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella18~COUT at LC_X7_Y11_N2
--operation mode is arithmetic

R2L25_cout_0 = R2_safe_q[18] & !R2L94;
R2L25 = CARRY(R2L25_cout_0);

--R2L35 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella18~COUTCOUT1_1 at LC_X7_Y11_N2
--operation mode is arithmetic

R2L35_cout_1 = R2_safe_q[18] & !R2L05;
R2L35 = CARRY(R2L35_cout_1);


--R2_safe_q[19] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[19] at LC_X7_Y11_N3
--operation mode is arithmetic

R2_safe_q[19]_carry_eqn = (!R2L44 & R2L25) # (R2L44 & R2L35);
R2_safe_q[19]_lut_out = R2_safe_q[19] $ R2_safe_q[19]_carry_eqn;
R2_safe_q[19] = DFFEAS(R2_safe_q[19]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L55 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella19~COUT at LC_X7_Y11_N3
--operation mode is arithmetic

R2L55_cout_0 = !R2L25 # !R2_safe_q[19];
R2L55 = CARRY(R2L55_cout_0);

--R2L65 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella19~COUTCOUT1_1 at LC_X7_Y11_N3
--operation mode is arithmetic

R2L65_cout_1 = !R2L35 # !R2_safe_q[19];
R2L65 = CARRY(R2L65_cout_1);


--R2_safe_q[20] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[20] at LC_X7_Y11_N4
--operation mode is arithmetic

R2_safe_q[20]_carry_eqn = (!R2L44 & R2L55) # (R2L44 & R2L65);
R2_safe_q[20]_lut_out = R2_safe_q[20] $ !R2_safe_q[20]_carry_eqn;
R2_safe_q[20] = DFFEAS(R2_safe_q[20]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L85 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella20~COUT at LC_X7_Y11_N4
--operation mode is arithmetic

R2L85 = CARRY(R2_safe_q[20] & !R2L65);


--R2_safe_q[21] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[21] at LC_X7_Y11_N5
--operation mode is arithmetic

R2_safe_q[21]_carry_eqn = R2L85;
R2_safe_q[21]_lut_out = R2_safe_q[21] $ R2_safe_q[21]_carry_eqn;
R2_safe_q[21] = DFFEAS(R2_safe_q[21]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L06 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella21~COUT at LC_X7_Y11_N5
--operation mode is arithmetic

R2L06_cout_0 = !R2L85 # !R2_safe_q[21];
R2L06 = CARRY(R2L06_cout_0);

--R2L16 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella21~COUTCOUT1_1 at LC_X7_Y11_N5
--operation mode is arithmetic

R2L16_cout_1 = !R2L85 # !R2_safe_q[21];
R2L16 = CARRY(R2L16_cout_1);


--L1L8 is fdiv1khz:inst12|LessThan~477 at LC_X6_Y11_N2
--operation mode is normal

L1L8 = !R2_safe_q[18] & !R2_safe_q[20] & !R2_safe_q[21] & !R2_safe_q[19];


--R2_safe_q[22] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[22] at LC_X7_Y11_N6
--operation mode is arithmetic

R2_safe_q[22]_carry_eqn = (!R2L85 & R2L06) # (R2L85 & R2L16);
R2_safe_q[22]_lut_out = R2_safe_q[22] $ (!R2_safe_q[22]_carry_eqn);
R2_safe_q[22] = DFFEAS(R2_safe_q[22]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L36 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella22~COUT at LC_X7_Y11_N6
--operation mode is arithmetic

R2L36_cout_0 = R2_safe_q[22] & !R2L06;
R2L36 = CARRY(R2L36_cout_0);

--R2L46 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella22~COUTCOUT1_1 at LC_X7_Y11_N6
--operation mode is arithmetic

R2L46_cout_1 = R2_safe_q[22] & !R2L16;
R2L46 = CARRY(R2L46_cout_1);


--R2_safe_q[23] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[23] at LC_X7_Y11_N7
--operation mode is arithmetic

R2_safe_q[23]_carry_eqn = (!R2L85 & R2L36) # (R2L85 & R2L46);
R2_safe_q[23]_lut_out = R2_safe_q[23] $ (R2_safe_q[23]_carry_eqn);
R2_safe_q[23] = DFFEAS(R2_safe_q[23]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L66 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella23~COUT at LC_X7_Y11_N7
--operation mode is arithmetic

R2L66_cout_0 = !R2L36 # !R2_safe_q[23];
R2L66 = CARRY(R2L66_cout_0);

--R2L76 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella23~COUTCOUT1_1 at LC_X7_Y11_N7
--operation mode is arithmetic

R2L76_cout_1 = !R2L46 # !R2_safe_q[23];
R2L76 = CARRY(R2L76_cout_1);


--R2_safe_q[24] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[24] at LC_X7_Y11_N8
--operation mode is arithmetic

R2_safe_q[24]_carry_eqn = (!R2L85 & R2L66) # (R2L85 & R2L76);
R2_safe_q[24]_lut_out = R2_safe_q[24] $ !R2_safe_q[24]_carry_eqn;
R2_safe_q[24] = DFFEAS(R2_safe_q[24]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L96 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella24~COUT at LC_X7_Y11_N8
--operation mode is arithmetic

R2L96_cout_0 = R2_safe_q[24] & !R2L66;
R2L96 = CARRY(R2L96_cout_0);

--R2L07 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella24~COUTCOUT1_1 at LC_X7_Y11_N8
--operation mode is arithmetic

R2L07_cout_1 = R2_safe_q[24] & !R2L76;
R2L07 = CARRY(R2L07_cout_1);


--R2_safe_q[25] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[25] at LC_X7_Y11_N9
--operation mode is arithmetic

R2_safe_q[25]_carry_eqn = (!R2L85 & R2L96) # (R2L85 & R2L07);
R2_safe_q[25]_lut_out = R2_safe_q[25] $ (R2_safe_q[25]_carry_eqn);
R2_safe_q[25] = DFFEAS(R2_safe_q[25]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L27 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella25~COUT at LC_X7_Y11_N9
--operation mode is arithmetic

R2L27 = CARRY(!R2L07 # !R2_safe_q[25]);


--L1L9 is fdiv1khz:inst12|LessThan~478 at LC_X8_Y11_N2
--operation mode is normal

L1L9 = !R2_safe_q[22] & !R2_safe_q[23] & !R2_safe_q[24] & !R2_safe_q[25];


--R2_safe_q[26] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[26] at LC_X7_Y10_N0
--operation mode is arithmetic

R2_safe_q[26]_carry_eqn = R2L27;
R2_safe_q[26]_lut_out = R2_safe_q[26] $ !R2_safe_q[26]_carry_eqn;
R2_safe_q[26] = DFFEAS(R2_safe_q[26]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L47 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella26~COUT at LC_X7_Y10_N0
--operation mode is arithmetic

R2L47_cout_0 = R2_safe_q[26] & !R2L27;
R2L47 = CARRY(R2L47_cout_0);

--R2L57 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella26~COUTCOUT1_1 at LC_X7_Y10_N0
--operation mode is arithmetic

R2L57_cout_1 = R2_safe_q[26] & !R2L27;
R2L57 = CARRY(R2L57_cout_1);


--R2_safe_q[27] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[27] at LC_X7_Y10_N1
--operation mode is arithmetic

R2_safe_q[27]_carry_eqn = (!R2L27 & R2L47) # (R2L27 & R2L57);
R2_safe_q[27]_lut_out = R2_safe_q[27] $ (R2_safe_q[27]_carry_eqn);
R2_safe_q[27] = DFFEAS(R2_safe_q[27]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L77 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella27~COUT at LC_X7_Y10_N1
--operation mode is arithmetic

R2L77_cout_0 = !R2L47 # !R2_safe_q[27];
R2L77 = CARRY(R2L77_cout_0);

--R2L87 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella27~COUTCOUT1_1 at LC_X7_Y10_N1
--operation mode is arithmetic

R2L87_cout_1 = !R2L57 # !R2_safe_q[27];
R2L87 = CARRY(R2L87_cout_1);


--R2_safe_q[28] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[28] at LC_X7_Y10_N2
--operation mode is arithmetic

R2_safe_q[28]_carry_eqn = (!R2L27 & R2L77) # (R2L27 & R2L87);
R2_safe_q[28]_lut_out = R2_safe_q[28] $ (!R2_safe_q[28]_carry_eqn);
R2_safe_q[28] = DFFEAS(R2_safe_q[28]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L08 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella28~COUT at LC_X7_Y10_N2
--operation mode is arithmetic

R2L08_cout_0 = R2_safe_q[28] & !R2L77;
R2L08 = CARRY(R2L08_cout_0);

--R2L18 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella28~COUTCOUT1_1 at LC_X7_Y10_N2
--operation mode is arithmetic

R2L18_cout_1 = R2_safe_q[28] & !R2L87;
R2L18 = CARRY(R2L18_cout_1);


--R2_safe_q[29] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[29] at LC_X7_Y10_N3
--operation mode is arithmetic

R2_safe_q[29]_carry_eqn = (!R2L27 & R2L08) # (R2L27 & R2L18);
R2_safe_q[29]_lut_out = R2_safe_q[29] $ R2_safe_q[29]_carry_eqn;
R2_safe_q[29] = DFFEAS(R2_safe_q[29]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L38 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella29~COUT at LC_X7_Y10_N3
--operation mode is arithmetic

R2L38_cout_0 = !R2L08 # !R2_safe_q[29];
R2L38 = CARRY(R2L38_cout_0);

--R2L48 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella29~COUTCOUT1_1 at LC_X7_Y10_N3
--operation mode is arithmetic

R2L48_cout_1 = !R2L18 # !R2_safe_q[29];
R2L48 = CARRY(R2L48_cout_1);


--L1L01 is fdiv1khz:inst12|LessThan~479 at LC_X8_Y10_N2
--operation mode is normal

L1L01 = !R2_safe_q[27] & !R2_safe_q[26] & !R2_safe_q[29] & !R2_safe_q[28];


--L1L11 is fdiv1khz:inst12|LessThan~480 at LC_X7_Y10_N9
--operation mode is normal

L1L11 = L1L9 & L1L7 & L1L01 & L1L8;


--R2_safe_q[30] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[30] at LC_X7_Y10_N4
--operation mode is arithmetic

R2_safe_q[30]_carry_eqn = (!R2L27 & R2L38) # (R2L27 & R2L48);
R2_safe_q[30]_lut_out = R2_safe_q[30] $ !R2_safe_q[30]_carry_eqn;
R2_safe_q[30] = DFFEAS(R2_safe_q[30]_lut_out, GLOBAL(CLK), VCC, , , , , L1L1, );

--R2L68 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella30~COUT at LC_X7_Y10_N4
--operation mode is arithmetic

R2L68 = CARRY(R2_safe_q[30] & !R2L48);


--L1L1 is fdiv1khz:inst12|LessThan~256 at LC_X7_Y10_N6
--operation mode is normal

L1L1 = !R2_safe_q[31] & R2_safe_q[30] # !L1L6 # !L1L11;

--L1_clk_out is fdiv1khz:inst12|clk_out at LC_X7_Y10_N6
--operation mode is normal

L1_clk_out = DFFEAS(L1L1, GLOBAL(CLK), VCC, , , , , , );


--R1_safe_q[31] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[31] at LC_X10_Y6_N5
--operation mode is normal

R1_safe_q[31]_carry_eqn = R1L68;
R1_safe_q[31]_lut_out = R1_safe_q[31]_carry_eqn $ R1_safe_q[31];
R1_safe_q[31] = DFFEAS(R1_safe_q[31]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );


--R1_safe_q[5] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[5] at LC_X10_Y9_N9
--operation mode is arithmetic

R1_safe_q[5]_carry_eqn = (!R1L2 & R1L31) # (R1L2 & R1L41);
R1_safe_q[5]_lut_out = R1_safe_q[5] $ (R1_safe_q[5]_carry_eqn);
R1_safe_q[5] = DFFEAS(R1_safe_q[5]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L61 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella5~COUT at LC_X10_Y9_N9
--operation mode is arithmetic

R1L61 = CARRY(!R1L41 # !R1_safe_q[5]);


--R1_safe_q[6] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[6] at LC_X10_Y8_N0
--operation mode is arithmetic

R1_safe_q[6]_carry_eqn = R1L61;
R1_safe_q[6]_lut_out = R1_safe_q[6] $ !R1_safe_q[6]_carry_eqn;
R1_safe_q[6] = DFFEAS(R1_safe_q[6]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L81 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella6~COUT at LC_X10_Y8_N0
--operation mode is arithmetic

R1L81_cout_0 = R1_safe_q[6] & !R1L61;
R1L81 = CARRY(R1L81_cout_0);

--R1L91 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella6~COUTCOUT1_1 at LC_X10_Y8_N0
--operation mode is arithmetic

R1L91_cout_1 = R1_safe_q[6] & !R1L61;
R1L91 = CARRY(R1L91_cout_1);


--R1_safe_q[7] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[7] at LC_X10_Y8_N1
--operation mode is arithmetic

R1_safe_q[7]_carry_eqn = (!R1L61 & R1L81) # (R1L61 & R1L91);
R1_safe_q[7]_lut_out = R1_safe_q[7] $ (R1_safe_q[7]_carry_eqn);
R1_safe_q[7] = DFFEAS(R1_safe_q[7]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L12 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella7~COUT at LC_X10_Y8_N1
--operation mode is arithmetic

R1L12_cout_0 = !R1L81 # !R1_safe_q[7];
R1L12 = CARRY(R1L12_cout_0);

--R1L22 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella7~COUTCOUT1_1 at LC_X10_Y8_N1
--operation mode is arithmetic

R1L22_cout_1 = !R1L91 # !R1_safe_q[7];
R1L22 = CARRY(R1L22_cout_1);


--R1_safe_q[8] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[8] at LC_X10_Y8_N2
--operation mode is arithmetic

R1_safe_q[8]_carry_eqn = (!R1L61 & R1L12) # (R1L61 & R1L22);
R1_safe_q[8]_lut_out = R1_safe_q[8] $ (!R1_safe_q[8]_carry_eqn);
R1_safe_q[8] = DFFEAS(R1_safe_q[8]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L42 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella8~COUT at LC_X10_Y8_N2
--operation mode is arithmetic

R1L42_cout_0 = R1_safe_q[8] & !R1L12;
R1L42 = CARRY(R1L42_cout_0);

--R1L52 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella8~COUTCOUT1_1 at LC_X10_Y8_N2
--operation mode is arithmetic

R1L52_cout_1 = R1_safe_q[8] & !R1L22;
R1L52 = CARRY(R1L52_cout_1);


--K1L2 is fdiv1hz:inst11|LessThan~500 at LC_X10_Y9_N2
--operation mode is normal

K1L2 = !R1_safe_q[6] # !R1_safe_q[7] # !R1_safe_q[8] # !R1_safe_q[5];


--R1_safe_q[0] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[0] at LC_X10_Y9_N4
--operation mode is arithmetic

R1_safe_q[0]_lut_out = !R1_safe_q[0];
R1_safe_q[0] = DFFEAS(R1_safe_q[0]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L2 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella0~COUT at LC_X10_Y9_N4
--operation mode is arithmetic

R1L2 = CARRY(R1_safe_q[0]);


--R1_safe_q[1] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[1] at LC_X10_Y9_N5
--operation mode is arithmetic

R1_safe_q[1]_carry_eqn = R1L2;
R1_safe_q[1]_lut_out = R1_safe_q[1] $ R1_safe_q[1]_carry_eqn;
R1_safe_q[1] = DFFEAS(R1_safe_q[1]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L4 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella1~COUT at LC_X10_Y9_N5
--operation mode is arithmetic

R1L4_cout_0 = !R1L2 # !R1_safe_q[1];
R1L4 = CARRY(R1L4_cout_0);

--R1L5 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella1~COUTCOUT1_1 at LC_X10_Y9_N5
--operation mode is arithmetic

R1L5_cout_1 = !R1L2 # !R1_safe_q[1];
R1L5 = CARRY(R1L5_cout_1);


--R1_safe_q[2] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[2] at LC_X10_Y9_N6
--operation mode is arithmetic

R1_safe_q[2]_carry_eqn = (!R1L2 & R1L4) # (R1L2 & R1L5);
R1_safe_q[2]_lut_out = R1_safe_q[2] $ (!R1_safe_q[2]_carry_eqn);
R1_safe_q[2] = DFFEAS(R1_safe_q[2]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L7 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella2~COUT at LC_X10_Y9_N6
--operation mode is arithmetic

R1L7_cout_0 = R1_safe_q[2] & !R1L4;
R1L7 = CARRY(R1L7_cout_0);

--R1L8 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella2~COUTCOUT1_1 at LC_X10_Y9_N6
--operation mode is arithmetic

R1L8_cout_1 = R1_safe_q[2] & !R1L5;
R1L8 = CARRY(R1L8_cout_1);


--R1_safe_q[3] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[3] at LC_X10_Y9_N7
--operation mode is arithmetic

R1_safe_q[3]_carry_eqn = (!R1L2 & R1L7) # (R1L2 & R1L8);
R1_safe_q[3]_lut_out = R1_safe_q[3] $ (R1_safe_q[3]_carry_eqn);
R1_safe_q[3] = DFFEAS(R1_safe_q[3]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L01 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella3~COUT at LC_X10_Y9_N7
--operation mode is arithmetic

R1L01_cout_0 = !R1L7 # !R1_safe_q[3];
R1L01 = CARRY(R1L01_cout_0);

--R1L11 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella3~COUTCOUT1_1 at LC_X10_Y9_N7
--operation mode is arithmetic

R1L11_cout_1 = !R1L8 # !R1_safe_q[3];
R1L11 = CARRY(R1L11_cout_1);


--K1L3 is fdiv1hz:inst11|LessThan~501 at LC_X10_Y9_N3
--operation mode is normal

K1L3 = !R1_safe_q[3] & !R1_safe_q[2] # !R1_safe_q[0] # !R1_safe_q[1];


--R1_safe_q[4] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[4] at LC_X10_Y9_N8
--operation mode is arithmetic

R1_safe_q[4]_carry_eqn = (!R1L2 & R1L01) # (R1L2 & R1L11);
R1_safe_q[4]_lut_out = R1_safe_q[4] $ !R1_safe_q[4]_carry_eqn;
R1_safe_q[4] = DFFEAS(R1_safe_q[4]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L31 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella4~COUT at LC_X10_Y9_N8
--operation mode is arithmetic

R1L31_cout_0 = R1_safe_q[4] & !R1L01;
R1L31 = CARRY(R1L31_cout_0);

--R1L41 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella4~COUTCOUT1_1 at LC_X10_Y9_N8
--operation mode is arithmetic

R1L41_cout_1 = R1_safe_q[4] & !R1L11;
R1L41 = CARRY(R1L41_cout_1);


--R1_safe_q[9] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[9] at LC_X10_Y8_N3
--operation mode is arithmetic

R1_safe_q[9]_carry_eqn = (!R1L61 & R1L42) # (R1L61 & R1L52);
R1_safe_q[9]_lut_out = R1_safe_q[9] $ R1_safe_q[9]_carry_eqn;
R1_safe_q[9] = DFFEAS(R1_safe_q[9]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L72 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella9~COUT at LC_X10_Y8_N3
--operation mode is arithmetic

R1L72_cout_0 = !R1L42 # !R1_safe_q[9];
R1L72 = CARRY(R1L72_cout_0);

--R1L82 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella9~COUTCOUT1_1 at LC_X10_Y8_N3
--operation mode is arithmetic

R1L82_cout_1 = !R1L52 # !R1_safe_q[9];
R1L82 = CARRY(R1L82_cout_1);


--K1L4 is fdiv1hz:inst11|LessThan~502 at LC_X10_Y6_N7
--operation mode is normal

K1L4 = K1L2 # !R1_safe_q[4] & K1L3 # !R1_safe_q[9];


--R1_safe_q[10] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[10] at LC_X10_Y8_N4
--operation mode is arithmetic

R1_safe_q[10]_carry_eqn = (!R1L61 & R1L72) # (R1L61 & R1L82);
R1_safe_q[10]_lut_out = R1_safe_q[10] $ !R1_safe_q[10]_carry_eqn;
R1_safe_q[10] = DFFEAS(R1_safe_q[10]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L03 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella10~COUT at LC_X10_Y8_N4
--operation mode is arithmetic

R1L03 = CARRY(R1_safe_q[10] & !R1L82);


--R1_safe_q[11] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[11] at LC_X10_Y8_N5
--operation mode is arithmetic

R1_safe_q[11]_carry_eqn = R1L03;
R1_safe_q[11]_lut_out = R1_safe_q[11] $ R1_safe_q[11]_carry_eqn;
R1_safe_q[11] = DFFEAS(R1_safe_q[11]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L23 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella11~COUT at LC_X10_Y8_N5
--operation mode is arithmetic

R1L23_cout_0 = !R1L03 # !R1_safe_q[11];
R1L23 = CARRY(R1L23_cout_0);

--R1L33 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella11~COUTCOUT1_1 at LC_X10_Y8_N5
--operation mode is arithmetic

R1L33_cout_1 = !R1L03 # !R1_safe_q[11];
R1L33 = CARRY(R1L33_cout_1);


--R1_safe_q[12] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[12] at LC_X10_Y8_N6
--operation mode is arithmetic

R1_safe_q[12]_carry_eqn = (!R1L03 & R1L23) # (R1L03 & R1L33);
R1_safe_q[12]_lut_out = R1_safe_q[12] $ (!R1_safe_q[12]_carry_eqn);
R1_safe_q[12] = DFFEAS(R1_safe_q[12]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L53 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella12~COUT at LC_X10_Y8_N6
--operation mode is arithmetic

R1L53_cout_0 = R1_safe_q[12] & !R1L23;
R1L53 = CARRY(R1L53_cout_0);

--R1L63 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella12~COUTCOUT1_1 at LC_X10_Y8_N6
--operation mode is arithmetic

R1L63_cout_1 = R1_safe_q[12] & !R1L33;
R1L63 = CARRY(R1L63_cout_1);


--R1_safe_q[13] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[13] at LC_X10_Y8_N7
--operation mode is arithmetic

R1_safe_q[13]_carry_eqn = (!R1L03 & R1L53) # (R1L03 & R1L63);
R1_safe_q[13]_lut_out = R1_safe_q[13] $ (R1_safe_q[13]_carry_eqn);
R1_safe_q[13] = DFFEAS(R1_safe_q[13]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L83 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella13~COUT at LC_X10_Y8_N7
--operation mode is arithmetic

R1L83_cout_0 = !R1L53 # !R1_safe_q[13];
R1L83 = CARRY(R1L83_cout_0);

--R1L93 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella13~COUTCOUT1_1 at LC_X10_Y8_N7
--operation mode is arithmetic

R1L93_cout_1 = !R1L63 # !R1_safe_q[13];
R1L93 = CARRY(R1L93_cout_1);


--K1L5 is fdiv1hz:inst11|LessThan~503 at LC_X9_Y8_N2
--operation mode is normal

K1L5 = !R1_safe_q[13] & !R1_safe_q[10] & !R1_safe_q[11] & !R1_safe_q[12];


--R1_safe_q[14] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[14] at LC_X10_Y8_N8
--operation mode is arithmetic

R1_safe_q[14]_carry_eqn = (!R1L03 & R1L83) # (R1L03 & R1L93);
R1_safe_q[14]_lut_out = R1_safe_q[14] $ !R1_safe_q[14]_carry_eqn;
R1_safe_q[14] = DFFEAS(R1_safe_q[14]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L14 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella14~COUT at LC_X10_Y8_N8
--operation mode is arithmetic

R1L14_cout_0 = R1_safe_q[14] & !R1L83;
R1L14 = CARRY(R1L14_cout_0);

--R1L24 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella14~COUTCOUT1_1 at LC_X10_Y8_N8
--operation mode is arithmetic

R1L24_cout_1 = R1_safe_q[14] & !R1L93;
R1L24 = CARRY(R1L24_cout_1);


--R1_safe_q[15] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[15] at LC_X10_Y8_N9
--operation mode is arithmetic

R1_safe_q[15]_carry_eqn = (!R1L03 & R1L14) # (R1L03 & R1L24);
R1_safe_q[15]_lut_out = R1_safe_q[15] $ (R1_safe_q[15]_carry_eqn);
R1_safe_q[15] = DFFEAS(R1_safe_q[15]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L44 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella15~COUT at LC_X10_Y8_N9
--operation mode is arithmetic

R1L44 = CARRY(!R1L24 # !R1_safe_q[15]);


--R1_safe_q[16] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[16] at LC_X10_Y7_N0
--operation mode is arithmetic

R1_safe_q[16]_carry_eqn = R1L44;
R1_safe_q[16]_lut_out = R1_safe_q[16] $ !R1_safe_q[16]_carry_eqn;
R1_safe_q[16] = DFFEAS(R1_safe_q[16]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L64 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella16~COUT at LC_X10_Y7_N0
--operation mode is arithmetic

R1L64_cout_0 = R1_safe_q[16] & !R1L44;
R1L64 = CARRY(R1L64_cout_0);

--R1L74 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella16~COUTCOUT1_1 at LC_X10_Y7_N0
--operation mode is arithmetic

R1L74_cout_1 = R1_safe_q[16] & !R1L44;
R1L74 = CARRY(R1L74_cout_1);


--R1_safe_q[17] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[17] at LC_X10_Y7_N1
--operation mode is arithmetic

R1_safe_q[17]_carry_eqn = (!R1L44 & R1L64) # (R1L44 & R1L74);
R1_safe_q[17]_lut_out = R1_safe_q[17] $ (R1_safe_q[17]_carry_eqn);
R1_safe_q[17] = DFFEAS(R1_safe_q[17]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L94 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella17~COUT at LC_X10_Y7_N1
--operation mode is arithmetic

R1L94_cout_0 = !R1L64 # !R1_safe_q[17];
R1L94 = CARRY(R1L94_cout_0);

--R1L05 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella17~COUTCOUT1_1 at LC_X10_Y7_N1
--operation mode is arithmetic

R1L05_cout_1 = !R1L74 # !R1_safe_q[17];
R1L05 = CARRY(R1L05_cout_1);


--K1L6 is fdiv1hz:inst11|LessThan~504 at LC_X11_Y8_N2
--operation mode is normal

K1L6 = !R1_safe_q[16] & !R1_safe_q[15] & !R1_safe_q[14] & !R1_safe_q[17];


--R1_safe_q[18] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[18] at LC_X10_Y7_N2
--operation mode is arithmetic

R1_safe_q[18]_carry_eqn = (!R1L44 & R1L94) # (R1L44 & R1L05);
R1_safe_q[18]_lut_out = R1_safe_q[18] $ (!R1_safe_q[18]_carry_eqn);
R1_safe_q[18] = DFFEAS(R1_safe_q[18]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L25 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella18~COUT at LC_X10_Y7_N2
--operation mode is arithmetic

R1L25_cout_0 = R1_safe_q[18] & !R1L94;
R1L25 = CARRY(R1L25_cout_0);

--R1L35 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella18~COUTCOUT1_1 at LC_X10_Y7_N2
--operation mode is arithmetic

R1L35_cout_1 = R1_safe_q[18] & !R1L05;
R1L35 = CARRY(R1L35_cout_1);


--R1_safe_q[19] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[19] at LC_X10_Y7_N3
--operation mode is arithmetic

R1_safe_q[19]_carry_eqn = (!R1L44 & R1L25) # (R1L44 & R1L35);
R1_safe_q[19]_lut_out = R1_safe_q[19] $ R1_safe_q[19]_carry_eqn;
R1_safe_q[19] = DFFEAS(R1_safe_q[19]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L55 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella19~COUT at LC_X10_Y7_N3
--operation mode is arithmetic

R1L55_cout_0 = !R1L25 # !R1_safe_q[19];
R1L55 = CARRY(R1L55_cout_0);

--R1L65 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella19~COUTCOUT1_1 at LC_X10_Y7_N3
--operation mode is arithmetic

R1L65_cout_1 = !R1L35 # !R1_safe_q[19];
R1L65 = CARRY(R1L65_cout_1);


--R1_safe_q[20] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[20] at LC_X10_Y7_N4
--operation mode is arithmetic

R1_safe_q[20]_carry_eqn = (!R1L44 & R1L55) # (R1L44 & R1L65);
R1_safe_q[20]_lut_out = R1_safe_q[20] $ !R1_safe_q[20]_carry_eqn;
R1_safe_q[20] = DFFEAS(R1_safe_q[20]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L85 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella20~COUT at LC_X10_Y7_N4
--operation mode is arithmetic

R1L85 = CARRY(R1_safe_q[20] & !R1L65);


--R1_safe_q[21] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[21] at LC_X10_Y7_N5
--operation mode is arithmetic

R1_safe_q[21]_carry_eqn = R1L85;
R1_safe_q[21]_lut_out = R1_safe_q[21] $ R1_safe_q[21]_carry_eqn;
R1_safe_q[21] = DFFEAS(R1_safe_q[21]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L06 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella21~COUT at LC_X10_Y7_N5
--operation mode is arithmetic

R1L06_cout_0 = !R1L85 # !R1_safe_q[21];
R1L06 = CARRY(R1L06_cout_0);

--R1L16 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella21~COUTCOUT1_1 at LC_X10_Y7_N5
--operation mode is arithmetic

R1L16_cout_1 = !R1L85 # !R1_safe_q[21];
R1L16 = CARRY(R1L16_cout_1);


--K1L7 is fdiv1hz:inst11|LessThan~505 at LC_X9_Y7_N2
--operation mode is normal

K1L7 = !R1_safe_q[18] & !R1_safe_q[20] & !R1_safe_q[21] & !R1_safe_q[19];


--R1_safe_q[22] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[22] at LC_X10_Y7_N6
--operation mode is arithmetic

R1_safe_q[22]_carry_eqn = (!R1L85 & R1L06) # (R1L85 & R1L16);
R1_safe_q[22]_lut_out = R1_safe_q[22] $ (!R1_safe_q[22]_carry_eqn);
R1_safe_q[22] = DFFEAS(R1_safe_q[22]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L36 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella22~COUT at LC_X10_Y7_N6
--operation mode is arithmetic

R1L36_cout_0 = R1_safe_q[22] & !R1L06;
R1L36 = CARRY(R1L36_cout_0);

--R1L46 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella22~COUTCOUT1_1 at LC_X10_Y7_N6
--operation mode is arithmetic

R1L46_cout_1 = R1_safe_q[22] & !R1L16;
R1L46 = CARRY(R1L46_cout_1);


--R1_safe_q[23] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[23] at LC_X10_Y7_N7
--operation mode is arithmetic

R1_safe_q[23]_carry_eqn = (!R1L85 & R1L36) # (R1L85 & R1L46);
R1_safe_q[23]_lut_out = R1_safe_q[23] $ (R1_safe_q[23]_carry_eqn);
R1_safe_q[23] = DFFEAS(R1_safe_q[23]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L66 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella23~COUT at LC_X10_Y7_N7
--operation mode is arithmetic

R1L66_cout_0 = !R1L36 # !R1_safe_q[23];
R1L66 = CARRY(R1L66_cout_0);

--R1L76 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella23~COUTCOUT1_1 at LC_X10_Y7_N7
--operation mode is arithmetic

R1L76_cout_1 = !R1L46 # !R1_safe_q[23];
R1L76 = CARRY(R1L76_cout_1);


--R1_safe_q[24] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[24] at LC_X10_Y7_N8
--operation mode is arithmetic

R1_safe_q[24]_carry_eqn = (!R1L85 & R1L66) # (R1L85 & R1L76);
R1_safe_q[24]_lut_out = R1_safe_q[24] $ !R1_safe_q[24]_carry_eqn;
R1_safe_q[24] = DFFEAS(R1_safe_q[24]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L96 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella24~COUT at LC_X10_Y7_N8
--operation mode is arithmetic

R1L96_cout_0 = R1_safe_q[24] & !R1L66;
R1L96 = CARRY(R1L96_cout_0);

--R1L07 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella24~COUTCOUT1_1 at LC_X10_Y7_N8
--operation mode is arithmetic

R1L07_cout_1 = R1_safe_q[24] & !R1L76;
R1L07 = CARRY(R1L07_cout_1);


--R1_safe_q[25] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[25] at LC_X10_Y7_N9
--operation mode is arithmetic

R1_safe_q[25]_carry_eqn = (!R1L85 & R1L96) # (R1L85 & R1L07);
R1_safe_q[25]_lut_out = R1_safe_q[25] $ (R1_safe_q[25]_carry_eqn);
R1_safe_q[25] = DFFEAS(R1_safe_q[25]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L27 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella25~COUT at LC_X10_Y7_N9
--operation mode is arithmetic

R1L27 = CARRY(!R1L07 # !R1_safe_q[25]);


--K1L8 is fdiv1hz:inst11|LessThan~506 at LC_X11_Y6_N2
--operation mode is normal

K1L8 = !R1_safe_q[24] & !R1_safe_q[22] & !R1_safe_q[23] & !R1_safe_q[25];


--K1L9 is fdiv1hz:inst11|LessThan~507 at LC_X10_Y6_N9
--operation mode is normal

K1L9 = K1L6 & K1L5 & K1L8 & K1L7;


--R1_safe_q[26] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[26] at LC_X10_Y6_N0
--operation mode is arithmetic

R1_safe_q[26]_carry_eqn = R1L27;
R1_safe_q[26]_lut_out = R1_safe_q[26] $ !R1_safe_q[26]_carry_eqn;
R1_safe_q[26] = DFFEAS(R1_safe_q[26]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L47 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella26~COUT at LC_X10_Y6_N0
--operation mode is arithmetic

R1L47_cout_0 = R1_safe_q[26] & !R1L27;
R1L47 = CARRY(R1L47_cout_0);

--R1L57 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella26~COUTCOUT1_1 at LC_X10_Y6_N0
--operation mode is arithmetic

R1L57_cout_1 = R1_safe_q[26] & !R1L27;
R1L57 = CARRY(R1L57_cout_1);


--R1_safe_q[27] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[27] at LC_X10_Y6_N1
--operation mode is arithmetic

R1_safe_q[27]_carry_eqn = (!R1L27 & R1L47) # (R1L27 & R1L57);
R1_safe_q[27]_lut_out = R1_safe_q[27] $ (R1_safe_q[27]_carry_eqn);
R1_safe_q[27] = DFFEAS(R1_safe_q[27]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L77 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella27~COUT at LC_X10_Y6_N1
--operation mode is arithmetic

R1L77_cout_0 = !R1L47 # !R1_safe_q[27];
R1L77 = CARRY(R1L77_cout_0);

--R1L87 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella27~COUTCOUT1_1 at LC_X10_Y6_N1
--operation mode is arithmetic

R1L87_cout_1 = !R1L57 # !R1_safe_q[27];
R1L87 = CARRY(R1L87_cout_1);


--K1L01 is fdiv1hz:inst11|LessThan~508 at LC_X9_Y6_N6
--operation mode is normal

K1L01 = !R1_safe_q[26] & !R1_safe_q[27];


--R1_safe_q[30] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[30] at LC_X10_Y6_N4
--operation mode is arithmetic

R1_safe_q[30]_carry_eqn = (!R1L27 & R1L38) # (R1L27 & R1L48);
R1_safe_q[30]_lut_out = R1_safe_q[30] $ !R1_safe_q[30]_carry_eqn;
R1_safe_q[30] = DFFEAS(R1_safe_q[30]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L68 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella30~COUT at LC_X10_Y6_N4
--operation mode is arithmetic

R1L68 = CARRY(R1_safe_q[30] & !R1L48);


--R1_safe_q[28] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[28] at LC_X10_Y6_N2
--operation mode is arithmetic

R1_safe_q[28]_carry_eqn = (!R1L27 & R1L77) # (R1L27 & R1L87);
R1_safe_q[28]_lut_out = R1_safe_q[28] $ (!R1_safe_q[28]_carry_eqn);
R1_safe_q[28] = DFFEAS(R1_safe_q[28]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L08 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella28~COUT at LC_X10_Y6_N2
--operation mode is arithmetic

R1L08_cout_0 = R1_safe_q[28] & !R1L77;
R1L08 = CARRY(R1L08_cout_0);

--R1L18 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella28~COUTCOUT1_1 at LC_X10_Y6_N2
--operation mode is arithmetic

R1L18_cout_1 = R1_safe_q[28] & !R1L87;
R1L18 = CARRY(R1L18_cout_1);


--R1_safe_q[29] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[29] at LC_X10_Y6_N3
--operation mode is arithmetic

R1_safe_q[29]_carry_eqn = (!R1L27 & R1L08) # (R1L27 & R1L18);
R1_safe_q[29]_lut_out = R1_safe_q[29] $ R1_safe_q[29]_carry_eqn;
R1_safe_q[29] = DFFEAS(R1_safe_q[29]_lut_out, GLOBAL(L1_clk_out), VCC, , , , , K1L1, );

--R1L38 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella29~COUT at LC_X10_Y6_N3
--operation mode is arithmetic

R1L38_cout_0 = !R1L08 # !R1_safe_q[29];
R1L38 = CARRY(R1L38_cout_0);

--R1L48 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella29~COUTCOUT1_1 at LC_X10_Y6_N3
--operation mode is arithmetic

R1L48_cout_1 = !R1L18 # !R1_safe_q[29];
R1L48 = CARRY(R1L48_cout_1);


--K1L11 is fdiv1hz:inst11|LessThan~509 at LC_X10_Y6_N8
--operation mode is normal

K1L11 = !R1_safe_q[28] & !R1_safe_q[29] & !R1_safe_q[30] & K1L01;


--K1L1 is fdiv1hz:inst11|LessThan~256 at LC_X10_Y6_N6
--operation mode is normal

K1L1 = !R1_safe_q[31] & !K1L11 # !K1L4 # !K1L9;

--K1_clk_out is fdiv1hz:inst11|clk_out at LC_X10_Y6_N6
--operation mode is normal

K1_clk_out = DFFEAS(K1L1, GLOBAL(L1_clk_out), VCC, , , , , , );


--H1L61 is dispmux:inst8|D_OUT[3]~747 at LC_X21_Y8_N8
--operation mode is normal

H1L61 = H1L51 & !H1L21 & B1_sdata[0] # !J1_D_OUT[0] # !H1L51 & B1_sdata[0] # !J1_D_OUT[0];


--D1L1 is counter55:inst2|CData0[0]~21 at LC_X19_Y8_N4
--operation mode is normal

D1L1 = B1_sdata[0] # D1L92 $ !D1L62 # !Reset;


--D1L3 is counter55:inst2|CData1[0]~45 at LC_X19_Y8_N1
--operation mode is normal

D1L3 = B1_sdata[0] # Q1L51 # !D1L92 # !Reset;


--H1L41 is dispmux:inst8|D_OUT[3]~730 at LC_X21_Y9_N9
--operation mode is normal

H1L41 = !B1_sdata[0] & J1_D_OUT[0] & D1L21 $ H1L31;


--Reset is Reset at PIN_84
--operation mode is input

Reset = INPUT();


--SW is SW at PIN_41
--operation mode is input

SW = INPUT();


--CLK is CLK at PIN_10
--operation mode is input

CLK = INPUT();


--Red1 is Red1 at PIN_40
--operation mode is output

Red1 = OUTPUT(M1L3);


--Red2 is Red2 at PIN_65
--operation mode is output

Red2 = OUTPUT(M1L4);


--Yellow1 is Yellow1 at PIN_39
--operation mode is output

Yellow1 = OUTPUT(M1L5);


--Yellow2 is Yellow2 at PIN_42
--operation mode is output

Yellow2 = OUTPUT(M1L6);


--Green1 is Green1 at PIN_38
--operation mode is output

Green1 = OUTPUT(!M1L1);


--Green2 is Green2 at PIN_47
--operation mode is output

Green2 = OUTPUT(M1L2);


--SEG_Data[7] is SEG_Data[7] at PIN_71
--operation mode is output

SEG_Data[7] = OUTPUT(!G1L5);


--SEG_Data[6] is SEG_Data[6] at PIN_85
--operation mode is output

SEG_Data[6] = OUTPUT(!G1L6);


--SEG_Data[5] is SEG_Data[5] at PIN_69
--operation mode is output

SEG_Data[5] = OUTPUT(!G1L7);


--SEG_Data[4] is SEG_Data[4] at PIN_72
--operation mode is output

SEG_Data[4] = OUTPUT(!G1L4);


--SEG_Data[3] is SEG_Data[3] at PIN_73
--operation mode is output

SEG_Data[3] = OUTPUT(!G1L3);


--SEG_Data[2] is SEG_Data[2] at PIN_79
--operation mode is output

SEG_Data[2] = OUTPUT(!G1L2);


--SEG_Data[1] is SEG_Data[1] at PIN_78
--operation mode is output

SEG_Data[1] = OUTPUT(G1L1);


--SEG_Data[0] is SEG_Data[0] at PIN_23
--operation mode is output

SEG_Data[0] = OUTPUT(GND);


--SEG_Sel[1] is SEG_Sel[1] at PIN_68
--operation mode is output

SEG_Sel[1] = OUTPUT(!J1_D_OUT[0]);


--SEG_Sel[0] is SEG_Sel[0] at PIN_70
--operation mode is output

SEG_Sel[0] = OUTPUT(J1_D_OUT[0]);




