--A1L4Q is QN~reg0 at LC1
A1L4Q_p1_out = !S & R & !A1L4Q;
A1L4Q_p2_out = S & !R & A1L4Q;
A1L4Q_or_out = A1L4Q_p1_out # A1L4Q_p2_out;
A1L4Q_reg_input = A1L4Q_or_out;
A1L4Q = TFFE(A1L4Q_reg_input, !GLOBAL(C), , , );


--A1L5Q is Q~reg0 at LC2
A1L5Q_p1_out = !R & S & !A1L5Q;
A1L5Q_p2_out = R & !S & A1L5Q;
A1L5Q_or_out = A1L5Q_p1_out # A1L5Q_p2_out;
A1L5Q_reg_input = A1L5Q_or_out;
A1L5Q = TFFE(A1L5Q_reg_input, !GLOBAL(C), , , );


--S is S at PIN_24
--operation mode is input

S = INPUT();


--R is R at PIN_21
--operation mode is input

R = INPUT();


--C is C at PIN_43
--operation mode is input

C = INPUT();


--Q is Q at PIN_5
--operation mode is output

Q = OUTPUT(A1L5Q);


--QN is QN at PIN_4
--operation mode is output

QN = OUTPUT(A1L4Q);






