--A1L22 is pulse_1[15]~450 at LC17
A1L22_p1_out = !Reset & Clock_65536Hz & pulse_16_data[15] & second_pulse_data[15];
A1L22_p2_out = Reset & A1L22;
A1L22_p3_out = A1L22 & Clock_65536Hz & pulse_16_data[15] & second_pulse_data[15];
A1L22_or_out = A1L22_p1_out # A1L22_p2_out # A1L22_p3_out;
A1L22 = A1L22_or_out;


--A1L12 is pulse_1[14]~454 at LC18
A1L12_p1_out = !Reset & Clock_65536Hz & pulse_16_data[14] & second_pulse_data[14];
A1L12_p2_out = Reset & A1L12;
A1L12_p3_out = A1L12 & Clock_65536Hz & pulse_16_data[14] & second_pulse_data[14];
A1L12_or_out = A1L12_p1_out # A1L12_p2_out # A1L12_p3_out;
A1L12 = A1L12_or_out;


--A1L02 is pulse_1[13]~458 at LC25
A1L02_p1_out = !Reset & Clock_65536Hz & pulse_16_data[13] & second_pulse_data[13];
A1L02_p2_out = Reset & A1L02;
A1L02_p3_out = A1L02 & Clock_65536Hz & pulse_16_data[13] & second_pulse_data[13];
A1L02_or_out = A1L02_p1_out # A1L02_p2_out # A1L02_p3_out;
A1L02 = A1L02_or_out;


--A1L91 is pulse_1[12]~462 at LC26
A1L91_p1_out = !Reset & Clock_65536Hz & pulse_16_data[12] & second_pulse_data[12];
A1L91_p2_out = Reset & A1L91;
A1L91_p3_out = A1L91 & Clock_65536Hz & pulse_16_data[12] & second_pulse_data[12];
A1L91_or_out = A1L91_p1_out # A1L91_p2_out # A1L91_p3_out;
A1L91 = A1L91_or_out;


--A1L81 is pulse_1[11]~466 at LC28
A1L81_p1_out = !Reset & Clock_65536Hz & pulse_16_data[11] & second_pulse_data[11];
A1L81_p2_out = Reset & A1L81;
A1L81_p3_out = A1L81 & Clock_65536Hz & pulse_16_data[11] & second_pulse_data[11];
A1L81_or_out = A1L81_p1_out # A1L81_p2_out # A1L81_p3_out;
A1L81 = A1L81_or_out;


--A1L71 is pulse_1[10]~470 at LC29
A1L71_p1_out = !Reset & Clock_65536Hz & pulse_16_data[10] & second_pulse_data[10];
A1L71_p2_out = Reset & A1L71;
A1L71_p3_out = A1L71 & Clock_65536Hz & pulse_16_data[10] & second_pulse_data[10];
A1L71_or_out = A1L71_p1_out # A1L71_p2_out # A1L71_p3_out;
A1L71 = A1L71_or_out;


--A1L61 is pulse_1[9]~474 at LC19
A1L61_p1_out = !Reset & Clock_65536Hz & pulse_16_data[9] & second_pulse_data[9];
A1L61_p2_out = Reset & A1L61;
A1L61_p3_out = A1L61 & Clock_65536Hz & pulse_16_data[9] & second_pulse_data[9];
A1L61_or_out = A1L61_p1_out # A1L61_p2_out # A1L61_p3_out;
A1L61 = A1L61_or_out;


--A1L51 is pulse_1[8]~478 at LC12
A1L51_p1_out = !Reset & Clock_65536Hz & pulse_16_data[8] & second_pulse_data[8];
A1L51_p2_out = Reset & A1L51;
A1L51_p3_out = A1L51 & Clock_65536Hz & pulse_16_data[8] & second_pulse_data[8];
A1L51_or_out = A1L51_p1_out # A1L51_p2_out # A1L51_p3_out;
A1L51 = A1L51_or_out;


--A1L41 is pulse_1[7]~482 at LC11
A1L41_p1_out = !Reset & Clock_65536Hz & pulse_16_data[7] & second_pulse_data[7];
A1L41_p2_out = Reset & A1L41;
A1L41_p3_out = A1L41 & Clock_65536Hz & pulse_16_data[7] & second_pulse_data[7];
A1L41_or_out = A1L41_p1_out # A1L41_p2_out # A1L41_p3_out;
A1L41 = A1L41_or_out;


--A1L31 is pulse_1[6]~486 at LC10
A1L31_p1_out = !Reset & Clock_65536Hz & pulse_16_data[6] & second_pulse_data[6];
A1L31_p2_out = Reset & A1L31;
A1L31_p3_out = A1L31 & Clock_65536Hz & pulse_16_data[6] & second_pulse_data[6];
A1L31_or_out = A1L31_p1_out # A1L31_p2_out # A1L31_p3_out;
A1L31 = A1L31_or_out;


--A1L21 is pulse_1[5]~490 at LC9
A1L21_p1_out = !Reset & Clock_65536Hz & pulse_16_data[5] & second_pulse_data[5];
A1L21_p2_out = Reset & A1L21;
A1L21_p3_out = A1L21 & Clock_65536Hz & pulse_16_data[5] & second_pulse_data[5];
A1L21_or_out = A1L21_p1_out # A1L21_p2_out # A1L21_p3_out;
A1L21 = A1L21_or_out;


--A1L11 is pulse_1[4]~494 at LC8
A1L11_p1_out = !Reset & Clock_65536Hz & pulse_16_data[4] & second_pulse_data[4];
A1L11_p2_out = Reset & A1L11;
A1L11_p3_out = A1L11 & Clock_65536Hz & pulse_16_data[4] & second_pulse_data[4];
A1L11_or_out = A1L11_p1_out # A1L11_p2_out # A1L11_p3_out;
A1L11 = A1L11_or_out;


--A1L01 is pulse_1[3]~498 at LC4
A1L01_p1_out = !Reset & Clock_65536Hz & pulse_16_data[3] & second_pulse_data[3];
A1L01_p2_out = Reset & A1L01;
A1L01_p3_out = A1L01 & Clock_65536Hz & pulse_16_data[3] & second_pulse_data[3];
A1L01_or_out = A1L01_p1_out # A1L01_p2_out # A1L01_p3_out;
A1L01 = A1L01_or_out;


--A1L9 is pulse_1[2]~502 at LC3
A1L9_p1_out = !Reset & Clock_65536Hz & pulse_16_data[2] & second_pulse_data[2];
A1L9_p2_out = Reset & A1L9;
A1L9_p3_out = A1L9 & Clock_65536Hz & pulse_16_data[2] & second_pulse_data[2];
A1L9_or_out = A1L9_p1_out # A1L9_p2_out # A1L9_p3_out;
A1L9 = A1L9_or_out;


--A1L8 is pulse_1[1]~506 at LC2
A1L8_p1_out = !Reset & Clock_65536Hz & pulse_16_data[1] & second_pulse_data[1];
A1L8_p2_out = Reset & A1L8;
A1L8_p3_out = A1L8 & Clock_65536Hz & pulse_16_data[1] & second_pulse_data[1];
A1L8_or_out = A1L8_p1_out # A1L8_p2_out # A1L8_p3_out;
A1L8 = A1L8_or_out;


--A1L7 is pulse_1[0]~510 at LC1
A1L7_p1_out = !Reset & Clock_65536Hz & pulse_16_data[0] & second_pulse_data[0];
A1L7_p2_out = Reset & A1L7;
A1L7_p3_out = A1L7 & Clock_65536Hz & pulse_16_data[0] & second_pulse_data[0];
A1L7_or_out = A1L7_p1_out # A1L7_p2_out # A1L7_p3_out;
A1L7 = A1L7_or_out;


--A1L14 is pulse_out~25 at LC33
A1L14_p1_out = !A1L22 & !A1L12 & !A1L02 & !A1L91 & !A1L81 & !A1L71 & !A1L61 & !A1L51 & !A1L41 & !A1L31 & !A1L21 & !A1L11 & !A1L01 & !A1L9 & !A1L8 & !A1L7;
A1L14_or_out = A1L14_p1_out # Reset;
A1L14 = !(A1L14_or_out);


--Reset is Reset at PIN_85
--operation mode is input

Reset = INPUT();


--Clock_65536Hz is Clock_65536Hz at PIN_92
--operation mode is input

Clock_65536Hz = INPUT();


--pulse_16_data[15] is pulse_16_data[15] at PIN_84
--operation mode is input

pulse_16_data[15] = INPUT();


--pulse_16_data[14] is pulse_16_data[14] at PIN_93
--operation mode is input

pulse_16_data[14] = INPUT();


--pulse_16_data[13] is pulse_16_data[13] at PIN_61
--operation mode is input

pulse_16_data[13] = INPUT();


--pulse_16_data[12] is pulse_16_data[12] at PIN_16
--operation mode is input

pulse_16_data[12] = INPUT();


--pulse_16_data[11] is pulse_16_data[11] at PIN_45
--operation mode is input

pulse_16_data[11] = INPUT();


--pulse_16_data[10] is pulse_16_data[10] at PIN_9
--operation mode is input

pulse_16_data[10] = INPUT();


--pulse_16_data[9] is pulse_16_data[9] at PIN_17
--operation mode is input

pulse_16_data[9] = INPUT();


--pulse_16_data[8] is pulse_16_data[8] at PIN_83
--operation mode is input

pulse_16_data[8] = INPUT();


--pulse_16_data[7] is pulse_16_data[7] at PIN_96
--operation mode is input

pulse_16_data[7] = INPUT();


--pulse_16_data[6] is pulse_16_data[6] at PIN_58
--operation mode is input

pulse_16_data[6] = INPUT();


--pulse_16_data[5] is pulse_16_data[5] at PIN_20
--operation mode is input

pulse_16_data[5] = INPUT();


--pulse_16_data[4] is pulse_16_data[4] at PIN_97
--operation mode is input

pulse_16_data[4] = INPUT();


--pulse_16_data[3] is pulse_16_data[3] at PIN_99
--operation mode is input

pulse_16_data[3] = INPUT();


--pulse_16_data[2] is pulse_16_data[2] at PIN_25
--operation mode is input

pulse_16_data[2] = INPUT();


--pulse_16_data[1] is pulse_16_data[1] at PIN_30
--operation mode is input

pulse_16_data[1] = INPUT();


--pulse_16_data[0] is pulse_16_data[0] at PIN_69
--operation mode is input

pulse_16_data[0] = INPUT();


--second_pulse_data[15] is second_pulse_data[15] at PIN_31
--operation mode is input

second_pulse_data[15] = INPUT();


--second_pulse_data[14] is second_pulse_data[14] at PIN_32
--operation mode is input

second_pulse_data[14] = INPUT();


--second_pulse_data[13] is second_pulse_data[13] at PIN_68
--operation mode is input

second_pulse_data[13] = INPUT();


--second_pulse_data[12] is second_pulse_data[12] at PIN_10
--operation mode is input

second_pulse_data[12] = INPUT();


--second_pulse_data[11] is second_pulse_data[11] at PIN_33
--operation mode is input

second_pulse_data[11] = INPUT();


--second_pulse_data[10] is second_pulse_data[10] at PIN_46
--operation mode is input

second_pulse_data[10] = INPUT();


--second_pulse_data[9] is second_pulse_data[9] at PIN_8
--operation mode is input

second_pulse_data[9] = INPUT();


--second_pulse_data[8] is second_pulse_data[8] at PIN_6
--operation mode is input

second_pulse_data[8] = INPUT();


--second_pulse_data[7] is second_pulse_data[7] at PIN_71
--operation mode is input

second_pulse_data[7] = INPUT();


--second_pulse_data[6] is second_pulse_data[6] at PIN_47
--operation mode is input

second_pulse_data[6] = INPUT();


--second_pulse_data[5] is second_pulse_data[5] at PIN_29
--operation mode is input

second_pulse_data[5] = INPUT();


--second_pulse_data[4] is second_pulse_data[4] at PIN_48
--operation mode is input

second_pulse_data[4] = INPUT();


--second_pulse_data[3] is second_pulse_data[3] at PIN_19
--operation mode is input

second_pulse_data[3] = INPUT();


--second_pulse_data[2] is second_pulse_data[2] at PIN_81
--operation mode is input

second_pulse_data[2] = INPUT();


--second_pulse_data[1] is second_pulse_data[1] at PIN_94
--operation mode is input

second_pulse_data[1] = INPUT();


--second_pulse_data[0] is second_pulse_data[0] at PIN_60
--operation mode is input

second_pulse_data[0] = INPUT();


--pulse_out is pulse_out at PIN_40
--operation mode is output

pulse_out = OUTPUT(A1L14);






