--A1L33Q is Direction_Disp_Row2[1]~reg0 at LC21
A1L33Q_p1_out = !A1L33Q & A1L13Q & !A1L73Q & !A1L53Q;
A1L33Q_or_out = A1L33Q_p1_out;
A1L33Q_reg_input = A1L33Q_or_out;
A1L33Q = DFFE(A1L33Q_reg_input, GLOBAL(Clock_1KHz), , , );


--A1L73Q is Direction_Disp_Row2[3]~reg0 at LC13
A1L73Q_p1_out = A1L13Q & A1L33Q & !A1L73Q & !A1L53Q;
A1L73Q_or_out = A1L73Q_p1_out;
A1L73Q_reg_input = A1L73Q_or_out;
A1L73Q = DFFE(A1L73Q_reg_input, GLOBAL(Clock_1KHz), , , );


--A1L13Q is Direction_Disp_Row2[0]~reg0 at LC14
A1L13Q_p1_out = !A1L73Q & !A1L53Q & !A1L33Q & !A1L13Q;
A1L13Q_or_out = A1L13Q_p1_out;
A1L13Q_reg_input = A1L13Q_or_out;
A1L13Q = DFFE(A1L13Q_reg_input, GLOBAL(Clock_1KHz), , , );


--A1L53Q is Direction_Disp_Row2[2]~reg0 at LC15
A1L53Q_p1_out = !A1L13Q & A1L33Q & !A1L73Q & !A1L53Q;
A1L53Q_or_out = A1L53Q_p1_out;
A1L53Q_reg_input = A1L53Q_or_out;
A1L53Q = DFFE(A1L53Q_reg_input, GLOBAL(Clock_1KHz), , , );


--A1L93Q is Direction_Disp_Row2[4]~reg0 at LC16
A1L93Q_p1_out = !A1L73Q & A1L53Q & !A1L33Q & !A1L13Q;
A1L93Q_or_out = A1L93Q_p1_out;
A1L93Q_reg_input = A1L93Q_or_out;
A1L93Q = DFFE(A1L93Q_reg_input, GLOBAL(Clock_1KHz), , , );


--A1L41 is Direction_Disp_Row1[6]$latch$en_or~307 at LC12
A1L41_p0_out = !A1L33Q & !A1L93Q & !A1L13Q & A1L73Q & !A1L53Q;
A1L41_p3_out = Now_Direction[0] & Now_Direction[1];
A1L41_p4_out = !Now_Direction[0] & !Now_Direction[1];
A1L41_or_out = A1L51 # A1L41_p0_out # En # Reset # A1L41_p3_out # A1L41_p4_out;
A1L41 = A1L41_or_out;


--A1L91 is Direction_Disp_Row1~1070 at LC10
A1L91_p1_out = !A1L53Q & !A1L73Q & !A1L33Q & !A1L93Q & A1L13Q;
A1L91_p2_out = !Now_Direction[0] & !Now_Direction[1];
A1L91_p3_out = Now_Direction[0] & Now_Direction[1];
A1L91_or_out = A1L42 # En # A1L91_p1_out # A1L91_p2_out # A1L91_p3_out # Reset;
A1L91 = A1L91_or_out;


--A1L22 is Direction_Disp_Row1~1073 at LC8
A1L22_p1_out = !A1L53Q & A1L73Q & !A1L33Q & !A1L93Q & !A1L13Q;
A1L22_p2_out = !A1L53Q & !A1L73Q & A1L33Q & !A1L93Q & !A1L13Q;
A1L22_p3_out = !A1L53Q & !A1L73Q & !A1L33Q & A1L93Q & !A1L13Q & Now_Direction[1];
A1L22_p4_out = !A1L53Q & !A1L73Q & !A1L33Q & !A1L93Q & A1L13Q & Now_Direction[1];
A1L22_or_out = A1L52 # En # A1L22_p1_out # A1L22_p2_out # A1L22_p3_out # A1L22_p4_out;
A1L22 = A1L22_or_out;


--A1L32 is Direction_Disp_Row1~1074 at LC6
A1L32_p0_out = !Now_Direction[1] & !Now_Direction[0];
A1L32_p1_out = A1L33Q & !A1L93Q & !A1L13Q & !A1L73Q & !A1L53Q & Now_Direction[1];
A1L32_p2_out = Now_Direction[1] & Now_Direction[0];
A1L32_p3_out = !A1L33Q & A1L93Q & !A1L13Q & !A1L73Q & !A1L53Q;
A1L32_p4_out = !A1L33Q & !A1L93Q & A1L13Q & !A1L73Q & !A1L53Q;
A1L32_or_out = A1L62 # A1L32_p0_out # A1L32_p1_out # A1L32_p2_out # A1L32_p3_out # A1L32_p4_out;
A1L32 = A1L32_or_out;


--A1L02 is Direction_Disp_Row1~1071 at LC4
A1L02_p0_out = !Now_Direction[0] & !Now_Direction[1];
A1L02_p1_out = !A1L53Q & !A1L73Q & A1L33Q & !A1L93Q & !A1L13Q & Now_Direction[0];
A1L02_p2_out = Now_Direction[0] & Now_Direction[1];
A1L02_p3_out = !A1L53Q & !A1L73Q & !A1L33Q & A1L93Q & !A1L13Q;
A1L02_p4_out = !A1L53Q & !A1L73Q & !A1L33Q & !A1L93Q & A1L13Q;
A1L02_or_out = A1L72 # A1L02_p0_out # A1L02_p1_out # A1L02_p2_out # A1L02_p3_out # A1L02_p4_out;
A1L02 = A1L02_or_out;


--A1L12 is Direction_Disp_Row1~1072 at LC2
A1L12_p0_out = !A1L53Q & !A1L73Q & A1L33Q & !A1L93Q & !A1L13Q;
A1L12_p1_out = Now_Direction[0] & !A1L53Q & !A1L73Q & !A1L33Q & !A1L93Q & A1L13Q;
A1L12_p2_out = Now_Direction[0] & Now_Direction[1];
A1L12_p3_out = !Now_Direction[0] & !Now_Direction[1];
A1L12_p4_out = !A1L53Q & A1L73Q & !A1L33Q & !A1L93Q & !A1L13Q;
A1L12_or_out = A1L82 # A1L12_p0_out # A1L12_p1_out # A1L12_p2_out # A1L12_p3_out # A1L12_p4_out;
A1L12 = A1L12_or_out;


--A1L61 is Direction_Disp_Row1[6]$latch~14 at LC17
A1L61_p1_out = A1L91 & A1L41;
A1L61_p2_out = !A1L41 & A1L61;
A1L61_p3_out = A1L91 & A1L61;
A1L61_or_out = A1L61_p1_out # A1L61_p2_out # A1L61_p3_out;
A1L61 = A1L61_or_out;


--A1L21 is Direction_Disp_Row1[5]$latch~10 at LC18
A1L21_p1_out = A1L02 & A1L41;
A1L21_p2_out = !A1L41 & A1L21;
A1L21_p3_out = A1L02 & A1L21;
A1L21_or_out = A1L21_p1_out # A1L21_p2_out # A1L21_p3_out;
A1L21 = A1L21_or_out;


--A1L01 is Direction_Disp_Row1[4]$latch~10 at LC19
A1L01_p1_out = A1L12 & A1L41;
A1L01_p2_out = !A1L41 & A1L01;
A1L01_p3_out = A1L12 & A1L01;
A1L01_or_out = A1L01_p1_out # A1L01_p2_out # A1L01_p3_out;
A1L01 = A1L01_or_out;


--A1L7 is Direction_Disp_Row1[2]$latch~10 at LC24
A1L7_p1_out = A1L22 & A1L41;
A1L7_p2_out = !A1L41 & A1L7;
A1L7_p3_out = A1L22 & A1L7;
A1L7_or_out = A1L7_p1_out # A1L7_p2_out # A1L7_p3_out;
A1L7 = A1L7_or_out;


--A1L5 is Direction_Disp_Row1[1]$latch~10 at LC27
A1L5_p1_out = A1L32 & A1L41;
A1L5_p2_out = !A1L41 & A1L5;
A1L5_p3_out = A1L32 & A1L5;
A1L5_or_out = A1L5_p1_out # A1L5_p2_out # A1L5_p3_out;
A1L5 = A1L5_or_out;


--A1L71 is Direction_Disp_Row1[6]$latch~16 at LC23
A1L71_or_out = A1L61;
A1L71 = A1L71_or_out;


--A1L81 is Direction_Disp_Row1[6]$latch~18 at LC22
A1L81_or_out = A1L61;
A1L81 = A1L81_or_out;


--A1L51 is Direction_Disp_Row1[6]$latch$en_or~326 at LC11
A1L51_p1_out = !A1L33Q & !A1L93Q & !A1L13Q & !A1L73Q & A1L53Q;
A1L51_p2_out = A1L33Q & !A1L93Q & !A1L13Q & !A1L73Q & !A1L53Q;
A1L51_p3_out = !A1L33Q & !A1L93Q & A1L13Q & !A1L73Q & !A1L53Q;
A1L51_p4_out = !A1L33Q & A1L93Q & !A1L13Q & !A1L73Q & !A1L53Q;
A1L51 = A1L51_p1_out # A1L51_p2_out # A1L51_p3_out # A1L51_p4_out;


--A1L42 is Direction_Disp_Row1~1105 at LC9
A1L42_p1_out = !A1L53Q & A1L73Q & !A1L33Q & !A1L93Q & !A1L13Q;
A1L42_p2_out = !A1L53Q & !A1L73Q & A1L33Q & !A1L93Q & !A1L13Q;
A1L42_p3_out = !A1L53Q & !A1L73Q & !A1L33Q & A1L93Q & !A1L13Q;
A1L42 = A1L42_p1_out # A1L42_p2_out # A1L42_p3_out;


--A1L52 is Direction_Disp_Row1~1109 at LC7
A1L52_p1_out = Now_Direction[0] & Now_Direction[1];
A1L52_p2_out = !Now_Direction[0] & !Now_Direction[1];
A1L52 = A1L52_p1_out # A1L52_p2_out # Reset;


--A1L62 is Direction_Disp_Row1~1113 at LC5
A1L62_p3_out = !A1L33Q & !A1L93Q & !A1L13Q & A1L73Q & !A1L53Q & Now_Direction[1];
A1L62 = Reset # En # A1L62_p3_out;


--A1L72 is Direction_Disp_Row1~1117 at LC3
A1L72_p3_out = !A1L53Q & A1L73Q & !A1L33Q & !A1L93Q & !A1L13Q & Now_Direction[0];
A1L72 = Reset # En # A1L72_p3_out;


--A1L82 is Direction_Disp_Row1~1121 at LC1
A1L82_p3_out = Now_Direction[0] & !A1L53Q & !A1L73Q & !A1L33Q & A1L93Q & !A1L13Q;
A1L82 = Reset # En # A1L82_p3_out;


--Reset is Reset at PIN_12
--operation mode is input

Reset = INPUT();


--En is En at PIN_16
--operation mode is input

En = INPUT();


--Clock_1KHz is Clock_1KHz at PIN_43
--operation mode is input

Clock_1KHz = INPUT();


--Now_Direction[1] is Now_Direction[1] at PIN_9
--operation mode is input

Now_Direction[1] = INPUT();


--Now_Direction[0] is Now_Direction[0] at PIN_44
--operation mode is input

Now_Direction[0] = INPUT();


--Direction_Disp_Row2[1] is Direction_Disp_Row2[1] at PIN_37
--operation mode is output

Direction_Disp_Row2[1] = OUTPUT(A1L33Q);


--Direction_Disp_Row2[3] is Direction_Disp_Row2[3] at PIN_18
--operation mode is output

Direction_Disp_Row2[3] = OUTPUT(A1L73Q);


--Direction_Disp_Row2[0] is Direction_Disp_Row2[0] at PIN_19
--operation mode is output

Direction_Disp_Row2[0] = OUTPUT(A1L13Q);


--Direction_Disp_Row2[2] is Direction_Disp_Row2[2] at PIN_20
--operation mode is output

Direction_Disp_Row2[2] = OUTPUT(A1L53Q);


--Direction_Disp_Row2[4] is Direction_Disp_Row2[4] at PIN_21
--operation mode is output

Direction_Disp_Row2[4] = OUTPUT(A1L93Q);


--Direction_Disp_Row1[6] is Direction_Disp_Row1[6] at PIN_41
--operation mode is output

Direction_Disp_Row1[6] = OUTPUT(A1L61);


--Direction_Disp_Row1[5] is Direction_Disp_Row1[5] at PIN_40
--operation mode is output

Direction_Disp_Row1[5] = OUTPUT(A1L21);


--Direction_Disp_Row1[4] is Direction_Disp_Row1[4] at PIN_39
--operation mode is output

Direction_Disp_Row1[4] = OUTPUT(A1L01);


--Direction_Disp_Row1[2] is Direction_Disp_Row1[2] at PIN_33
--operation mode is output

Direction_Disp_Row1[2] = OUTPUT(A1L7);


--Direction_Disp_Row1[1] is Direction_Disp_Row1[1] at PIN_29
--operation mode is output

Direction_Disp_Row1[1] = OUTPUT(A1L5);


--Direction_Disp_Row1[3] is Direction_Disp_Row1[3] at PIN_34
--operation mode is output

Direction_Disp_Row1[3] = OUTPUT(A1L71);


--Direction_Disp_Row1[0] is Direction_Disp_Row1[0] at PIN_36
--operation mode is output

Direction_Disp_Row1[0] = OUTPUT(A1L81);






