Timing Analyzer report for DC_Motor_Main
Fri Aug 04 19:03:55 2006
Version 4.2 Build 157 12/07/2004 SJ Full Version


---------------------
; Table of Contents ;
---------------------
  1. Legal Notice
  2. Timing Analyzer Summary
  3. Timing Analyzer Settings
  4. Clock Settings Summary
  5. Clock Setup: 'Clk_SCL'
  6. Clock Setup: 'Rate_Pulse'
  7. Clock Setup: 'Rate_Measure_Ctrl'
  8. tsu
  9. tco
 10. tpd
 11. th
 12. Timing Analyzer Messages



----------------
; Legal Notice ;
----------------
Copyright (C) 1991-2004 Altera Corporation
Any  megafunction  design,  and related netlist (encrypted  or  decrypted),
support information,  device programming or simulation file,  and any other
associated  documentation or information  provided by  Altera  or a partner
under  Altera's   Megafunction   Partnership   Program  may  be  used  only
to program  PLD  devices (but not masked  PLD  devices) from  Altera.   Any
other  use  of such  megafunction  design,  netlist,  support  information,
device programming or simulation file,  or any other  related documentation
or information  is prohibited  for  any  other purpose,  including, but not
limited to  modification,  reverse engineering,  de-compiling, or use  with
any other  silicon devices,  unless such use is  explicitly  licensed under
a separate agreement with  Altera  or a megafunction partner.  Title to the
intellectual property,  including patents,  copyrights,  trademarks,  trade
secrets,  or maskworks,  embodied in any such megafunction design, netlist,
support  information,  device programming or simulation file,  or any other
related documentation or information provided by  Altera  or a megafunction
partner, remains with Altera, the megafunction partner, or their respective
licensors. No other licenses, including any licenses needed under any third
party's intellectual property, are provided herein.



+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Timing Analyzer Summary                                                                                                                                                                                                                                                          ;
+----------------------------------+-------+---------------+----------------------------------+--------------------------------------------------------------+--------------------------------------------------------------+-------------------+-------------------+--------------+
; Type                             ; Slack ; Required Time ; Actual Time                      ; From                                                         ; To                                                           ; From Clock        ; To Clock          ; Failed Paths ;
+----------------------------------+-------+---------------+----------------------------------+--------------------------------------------------------------+--------------------------------------------------------------+-------------------+-------------------+--------------+
; Worst-case tsu                   ; N/A   ; None          ; 4.000 ns                         ; Reset                                                        ; main:inst3|Data_drive:b2v_inst|Adc_Conv                      ;                   ; Clk_SCL           ; 0            ;
; Worst-case tco                   ; N/A   ; None          ; 24.600 ns                        ; main:inst3|Data_Read:b2v_inst1|Data[13]                      ; Current_Adjust_Drive                                         ; Clk_SCL           ;                   ; 0            ;
; Worst-case tpd                   ; N/A   ; None          ; 11.400 ns                        ; Position_Set[11]                                             ; Position_Adjust_Drive                                        ;                   ;                   ; 0            ;
; Worst-case th                    ; N/A   ; None          ; 8.900 ns                         ; AD7895_Data                                                  ; main:inst3|Data_Read:b2v_inst1|Data[8]                       ;                   ; Clk_SCL           ; 0            ;
; Clock Setup: 'Clk_SCL'           ; N/A   ; None          ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; Clk_SCL           ; Clk_SCL           ; 0            ;
; Clock Setup: 'Rate_Measure_Ctrl' ; N/A   ; None          ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; 0            ;
; Clock Setup: 'Rate_Pulse'        ; N/A   ; None          ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0] ; Rate_Pulse        ; Rate_Pulse        ; 0            ;
; Total number of failed paths     ;       ;               ;                                  ;                                                              ;                                                              ;                   ;                   ; 0            ;
+----------------------------------+-------+---------------+----------------------------------+--------------------------------------------------------------+--------------------------------------------------------------+-------------------+-------------------+--------------+


+------------------------------------------------------------------------------------------------------+
; Timing Analyzer Settings                                                                             ;
+-------------------------------------------------------+--------------------+------+----+-------------+
; Option                                                ; Setting            ; From ; To ; Entity Name ;
+-------------------------------------------------------+--------------------+------+----+-------------+
; Device Name                                           ; EPM7128STC100-6    ;      ;    ;             ;
; Timing Models                                         ; Final              ;      ;    ;             ;
; Number of source nodes to report per destination node ; 10                 ;      ;    ;             ;
; Number of destination nodes to report                 ; 10                 ;      ;    ;             ;
; Number of paths to report                             ; 200                ;      ;    ;             ;
; Report Minumum Timing Checks                          ; Off                ;      ;    ;             ;
; Use Fast Timing Models                                ; Off                ;      ;    ;             ;
; Report IO Paths Separately                            ; Off                ;      ;    ;             ;
; Clock Analysis Only                                   ; Off                ;      ;    ;             ;
; Default hold multicycle                               ; Same as Multicycle ;      ;    ;             ;
; Cut paths between unrelated clock domains             ; On                 ;      ;    ;             ;
; Cut off read during write signal paths                ; On                 ;      ;    ;             ;
; Cut off clear and preset signal paths                 ; On                 ;      ;    ;             ;
; Cut off feedback from I/O pins                        ; On                 ;      ;    ;             ;
; Ignore Clock Settings                                 ; Off                ;      ;    ;             ;
; Analyze latches as synchronous elements               ; Off                ;      ;    ;             ;
; Do Min/Max analysis using Rise/Fall delays            ; Off                ;      ;    ;             ;
; Enable Recovery/Removal analysis                      ; Off                ;      ;    ;             ;
; Use Clock Latency for PLL offset                      ; Off                ;      ;    ;             ;
+-------------------------------------------------------+--------------------+------+----+-------------+


+----------------------------------------------------------------------------------------------------------------------------------------+
; Clock Settings Summary                                                                                                                 ;
+-------------------+--------------------+----------+------------------+----------+-----------------------+---------------------+--------+
; Clock Node Name   ; Clock Setting Name ; Type     ; Fmax Requirement ; Based on ; Multiply Base Fmax by ; Divide Base Fmax by ; Offset ;
+-------------------+--------------------+----------+------------------+----------+-----------------------+---------------------+--------+
; Clock             ;                    ; User Pin ; NONE             ; NONE     ; N/A                   ; N/A                 ; N/A    ;
; Clk_SCL           ;                    ; User Pin ; NONE             ; NONE     ; N/A                   ; N/A                 ; N/A    ;
; Rate_Pulse        ;                    ; User Pin ; NONE             ; NONE     ; N/A                   ; N/A                 ; N/A    ;
; Rate_Measure_Ctrl ;                    ; User Pin ; NONE             ; NONE     ; N/A                   ; N/A                 ; N/A    ;
+-------------------+--------------------+----------+------------------+----------+-----------------------+---------------------+--------+


+------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Clock Setup: 'Clk_SCL'                                                                                                                                                                                                                                                             ;
+-------+----------------------------------+--------------------------------------------------------------+--------------------------------------------------------------+------------+----------+-----------------------------+---------------------------+-------------------------+
; Slack ; Actual fmax (period)             ; From                                                         ; To                                                           ; From Clock ; To Clock ; Required Setup Relationship ; Required Longest P2P Time ; Actual Longest P2P Time ;
+-------+----------------------------------+--------------------------------------------------------------+--------------------------------------------------------------+------------+----------+-----------------------------+---------------------------+-------------------------+
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|Data[8]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|Data[8]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; main:inst3|Data_Read:b2v_inst1|Data[8]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; main:inst3|Data_Read:b2v_inst1|Data[8]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|Data[8]                       ; main:inst3|Data_Read:b2v_inst1|Data[8]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|Data[10]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|Data[10]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; main:inst3|Data_Read:b2v_inst1|Data[10]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; main:inst3|Data_Read:b2v_inst1|Data[10]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|Data[10]                      ; main:inst3|Data_Read:b2v_inst1|Data[10]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|Data[15]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|Data[15]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; main:inst3|Data_Read:b2v_inst1|Data[15]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; main:inst3|Data_Read:b2v_inst1|Data[15]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|Data[4]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|Data[4]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; main:inst3|Data_Read:b2v_inst1|Data[4]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; main:inst3|Data_Read:b2v_inst1|Data[4]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|Data[4]                       ; main:inst3|Data_Read:b2v_inst1|Data[4]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|Data[5]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|Data[5]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; main:inst3|Data_Read:b2v_inst1|Data[5]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; main:inst3|Data_Read:b2v_inst1|Data[5]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|Data[5]                       ; main:inst3|Data_Read:b2v_inst1|Data[5]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|Data[6]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|Data[6]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; main:inst3|Data_Read:b2v_inst1|Data[6]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; main:inst3|Data_Read:b2v_inst1|Data[6]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|Data[6]                       ; main:inst3|Data_Read:b2v_inst1|Data[6]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|Data[7]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|Data[7]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; main:inst3|Data_Read:b2v_inst1|Data[7]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; main:inst3|Data_Read:b2v_inst1|Data[7]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|Data[7]                       ; main:inst3|Data_Read:b2v_inst1|Data[7]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|Data[9]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|Data[9]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; main:inst3|Data_Read:b2v_inst1|Data[9]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; main:inst3|Data_Read:b2v_inst1|Data[9]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|Data[9]                       ; main:inst3|Data_Read:b2v_inst1|Data[9]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|Data[11]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|Data[11]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; main:inst3|Data_Read:b2v_inst1|Data[11]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; main:inst3|Data_Read:b2v_inst1|Data[11]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|Data[11]                      ; main:inst3|Data_Read:b2v_inst1|Data[11]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|Data[12]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|Data[12]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; main:inst3|Data_Read:b2v_inst1|Data[12]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; main:inst3|Data_Read:b2v_inst1|Data[12]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|Data[13]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|Data[13]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; main:inst3|Data_Read:b2v_inst1|Data[13]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; main:inst3|Data_Read:b2v_inst1|Data[13]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|Data[13]                      ; main:inst3|Data_Read:b2v_inst1|Data[13]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|Data[14]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|Data[14]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; main:inst3|Data_Read:b2v_inst1|Data[14]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; main:inst3|Data_Read:b2v_inst1|Data[14]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|Data[14]                      ; main:inst3|Data_Read:b2v_inst1|Data[14]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 97.09 MHz ( period = 10.300 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 98.04 MHz ( period = 10.200 ns ) ; main:inst3|Data_Read:b2v_inst1|Data[15]                      ; main:inst3|Data_Read:b2v_inst1|Data[15]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.400 ns                ;
; N/A   ; 98.04 MHz ( period = 10.200 ns ) ; main:inst3|Data_Read:b2v_inst1|Data[12]                      ; main:inst3|Data_Read:b2v_inst1|Data[12]                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.400 ns                ;
; N/A   ; 98.04 MHz ( period = 10.200 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[3] ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.400 ns                ;
; N/A   ; 98.04 MHz ( period = 10.200 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[2] ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.400 ns                ;
; N/A   ; 98.04 MHz ( period = 10.200 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[1] ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.400 ns                ;
; N/A   ; 98.04 MHz ( period = 10.200 ns ) ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0] ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.400 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[0]                       ; main:inst3|Data_drive:b2v_inst|Adc_Conv                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[1]                       ; main:inst3|Data_drive:b2v_inst|Adc_Conv                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[2]                       ; main:inst3|Data_drive:b2v_inst|Adc_Conv                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[3]                       ; main:inst3|Data_drive:b2v_inst|Adc_Conv                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[4]                       ; main:inst3|Data_drive:b2v_inst|Adc_Conv                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[5]                       ; main:inst3|Data_drive:b2v_inst|Adc_Conv                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[0]                       ; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select                ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[1]                       ; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select                ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[2]                       ; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select                ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[3]                       ; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select                ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[4]                       ; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select                ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[5]                       ; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select                ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[0]                       ; main:inst3|Data_drive:b2v_inst|cnt1[5]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[1]                       ; main:inst3|Data_drive:b2v_inst|cnt1[5]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[2]                       ; main:inst3|Data_drive:b2v_inst|cnt1[5]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[3]                       ; main:inst3|Data_drive:b2v_inst|cnt1[5]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[4]                       ; main:inst3|Data_drive:b2v_inst|cnt1[5]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[5]                       ; main:inst3|Data_drive:b2v_inst|cnt1[5]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[0]                       ; main:inst3|Data_drive:b2v_inst|cnt1[4]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[1]                       ; main:inst3|Data_drive:b2v_inst|cnt1[4]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[2]                       ; main:inst3|Data_drive:b2v_inst|cnt1[4]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[3]                       ; main:inst3|Data_drive:b2v_inst|cnt1[4]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[4]                       ; main:inst3|Data_drive:b2v_inst|cnt1[4]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[0]                       ; main:inst3|Data_drive:b2v_inst|cnt1[3]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[1]                       ; main:inst3|Data_drive:b2v_inst|cnt1[3]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[2]                       ; main:inst3|Data_drive:b2v_inst|cnt1[3]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[3]                       ; main:inst3|Data_drive:b2v_inst|cnt1[3]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[0]                       ; main:inst3|Data_drive:b2v_inst|cnt1[2]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[1]                       ; main:inst3|Data_drive:b2v_inst|cnt1[2]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[2]                       ; main:inst3|Data_drive:b2v_inst|cnt1[2]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[0]                       ; main:inst3|Data_drive:b2v_inst|cnt1[1]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[1]                       ; main:inst3|Data_drive:b2v_inst|cnt1[1]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 147.06 MHz ( period = 6.800 ns ) ; main:inst3|Data_drive:b2v_inst|Adc_Conv                      ; main:inst3|Data_drive:b2v_inst|Adc_Conv                      ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.400 ns                ;
; N/A   ; 147.06 MHz ( period = 6.800 ns ) ; main:inst3|Data_drive:b2v_inst|cnt1[0]                       ; main:inst3|Data_drive:b2v_inst|cnt1[0]                       ; Clk_SCL    ; Clk_SCL  ; None                        ; None                      ; 4.400 ns                ;
+-------+----------------------------------+--------------------------------------------------------------+--------------------------------------------------------------+------------+----------+-----------------------------+---------------------------+-------------------------+


+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Clock Setup: 'Rate_Pulse'                                                                                                                                                                                                                                                              ;
+-------+----------------------------------+---------------------------------------------------------------+---------------------------------------------------------------+------------+------------+-----------------------------+---------------------------+-------------------------+
; Slack ; Actual fmax (period)             ; From                                                          ; To                                                            ; From Clock ; To Clock   ; Required Setup Relationship ; Required Longest P2P Time ; Actual Longest P2P Time ;
+-------+----------------------------------+---------------------------------------------------------------+---------------------------------------------------------------+------------+------------+-----------------------------+---------------------------+-------------------------+
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Pulse ; Rate_Pulse ; None                        ; None                      ; 4.500 ns                ;
+-------+----------------------------------+---------------------------------------------------------------+---------------------------------------------------------------+------------+------------+-----------------------------+---------------------------+-------------------------+


+------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Clock Setup: 'Rate_Measure_Ctrl'                                                                                                                                                                                                                                                                     ;
+-------+----------------------------------+---------------------------------------------------------------+---------------------------------------------------------------+-------------------+-------------------+-----------------------------+---------------------------+-------------------------+
; Slack ; Actual fmax (period)             ; From                                                          ; To                                                            ; From Clock        ; To Clock          ; Required Setup Relationship ; Required Longest P2P Time ; Actual Longest P2P Time ;
+-------+----------------------------------+---------------------------------------------------------------+---------------------------------------------------------------+-------------------+-------------------+-----------------------------+---------------------------+-------------------------+
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 142.86 MHz ( period = 7.000 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.600 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
; N/A   ; 144.93 MHz ( period = 6.900 ns ) ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure_Ctrl ; Rate_Measure_Ctrl ; None                        ; None                      ; 4.500 ns                ;
+-------+----------------------------------+---------------------------------------------------------------+---------------------------------------------------------------+-------------------+-------------------+-----------------------------+---------------------------+-------------------------+


+-----------------------------------------------------------------------------------------------------------------------------------------+
; tsu                                                                                                                                     ;
+-------+--------------+------------+-----------------+---------------------------------------------------------------+-------------------+
; Slack ; Required tsu ; Actual tsu ; From            ; To                                                            ; To Clock          ;
+-------+--------------+------------+-----------------+---------------------------------------------------------------+-------------------+
; N/A   ; None         ; 4.000 ns   ; Reset           ; Position_adc_ctrl:inst6|Adc_Mode                              ; Clock             ;
; N/A   ; None         ; 4.000 ns   ; Reset           ; Position_adc_ctrl:inst6|Adc_Cs                                ; Clock             ;
; N/A   ; None         ; 4.000 ns   ; Reset           ; main:inst3|Data_drive:b2v_inst|cnt1[0]                        ; Clk_SCL           ;
; N/A   ; None         ; 4.000 ns   ; Reset           ; Position_adc_ctrl:inst6|Adc_Conv                              ; Clock             ;
; N/A   ; None         ; 4.000 ns   ; Reset           ; Position_adc_ctrl:inst6|Adc_Rd                                ; Clock             ;
; N/A   ; None         ; 4.000 ns   ; Reset           ; main:inst3|Data_drive:b2v_inst|cnt1[1]                        ; Clk_SCL           ;
; N/A   ; None         ; 4.000 ns   ; Reset           ; main:inst3|Data_drive:b2v_inst|cnt1[2]                        ; Clk_SCL           ;
; N/A   ; None         ; 4.000 ns   ; Reset           ; main:inst3|Data_drive:b2v_inst|cnt1[3]                        ; Clk_SCL           ;
; N/A   ; None         ; 4.000 ns   ; Reset           ; main:inst3|Data_drive:b2v_inst|cnt1[4]                        ; Clk_SCL           ;
; N/A   ; None         ; 4.000 ns   ; Reset           ; main:inst3|Data_drive:b2v_inst|cnt1[5]                        ; Clk_SCL           ;
; N/A   ; None         ; 4.000 ns   ; Reset           ; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select                 ; Clk_SCL           ;
; N/A   ; None         ; 4.000 ns   ; Reset           ; main:inst3|Data_drive:b2v_inst|Adc_Conv                       ; Clk_SCL           ;
; N/A   ; None         ; 3.600 ns   ; Current_SW      ; main:inst3|Data_drive:b2v_inst|cnt1[0]                        ; Clk_SCL           ;
; N/A   ; None         ; 3.600 ns   ; Current_SW      ; main:inst3|Data_drive:b2v_inst|cnt1[1]                        ; Clk_SCL           ;
; N/A   ; None         ; 3.600 ns   ; Current_SW      ; main:inst3|Data_drive:b2v_inst|cnt1[2]                        ; Clk_SCL           ;
; N/A   ; None         ; 3.600 ns   ; Current_SW      ; main:inst3|Data_drive:b2v_inst|cnt1[3]                        ; Clk_SCL           ;
; N/A   ; None         ; 3.600 ns   ; Current_SW      ; main:inst3|Data_drive:b2v_inst|cnt1[4]                        ; Clk_SCL           ;
; N/A   ; None         ; 3.600 ns   ; Current_SW      ; main:inst3|Data_drive:b2v_inst|cnt1[5]                        ; Clk_SCL           ;
; N/A   ; None         ; 3.600 ns   ; Current_SW      ; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select                 ; Clk_SCL           ;
; N/A   ; None         ; 3.600 ns   ; Current_SW      ; main:inst3|Data_drive:b2v_inst|Adc_Conv                       ; Clk_SCL           ;
; N/A   ; None         ; 3.500 ns   ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|cnt1[0]                        ; Clk_SCL           ;
; N/A   ; None         ; 3.500 ns   ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|cnt1[1]                        ; Clk_SCL           ;
; N/A   ; None         ; 3.500 ns   ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|cnt1[2]                        ; Clk_SCL           ;
; N/A   ; None         ; 3.500 ns   ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|cnt1[3]                        ; Clk_SCL           ;
; N/A   ; None         ; 3.500 ns   ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|cnt1[4]                        ; Clk_SCL           ;
; N/A   ; None         ; 3.500 ns   ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|cnt1[5]                        ; Clk_SCL           ;
; N/A   ; None         ; 3.500 ns   ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select                 ; Clk_SCL           ;
; N/A   ; None         ; 3.500 ns   ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|Adc_Conv                       ; Clk_SCL           ;
; N/A   ; None         ; 3.500 ns   ; Position_SW     ; Position_adc_ctrl:inst6|Adc_Mode                              ; Clock             ;
; N/A   ; None         ; 3.500 ns   ; Position_SW     ; Position_adc_ctrl:inst6|Adc_Cs                                ; Clock             ;
; N/A   ; None         ; 3.500 ns   ; Position_SW     ; Position_adc_ctrl:inst6|Adc_Conv                              ; Clock             ;
; N/A   ; None         ; 3.500 ns   ; Position_SW     ; Position_adc_ctrl:inst6|Adc_Rd                                ; Clock             ;
; N/A   ; None         ; 3.400 ns   ; AD7492_Busy     ; Position_adc_ctrl:inst6|Adc_Conv                              ; Clock             ;
; N/A   ; None         ; 3.400 ns   ; AD7492_Busy     ; Position_adc_ctrl:inst6|Adc_Rd                                ; Clock             ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse        ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.400 ns   ; Reset           ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse        ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 1.000 ns   ; Rate_SW         ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse        ;
; N/A   ; None         ; -2.500 ns  ; AD7492_Data[0]  ; Position_adc_ctrl:inst6|Position_Data[0]                      ; Clock             ;
; N/A   ; None         ; -2.500 ns  ; AD7492_Data[1]  ; Position_adc_ctrl:inst6|Position_Data[1]                      ; Clock             ;
; N/A   ; None         ; -2.500 ns  ; AD7492_Data[2]  ; Position_adc_ctrl:inst6|Position_Data[2]                      ; Clock             ;
; N/A   ; None         ; -2.500 ns  ; AD7492_Data[3]  ; Position_adc_ctrl:inst6|Position_Data[3]                      ; Clock             ;
; N/A   ; None         ; -2.500 ns  ; AD7492_Data[4]  ; Position_adc_ctrl:inst6|Position_Data[4]                      ; Clock             ;
; N/A   ; None         ; -2.500 ns  ; AD7492_Data[5]  ; Position_adc_ctrl:inst6|Position_Data[5]                      ; Clock             ;
; N/A   ; None         ; -2.500 ns  ; AD7492_Data[6]  ; Position_adc_ctrl:inst6|Position_Data[6]                      ; Clock             ;
; N/A   ; None         ; -2.500 ns  ; AD7492_Data[7]  ; Position_adc_ctrl:inst6|Position_Data[7]                      ; Clock             ;
; N/A   ; None         ; -2.500 ns  ; AD7492_Data[8]  ; Position_adc_ctrl:inst6|Position_Data[8]                      ; Clock             ;
; N/A   ; None         ; -2.500 ns  ; AD7492_Data[9]  ; Position_adc_ctrl:inst6|Position_Data[9]                      ; Clock             ;
; N/A   ; None         ; -2.500 ns  ; AD7492_Data[10] ; Position_adc_ctrl:inst6|Position_Data[10]                     ; Clock             ;
; N/A   ; None         ; -2.500 ns  ; AD7492_Data[11] ; Position_adc_ctrl:inst6|Position_Data[11]                     ; Clock             ;
; N/A   ; None         ; -2.800 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[14]                       ; Clk_SCL           ;
; N/A   ; None         ; -2.800 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[13]                       ; Clk_SCL           ;
; N/A   ; None         ; -2.800 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[12]                       ; Clk_SCL           ;
; N/A   ; None         ; -2.800 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[11]                       ; Clk_SCL           ;
; N/A   ; None         ; -2.800 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[9]                        ; Clk_SCL           ;
; N/A   ; None         ; -2.800 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[7]                        ; Clk_SCL           ;
; N/A   ; None         ; -2.800 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[6]                        ; Clk_SCL           ;
; N/A   ; None         ; -2.800 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[5]                        ; Clk_SCL           ;
; N/A   ; None         ; -2.800 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[4]                        ; Clk_SCL           ;
; N/A   ; None         ; -2.800 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[15]                       ; Clk_SCL           ;
; N/A   ; None         ; -2.800 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[10]                       ; Clk_SCL           ;
; N/A   ; None         ; -2.800 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[8]                        ; Clk_SCL           ;
+-------+--------------+------------+-----------------+---------------------------------------------------------------+-------------------+


+-----------------------------------------------------------------------------------------------------------------------------------------------+
; tco                                                                                                                                           ;
+-------+--------------+------------+---------------------------------------------------------------+-----------------------+-------------------+
; Slack ; Required tco ; Actual tco ; From                                                          ; To                    ; From Clock        ;
+-------+--------------+------------+---------------------------------------------------------------+-----------------------+-------------------+
; N/A   ; None         ; 24.600 ns  ; main:inst3|Data_Read:b2v_inst1|Data[14]                       ; Current_Adjust_Drive  ; Clk_SCL           ;
; N/A   ; None         ; 24.600 ns  ; main:inst3|Data_Read:b2v_inst1|Data[13]                       ; Current_Adjust_Drive  ; Clk_SCL           ;
; N/A   ; None         ; 24.500 ns  ; main:inst3|Data_Read:b2v_inst1|Data[12]                       ; Current_Adjust_Drive  ; Clk_SCL           ;
; N/A   ; None         ; 24.500 ns  ; main:inst3|Data_Read:b2v_inst1|Data[15]                       ; Current_Adjust_Drive  ; Clk_SCL           ;
; N/A   ; None         ; 22.900 ns  ; main:inst3|Data_Read:b2v_inst1|Data[11]                       ; Current_Adjust_Drive  ; Clk_SCL           ;
; N/A   ; None         ; 22.900 ns  ; main:inst3|Data_Read:b2v_inst1|Data[9]                        ; Current_Adjust_Drive  ; Clk_SCL           ;
; N/A   ; None         ; 22.900 ns  ; main:inst3|Data_Read:b2v_inst1|Data[7]                        ; Current_Adjust_Drive  ; Clk_SCL           ;
; N/A   ; None         ; 22.900 ns  ; main:inst3|Data_Read:b2v_inst1|Data[6]                        ; Current_Adjust_Drive  ; Clk_SCL           ;
; N/A   ; None         ; 22.900 ns  ; main:inst3|Data_Read:b2v_inst1|Data[5]                        ; Current_Adjust_Drive  ; Clk_SCL           ;
; N/A   ; None         ; 22.900 ns  ; main:inst3|Data_Read:b2v_inst1|Data[4]                        ; Current_Adjust_Drive  ; Clk_SCL           ;
; N/A   ; None         ; 22.900 ns  ; main:inst3|Data_Read:b2v_inst1|Data[10]                       ; Current_Adjust_Drive  ; Clk_SCL           ;
; N/A   ; None         ; 22.900 ns  ; main:inst3|Data_Read:b2v_inst1|Data[8]                        ; Current_Adjust_Drive  ; Clk_SCL           ;
; N/A   ; None         ; 20.700 ns  ; Position_adc_ctrl:inst6|Position_Data[11]                     ; Position_Adjust_Drive ; Clock             ;
; N/A   ; None         ; 20.700 ns  ; Position_adc_ctrl:inst6|Position_Data[10]                     ; Position_Adjust_Drive ; Clock             ;
; N/A   ; None         ; 20.700 ns  ; Position_adc_ctrl:inst6|Position_Data[9]                      ; Position_Adjust_Drive ; Clock             ;
; N/A   ; None         ; 20.700 ns  ; Position_adc_ctrl:inst6|Position_Data[8]                      ; Position_Adjust_Drive ; Clock             ;
; N/A   ; None         ; 19.000 ns  ; Position_adc_ctrl:inst6|Position_Data[7]                      ; Position_Adjust_Drive ; Clock             ;
; N/A   ; None         ; 19.000 ns  ; Position_adc_ctrl:inst6|Position_Data[6]                      ; Position_Adjust_Drive ; Clock             ;
; N/A   ; None         ; 19.000 ns  ; Position_adc_ctrl:inst6|Position_Data[5]                      ; Position_Adjust_Drive ; Clock             ;
; N/A   ; None         ; 19.000 ns  ; Position_adc_ctrl:inst6|Position_Data[4]                      ; Position_Adjust_Drive ; Clock             ;
; N/A   ; None         ; 19.000 ns  ; Position_adc_ctrl:inst6|Position_Data[3]                      ; Position_Adjust_Drive ; Clock             ;
; N/A   ; None         ; 19.000 ns  ; Position_adc_ctrl:inst6|Position_Data[2]                      ; Position_Adjust_Drive ; Clock             ;
; N/A   ; None         ; 19.000 ns  ; Position_adc_ctrl:inst6|Position_Data[1]                      ; Position_Adjust_Drive ; Clock             ;
; N/A   ; None         ; 19.000 ns  ; Position_adc_ctrl:inst6|Position_Data[0]                      ; Position_Adjust_Drive ; Clock             ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 17.500 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 15.900 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 15.900 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 15.900 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 15.900 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 15.800 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 15.800 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 15.800 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 15.800 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 15.800 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 15.800 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 15.800 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 15.800 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 15.800 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 15.800 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 15.800 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Adjust_Drive     ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 15.800 ns  ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Adjust_Drive     ; Rate_Pulse        ;
; N/A   ; None         ; 9.500 ns   ; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select                 ; AD7895_SCL            ; Clk_SCL           ;
; N/A   ; None         ; 6.600 ns   ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Over             ; Rate_Measure_Ctrl ;
; N/A   ; None         ; 6.600 ns   ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Over             ; Rate_Pulse        ;
; N/A   ; None         ; 4.000 ns   ; main:inst3|Data_drive:b2v_inst|Adc_Conv                       ; AD7895_Conv           ; Clk_SCL           ;
; N/A   ; None         ; 4.000 ns   ; Position_adc_ctrl:inst6|Adc_Conv                              ; AD7492_Conv           ; Clock             ;
; N/A   ; None         ; 4.000 ns   ; Position_adc_ctrl:inst6|Adc_Rd                                ; AD7492_RD             ; Clock             ;
; N/A   ; None         ; 4.000 ns   ; Position_adc_ctrl:inst6|Adc_Cs                                ; AD7492_CS             ; Clock             ;
; N/A   ; None         ; 4.000 ns   ; Position_adc_ctrl:inst6|Adc_Mode                              ; AD7492_Mode           ; Clock             ;
+-------+--------------+------------+---------------------------------------------------------------+-----------------------+-------------------+


+----------------------------------------------------------------------------------------+
; tpd                                                                                    ;
+-------+-------------------+-----------------+------------------+-----------------------+
; Slack ; Required P2P Time ; Actual P2P Time ; From             ; To                    ;
+-------+-------------------+-----------------+------------------+-----------------------+
; N/A   ; None              ; 11.400 ns       ; Rate_Set[8]      ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 11.400 ns       ; Rate_Set[9]      ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 11.400 ns       ; Rate_Set[10]     ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 11.400 ns       ; Rate_Set[11]     ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 11.400 ns       ; Rate_Set[12]     ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 11.400 ns       ; Rate_Set[13]     ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 11.400 ns       ; Rate_Set[14]     ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 11.400 ns       ; Rate_Set[15]     ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 11.400 ns       ; Current_Set[8]   ; Current_Adjust_Drive  ;
; N/A   ; None              ; 11.400 ns       ; Current_Set[9]   ; Current_Adjust_Drive  ;
; N/A   ; None              ; 11.400 ns       ; Current_Set[10]  ; Current_Adjust_Drive  ;
; N/A   ; None              ; 11.400 ns       ; Current_Set[11]  ; Current_Adjust_Drive  ;
; N/A   ; None              ; 11.400 ns       ; Position_Set[8]  ; Position_Adjust_Drive ;
; N/A   ; None              ; 11.400 ns       ; Position_Set[9]  ; Position_Adjust_Drive ;
; N/A   ; None              ; 11.400 ns       ; Position_Set[10] ; Position_Adjust_Drive ;
; N/A   ; None              ; 11.400 ns       ; Position_Set[11] ; Position_Adjust_Drive ;
; N/A   ; None              ; 9.700 ns        ; Rate_Set[0]      ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 9.700 ns        ; Rate_Set[1]      ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 9.700 ns        ; Rate_Set[2]      ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 9.700 ns        ; Rate_Set[3]      ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 9.700 ns        ; Rate_Set[4]      ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 9.700 ns        ; Rate_Set[5]      ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 9.700 ns        ; Rate_Set[6]      ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 9.700 ns        ; Rate_Set[7]      ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 9.700 ns        ; Current_Set[0]   ; Current_Adjust_Drive  ;
; N/A   ; None              ; 9.700 ns        ; Current_Set[1]   ; Current_Adjust_Drive  ;
; N/A   ; None              ; 9.700 ns        ; Current_Set[2]   ; Current_Adjust_Drive  ;
; N/A   ; None              ; 9.700 ns        ; Current_Set[3]   ; Current_Adjust_Drive  ;
; N/A   ; None              ; 9.700 ns        ; Current_Set[4]   ; Current_Adjust_Drive  ;
; N/A   ; None              ; 9.700 ns        ; Current_Set[5]   ; Current_Adjust_Drive  ;
; N/A   ; None              ; 9.700 ns        ; Current_Set[6]   ; Current_Adjust_Drive  ;
; N/A   ; None              ; 9.700 ns        ; Current_Set[7]   ; Current_Adjust_Drive  ;
; N/A   ; None              ; 9.700 ns        ; Position_Set[0]  ; Position_Adjust_Drive ;
; N/A   ; None              ; 9.700 ns        ; Position_Set[1]  ; Position_Adjust_Drive ;
; N/A   ; None              ; 9.700 ns        ; Position_Set[2]  ; Position_Adjust_Drive ;
; N/A   ; None              ; 9.700 ns        ; Position_Set[3]  ; Position_Adjust_Drive ;
; N/A   ; None              ; 9.700 ns        ; Position_Set[4]  ; Position_Adjust_Drive ;
; N/A   ; None              ; 9.700 ns        ; Position_Set[5]  ; Position_Adjust_Drive ;
; N/A   ; None              ; 9.700 ns        ; Position_Set[6]  ; Position_Adjust_Drive ;
; N/A   ; None              ; 9.700 ns        ; Position_Set[7]  ; Position_Adjust_Drive ;
; N/A   ; None              ; 6.600 ns        ; Reset            ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 6.600 ns        ; Reset            ; Current_Adjust_Drive  ;
; N/A   ; None              ; 6.600 ns        ; Reset            ; Position_Adjust_Drive ;
; N/A   ; None              ; 6.200 ns        ; Rate_SW          ; Rate_Adjust_Drive     ;
; N/A   ; None              ; 6.200 ns        ; Current_SW       ; Current_Adjust_Drive  ;
; N/A   ; None              ; 6.100 ns        ; Clk_SCL          ; AD7895_SCL            ;
; N/A   ; None              ; 6.100 ns        ; Position_SW      ; Position_Adjust_Drive ;
+-------+-------------------+-----------------+------------------+-----------------------+


+-----------------------------------------------------------------------------------------------------------------------------------------------+
; th                                                                                                                                            ;
+---------------+-------------+-----------+-----------------+---------------------------------------------------------------+-------------------+
; Minimum Slack ; Required th ; Actual th ; From            ; To                                                            ; To Clock          ;
+---------------+-------------+-----------+-----------------+---------------------------------------------------------------+-------------------+
; N/A           ; None        ; 8.900 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[14]                       ; Clk_SCL           ;
; N/A           ; None        ; 8.900 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[13]                       ; Clk_SCL           ;
; N/A           ; None        ; 8.900 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[12]                       ; Clk_SCL           ;
; N/A           ; None        ; 8.900 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[11]                       ; Clk_SCL           ;
; N/A           ; None        ; 8.900 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[9]                        ; Clk_SCL           ;
; N/A           ; None        ; 8.900 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[7]                        ; Clk_SCL           ;
; N/A           ; None        ; 8.900 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[6]                        ; Clk_SCL           ;
; N/A           ; None        ; 8.900 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[5]                        ; Clk_SCL           ;
; N/A           ; None        ; 8.900 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[4]                        ; Clk_SCL           ;
; N/A           ; None        ; 8.900 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[15]                       ; Clk_SCL           ;
; N/A           ; None        ; 8.900 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[10]                       ; Clk_SCL           ;
; N/A           ; None        ; 8.900 ns  ; AD7895_Data     ; main:inst3|Data_Read:b2v_inst1|Data[8]                        ; Clk_SCL           ;
; N/A           ; None        ; 5.200 ns  ; AD7492_Data[0]  ; Position_adc_ctrl:inst6|Position_Data[0]                      ; Clock             ;
; N/A           ; None        ; 5.200 ns  ; AD7492_Data[1]  ; Position_adc_ctrl:inst6|Position_Data[1]                      ; Clock             ;
; N/A           ; None        ; 5.200 ns  ; AD7492_Data[2]  ; Position_adc_ctrl:inst6|Position_Data[2]                      ; Clock             ;
; N/A           ; None        ; 5.200 ns  ; AD7492_Data[3]  ; Position_adc_ctrl:inst6|Position_Data[3]                      ; Clock             ;
; N/A           ; None        ; 5.200 ns  ; AD7492_Data[4]  ; Position_adc_ctrl:inst6|Position_Data[4]                      ; Clock             ;
; N/A           ; None        ; 5.200 ns  ; AD7492_Data[5]  ; Position_adc_ctrl:inst6|Position_Data[5]                      ; Clock             ;
; N/A           ; None        ; 5.200 ns  ; AD7492_Data[6]  ; Position_adc_ctrl:inst6|Position_Data[6]                      ; Clock             ;
; N/A           ; None        ; 5.200 ns  ; AD7492_Data[7]  ; Position_adc_ctrl:inst6|Position_Data[7]                      ; Clock             ;
; N/A           ; None        ; 5.200 ns  ; AD7492_Data[8]  ; Position_adc_ctrl:inst6|Position_Data[8]                      ; Clock             ;
; N/A           ; None        ; 5.200 ns  ; AD7492_Data[9]  ; Position_adc_ctrl:inst6|Position_Data[9]                      ; Clock             ;
; N/A           ; None        ; 5.200 ns  ; AD7492_Data[10] ; Position_adc_ctrl:inst6|Position_Data[10]                     ; Clock             ;
; N/A           ; None        ; 5.200 ns  ; AD7492_Data[11] ; Position_adc_ctrl:inst6|Position_Data[11]                     ; Clock             ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse        ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.700 ns  ; Rate_SW         ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]  ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10] ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11] ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12] ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13] ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14] ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15] ; Rate_Pulse        ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Measure_Ctrl ;
; N/A           ; None        ; 1.300 ns  ; Reset           ; Rate_Measure:inst2|Rate_Pulse_Alarm                           ; Rate_Pulse        ;
; N/A           ; None        ; -0.700 ns ; AD7492_Busy     ; Position_adc_ctrl:inst6|Adc_Conv                              ; Clock             ;
; N/A           ; None        ; -0.700 ns ; AD7492_Busy     ; Position_adc_ctrl:inst6|Adc_Rd                                ; Clock             ;
; N/A           ; None        ; -0.800 ns ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|cnt1[0]                        ; Clk_SCL           ;
; N/A           ; None        ; -0.800 ns ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|cnt1[1]                        ; Clk_SCL           ;
; N/A           ; None        ; -0.800 ns ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|cnt1[2]                        ; Clk_SCL           ;
; N/A           ; None        ; -0.800 ns ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|cnt1[3]                        ; Clk_SCL           ;
; N/A           ; None        ; -0.800 ns ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|cnt1[4]                        ; Clk_SCL           ;
; N/A           ; None        ; -0.800 ns ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|cnt1[5]                        ; Clk_SCL           ;
; N/A           ; None        ; -0.800 ns ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select                 ; Clk_SCL           ;
; N/A           ; None        ; -0.800 ns ; AD7895_Busy     ; main:inst3|Data_drive:b2v_inst|Adc_Conv                       ; Clk_SCL           ;
; N/A           ; None        ; -0.800 ns ; Position_SW     ; Position_adc_ctrl:inst6|Adc_Mode                              ; Clock             ;
; N/A           ; None        ; -0.800 ns ; Position_SW     ; Position_adc_ctrl:inst6|Adc_Cs                                ; Clock             ;
; N/A           ; None        ; -0.800 ns ; Position_SW     ; Position_adc_ctrl:inst6|Adc_Conv                              ; Clock             ;
; N/A           ; None        ; -0.800 ns ; Position_SW     ; Position_adc_ctrl:inst6|Adc_Rd                                ; Clock             ;
; N/A           ; None        ; -0.900 ns ; Current_SW      ; main:inst3|Data_drive:b2v_inst|cnt1[0]                        ; Clk_SCL           ;
; N/A           ; None        ; -0.900 ns ; Current_SW      ; main:inst3|Data_drive:b2v_inst|cnt1[1]                        ; Clk_SCL           ;
; N/A           ; None        ; -0.900 ns ; Current_SW      ; main:inst3|Data_drive:b2v_inst|cnt1[2]                        ; Clk_SCL           ;
; N/A           ; None        ; -0.900 ns ; Current_SW      ; main:inst3|Data_drive:b2v_inst|cnt1[3]                        ; Clk_SCL           ;
; N/A           ; None        ; -0.900 ns ; Current_SW      ; main:inst3|Data_drive:b2v_inst|cnt1[4]                        ; Clk_SCL           ;
; N/A           ; None        ; -0.900 ns ; Current_SW      ; main:inst3|Data_drive:b2v_inst|cnt1[5]                        ; Clk_SCL           ;
; N/A           ; None        ; -0.900 ns ; Current_SW      ; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select                 ; Clk_SCL           ;
; N/A           ; None        ; -0.900 ns ; Current_SW      ; main:inst3|Data_drive:b2v_inst|Adc_Conv                       ; Clk_SCL           ;
; N/A           ; None        ; -1.300 ns ; Reset           ; Position_adc_ctrl:inst6|Adc_Mode                              ; Clock             ;
; N/A           ; None        ; -1.300 ns ; Reset           ; Position_adc_ctrl:inst6|Adc_Cs                                ; Clock             ;
; N/A           ; None        ; -1.300 ns ; Reset           ; main:inst3|Data_drive:b2v_inst|cnt1[0]                        ; Clk_SCL           ;
; N/A           ; None        ; -1.300 ns ; Reset           ; Position_adc_ctrl:inst6|Adc_Conv                              ; Clock             ;
; N/A           ; None        ; -1.300 ns ; Reset           ; Position_adc_ctrl:inst6|Adc_Rd                                ; Clock             ;
; N/A           ; None        ; -1.300 ns ; Reset           ; main:inst3|Data_drive:b2v_inst|cnt1[1]                        ; Clk_SCL           ;
; N/A           ; None        ; -1.300 ns ; Reset           ; main:inst3|Data_drive:b2v_inst|cnt1[2]                        ; Clk_SCL           ;
; N/A           ; None        ; -1.300 ns ; Reset           ; main:inst3|Data_drive:b2v_inst|cnt1[3]                        ; Clk_SCL           ;
; N/A           ; None        ; -1.300 ns ; Reset           ; main:inst3|Data_drive:b2v_inst|cnt1[4]                        ; Clk_SCL           ;
; N/A           ; None        ; -1.300 ns ; Reset           ; main:inst3|Data_drive:b2v_inst|cnt1[5]                        ; Clk_SCL           ;
; N/A           ; None        ; -1.300 ns ; Reset           ; main:inst3|Data_drive:b2v_inst|Adc_SCL_Select                 ; Clk_SCL           ;
; N/A           ; None        ; -1.300 ns ; Reset           ; main:inst3|Data_drive:b2v_inst|Adc_Conv                       ; Clk_SCL           ;
+---------------+-------------+-----------+-----------------+---------------------------------------------------------------+-------------------+


+--------------------------+
; Timing Analyzer Messages ;
+--------------------------+
Info: *******************************************************************
Info: Running Quartus II Timing Analyzer
    Info: Version 4.2 Build 157 12/07/2004 SJ Full Version
    Info: Processing started: Fri Aug 04 19:03:53 2006
Info: Command: quartus_tan --import_settings_files=off --export_settings_files=off DC_Motor_Main -c DC_Motor_Main
Info: Started post-fitting delay annotation
Info: Delay annotation completed successfully
Warning: Found pins functioning as undefined clocks and/or memory enables
    Info: Assuming node "Clock" is an undefined clock
    Info: Assuming node "Clk_SCL" is an undefined clock
    Info: Assuming node "Rate_Pulse" is an undefined clock
    Info: Assuming node "Rate_Measure_Ctrl" is an undefined clock
Warning: Found 4 node(s) in clock paths which may be acting as ripple and/or gated clocks -- node(s) analyzed as buffer(s) resulting in clock skew
    Info: Detected gated clock "main:inst3|Data_drive:b2v_inst|Adc_SCL~58" as buffer
    Info: Detected gated clock "main:inst3|Data_drive:b2v_inst|Adc_SCL~42" as buffer
    Info: Detected ripple clock "main:inst3|Data_drive:b2v_inst|Adc_SCL_Select" as buffer
    Info: Detected ripple clock "Position_adc_ctrl:inst6|Adc_Rd" as buffer
Info: No valid register-to-register data paths exist for clock "Clock"
Info: Clock "Clk_SCL" has Internal fmax of 97.09 MHz between source register "main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0]" and destination register "main:inst3|Data_Read:b2v_inst1|Data[8]" (period= 10.3 ns)
    Info: + Longest register to register delay is 4.500 ns
        Info: 1: + IC(0.000 ns) + CELL(0.000 ns) = 0.000 ns; Loc. = LC61; Fanout = 28; REG Node = 'main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0]'
        Info: 2: + IC(1.500 ns) + CELL(3.000 ns) = 4.500 ns; Loc. = LC59; Fanout = 5; REG Node = 'main:inst3|Data_Read:b2v_inst1|Data[8]'
        Info: Total cell delay = 3.000 ns ( 66.67 % )
        Info: Total interconnect delay = 1.500 ns ( 33.33 % )
    Info: - Smallest clock skew is -3.400 ns
        Info: + Shortest clock path from clock "Clk_SCL" to destination register is 8.500 ns
            Info: 1: + IC(0.000 ns) + CELL(1.600 ns) = 1.600 ns; Loc. = PIN_87; Fanout = 11; CLK Node = 'Clk_SCL'
            Info: 2: + IC(0.100 ns) + CELL(3.700 ns) = 5.400 ns; Loc. = SEXP50; Fanout = 14; COMB Node = 'main:inst3|Data_drive:b2v_inst|Adc_SCL~42'
            Info: 3: + IC(0.000 ns) + CELL(3.100 ns) = 8.500 ns; Loc. = LC59; Fanout = 5; REG Node = 'main:inst3|Data_Read:b2v_inst1|Data[8]'
            Info: Total cell delay = 8.400 ns ( 98.82 % )
            Info: Total interconnect delay = 0.100 ns ( 1.18 % )
        Info: - Longest clock path from clock "Clk_SCL" to source register is 11.900 ns
            Info: 1: + IC(0.000 ns) + CELL(1.600 ns) = 1.600 ns; Loc. = PIN_87; Fanout = 11; CLK Node = 'Clk_SCL'
            Info: 2: + IC(0.000 ns) + CELL(2.000 ns) = 3.600 ns; Loc. = LC60; Fanout = 3; REG Node = 'main:inst3|Data_drive:b2v_inst|Adc_SCL_Select'
            Info: 3: + IC(1.500 ns) + CELL(3.700 ns) = 8.800 ns; Loc. = SEXP50; Fanout = 14; COMB Node = 'main:inst3|Data_drive:b2v_inst|Adc_SCL~42'
            Info: 4: + IC(0.000 ns) + CELL(3.100 ns) = 11.900 ns; Loc. = LC61; Fanout = 28; REG Node = 'main:inst3|Data_Read:b2v_inst1|lpm_counter:cnt_rtl_1|dffs[0]'
            Info: Total cell delay = 10.400 ns ( 87.39 % )
            Info: Total interconnect delay = 1.500 ns ( 12.61 % )
    Info: + Micro clock to output delay of source is 1.400 ns
    Info: + Micro setup delay of destination is 1.000 ns
Info: Clock "Rate_Pulse" has Internal fmax of 142.86 MHz between source register "Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]" and destination register "Rate_Measure:inst2|Rate_Pulse_Alarm" (period= 7.0 ns)
    Info: + Longest register to register delay is 4.600 ns
        Info: 1: + IC(0.000 ns) + CELL(0.000 ns) = 0.000 ns; Loc. = LC67; Fanout = 21; REG Node = 'Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]'
        Info: 2: + IC(1.600 ns) + CELL(3.000 ns) = 4.600 ns; Loc. = LC1; Fanout = 1; REG Node = 'Rate_Measure:inst2|Rate_Pulse_Alarm'
        Info: Total cell delay = 3.000 ns ( 65.22 % )
        Info: Total interconnect delay = 1.600 ns ( 34.78 % )
    Info: - Smallest clock skew is 0.000 ns
        Info: + Shortest clock path from clock "Rate_Pulse" to destination register is 4.800 ns
            Info: 1: + IC(0.000 ns) + CELL(0.200 ns) = 0.200 ns; Loc. = PIN_60; Fanout = 17; CLK Node = 'Rate_Pulse'
            Info: 2: + IC(1.500 ns) + CELL(3.100 ns) = 4.800 ns; Loc. = LC1; Fanout = 1; REG Node = 'Rate_Measure:inst2|Rate_Pulse_Alarm'
            Info: Total cell delay = 3.300 ns ( 68.75 % )
            Info: Total interconnect delay = 1.500 ns ( 31.25 % )
        Info: - Longest clock path from clock "Rate_Pulse" to source register is 4.800 ns
            Info: 1: + IC(0.000 ns) + CELL(0.200 ns) = 0.200 ns; Loc. = PIN_60; Fanout = 17; CLK Node = 'Rate_Pulse'
            Info: 2: + IC(1.500 ns) + CELL(3.100 ns) = 4.800 ns; Loc. = LC67; Fanout = 21; REG Node = 'Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]'
            Info: Total cell delay = 3.300 ns ( 68.75 % )
            Info: Total interconnect delay = 1.500 ns ( 31.25 % )
    Info: + Micro clock to output delay of source is 1.400 ns
    Info: + Micro setup delay of destination is 1.000 ns
Info: Clock "Rate_Measure_Ctrl" has Internal fmax of 142.86 MHz between source register "Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]" and destination register "Rate_Measure:inst2|Rate_Pulse_Alarm" (period= 7.0 ns)
    Info: + Longest register to register delay is 4.600 ns
        Info: 1: + IC(0.000 ns) + CELL(0.000 ns) = 0.000 ns; Loc. = LC67; Fanout = 21; REG Node = 'Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]'
        Info: 2: + IC(1.600 ns) + CELL(3.000 ns) = 4.600 ns; Loc. = LC1; Fanout = 1; REG Node = 'Rate_Measure:inst2|Rate_Pulse_Alarm'
        Info: Total cell delay = 3.000 ns ( 65.22 % )
        Info: Total interconnect delay = 1.600 ns ( 34.78 % )
    Info: - Smallest clock skew is 0.000 ns
        Info: + Shortest clock path from clock "Rate_Measure_Ctrl" to destination register is 4.800 ns
            Info: 1: + IC(0.000 ns) + CELL(0.200 ns) = 0.200 ns; Loc. = PIN_68; Fanout = 17; CLK Node = 'Rate_Measure_Ctrl'
            Info: 2: + IC(1.500 ns) + CELL(3.100 ns) = 4.800 ns; Loc. = LC1; Fanout = 1; REG Node = 'Rate_Measure:inst2|Rate_Pulse_Alarm'
            Info: Total cell delay = 3.300 ns ( 68.75 % )
            Info: Total interconnect delay = 1.500 ns ( 31.25 % )
        Info: - Longest clock path from clock "Rate_Measure_Ctrl" to source register is 4.800 ns
            Info: 1: + IC(0.000 ns) + CELL(0.200 ns) = 0.200 ns; Loc. = PIN_68; Fanout = 17; CLK Node = 'Rate_Measure_Ctrl'
            Info: 2: + IC(1.500 ns) + CELL(3.100 ns) = 4.800 ns; Loc. = LC67; Fanout = 21; REG Node = 'Rate_Measure:inst2|lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]'
            Info: Total cell delay = 3.300 ns ( 68.75 % )
            Info: Total interconnect delay = 1.500 ns ( 31.25 % )
    Info: + Micro clock to output delay of source is 1.400 ns
    Info: + Micro setup delay of destination is 1.000 ns
Info: tsu for register "Position_adc_ctrl:inst6|Adc_Mode" (data pin = "Reset", clock pin = "Clock") is 4.000 ns
    Info: + Longest pin to register delay is 5.200 ns
        Info: 1: + IC(0.000 ns) + CELL(0.200 ns) = 0.200 ns; Loc. = PIN_27; Fanout = 52; PIN Node = 'Reset'
        Info: 2: + IC(2.000 ns) + CELL(3.000 ns) = 5.200 ns; Loc. = LC19; Fanout = 1; REG Node = 'Position_adc_ctrl:inst6|Adc_Mode'
        Info: Total cell delay = 3.200 ns ( 61.54 % )
        Info: Total interconnect delay = 2.000 ns ( 38.46 % )
    Info: + Micro setup delay of destination is 1.000 ns
    Info: - Shortest clock path from clock "Clock" to destination register is 2.200 ns
        Info: 1: + IC(0.000 ns) + CELL(1.600 ns) = 1.600 ns; Loc. = PIN_90; Fanout = 4; CLK Node = 'Clock'
        Info: 2: + IC(0.000 ns) + CELL(0.600 ns) = 2.200 ns; Loc. = LC19; Fanout = 1; REG Node = 'Position_adc_ctrl:inst6|Adc_Mode'
        Info: Total cell delay = 2.200 ns ( 100.00 % )
Info: tco from clock "Clk_SCL" to destination pin "Current_Adjust_Drive" through register "main:inst3|Data_Read:b2v_inst1|Data[14]" is 24.600 ns
    Info: + Longest clock path from clock "Clk_SCL" to source register is 11.900 ns
        Info: 1: + IC(0.000 ns) + CELL(1.600 ns) = 1.600 ns; Loc. = PIN_87; Fanout = 11; CLK Node = 'Clk_SCL'
        Info: 2: + IC(0.000 ns) + CELL(2.000 ns) = 3.600 ns; Loc. = LC60; Fanout = 3; REG Node = 'main:inst3|Data_drive:b2v_inst|Adc_SCL_Select'
        Info: 3: + IC(1.500 ns) + CELL(3.700 ns) = 8.800 ns; Loc. = SEXP50; Fanout = 14; COMB Node = 'main:inst3|Data_drive:b2v_inst|Adc_SCL~42'
        Info: 4: + IC(0.000 ns) + CELL(3.100 ns) = 11.900 ns; Loc. = LC50; Fanout = 4; REG Node = 'main:inst3|Data_Read:b2v_inst1|Data[14]'
        Info: Total cell delay = 10.400 ns ( 87.39 % )
        Info: Total interconnect delay = 1.500 ns ( 12.61 % )
    Info: + Micro clock to output delay of source is 1.400 ns
    Info: + Longest register to pin delay is 11.300 ns
        Info: 1: + IC(0.000 ns) + CELL(0.000 ns) = 0.000 ns; Loc. = LC50; Fanout = 4; REG Node = 'main:inst3|Data_Read:b2v_inst1|Data[14]'
        Info: 2: + IC(1.500 ns) + CELL(4.000 ns) = 5.500 ns; Loc. = LC89; Fanout = 1; COMB Node = 'Current_Adjust:inst5|always0~139'
        Info: 3: + IC(1.400 ns) + CELL(4.000 ns) = 10.900 ns; Loc. = LC81; Fanout = 1; COMB Node = 'Current_Adjust:inst5|Current_Adjust_Out~14'
        Info: 4: + IC(0.000 ns) + CELL(0.400 ns) = 11.300 ns; Loc. = PIN_52; Fanout = 0; PIN Node = 'Current_Adjust_Drive'
        Info: Total cell delay = 8.400 ns ( 74.34 % )
        Info: Total interconnect delay = 2.900 ns ( 25.66 % )
Info: Longest tpd from source pin "Rate_Set[8]" to destination pin "Rate_Adjust_Drive" is 11.400 ns
    Info: 1: + IC(0.000 ns) + CELL(0.200 ns) = 0.200 ns; Loc. = PIN_61; Fanout = 1; PIN Node = 'Rate_Set[8]'
    Info: 2: + IC(1.400 ns) + CELL(4.000 ns) = 5.600 ns; Loc. = LC24; Fanout = 1; COMB Node = 'Rate_Adjust:inst11|always0~163'
    Info: 3: + IC(1.400 ns) + CELL(4.000 ns) = 11.000 ns; Loc. = LC113; Fanout = 1; COMB Node = 'Rate_Adjust:inst11|Rate_Adjust_Out~14'
    Info: 4: + IC(0.000 ns) + CELL(0.400 ns) = 11.400 ns; Loc. = PIN_75; Fanout = 0; PIN Node = 'Rate_Adjust_Drive'
    Info: Total cell delay = 8.600 ns ( 75.44 % )
    Info: Total interconnect delay = 2.800 ns ( 24.56 % )
Info: th for register "main:inst3|Data_Read:b2v_inst1|Data[14]" (data pin = "AD7895_Data", clock pin = "Clk_SCL") is 8.900 ns
    Info: + Longest clock path from clock "Clk_SCL" to destination register is 11.900 ns
        Info: 1: + IC(0.000 ns) + CELL(1.600 ns) = 1.600 ns; Loc. = PIN_87; Fanout = 11; CLK Node = 'Clk_SCL'
        Info: 2: + IC(0.000 ns) + CELL(2.000 ns) = 3.600 ns; Loc. = LC60; Fanout = 3; REG Node = 'main:inst3|Data_drive:b2v_inst|Adc_SCL_Select'
        Info: 3: + IC(1.500 ns) + CELL(3.700 ns) = 8.800 ns; Loc. = SEXP50; Fanout = 14; COMB Node = 'main:inst3|Data_drive:b2v_inst|Adc_SCL~42'
        Info: 4: + IC(0.000 ns) + CELL(3.100 ns) = 11.900 ns; Loc. = LC50; Fanout = 4; REG Node = 'main:inst3|Data_Read:b2v_inst1|Data[14]'
        Info: Total cell delay = 10.400 ns ( 87.39 % )
        Info: Total interconnect delay = 1.500 ns ( 12.61 % )
    Info: + Micro hold delay of destination is 1.700 ns
    Info: - Shortest pin to register delay is 4.700 ns
        Info: 1: + IC(0.000 ns) + CELL(0.200 ns) = 0.200 ns; Loc. = PIN_5; Fanout = 24; PIN Node = 'AD7895_Data'
        Info: 2: + IC(1.500 ns) + CELL(3.000 ns) = 4.700 ns; Loc. = LC50; Fanout = 4; REG Node = 'main:inst3|Data_Read:b2v_inst1|Data[14]'
        Info: Total cell delay = 3.200 ns ( 68.09 % )
        Info: Total interconnect delay = 1.500 ns ( 31.91 % )
Info: Quartus II Timing Analyzer was successful. 0 errors, 2 warnings
    Info: Processing ended: Fri Aug 04 19:03:55 2006
    Info: Elapsed time: 00:00:03


