--B1_dffs[0] is lpm_counter:hour_data0_rtl_1|dffs[0]
B1_dffs[0]_p1_out = !B1_dffs[1] & !B2_dffs[1] & !B1_dffs[0] & !B1_dffs[2];
B1_dffs[0]_p2_out = !B2_dffs[1] & !B1_dffs[0] & !B1_dffs[3];
B1_dffs[0]_p4_out = !B1_dffs[0] & !B1_dffs[2] & !B1_dffs[3] & !B2_dffs[0];
B1_dffs[0]_or_out = B1_dffs[0]_p1_out # B1_dffs[0]_p2_out # B1_dffs[0]_p4_out;
B1_dffs[0]_reg_input = B1_dffs[0]_or_out;
B1_dffs[0] = DFFE(B1_dffs[0]_reg_input, GLOBAL(clk), , , EN);


--B2_dffs[0] is lpm_counter:hour_data1_rtl_0|dffs[0]
B2_dffs[0]_p0_out = !B2_dffs[1] & !B1_dffs[3] & B2_dffs[0];
B2_dffs[0]_p1_out = EN & !B2_dffs[1] & B1_dffs[3] & !B2_dffs[0] & B1_dffs[2];
B2_dffs[0]_p2_out = !EN & B2_dffs[0];
B2_dffs[0]_p3_out = EN & !B2_dffs[1] & B1_dffs[3] & !B2_dffs[0] & B1_dffs[0];
B2_dffs[0]_p4_out = EN & B1_dffs[1] & !B2_dffs[1] & B1_dffs[3] & !B2_dffs[0];
B2_dffs[0]_or_out = B2L3 # B2_dffs[0]_p0_out # B2_dffs[0]_p1_out # B2_dffs[0]_p2_out # B2_dffs[0]_p3_out # B2_dffs[0]_p4_out;
B2_dffs[0]_reg_input = B2_dffs[0]_or_out;
B2_dffs[0] = DFFE(B2_dffs[0]_reg_input, GLOBAL(clk), , , );


--B1_dffs[1] is lpm_counter:hour_data0_rtl_1|dffs[1]
B1_dffs[1]_p0_out = !B1_dffs[3] & !B1_dffs[1] & B1_dffs[0] & !B2_dffs[0] & !B1_dffs[2];
B1_dffs[1]_p1_out = !B2_dffs[1] & !B1_dffs[3] & B1_dffs[1] & !B1_dffs[0];
B1_dffs[1]_p2_out = !B2_dffs[1] & !B1_dffs[3] & !B1_dffs[1] & B1_dffs[0];
B1_dffs[1]_p4_out = !B1_dffs[3] & B1_dffs[1] & !B1_dffs[0] & !B2_dffs[0] & !B1_dffs[2];
B1_dffs[1]_or_out = B1_dffs[1]_p0_out # B1_dffs[1]_p1_out # B1_dffs[1]_p2_out # B1_dffs[1]_p4_out;
B1_dffs[1]_reg_input = B1_dffs[1]_or_out;
B1_dffs[1] = DFFE(B1_dffs[1]_reg_input, GLOBAL(clk), , , EN);


--B1_dffs[2] is lpm_counter:hour_data0_rtl_1|dffs[2]
B1_dffs[2]_p0_out = !B1_dffs[3] & !B1_dffs[2] & B1_dffs[1] & B1_dffs[0] & !B2_dffs[0];
B1_dffs[2]_p1_out = !B2_dffs[1] & !B1_dffs[3] & B1_dffs[2] & !B1_dffs[1];
B1_dffs[2]_p2_out = !B2_dffs[1] & !B1_dffs[3] & B1_dffs[2] & !B1_dffs[0];
B1_dffs[2]_p4_out = !B2_dffs[1] & !B1_dffs[3] & !B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[2]_or_out = B1_dffs[2]_p0_out # B1_dffs[2]_p1_out # B1_dffs[2]_p2_out # B1_dffs[2]_p4_out;
B1_dffs[2]_reg_input = B1_dffs[2]_or_out;
B1_dffs[2] = DFFE(B1_dffs[2]_reg_input, GLOBAL(clk), , , EN);


--B1_dffs[3] is lpm_counter:hour_data0_rtl_1|dffs[3]
B1_dffs[3]_p1_out = !B2_dffs[1] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & !B1_dffs[0];
B1_dffs[3]_p2_out = !B2_dffs[1] & !B1_dffs[3] & B1_dffs[2] & B1_dffs[1] & B1_dffs[0];
B1_dffs[3]_or_out = B1_dffs[3]_p1_out # B1_dffs[3]_p2_out;
B1_dffs[3]_reg_input = B1_dffs[3]_or_out;
B1_dffs[3] = DFFE(B1_dffs[3]_reg_input, GLOBAL(clk), , , EN);


--B2_dffs[1] is lpm_counter:hour_data1_rtl_0|dffs[1]
B2_dffs[1]_p0_out = !B1_dffs[3] & !B2_dffs[0] & !B1_dffs[2] & B2_dffs[1];
B2_dffs[1]_p1_out = EN & B1_dffs[3] & B2_dffs[0] & B1_dffs[2] & !B2_dffs[1];
B2_dffs[1]_p2_out = EN & B1_dffs[3] & B2_dffs[0] & !B2_dffs[1] & B1_dffs[1];
B2_dffs[1]_p3_out = EN & B1_dffs[3] & B2_dffs[0] & !B2_dffs[1] & B1_dffs[0];
B2_dffs[1]_p4_out = !EN & B2_dffs[1];
B2_dffs[1]_or_out = B2_dffs[1]_p0_out # B2_dffs[1]_p1_out # B2_dffs[1]_p2_out # B2_dffs[1]_p3_out # B2_dffs[1]_p4_out;
B2_dffs[1]_reg_input = B2_dffs[1]_or_out;
B2_dffs[1] = DFFE(B2_dffs[1]_reg_input, GLOBAL(clk), , , );


--A1L3Q is EO~reg0
A1L3Q_p0_out = !B1_dffs[2] & A1L3Q & !B1_dffs[1] & !B1_dffs[0];
A1L3Q_p1_out = EN & B2_dffs[1] & B1_dffs[3];
A1L3Q_p2_out = EN & B2_dffs[1] & B2_dffs[0];
A1L3Q_p3_out = EN & B2_dffs[1] & B1_dffs[2];
A1L3Q_p4_out = !EN & A1L3Q;
A1L3Q_or_out = B2L5 # A1L3Q_p0_out # A1L3Q_p1_out # A1L3Q_p2_out # A1L3Q_p3_out # A1L3Q_p4_out;
A1L3Q_reg_input = A1L3Q_or_out;
A1L3Q = DFFE(A1L3Q_reg_input, GLOBAL(clk), , , );


--B2L3 is lpm_counter:hour_data1_rtl_0|dffs[0]~93
B2L3_p1_out = !B1_dffs[2] & !B2_dffs[1] & B2_dffs[0] & !B1_dffs[1] & !B1_dffs[0];
B2L3 = B2L3_p1_out;


--B2L5 is lpm_counter:hour_data1_rtl_0|dffs[1]~95
B2L5_p1_out = !B1_dffs[3] & A1L3Q;
B2L5 = B2L5_p1_out;


--~GND~0 is ~GND~0
~GND~0_or_out = GND;
~GND~0 = ~GND~0_or_out;


--~GND~1 is ~GND~1
~GND~1_or_out = GND;
~GND~1 = ~GND~1_or_out;


--clk is clk
--operation mode is input

clk = INPUT();


--EN is EN
--operation mode is input

EN = INPUT();


--SW1 is SW1
--operation mode is input

SW1 = INPUT();


--SW2 is SW2
--operation mode is input

SW2 = INPUT();


--hour_data1[3] is hour_data1[3]
--operation mode is output

hour_data1[3] = OUTPUT(~GND~0);


--hour_data1[2] is hour_data1[2]
--operation mode is output

hour_data1[2] = OUTPUT(~GND~1);


--hour_data0[0] is hour_data0[0]
--operation mode is output

hour_data0[0] = OUTPUT(B1_dffs[0]);


--hour_data1[0] is hour_data1[0]
--operation mode is output

hour_data1[0] = OUTPUT(B2_dffs[0]);


--hour_data0[1] is hour_data0[1]
--operation mode is output

hour_data0[1] = OUTPUT(B1_dffs[1]);


--hour_data0[2] is hour_data0[2]
--operation mode is output

hour_data0[2] = OUTPUT(B1_dffs[2]);


--hour_data0[3] is hour_data0[3]
--operation mode is output

hour_data0[3] = OUTPUT(B1_dffs[3]);


--hour_data1[1] is hour_data1[1]
--operation mode is output

hour_data1[1] = OUTPUT(B2_dffs[1]);


--EO is EO
--operation mode is output

EO = OUTPUT(A1L3Q);


