--B1_dffs[0] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[0]
B1_dffs[0]_p1_out = !B1_dffs[0] & !En & !Reset;
B1_dffs[0]_or_out = B1_dffs[0]_p1_out;
B1_dffs[0]_reg_input = B1_dffs[0]_or_out;
B1_dffs[0]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[0] = DFFE(B1_dffs[0]_reg_input, B1_dffs[0]_p3_out, , , );


--B1_dffs[1] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[1]
B1_dffs[1]_p1_out = B1_dffs[0] & !En & !Reset & !B1_dffs[1];
B1_dffs[1]_p2_out = !B1_dffs[0] & !En & !Reset & B1_dffs[1];
B1_dffs[1]_or_out = B1_dffs[1]_p1_out # B1_dffs[1]_p2_out;
B1_dffs[1]_reg_input = B1_dffs[1]_or_out;
B1_dffs[1]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[1] = DFFE(B1_dffs[1]_reg_input, B1_dffs[1]_p3_out, , , );


--B1_dffs[2] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[2]
B1_dffs[2]_p1_out = B1_dffs[1] & B1_dffs[0] & !En & !Reset & !B1_dffs[2];
B1_dffs[2]_p2_out = !B1_dffs[1] & !En & !Reset & B1_dffs[2];
B1_dffs[2]_p4_out = !B1_dffs[0] & !En & !Reset & B1_dffs[2];
B1_dffs[2]_or_out = B1_dffs[2]_p1_out # B1_dffs[2]_p2_out # B1_dffs[2]_p4_out;
B1_dffs[2]_reg_input = B1_dffs[2]_or_out;
B1_dffs[2]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[2] = DFFE(B1_dffs[2]_reg_input, B1_dffs[2]_p3_out, , , );


--B1_dffs[3] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[3]
B1_dffs[3]_p1_out = !En & !Reset & B1_dffs[0] & B1_dffs[1] & B1_dffs[2];
B1_dffs[3]_p2_out = En & B1_dffs[3];
B1_dffs[3]_p4_out = Reset & B1_dffs[3];
B1_dffs[3]_or_out = B1_dffs[3]_p1_out # B1_dffs[3]_p2_out # B1_dffs[3]_p4_out;
B1_dffs[3]_reg_input = B1_dffs[3]_or_out;
B1_dffs[3]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[3] = TFFE(B1_dffs[3]_reg_input, B1_dffs[3]_p3_out, , , );


--B1_dffs[4] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[4]
B1_dffs[4]_p1_out = !En & !Reset & B1_dffs[0] & B1_dffs[1] & B1_dffs[2] & B1_dffs[3];
B1_dffs[4]_p2_out = En & B1_dffs[4];
B1_dffs[4]_p4_out = Reset & B1_dffs[4];
B1_dffs[4]_or_out = B1_dffs[4]_p1_out # B1_dffs[4]_p2_out # B1_dffs[4]_p4_out;
B1_dffs[4]_reg_input = B1_dffs[4]_or_out;
B1_dffs[4]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[4] = TFFE(B1_dffs[4]_reg_input, B1_dffs[4]_p3_out, , , );


--B1_dffs[5] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[5]
B1_dffs[5]_p1_out = !En & !Reset & B1_dffs[0] & B1_dffs[1] & B1_dffs[2] & B1_dffs[3] & B1_dffs[4];
B1_dffs[5]_p2_out = En & B1_dffs[5];
B1_dffs[5]_p4_out = Reset & B1_dffs[5];
B1_dffs[5]_or_out = B1_dffs[5]_p1_out # B1_dffs[5]_p2_out # B1_dffs[5]_p4_out;
B1_dffs[5]_reg_input = B1_dffs[5]_or_out;
B1_dffs[5]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[5] = TFFE(B1_dffs[5]_reg_input, B1_dffs[5]_p3_out, , , );


--B1_dffs[6] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[6]
B1_dffs[6]_p1_out = !En & !Reset & B1_dffs[0] & B1_dffs[1] & B1_dffs[2] & B1_dffs[3] & B1_dffs[4] & B1_dffs[5];
B1_dffs[6]_p2_out = En & B1_dffs[6];
B1_dffs[6]_p4_out = Reset & B1_dffs[6];
B1_dffs[6]_or_out = B1_dffs[6]_p1_out # B1_dffs[6]_p2_out # B1_dffs[6]_p4_out;
B1_dffs[6]_reg_input = B1_dffs[6]_or_out;
B1_dffs[6]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[6] = TFFE(B1_dffs[6]_reg_input, B1_dffs[6]_p3_out, , , );


--B1_dffs[7] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[7]
B1_dffs[7]_p1_out = !En & !Reset & B1_dffs[0] & B1_dffs[1] & B1_dffs[2] & B1_dffs[3] & B1_dffs[4] & B1_dffs[5] & B1_dffs[6];
B1_dffs[7]_p2_out = En & B1_dffs[7];
B1_dffs[7]_p4_out = Reset & B1_dffs[7];
B1_dffs[7]_or_out = B1_dffs[7]_p1_out # B1_dffs[7]_p2_out # B1_dffs[7]_p4_out;
B1_dffs[7]_reg_input = B1_dffs[7]_or_out;
B1_dffs[7]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[7] = TFFE(B1_dffs[7]_reg_input, B1_dffs[7]_p3_out, , , );


--B1_dffs[8] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[8]
B1_dffs[8]_p1_out = !En & !Reset & B1_dffs[0] & B1_dffs[1] & B1_dffs[2] & B1_dffs[3] & B1_dffs[4] & B1_dffs[5] & B1_dffs[6] & B1_dffs[7];
B1_dffs[8]_p2_out = En & B1_dffs[8];
B1_dffs[8]_p4_out = Reset & B1_dffs[8];
B1_dffs[8]_or_out = B1_dffs[8]_p1_out # B1_dffs[8]_p2_out # B1_dffs[8]_p4_out;
B1_dffs[8]_reg_input = B1_dffs[8]_or_out;
B1_dffs[8]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[8] = TFFE(B1_dffs[8]_reg_input, B1_dffs[8]_p3_out, , , );


--B1_dffs[9] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[9]
B1_dffs[9]_p1_out = !En & !Reset & B1_dffs[0] & B1_dffs[1] & B1_dffs[2] & B1_dffs[3] & B1_dffs[4] & B1_dffs[5] & B1_dffs[6] & B1_dffs[7] & B1_dffs[8];
B1_dffs[9]_p2_out = En & B1_dffs[9];
B1_dffs[9]_p4_out = Reset & B1_dffs[9];
B1_dffs[9]_or_out = B1_dffs[9]_p1_out # B1_dffs[9]_p2_out # B1_dffs[9]_p4_out;
B1_dffs[9]_reg_input = B1_dffs[9]_or_out;
B1_dffs[9]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[9] = TFFE(B1_dffs[9]_reg_input, B1_dffs[9]_p3_out, , , );


--B1_dffs[10] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[10]
B1_dffs[10]_p1_out = !En & !Reset & B1_dffs[0] & B1_dffs[1] & B1_dffs[2] & B1_dffs[3] & B1_dffs[4] & B1_dffs[5] & B1_dffs[6] & B1_dffs[7] & B1_dffs[8] & B1_dffs[9];
B1_dffs[10]_p2_out = En & B1_dffs[10];
B1_dffs[10]_p4_out = Reset & B1_dffs[10];
B1_dffs[10]_or_out = B1_dffs[10]_p1_out # B1_dffs[10]_p2_out # B1_dffs[10]_p4_out;
B1_dffs[10]_reg_input = B1_dffs[10]_or_out;
B1_dffs[10]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[10] = TFFE(B1_dffs[10]_reg_input, B1_dffs[10]_p3_out, , , );


--B1_dffs[11] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[11]
B1_dffs[11]_p1_out = !En & !Reset & B1_dffs[0] & B1_dffs[1] & B1_dffs[2] & B1_dffs[3] & B1_dffs[4] & B1_dffs[5] & B1_dffs[6] & B1_dffs[7] & B1_dffs[8] & B1_dffs[9] & B1_dffs[10];
B1_dffs[11]_p2_out = En & B1_dffs[11];
B1_dffs[11]_p4_out = Reset & B1_dffs[11];
B1_dffs[11]_or_out = B1_dffs[11]_p1_out # B1_dffs[11]_p2_out # B1_dffs[11]_p4_out;
B1_dffs[11]_reg_input = B1_dffs[11]_or_out;
B1_dffs[11]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[11] = TFFE(B1_dffs[11]_reg_input, B1_dffs[11]_p3_out, , , );


--B1_dffs[12] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[12]
B1_dffs[12]_p1_out = !En & !Reset & B1_dffs[0] & B1_dffs[1] & B1_dffs[2] & B1_dffs[3] & B1_dffs[4] & B1_dffs[5] & B1_dffs[6] & B1_dffs[7] & B1_dffs[8] & B1_dffs[9] & B1_dffs[10] & B1_dffs[11];
B1_dffs[12]_p2_out = En & B1_dffs[12];
B1_dffs[12]_p4_out = Reset & B1_dffs[12];
B1_dffs[12]_or_out = B1_dffs[12]_p1_out # B1_dffs[12]_p2_out # B1_dffs[12]_p4_out;
B1_dffs[12]_reg_input = B1_dffs[12]_or_out;
B1_dffs[12]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[12] = TFFE(B1_dffs[12]_reg_input, B1_dffs[12]_p3_out, , , );


--B1_dffs[13] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[13]
B1_dffs[13]_p1_out = !En & !Reset & B1_dffs[0] & B1_dffs[1] & B1_dffs[2] & B1_dffs[3] & B1_dffs[4] & B1_dffs[5] & B1_dffs[6] & B1_dffs[7] & B1_dffs[8] & B1_dffs[9] & B1_dffs[10] & B1_dffs[11] & B1_dffs[12];
B1_dffs[13]_p2_out = En & B1_dffs[13];
B1_dffs[13]_p4_out = Reset & B1_dffs[13];
B1_dffs[13]_or_out = B1_dffs[13]_p1_out # B1_dffs[13]_p2_out # B1_dffs[13]_p4_out;
B1_dffs[13]_reg_input = B1_dffs[13]_or_out;
B1_dffs[13]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[13] = TFFE(B1_dffs[13]_reg_input, B1_dffs[13]_p3_out, , , );


--B1_dffs[14] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[14]
B1_dffs[14]_p1_out = !En & !Reset & B1_dffs[0] & B1_dffs[1] & B1_dffs[2] & B1_dffs[3] & B1_dffs[4] & B1_dffs[5] & B1_dffs[6] & B1_dffs[7] & B1_dffs[8] & B1_dffs[9] & B1_dffs[10] & B1_dffs[11] & B1_dffs[12] & B1_dffs[13];
B1_dffs[14]_p2_out = En & B1_dffs[14];
B1_dffs[14]_p4_out = Reset & B1_dffs[14];
B1_dffs[14]_or_out = B1_dffs[14]_p1_out # B1_dffs[14]_p2_out # B1_dffs[14]_p4_out;
B1_dffs[14]_reg_input = B1_dffs[14]_or_out;
B1_dffs[14]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[14] = TFFE(B1_dffs[14]_reg_input, B1_dffs[14]_p3_out, , , );


--A1L5Q is Rate_Pulse_Alarm~reg0
A1L5Q_p1_out = B1_dffs[15] & B1_dffs[14] & B1_dffs[13] & B1_dffs[12] & B1_dffs[11] & B1_dffs[10] & B1_dffs[9] & B1_dffs[8] & B1_dffs[7] & B1_dffs[6] & B1_dffs[5] & B1_dffs[4] & B1_dffs[3] & B1_dffs[2] & B1_dffs[1] & B1_dffs[0] & !En & !Reset;
A1L5Q_or_out = A1L5Q_p1_out;
A1L5Q_reg_input = A1L5Q_or_out;
A1L5Q_p3_out = Rate_Pulse & Measure_Ctrl;
A1L5Q = DFFE(A1L5Q_reg_input, A1L5Q_p3_out, , , );


--B1_dffs[15] is lpm_counter:Rate_Pulse_Data_rtl_0|dffs[15]
B1_dffs[15]_p1_out = !En & !Reset & B1_dffs[0] & B1_dffs[1] & B1_dffs[2] & B1_dffs[3] & B1_dffs[4] & B1_dffs[5] & B1_dffs[6] & B1_dffs[7] & B1_dffs[8] & B1_dffs[9] & B1_dffs[10] & B1_dffs[11] & B1_dffs[12] & B1_dffs[13] & B1_dffs[14];
B1_dffs[15]_p2_out = En & B1_dffs[15];
B1_dffs[15]_p4_out = Reset & B1_dffs[15];
B1_dffs[15]_or_out = B1_dffs[15]_p1_out # B1_dffs[15]_p2_out # B1_dffs[15]_p4_out;
B1_dffs[15]_reg_input = B1_dffs[15]_or_out;
B1_dffs[15]_p3_out = Rate_Pulse & Measure_Ctrl;
B1_dffs[15] = TFFE(B1_dffs[15]_reg_input, B1_dffs[15]_p3_out, , , );


--En is En
--operation mode is input

En = INPUT();


--Reset is Reset
--operation mode is input

Reset = INPUT();


--Rate_Pulse is Rate_Pulse
--operation mode is input

Rate_Pulse = INPUT();


--Measure_Ctrl is Measure_Ctrl
--operation mode is input

Measure_Ctrl = INPUT();


--Rate_Pulse_Data[0] is Rate_Pulse_Data[0]
--operation mode is output

Rate_Pulse_Data[0] = OUTPUT(B1_dffs[0]);


--Rate_Pulse_Data[1] is Rate_Pulse_Data[1]
--operation mode is output

Rate_Pulse_Data[1] = OUTPUT(B1_dffs[1]);


--Rate_Pulse_Data[2] is Rate_Pulse_Data[2]
--operation mode is output

Rate_Pulse_Data[2] = OUTPUT(B1_dffs[2]);


--Rate_Pulse_Data[3] is Rate_Pulse_Data[3]
--operation mode is output

Rate_Pulse_Data[3] = OUTPUT(B1_dffs[3]);


--Rate_Pulse_Data[4] is Rate_Pulse_Data[4]
--operation mode is output

Rate_Pulse_Data[4] = OUTPUT(B1_dffs[4]);


--Rate_Pulse_Data[5] is Rate_Pulse_Data[5]
--operation mode is output

Rate_Pulse_Data[5] = OUTPUT(B1_dffs[5]);


--Rate_Pulse_Data[6] is Rate_Pulse_Data[6]
--operation mode is output

Rate_Pulse_Data[6] = OUTPUT(B1_dffs[6]);


--Rate_Pulse_Data[7] is Rate_Pulse_Data[7]
--operation mode is output

Rate_Pulse_Data[7] = OUTPUT(B1_dffs[7]);


--Rate_Pulse_Data[8] is Rate_Pulse_Data[8]
--operation mode is output

Rate_Pulse_Data[8] = OUTPUT(B1_dffs[8]);


--Rate_Pulse_Data[9] is Rate_Pulse_Data[9]
--operation mode is output

Rate_Pulse_Data[9] = OUTPUT(B1_dffs[9]);


--Rate_Pulse_Data[10] is Rate_Pulse_Data[10]
--operation mode is output

Rate_Pulse_Data[10] = OUTPUT(B1_dffs[10]);


--Rate_Pulse_Data[11] is Rate_Pulse_Data[11]
--operation mode is output

Rate_Pulse_Data[11] = OUTPUT(B1_dffs[11]);


--Rate_Pulse_Data[12] is Rate_Pulse_Data[12]
--operation mode is output

Rate_Pulse_Data[12] = OUTPUT(B1_dffs[12]);


--Rate_Pulse_Data[13] is Rate_Pulse_Data[13]
--operation mode is output

Rate_Pulse_Data[13] = OUTPUT(B1_dffs[13]);


--Rate_Pulse_Data[14] is Rate_Pulse_Data[14]
--operation mode is output

Rate_Pulse_Data[14] = OUTPUT(B1_dffs[14]);


--Rate_Pulse_Alarm is Rate_Pulse_Alarm
--operation mode is output

Rate_Pulse_Alarm = OUTPUT(A1L5Q);


--Rate_Pulse_Data[15] is Rate_Pulse_Data[15]
--operation mode is output

Rate_Pulse_Data[15] = OUTPUT(B1_dffs[15]);


