--A1L81 is Y_1~202 at LC1
A1L81_p1_out = C1_2 & B & !A & !G2_L & !G1_L;
A1L81_p2_out = B & A & C1_3 & !G2_L & !G1_L;
A1L81_p3_out = !B & !A & C1_0 & !G2_L & !G1_L;
A1L81_p4_out = !B & A & C1_1 & !G2_L & !G1_L;
A1L81_or_out = A1L81_p1_out # A1L81_p2_out # A1L81_p3_out # A1L81_p4_out;
A1L81 = A1L81_or_out;


--A1L02 is Y_2$latch$d_and~200 at LC3
A1L02_p1_out = C2_1 & A & !B;
A1L02_p2_out = A & B & C2_3;
A1L02_p3_out = !A & !B & C2_0;
A1L02_p4_out = !A & B & C2_2;
A1L02_or_out = A1L02_p1_out # A1L02_p2_out # A1L02_p3_out # A1L02_p4_out;
A1L02 = A1L02_or_out;


--A1L22 is Y_2$latch~10 at LC2
A1L22_p1_out = A1L12 & !G2_L & !G1_L & A1L02;
A1L22_p2_out = A1L22 & !G2_L & !G1_L;
A1L22_p3_out = A1L22 & !G2_L & !G1_L & A1L02;
A1L22_or_out = A1L22_p1_out # A1L22_p2_out # A1L22_p3_out;
A1L22 = A1L22_or_out;


--A1L12 is Y_2$latch$en_or~2sexp at SEXP1
A1L12 = EXP(!G2_L & !G1_L);


--G1_L is G1_L at PIN_11
--operation mode is input

G1_L = INPUT();


--G2_L is G2_L at PIN_34
--operation mode is input

G2_L = INPUT();


--B is B at PIN_12
--operation mode is input

B = INPUT();


--A is A at PIN_33
--operation mode is input

A = INPUT();


--C1_0 is C1_0 at PIN_16
--operation mode is input

C1_0 = INPUT();


--C1_1 is C1_1 at PIN_28
--operation mode is input

C1_1 = INPUT();


--C1_2 is C1_2 at PIN_18
--operation mode is input

C1_2 = INPUT();


--C1_3 is C1_3 at PIN_19
--operation mode is input

C1_3 = INPUT();


--C2_0 is C2_0 at PIN_20
--operation mode is input

C2_0 = INPUT();


--C2_1 is C2_1 at PIN_25
--operation mode is input

C2_1 = INPUT();


--C2_2 is C2_2 at PIN_21
--operation mode is input

C2_2 = INPUT();


--C2_3 is C2_3 at PIN_24
--operation mode is input

C2_3 = INPUT();


--Y_1 is Y_1 at PIN_4
--operation mode is output

Y_1 = OUTPUT(A1L81);


--Y_2 is Y_2 at PIN_5
--operation mode is output

Y_2 = OUTPUT(A1L22);






