--A1L91 is reduce_or~347
A1L91_p1_out = EN & !A & !C;
A1L91_p2_out = EN & !A & B;
A1L91_or_out = A1L91_p1_out # A1L91_p2_out;
A1L91 = A1L91_or_out;


--A1L81 is g_~47
A1L81_p1_out = EN & !C & B;
A1L81_p2_out = EN & !C & D;
A1L81_p3_out = EN & C & !A;
A1L81_p4_out = EN & C & !B;
A1L81_or_out = A1L81_p1_out # A1L81_p2_out # A1L81_p3_out # A1L81_p4_out;
A1L81 = A1L81_or_out;


--A1L31 is d_~123
A1L31_p1_out = C & EN & A & !B;
A1L31_p2_out = !C & EN & B;
A1L31_p3_out = !C & EN & !A;
A1L31_p4_out = EN & !A & B;
A1L31_or_out = A1L31_p1_out # A1L31_p2_out # A1L31_p3_out # A1L31_p4_out;
A1L31 = A1L31_or_out;


--A1L11 is c_~38
A1L11_p1_out = !C & A & EN;
A1L11_p2_out = !C & EN & !B;
A1L11_p3_out = C & EN & !D;
A1L11_or_out = A1L11_p1_out # A1L11_p2_out # A1L11_p3_out;
A1L11 = A1L11_or_out;


--A1L61 is f_~83
A1L61_p1_out = C & EN & !A;
A1L61_p2_out = EN & D & !B;
A1L61_p3_out = C & EN & !B;
A1L61_p4_out = EN & !A & !B;
A1L61_or_out = A1L61_p1_out # A1L61_p2_out # A1L61_p3_out # A1L61_p4_out;
A1L61 = A1L61_or_out;


--A1L9 is b_~49
A1L9_p1_out = EN & !D & !C;
A1L9_p2_out = EN & !D & A & B;
A1L9_p3_out = EN & !A & !B;
A1L9_p4_out = EN & !C & !B;
A1L9_or_out = A1L9_p1_out # A1L9_p2_out # A1L9_p3_out # A1L9_p4_out;
A1L9 = A1L9_or_out;


--A1L7 is a_~74
A1L7_p1_out = !A & !C & EN & !B;
A1L7_p2_out = A & C & EN & !D;
A1L7_p3_out = !C & EN & B & !D;
A1L7_p4_out = A & EN & !B & D;
A1L7_or_out = A1L7_p1_out # A1L7_p2_out # A1L7_p3_out # A1L7_p4_out;
A1L7 = A1L7_or_out;


--EN is EN
--operation mode is input

EN = INPUT();


--D is D
--operation mode is input

D = INPUT();


--C is C
--operation mode is input

C = INPUT();


--B is B
--operation mode is input

B = INPUT();


--A is A
--operation mode is input

A = INPUT();


--e_ is e_
--operation mode is output

e_ = OUTPUT(A1L91);


--d_ is d_
--operation mode is output

d_ = OUTPUT(A1L31);


--g_ is g_
--operation mode is output

g_ = OUTPUT(A1L81);


--c_ is c_
--operation mode is output

c_ = OUTPUT(A1L11);


--f_ is f_
--operation mode is output

f_ = OUTPUT(A1L61);


--a_ is a_
--operation mode is output

a_ = OUTPUT(A1L7);


--b_ is b_
--operation mode is output

b_ = OUTPUT(A1L9);


