/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/

/*
Copyright (C) 1991-2004 Altera Corporation
Any  megafunction  design,  and related netlist (encrypted  or  decrypted),
support information,  device programming or simulation file,  and any other
associated  documentation or information  provided by  Altera  or a partner
under  Altera's   Megafunction   Partnership   Program  may  be  used  only
to program  PLD  devices (but not masked  PLD  devices) from  Altera.   Any
other  use  of such  megafunction  design,  netlist,  support  information,
device programming or simulation file,  or any other  related documentation
or information  is prohibited  for  any  other purpose,  including, but not
limited to  modification,  reverse engineering,  de-compiling, or use  with
any other  silicon devices,  unless such use is  explicitly  licensed under
a separate agreement with  Altera  or a megafunction partner.  Title to the
intellectual property,  including patents,  copyrights,  trademarks,  trade
secrets,  or maskworks,  embodied in any such megafunction design, netlist,
support  information,  device programming or simulation file,  or any other
related documentation or information provided by  Altera  or a megafunction
partner, remains with Altera, the megafunction partner, or their respective
licensors. No other licenses, including any licenses needed under any third
party's intellectual property, are provided herein.
*/

HEADER
{
	VERSION = 1;
	TIME_UNIT = ns;
	SIMULATION_TIME = 0.0;
	GRID_PHASE = 0.0;
	GRID_PERIOD = 10.0;
	GRID_DUTY_CYCLE = 50;
}

SIGNAL("Clk_1Hz")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("Reset")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("acceleration")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 17;
	LSB_INDEX = 0;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("acceleration[16]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[15]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[14]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[13]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[12]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[11]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[10]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[9]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[8]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("acceleration[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "acceleration";
}

SIGNAL("second_pulse_out")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 16;
	LSB_INDEX = 0;
	DIRECTION = OUTPUT;
	PARENT = "";
}

SIGNAL("second_pulse_out[15]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[14]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[13]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[12]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[11]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[10]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[9]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[8]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("second_pulse_out[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = OUTPUT;
	PARENT = "second_pulse_out";
}

SIGNAL("speed")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = BUS;
	WIDTH = 16;
	LSB_INDEX = 0;
	DIRECTION = INPUT;
	PARENT = "";
}

SIGNAL("speed[15]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[14]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[13]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[12]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[11]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[10]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[9]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[8]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[7]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[6]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[5]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[4]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[3]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[2]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[1]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

SIGNAL("speed[0]")
{
	VALUE_TYPE = NINE_LEVEL_BIT;
	SIGNAL_TYPE = SINGLE_BIT;
	WIDTH = 1;
	LSB_INDEX = -1;
	DIRECTION = INPUT;
	PARENT = "speed";
}

TRANSITION_LIST("Clk_1Hz")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 50;
			LEVEL 0 FOR 10.0;
			LEVEL 1 FOR 10.0;
		}
	}
}

TRANSITION_LIST("Reset")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("acceleration[16]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("acceleration[15]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("acceleration[14]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("acceleration[13]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("acceleration[12]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("acceleration[11]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("acceleration[10]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("acceleration[9]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("acceleration[8]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("acceleration[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("acceleration[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 640.0;
		LEVEL 1 FOR 360.0;
	}
}

TRANSITION_LIST("acceleration[5]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 1;
			LEVEL 0 FOR 320.0;
			LEVEL 1 FOR 320.0;
		}
		LEVEL 0 FOR 320.0;
		LEVEL 1 FOR 40.0;
	}
}

TRANSITION_LIST("acceleration[4]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 3;
			LEVEL 0 FOR 160.0;
			LEVEL 1 FOR 160.0;
		}
		LEVEL 0 FOR 40.0;
	}
}

TRANSITION_LIST("acceleration[3]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 6;
			LEVEL 0 FOR 80.0;
			LEVEL 1 FOR 80.0;
		}
		LEVEL 0 FOR 40.0;
	}
}

TRANSITION_LIST("acceleration[2]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 12;
			LEVEL 0 FOR 40.0;
			LEVEL 1 FOR 40.0;
		}
		LEVEL 0 FOR 40.0;
	}
}

TRANSITION_LIST("acceleration[1]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 25;
			LEVEL 0 FOR 20.0;
			LEVEL 1 FOR 20.0;
		}
	}
}

TRANSITION_LIST("acceleration[0]")
{
	NODE
	{
		REPEAT = 1;
		NODE
		{
			REPEAT = 50;
			LEVEL 0 FOR 10.0;
			LEVEL 1 FOR 10.0;
		}
	}
}

TRANSITION_LIST("second_pulse_out[15]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[14]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[13]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[12]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[11]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[10]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[9]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[8]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("second_pulse_out[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL X FOR 1000.0;
	}
}

TRANSITION_LIST("speed[15]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[14]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[13]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[12]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[11]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[10]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[9]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[8]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[7]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[6]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[5]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[4]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[3]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[2]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 0 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[1]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 1 FOR 1000.0;
	}
}

TRANSITION_LIST("speed[0]")
{
	NODE
	{
		REPEAT = 1;
		LEVEL 1 FOR 1000.0;
	}
}

DISPLAY_LINE
{
	CHANNEL = "Clk_1Hz";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 0;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "Reset";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 1;
	TREE_LEVEL = 0;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 2;
	TREE_LEVEL = 0;
	CHILDREN = 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[16]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 3;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[15]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 4;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[14]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 5;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[13]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 6;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[12]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 7;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[11]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 8;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[10]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 9;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[9]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 10;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[8]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 11;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 12;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 13;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 14;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 15;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 16;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 17;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 18;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "acceleration[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 19;
	TREE_LEVEL = 1;
	PARENT = 2;
}

DISPLAY_LINE
{
	CHANNEL = "speed";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 20;
	TREE_LEVEL = 0;
	CHILDREN = 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36;
}

DISPLAY_LINE
{
	CHANNEL = "speed[15]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 21;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[14]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 22;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[13]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 23;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[12]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 24;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[11]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 25;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[10]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 26;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[9]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 27;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[8]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 28;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 29;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 30;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 31;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 32;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 33;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 34;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 35;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "speed[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 36;
	TREE_LEVEL = 1;
	PARENT = 20;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Hexadecimal;
	TREE_INDEX = 37;
	TREE_LEVEL = 0;
	CHILDREN = 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 49, 50, 51, 52, 53;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[15]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 38;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[14]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 39;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[13]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 40;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[12]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 41;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[11]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 42;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[10]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 43;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[9]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 44;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[8]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 45;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[7]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 46;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[6]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 47;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[5]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 48;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[4]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 49;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[3]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 50;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[2]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 51;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[1]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 52;
	TREE_LEVEL = 1;
	PARENT = 37;
}

DISPLAY_LINE
{
	CHANNEL = "second_pulse_out[0]";
	EXPAND_STATUS = COLLAPSED;
	RADIX = Binary;
	TREE_INDEX = 53;
	TREE_LEVEL = 1;
	PARENT = 37;
}

TIME_BAR
{
	TIME = 10050;
	MASTER = TRUE;
}
;
