--B1_dffs[0] is lpm_counter:Q0_rtl_0|dffs[0] at LC67
B1_dffs[0]_p1_out = !B1_dffs[0] & EN & !CLR;
B1_dffs[0]_or_out = B1_dffs[0]_p1_out;
B1_dffs[0]_reg_input = B1_dffs[0]_or_out;
B1_dffs[0] = DFFE(B1_dffs[0]_reg_input, GLOBAL(F_IN), , , );


--B1_dffs[1] is lpm_counter:Q0_rtl_0|dffs[1] at LC70
B1_dffs[1]_p1_out = !B1_dffs[3] & B1_dffs[0] & EN & !CLR & !B1_dffs[1];
B1_dffs[1]_p2_out = B1_dffs[0] & EN & !CLR & !B1_dffs[1] & B1_dffs[2];
B1_dffs[1]_p3_out = !B1_dffs[0] & EN & !CLR & B1_dffs[1];
B1_dffs[1]_or_out = B1_dffs[1]_p1_out # B1_dffs[1]_p2_out # B1_dffs[1]_p3_out;
B1_dffs[1]_reg_input = B1_dffs[1]_or_out;
B1_dffs[1] = DFFE(B1_dffs[1]_reg_input, GLOBAL(F_IN), , , );


--B1_dffs[2] is lpm_counter:Q0_rtl_0|dffs[2] at LC72
B1_dffs[2]_p1_out = !B1_dffs[1] & EN & !CLR & B1_dffs[2];
B1_dffs[2]_p2_out = B1_dffs[1] & EN & !CLR & !B1_dffs[2] & B1_dffs[0];
B1_dffs[2]_p3_out = EN & !CLR & B1_dffs[2] & !B1_dffs[0];
B1_dffs[2]_or_out = B1_dffs[2]_p1_out # B1_dffs[2]_p2_out # B1_dffs[2]_p3_out;
B1_dffs[2]_reg_input = B1_dffs[2]_or_out;
B1_dffs[2] = DFFE(B1_dffs[2]_reg_input, GLOBAL(F_IN), , , );


--B1_dffs[3] is lpm_counter:Q0_rtl_0|dffs[3] at LC51
B1_dffs[3]_p1_out = B1_dffs[2] & !B1_dffs[1] & EN & !CLR & B1_dffs[3];
B1_dffs[3]_p2_out = !B1_dffs[2] & B1_dffs[1] & EN & !CLR & B1_dffs[3];
B1_dffs[3]_p3_out = B1_dffs[2] & B1_dffs[1] & EN & !CLR & !B1_dffs[3] & B1_dffs[0];
B1_dffs[3]_p4_out = EN & !CLR & B1_dffs[3] & !B1_dffs[0];
B1_dffs[3]_or_out = B1_dffs[3]_p1_out # B1_dffs[3]_p2_out # B1_dffs[3]_p3_out # B1_dffs[3]_p4_out;
B1_dffs[3]_reg_input = B1_dffs[3]_or_out;
B1_dffs[3] = DFFE(B1_dffs[3]_reg_input, GLOBAL(F_IN), , , );


--B2_dffs[0] is lpm_counter:Q1_rtl_1|dffs[0] at LC54
B2_dffs[0]_p1_out = EN & !CLR & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3];
B2_dffs[0]_p2_out = !EN & B2_dffs[0];
B2_dffs[0]_p3_out = CLR & B2_dffs[0];
B2_dffs[0]_or_out = B2_dffs[0]_p1_out # B2_dffs[0]_p2_out # B2_dffs[0]_p3_out;
B2_dffs[0]_reg_input = B2_dffs[0]_or_out;
B2_dffs[0] = TFFE(B2_dffs[0]_reg_input, GLOBAL(F_IN), , , );


--B2_dffs[1] is lpm_counter:Q1_rtl_1|dffs[1] at LC56
B2_dffs[1]_p0_out = B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B2_dffs[0] & B2_dffs[1];
B2_dffs[1]_p1_out = !B2_dffs[3] & EN & !CLR & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B2_dffs[0];
B2_dffs[1]_p2_out = EN & !CLR & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B2_dffs[0] & B2_dffs[2];
B2_dffs[1]_p3_out = !EN & B2_dffs[1];
B2_dffs[1]_p4_out = CLR & B2_dffs[1];
B2_dffs[1]_or_out = B2_dffs[1]_p0_out # B2_dffs[1]_p1_out # B2_dffs[1]_p2_out # B2_dffs[1]_p3_out # B2_dffs[1]_p4_out;
B2_dffs[1]_reg_input = B2_dffs[1]_or_out;
B2_dffs[1] = TFFE(B2_dffs[1]_reg_input, GLOBAL(F_IN), , , );


--B2_dffs[2] is lpm_counter:Q1_rtl_1|dffs[2] at LC59
B2_dffs[2]_p1_out = B2_dffs[1] & B2_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & EN & !CLR;
B2_dffs[2]_p2_out = !EN & B2_dffs[2];
B2_dffs[2]_p3_out = CLR & B2_dffs[2];
B2_dffs[2]_or_out = B2_dffs[2]_p1_out # B2_dffs[2]_p2_out # B2_dffs[2]_p3_out;
B2_dffs[2]_reg_input = B2_dffs[2]_or_out;
B2_dffs[2] = TFFE(B2_dffs[2]_reg_input, GLOBAL(F_IN), , , );


--B2_dffs[3] is lpm_counter:Q1_rtl_1|dffs[3] at LC62
B2_dffs[3]_p1_out = B2_dffs[2] & B2_dffs[1] & B2_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & EN & !CLR;
B2_dffs[3]_p2_out = !B2_dffs[2] & !B2_dffs[1] & B2_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & B2_dffs[3];
B2_dffs[3]_p3_out = !EN & B2_dffs[3];
B2_dffs[3]_p4_out = CLR & B2_dffs[3];
B2_dffs[3]_or_out = B2_dffs[3]_p1_out # B2_dffs[3]_p2_out # B2_dffs[3]_p3_out # B2_dffs[3]_p4_out;
B2_dffs[3]_reg_input = B2_dffs[3]_or_out;
B2_dffs[3] = TFFE(B2_dffs[3]_reg_input, GLOBAL(F_IN), , , );


--B3_dffs[0] is lpm_counter:Q2_rtl_2|dffs[0] at LC64
B3_dffs[0]_p1_out = EN & !CLR & B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3];
B3_dffs[0]_p2_out = !EN & B3_dffs[0];
B3_dffs[0]_p3_out = CLR & B3_dffs[0];
B3_dffs[0]_or_out = B3_dffs[0]_p1_out # B3_dffs[0]_p2_out # B3_dffs[0]_p3_out;
B3_dffs[0]_reg_input = B3_dffs[0]_or_out;
B3_dffs[0] = TFFE(B3_dffs[0]_reg_input, GLOBAL(F_IN), , , );


--B3_dffs[1] is lpm_counter:Q2_rtl_2|dffs[1] at LC35
B3_dffs[1]_p0_out = B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0] & B3_dffs[1];
B3_dffs[1]_p1_out = !B3_dffs[3] & EN & !CLR & B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0];
B3_dffs[1]_p2_out = EN & !CLR & B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0] & B3_dffs[2];
B3_dffs[1]_p3_out = !EN & B3_dffs[1];
B3_dffs[1]_p4_out = CLR & B3_dffs[1];
B3_dffs[1]_or_out = B3_dffs[1]_p0_out # B3_dffs[1]_p1_out # B3_dffs[1]_p2_out # B3_dffs[1]_p3_out # B3_dffs[1]_p4_out;
B3_dffs[1]_reg_input = B3_dffs[1]_or_out;
B3_dffs[1] = TFFE(B3_dffs[1]_reg_input, GLOBAL(F_IN), , , );


--B3_dffs[2] is lpm_counter:Q2_rtl_2|dffs[2] at LC38
B3_dffs[2]_p1_out = B3_dffs[1] & B3_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & B2_dffs[3] & !B2_dffs[2] & !B2_dffs[1] & B2_dffs[0] & EN & !CLR;
B3_dffs[2]_p2_out = !EN & B3_dffs[2];
B3_dffs[2]_p3_out = CLR & B3_dffs[2];
B3_dffs[2]_or_out = B3_dffs[2]_p1_out # B3_dffs[2]_p2_out # B3_dffs[2]_p3_out;
B3_dffs[2]_reg_input = B3_dffs[2]_or_out;
B3_dffs[2] = TFFE(B3_dffs[2]_reg_input, GLOBAL(F_IN), , , );


--B3_dffs[3] is lpm_counter:Q2_rtl_2|dffs[3] at LC43
B3_dffs[3]_p1_out = B3_dffs[2] & B3_dffs[1] & B3_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & B2_dffs[3] & !B2_dffs[2] & !B2_dffs[1] & B2_dffs[0] & EN & !CLR;
B3_dffs[3]_p2_out = !B3_dffs[2] & !B3_dffs[1] & B3_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & B2_dffs[3] & !B2_dffs[2] & !B2_dffs[1] & B2_dffs[0] & B3_dffs[3];
B3_dffs[3]_p3_out = !EN & B3_dffs[3];
B3_dffs[3]_p4_out = CLR & B3_dffs[3];
B3_dffs[3]_or_out = B3_dffs[3]_p1_out # B3_dffs[3]_p2_out # B3_dffs[3]_p3_out # B3_dffs[3]_p4_out;
B3_dffs[3]_reg_input = B3_dffs[3]_or_out;
B3_dffs[3] = TFFE(B3_dffs[3]_reg_input, GLOBAL(F_IN), , , );


--B4_dffs[0] is lpm_counter:Q3_rtl_3|dffs[0] at LC46
B4_dffs[0]_p1_out = EN & !CLR & B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2] & B3_dffs[3];
B4_dffs[0]_p2_out = !EN & B4_dffs[0];
B4_dffs[0]_p3_out = CLR & B4_dffs[0];
B4_dffs[0]_or_out = B4_dffs[0]_p1_out # B4_dffs[0]_p2_out # B4_dffs[0]_p3_out;
B4_dffs[0]_reg_input = B4_dffs[0]_or_out;
B4_dffs[0] = TFFE(B4_dffs[0]_reg_input, GLOBAL(F_IN), , , );


--B4_dffs[1] is lpm_counter:Q3_rtl_3|dffs[1] at LC17
B4_dffs[1]_p0_out = B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2] & B3_dffs[3] & B4_dffs[0] & B4_dffs[1];
B4_dffs[1]_p1_out = !B4_dffs[3] & EN & !CLR & B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2] & B3_dffs[3] & B4_dffs[0];
B4_dffs[1]_p2_out = EN & !CLR & B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2] & B3_dffs[3] & B4_dffs[0] & B4_dffs[2];
B4_dffs[1]_p3_out = !EN & B4_dffs[1];
B4_dffs[1]_p4_out = CLR & B4_dffs[1];
B4_dffs[1]_or_out = B4_dffs[1]_p0_out # B4_dffs[1]_p1_out # B4_dffs[1]_p2_out # B4_dffs[1]_p3_out # B4_dffs[1]_p4_out;
B4_dffs[1]_reg_input = B4_dffs[1]_or_out;
B4_dffs[1] = TFFE(B4_dffs[1]_reg_input, GLOBAL(F_IN), , , );


--B4_dffs[2] is lpm_counter:Q3_rtl_3|dffs[2] at LC48
B4_dffs[2]_p1_out = B4_dffs[1] & B4_dffs[0] & B3_dffs[3] & !B3_dffs[2] & !B3_dffs[1] & B3_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & B2_dffs[3] & !B2_dffs[2] & !B2_dffs[1] & B2_dffs[0] & EN & !CLR;
B4_dffs[2]_p2_out = !EN & B4_dffs[2];
B4_dffs[2]_p3_out = CLR & B4_dffs[2];
B4_dffs[2]_or_out = B4_dffs[2]_p1_out # B4_dffs[2]_p2_out # B4_dffs[2]_p3_out;
B4_dffs[2]_reg_input = B4_dffs[2]_or_out;
B4_dffs[2] = TFFE(B4_dffs[2]_reg_input, GLOBAL(F_IN), , , );


--B4_dffs[3] is lpm_counter:Q3_rtl_3|dffs[3] at LC19
B4_dffs[3]_p1_out = B4_dffs[2] & B4_dffs[1] & B4_dffs[0] & B3_dffs[3] & !B3_dffs[2] & !B3_dffs[1] & B3_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & B2_dffs[3] & !B2_dffs[2] & !B2_dffs[1] & B2_dffs[0] & EN & !CLR;
B4_dffs[3]_p2_out = !B4_dffs[2] & !B4_dffs[1] & B4_dffs[0] & B3_dffs[3] & !B3_dffs[2] & !B3_dffs[1] & B3_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & B2_dffs[3] & !B2_dffs[2] & !B2_dffs[1] & B2_dffs[0] & B4_dffs[3];
B4_dffs[3]_p3_out = !EN & B4_dffs[3];
B4_dffs[3]_p4_out = CLR & B4_dffs[3];
B4_dffs[3]_or_out = B4_dffs[3]_p1_out # B4_dffs[3]_p2_out # B4_dffs[3]_p3_out # B4_dffs[3]_p4_out;
B4_dffs[3]_reg_input = B4_dffs[3]_or_out;
B4_dffs[3] = TFFE(B4_dffs[3]_reg_input, GLOBAL(F_IN), , , );


--B5_dffs[0] is lpm_counter:Q4_rtl_4|dffs[0] at LC24
B5_dffs[0]_p1_out = EN & !CLR & B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2] & B3_dffs[3] & B4_dffs[0] & !B4_dffs[1] & !B4_dffs[2] & B4_dffs[3];
B5_dffs[0]_p2_out = !EN & B5_dffs[0];
B5_dffs[0]_p3_out = CLR & B5_dffs[0];
B5_dffs[0]_or_out = B5_dffs[0]_p1_out # B5_dffs[0]_p2_out # B5_dffs[0]_p3_out;
B5_dffs[0]_reg_input = B5_dffs[0]_or_out;
B5_dffs[0] = TFFE(B5_dffs[0]_reg_input, GLOBAL(F_IN), , , );


--B5_dffs[1] is lpm_counter:Q4_rtl_4|dffs[1] at LC25
B5_dffs[1]_p0_out = B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2] & B3_dffs[3] & B4_dffs[0] & !B4_dffs[1] & !B4_dffs[2] & B4_dffs[3] & B5_dffs[0] & B5_dffs[1];
B5_dffs[1]_p1_out = !B5_dffs[3] & EN & !CLR & B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2] & B3_dffs[3] & B4_dffs[0] & !B4_dffs[1] & !B4_dffs[2] & B4_dffs[3] & B5_dffs[0];
B5_dffs[1]_p2_out = EN & !CLR & B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2] & B3_dffs[3] & B4_dffs[0] & !B4_dffs[1] & !B4_dffs[2] & B4_dffs[3] & B5_dffs[0] & B5_dffs[2];
B5_dffs[1]_p3_out = !EN & B5_dffs[1];
B5_dffs[1]_p4_out = CLR & B5_dffs[1];
B5_dffs[1]_or_out = B5_dffs[1]_p0_out # B5_dffs[1]_p1_out # B5_dffs[1]_p2_out # B5_dffs[1]_p3_out # B5_dffs[1]_p4_out;
B5_dffs[1]_reg_input = B5_dffs[1]_or_out;
B5_dffs[1] = TFFE(B5_dffs[1]_reg_input, GLOBAL(F_IN), , , );


--B5_dffs[2] is lpm_counter:Q4_rtl_4|dffs[2] at LC32
B5_dffs[2]_p1_out = B5_dffs[1] & B5_dffs[0] & B4_dffs[3] & !B4_dffs[2] & !B4_dffs[1] & B4_dffs[0] & B3_dffs[3] & !B3_dffs[2] & !B3_dffs[1] & B3_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & B2_dffs[3] & !B2_dffs[2] & !B2_dffs[1] & B2_dffs[0] & EN & !CLR;
B5_dffs[2]_p2_out = !EN & B5_dffs[2];
B5_dffs[2]_p3_out = CLR & B5_dffs[2];
B5_dffs[2]_or_out = B5_dffs[2]_p1_out # B5_dffs[2]_p2_out # B5_dffs[2]_p3_out;
B5_dffs[2]_reg_input = B5_dffs[2]_or_out;
B5_dffs[2] = TFFE(B5_dffs[2]_reg_input, GLOBAL(F_IN), , , );


--B5_dffs[3] is lpm_counter:Q4_rtl_4|dffs[3] at LC1
B5_dffs[3]_p1_out = B5_dffs[2] & B5_dffs[1] & B5_dffs[0] & B4_dffs[3] & !B4_dffs[2] & !B4_dffs[1] & B4_dffs[0] & B3_dffs[3] & !B3_dffs[2] & !B3_dffs[1] & B3_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & B2_dffs[3] & !B2_dffs[2] & !B2_dffs[1] & B2_dffs[0] & EN & !CLR;
B5_dffs[3]_p2_out = !B5_dffs[2] & !B5_dffs[1] & B5_dffs[0] & B4_dffs[3] & !B4_dffs[2] & !B4_dffs[1] & B4_dffs[0] & B3_dffs[3] & !B3_dffs[2] & !B3_dffs[1] & B3_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & B2_dffs[3] & !B2_dffs[2] & !B2_dffs[1] & B2_dffs[0] & B5_dffs[3];
B5_dffs[3]_p3_out = !EN & B5_dffs[3];
B5_dffs[3]_p4_out = CLR & B5_dffs[3];
B5_dffs[3]_or_out = B5_dffs[3]_p1_out # B5_dffs[3]_p2_out # B5_dffs[3]_p3_out # B5_dffs[3]_p4_out;
B5_dffs[3]_reg_input = B5_dffs[3]_or_out;
B5_dffs[3] = TFFE(B5_dffs[3]_reg_input, GLOBAL(F_IN), , , );


--B6_dffs[0] is lpm_counter:Q5_rtl_5|dffs[0] at LC3
B6_dffs[0]_p1_out = EN & !CLR & B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2] & B3_dffs[3] & B4_dffs[0] & !B4_dffs[1] & !B4_dffs[2] & B4_dffs[3] & B5_dffs[0] & !B5_dffs[1] & !B5_dffs[2] & B5_dffs[3];
B6_dffs[0]_p2_out = !EN & B6_dffs[0];
B6_dffs[0]_p3_out = CLR & B6_dffs[0];
B6_dffs[0]_or_out = B6_dffs[0]_p1_out # B6_dffs[0]_p2_out # B6_dffs[0]_p3_out;
B6_dffs[0]_reg_input = B6_dffs[0]_or_out;
B6_dffs[0] = TFFE(B6_dffs[0]_reg_input, GLOBAL(F_IN), , , );


--B6_dffs[1] is lpm_counter:Q5_rtl_5|dffs[1] at LC8
B6_dffs[1]_p0_out = B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2] & B3_dffs[3] & B4_dffs[0] & !B4_dffs[1] & !B4_dffs[2] & B4_dffs[3] & B5_dffs[0] & !B5_dffs[1] & !B5_dffs[2] & B5_dffs[3] & B6_dffs[0] & B6_dffs[1];
B6_dffs[1]_p1_out = !B6_dffs[3] & EN & !CLR & B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2] & B3_dffs[3] & B4_dffs[0] & !B4_dffs[1] & !B4_dffs[2] & B4_dffs[3] & B5_dffs[0] & !B5_dffs[1] & !B5_dffs[2] & B5_dffs[3] & B6_dffs[0];
B6_dffs[1]_p2_out = EN & !CLR & B2_dffs[0] & !B2_dffs[1] & !B2_dffs[2] & B2_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & B1_dffs[3] & B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2] & B3_dffs[3] & B4_dffs[0] & !B4_dffs[1] & !B4_dffs[2] & B4_dffs[3] & B5_dffs[0] & !B5_dffs[1] & !B5_dffs[2] & B5_dffs[3] & B6_dffs[0] & B6_dffs[2];
B6_dffs[1]_p3_out = !EN & B6_dffs[1];
B6_dffs[1]_p4_out = CLR & B6_dffs[1];
B6_dffs[1]_or_out = B6_dffs[1]_p0_out # B6_dffs[1]_p1_out # B6_dffs[1]_p2_out # B6_dffs[1]_p3_out # B6_dffs[1]_p4_out;
B6_dffs[1]_reg_input = B6_dffs[1]_or_out;
B6_dffs[1] = TFFE(B6_dffs[1]_reg_input, GLOBAL(F_IN), , , );


--B6_dffs[2] is lpm_counter:Q5_rtl_5|dffs[2] at LC11
B6_dffs[2]_p1_out = B6_dffs[1] & B6_dffs[0] & B5_dffs[3] & !B5_dffs[2] & !B5_dffs[1] & B5_dffs[0] & B4_dffs[3] & !B4_dffs[2] & !B4_dffs[1] & B4_dffs[0] & B3_dffs[3] & !B3_dffs[2] & !B3_dffs[1] & B3_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & B2_dffs[3] & !B2_dffs[2] & !B2_dffs[1] & B2_dffs[0] & EN & !CLR;
B6_dffs[2]_p2_out = !EN & B6_dffs[2];
B6_dffs[2]_p3_out = CLR & B6_dffs[2];
B6_dffs[2]_or_out = B6_dffs[2]_p1_out # B6_dffs[2]_p2_out # B6_dffs[2]_p3_out;
B6_dffs[2]_reg_input = B6_dffs[2]_or_out;
B6_dffs[2] = TFFE(B6_dffs[2]_reg_input, GLOBAL(F_IN), , , );


--B6_dffs[3] is lpm_counter:Q5_rtl_5|dffs[3] at LC16
B6_dffs[3]_p1_out = B6_dffs[2] & B6_dffs[1] & B6_dffs[0] & B5_dffs[3] & !B5_dffs[2] & !B5_dffs[1] & B5_dffs[0] & B4_dffs[3] & !B4_dffs[2] & !B4_dffs[1] & B4_dffs[0] & B3_dffs[3] & !B3_dffs[2] & !B3_dffs[1] & B3_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & B2_dffs[3] & !B2_dffs[2] & !B2_dffs[1] & B2_dffs[0] & EN & !CLR;
B6_dffs[3]_p2_out = !B6_dffs[2] & !B6_dffs[1] & B6_dffs[0] & B5_dffs[3] & !B5_dffs[2] & !B5_dffs[1] & B5_dffs[0] & B4_dffs[3] & !B4_dffs[2] & !B4_dffs[1] & B4_dffs[0] & B3_dffs[3] & !B3_dffs[2] & !B3_dffs[1] & B3_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & B2_dffs[3] & !B2_dffs[2] & !B2_dffs[1] & B2_dffs[0] & B6_dffs[3];
B6_dffs[3]_p3_out = !EN & B6_dffs[3];
B6_dffs[3]_p4_out = CLR & B6_dffs[3];
B6_dffs[3]_or_out = B6_dffs[3]_p1_out # B6_dffs[3]_p2_out # B6_dffs[3]_p3_out # B6_dffs[3]_p4_out;
B6_dffs[3]_reg_input = B6_dffs[3]_or_out;
B6_dffs[3] = TFFE(B6_dffs[3]_reg_input, GLOBAL(F_IN), , , );


--A1L5Q is F_OUT~reg0 at LC9
A1L5Q_p1_out = B5_dffs[3] & !B5_dffs[2] & !B5_dffs[1] & B5_dffs[0] & B4_dffs[3] & !B4_dffs[2] & !B4_dffs[1] & B4_dffs[0] & B3_dffs[3] & !B3_dffs[2] & !B3_dffs[1] & B3_dffs[0] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[1] & B1_dffs[0] & B2_dffs[3] & !B2_dffs[2] & !B2_dffs[1] & B2_dffs[0] & B6_dffs[3] & !B6_dffs[2] & !B6_dffs[1] & B6_dffs[0];
A1L5Q_or_out = A1L5Q_p1_out # !EN # CLR;
A1L5Q_reg_input = A1L5Q_or_out;
A1L5Q = DFFE(A1L5Q_reg_input, GLOBAL(F_IN), , , );


--EN is EN at PIN_63
--operation mode is input

EN = INPUT();


--CLR is CLR at PIN_81
--operation mode is input

CLR = INPUT();


--F_IN is F_IN at PIN_83
--operation mode is input

F_IN = INPUT();


--Q0[0] is Q0[0] at PIN_41
--operation mode is output

Q0[0] = OUTPUT(B1_dffs[0]);


--Q0[1] is Q0[1] at PIN_40
--operation mode is output

Q0[1] = OUTPUT(B1_dffs[1]);


--Q0[2] is Q0[2] at PIN_37
--operation mode is output

Q0[2] = OUTPUT(B1_dffs[2]);


--Q0[3] is Q0[3] at PIN_33
--operation mode is output

Q0[3] = OUTPUT(B1_dffs[3]);


--Q1[0] is Q1[0] at PIN_31
--operation mode is output

Q1[0] = OUTPUT(B2_dffs[0]);


--Q1[1] is Q1[1] at PIN_30
--operation mode is output

Q1[1] = OUTPUT(B2_dffs[1]);


--Q1[2] is Q1[2] at PIN_29
--operation mode is output

Q1[2] = OUTPUT(B2_dffs[2]);


--Q1[3] is Q1[3] at PIN_28
--operation mode is output

Q1[3] = OUTPUT(B2_dffs[3]);


--Q2[0] is Q2[0] at PIN_27
--operation mode is output

Q2[0] = OUTPUT(B3_dffs[0]);


--Q2[1] is Q2[1] at PIN_25
--operation mode is output

Q2[1] = OUTPUT(B3_dffs[1]);


--Q2[2] is Q2[2] at PIN_24
--operation mode is output

Q2[2] = OUTPUT(B3_dffs[2]);


--Q2[3] is Q2[3] at PIN_20
--operation mode is output

Q2[3] = OUTPUT(B3_dffs[3]);


--Q3[0] is Q3[0] at PIN_21
--operation mode is output

Q3[0] = OUTPUT(B4_dffs[0]);


--Q3[1] is Q3[1] at PIN_18
--operation mode is output

Q3[1] = OUTPUT(B4_dffs[1]);


--Q3[2] is Q3[2] at PIN_22
--operation mode is output

Q3[2] = OUTPUT(B4_dffs[2]);


--Q3[3] is Q3[3] at PIN_17
--operation mode is output

Q3[3] = OUTPUT(B4_dffs[3]);


--Q4[0] is Q4[0] at PIN_16
--operation mode is output

Q4[0] = OUTPUT(B5_dffs[0]);


--Q4[1] is Q4[1] at PIN_15
--operation mode is output

Q4[1] = OUTPUT(B5_dffs[1]);


--Q4[2] is Q4[2] at PIN_12
--operation mode is output

Q4[2] = OUTPUT(B5_dffs[2]);


--Q4[3] is Q4[3] at PIN_11
--operation mode is output

Q4[3] = OUTPUT(B5_dffs[3]);


--Q5[0] is Q5[0] at PIN_10
--operation mode is output

Q5[0] = OUTPUT(B6_dffs[0]);


--Q5[1] is Q5[1] at PIN_9
--operation mode is output

Q5[1] = OUTPUT(B6_dffs[1]);


--Q5[2] is Q5[2] at PIN_5
--operation mode is output

Q5[2] = OUTPUT(B6_dffs[2]);


--Q5[3] is Q5[3] at PIN_4
--operation mode is output

Q5[3] = OUTPUT(B6_dffs[3]);


--F_OUT is F_OUT at PIN_8
--operation mode is output

F_OUT = OUTPUT(A1L5Q);






