--A1L32 is reduce_or~347 at LC2
A1L32_p1_out = EN & !A & !C;
A1L32_p2_out = EN & !A & B;
A1L32_or_out = A1L32_p1_out # A1L32_p2_out;
A1L32 = A1L32_or_out;


--A1L22 is g_~47 at LC3
A1L22_p1_out = EN & !C & B;
A1L22_p2_out = EN & !C & D;
A1L22_p3_out = EN & C & !A;
A1L22_p4_out = EN & C & !B;
A1L22_or_out = A1L22_p1_out # A1L22_p2_out # A1L22_p3_out # A1L22_p4_out;
A1L22 = A1L22_or_out;


--A1L71 is d_~123 at LC5
A1L71_p1_out = C & EN & A & !B;
A1L71_p2_out = !C & EN & B;
A1L71_p3_out = !C & EN & !A;
A1L71_p4_out = EN & !A & B;
A1L71_or_out = A1L71_p1_out # A1L71_p2_out # A1L71_p3_out # A1L71_p4_out;
A1L71 = A1L71_or_out;


--A1L51 is c_~38 at LC6
A1L51_p1_out = !C & A & EN;
A1L51_p2_out = !C & EN & !B;
A1L51_p3_out = C & EN & !D;
A1L51_or_out = A1L51_p1_out # A1L51_p2_out # A1L51_p3_out;
A1L51 = A1L51_or_out;


--A1L02 is f_~83 at LC7
A1L02_p1_out = C & EN & !A;
A1L02_p2_out = EN & D & !B;
A1L02_p3_out = C & EN & !B;
A1L02_p4_out = EN & !A & !B;
A1L02_or_out = A1L02_p1_out # A1L02_p2_out # A1L02_p3_out # A1L02_p4_out;
A1L02 = A1L02_or_out;


--A1L31 is b_~49 at LC8
A1L31_p1_out = EN & !D & !C;
A1L31_p2_out = EN & !D & A & B;
A1L31_p3_out = EN & !A & !B;
A1L31_p4_out = EN & !C & !B;
A1L31_or_out = A1L31_p1_out # A1L31_p2_out # A1L31_p3_out # A1L31_p4_out;
A1L31 = A1L31_or_out;


--A1L11 is a_~74 at LC1
A1L11_p1_out = !A & !C & EN & !B;
A1L11_p2_out = A & C & EN & !D;
A1L11_p3_out = !C & EN & B & !D;
A1L11_p4_out = A & EN & !B & D;
A1L11_or_out = A1L11_p1_out # A1L11_p2_out # A1L11_p3_out # A1L11_p4_out;
A1L11 = A1L11_or_out;


--EN is EN at PIN_36
--operation mode is input

EN = INPUT();


--D is D at PIN_33
--operation mode is input

D = INPUT();


--C is C at PIN_21
--operation mode is input

C = INPUT();


--B is B at PIN_28
--operation mode is input

B = INPUT();


--A is A at PIN_16
--operation mode is input

A = INPUT();


--e_ is e_ at PIN_5
--operation mode is output

e_ = OUTPUT(A1L32);


--d_ is d_ at PIN_8
--operation mode is output

d_ = OUTPUT(A1L71);


--g_ is g_ at PIN_6
--operation mode is output

g_ = OUTPUT(A1L22);


--c_ is c_ at PIN_9
--operation mode is output

c_ = OUTPUT(A1L51);


--f_ is f_ at PIN_11
--operation mode is output

f_ = OUTPUT(A1L02);


--a_ is a_ at PIN_4
--operation mode is output

a_ = OUTPUT(A1L11);


--b_ is b_ at PIN_12
--operation mode is output

b_ = OUTPUT(A1L31);






