--B1_dffs[0] is lpm_counter:CNT_rtl_0|dffs[0] at LC3
B1_dffs[0]_p1_out = !B1_dffs[0] & !Reset;
B1_dffs[0]_or_out = B1_dffs[0]_p1_out;
B1_dffs[0]_reg_input = B1_dffs[0]_or_out;
B1_dffs[0] = DFFE(B1_dffs[0]_reg_input, GLOBAL(Clock_8MHz), , , );


--B1_dffs[2] is lpm_counter:CNT_rtl_0|dffs[2] at LC4
B1_dffs[2]_p1_out = !Reset & B1_dffs[1] & B1_dffs[0];
B1_dffs[2]_p2_out = Reset & B1_dffs[2];
B1_dffs[2]_or_out = B1_dffs[2]_p1_out # B1_dffs[2]_p2_out;
B1_dffs[2]_reg_input = B1_dffs[2]_or_out;
B1_dffs[2] = TFFE(B1_dffs[2]_reg_input, GLOBAL(Clock_8MHz), , , );


--B1_dffs[3] is lpm_counter:CNT_rtl_0|dffs[3] at LC1
B1_dffs[3]_p1_out = !Reset & B1_dffs[1] & B1_dffs[2] & B1_dffs[0];
B1_dffs[3]_p2_out = Reset & B1_dffs[3];
B1_dffs[3]_or_out = B1_dffs[3]_p1_out # B1_dffs[3]_p2_out;
B1_dffs[3]_reg_input = B1_dffs[3]_or_out;
B1_dffs[3] = TFFE(B1_dffs[3]_reg_input, GLOBAL(Clock_8MHz), , , );


--B1_dffs[1] is lpm_counter:CNT_rtl_0|dffs[1] at LC2
B1_dffs[1]_p1_out = !Reset & B1_dffs[0] & !B1_dffs[1];
B1_dffs[1]_p2_out = !Reset & !B1_dffs[0] & B1_dffs[1];
B1_dffs[1]_or_out = B1_dffs[1]_p1_out # B1_dffs[1]_p2_out;
B1_dffs[1]_reg_input = B1_dffs[1]_or_out;
B1_dffs[1] = DFFE(B1_dffs[1]_reg_input, GLOBAL(Clock_8MHz), , , );


--Reset is Reset at PIN_24
--operation mode is input

Reset = INPUT();


--Clock_8MHz is Clock_8MHz at PIN_43
--operation mode is input

Clock_8MHz = INPUT();


--F_1Hz is F_1Hz at PIN_4
--operation mode is output

F_1Hz = OUTPUT(B1_dffs[3]);


--F_65536Hz is F_65536Hz at PIN_5
--operation mode is output

F_65536Hz = OUTPUT(B1_dffs[1]);






