--S22_safe_q[0] is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S22_safe_q[0]_lut_out = !S22_safe_q[0];
S22_safe_q[0] = DFFEAS(S22_safe_q[0]_lut_out, SW2, VCC, , J1L4, , , J1L8, );

--S22L2 is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S22L2 = CARRY(S22_safe_q[0]);


--S9_safe_q[0] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S9_safe_q[0]_lut_out = !S9_safe_q[0];
S9_safe_q[0] = DFFEAS(S9_safe_q[0]_lut_out, SW2, VCC, , M1L5, , , M1L8, );

--S9L2 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S9L2 = CARRY(S9_safe_q[0]);


--S3_safe_q[0] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S3_safe_q[0]_lut_out = !S3_safe_q[0];
S3_safe_q[0] = DFFEAS(S3_safe_q[0]_lut_out, Q1_EO, VCC, , D1_Timepiece_EN, , , P1L2, );

--S3L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S3L2 = CARRY(S3_safe_q[0]);


--D1_TimeSet_EN is maincontrol:inst3|TimeSet_EN
--operation mode is normal

D1_TimeSet_EN_lut_out = D1_Function[0] & !D1_Function[2] & !D1_Function[1];
D1_TimeSet_EN = DFFEAS(D1_TimeSet_EN_lut_out, SW3, VCC, , , , , , );


--L1L9 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_0[0]~36
--operation mode is normal

L1L9 = D1_TimeSet_EN & S9_safe_q[0] # !D1_TimeSet_EN & S3_safe_q[0];


--S02_safe_q[0] is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S02_safe_q[0]_lut_out = !S02_safe_q[0];
S02_safe_q[0] = DFFEAS(S02_safe_q[0]_lut_out, SW2, VCC, , J1L2, , , J1L14, );

--S02L2 is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S02L2 = CARRY(S02_safe_q[0]);


--S7_safe_q[0] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S7_safe_q[0]_lut_out = !S7_safe_q[0];
S7_safe_q[0] = DFFEAS(S7_safe_q[0]_lut_out, SW2, VCC, , M1L2, , , M1L9, );

--S7L2 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S7L2 = CARRY(S7_safe_q[0]);


--S1_safe_q[0] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S1_safe_q[0]_lut_out = !S1_safe_q[0];
S1_safe_q[0] = DFFEAS(S1_safe_q[0]_lut_out, P1_EO, VCC, , D1_Timepiece_EN, , , N1L6, );

--S1L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S1L2 = CARRY(S1_safe_q[0]);


--L1L1 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_0[0]~36
--operation mode is normal

L1L1 = D1_TimeSet_EN & S7_safe_q[0] # !D1_TimeSet_EN & S1_safe_q[0];


--J1L02 is alarmclock:inst11|alarm~459
--operation mode is normal

J1L02 = S22_safe_q[0] & S02_safe_q[0] $ L1L1 # !L1L9 # !S22_safe_q[0] & L1L9 # S02_safe_q[0] $ L1L1;


--S22_safe_q[1] is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S22_safe_q[1]_carry_eqn = S22L2;
S22_safe_q[1]_lut_out = S22_safe_q[1] $ (S22_safe_q[1]_carry_eqn);
S22_safe_q[1] = DFFEAS(S22_safe_q[1]_lut_out, SW2, VCC, , J1L4, , , J1L8, );

--S22L4 is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S22L4 = CARRY(!S22L2 # !S22_safe_q[1]);


--S9_safe_q[1] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S9_safe_q[1]_carry_eqn = S9L2;
S9_safe_q[1]_lut_out = S9_safe_q[1] $ (S9_safe_q[1]_carry_eqn);
S9_safe_q[1] = DFFEAS(S9_safe_q[1]_lut_out, SW2, VCC, , M1L5, , , M1L8, );

--S9L4 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S9L4 = CARRY(!S9L2 # !S9_safe_q[1]);


--S3_safe_q[1] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S3_safe_q[1]_carry_eqn = S3L2;
S3_safe_q[1]_lut_out = S3_safe_q[1] $ (S3_safe_q[1]_carry_eqn);
S3_safe_q[1] = DFFEAS(S3_safe_q[1]_lut_out, Q1_EO, VCC, , D1_Timepiece_EN, , , P1L2, );

--S3L4 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S3L4 = CARRY(!S3L2 # !S3_safe_q[1]);


--L1L01 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_0[1]~37
--operation mode is normal

L1L01 = D1_TimeSet_EN & S9_safe_q[1] # !D1_TimeSet_EN & S3_safe_q[1];


--S32_safe_q[0] is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S32_safe_q[0]_lut_out = !S32_safe_q[0];
S32_safe_q[0] = DFFEAS(S32_safe_q[0]_lut_out, SW2, VCC, , J1L3, , , J1L01, );

--S32L2 is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S32L2 = CARRY(S32_safe_q[0]);


--S01_safe_q[0] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S01_safe_q[0]_lut_out = !S01_safe_q[0];
S01_safe_q[0] = DFFEAS(S01_safe_q[0]_lut_out, SW2, VCC, , M1L3, , , M1L01, );

--S01L2 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S01L2 = CARRY(S01_safe_q[0]);


--S4_safe_q[0] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S4_safe_q[0]_lut_out = !S4_safe_q[0];
S4_safe_q[0] = DFFEAS(S4_safe_q[0]_lut_out, Q1_EO, VCC, , P1L4, , , P1L3, );

--S4L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S4L2 = CARRY(S4_safe_q[0]);


--L1L31 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_1[0]~36
--operation mode is normal

L1L31 = D1_TimeSet_EN & S01_safe_q[0] # !D1_TimeSet_EN & S4_safe_q[0];


--J1L12 is alarmclock:inst11|alarm~460
--operation mode is normal

J1L12 = S22_safe_q[1] & S32_safe_q[0] $ L1L31 # !L1L01 # !S22_safe_q[1] & L1L01 # S32_safe_q[0] $ L1L31;


--S22_safe_q[3] is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S22_safe_q[3]_carry_eqn = S22L6;
S22_safe_q[3]_lut_out = S22_safe_q[3] $ (S22_safe_q[3]_carry_eqn);
S22_safe_q[3] = DFFEAS(S22_safe_q[3]_lut_out, SW2, VCC, , J1L4, , , J1L8, );


--S9_safe_q[3] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S9_safe_q[3]_carry_eqn = S9L6;
S9_safe_q[3]_lut_out = S9_safe_q[3] $ (S9_safe_q[3]_carry_eqn);
S9_safe_q[3] = DFFEAS(S9_safe_q[3]_lut_out, SW2, VCC, , M1L5, , , M1L8, );


--S3_safe_q[3] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S3_safe_q[3]_carry_eqn = S3L6;
S3_safe_q[3]_lut_out = S3_safe_q[3] $ (S3_safe_q[3]_carry_eqn);
S3_safe_q[3] = DFFEAS(S3_safe_q[3]_lut_out, Q1_EO, VCC, , D1_Timepiece_EN, , , P1L2, );


--L1L21 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_0[3]~38
--operation mode is normal

L1L21 = D1_TimeSet_EN & S9_safe_q[3] # !D1_TimeSet_EN & S3_safe_q[3];


--S42_safe_q[1] is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S42_safe_q[1]_carry_eqn = S42L2;
S42_safe_q[1]_lut_out = S42_safe_q[1] $ (S42_safe_q[1]_carry_eqn);
S42_safe_q[1] = DFFEAS(S42_safe_q[1]_lut_out, SW2, VCC, , J1L6, , , J1L7, );

--S42L4 is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S42L4 = CARRY(!S42L2 # !S42_safe_q[1]);


--S11_safe_q[1] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S11_safe_q[1]_carry_eqn = S11L2;
S11_safe_q[1]_lut_out = S11_safe_q[1] $ (S11_safe_q[1]_carry_eqn);
S11_safe_q[1] = DFFEAS(S11_safe_q[1]_lut_out, SW2, VCC, , M1L4, , , M1L7, );

--S11L4 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S11L4 = CARRY(!S11L2 # !S11_safe_q[1]);


--S5_safe_q[1] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S5_safe_q[1]_carry_eqn = S5L2;
S5_safe_q[1]_lut_out = S5_safe_q[1] $ (S5_safe_q[1]_carry_eqn);
S5_safe_q[1] = DFFEAS(S5_safe_q[1]_lut_out, C1L1, VCC, , D1_Timepiece_EN, , , Q1L2, );

--S5L4 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S5L4 = CARRY(!S5L2 # !S5_safe_q[1]);


--L1L81 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_0[1]~36
--operation mode is normal

L1L81 = D1_TimeSet_EN & S11_safe_q[1] # !D1_TimeSet_EN & S5_safe_q[1];


--J1L22 is alarmclock:inst11|alarm~461
--operation mode is normal

J1L22 = S22_safe_q[3] & S42_safe_q[1] $ L1L81 # !L1L21 # !S22_safe_q[3] & L1L21 # S42_safe_q[1] $ L1L81;


--S32_safe_q[2] is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S32_safe_q[2]_carry_eqn = S32L4;
S32_safe_q[2]_lut_out = S32_safe_q[2] $ (!S32_safe_q[2]_carry_eqn);
S32_safe_q[2] = DFFEAS(S32_safe_q[2]_lut_out, SW2, VCC, , J1L3, , , J1L01, );

--S32L6 is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S32L6 = CARRY(S32_safe_q[2] & !S32L4);


--S01_safe_q[2] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S01_safe_q[2]_carry_eqn = S01L4;
S01_safe_q[2]_lut_out = S01_safe_q[2] $ (!S01_safe_q[2]_carry_eqn);
S01_safe_q[2] = DFFEAS(S01_safe_q[2]_lut_out, SW2, VCC, , M1L3, , , M1L01, );

--S01L6 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S01L6 = CARRY(S01_safe_q[2] & !S01L4);


--S4_safe_q[2] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S4_safe_q[2]_carry_eqn = S4L4;
S4_safe_q[2]_lut_out = S4_safe_q[2] $ (!S4_safe_q[2]_carry_eqn);
S4_safe_q[2] = DFFEAS(S4_safe_q[2]_lut_out, Q1_EO, VCC, , P1L4, , , P1L3, );

--S4L6 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S4L6 = CARRY(S4_safe_q[2] & !S4L4);


--L1L51 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_1[2]~37
--operation mode is normal

L1L51 = D1_TimeSet_EN & S01_safe_q[2] # !D1_TimeSet_EN & S4_safe_q[2];


--S52_safe_q[2] is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S52_safe_q[2]_carry_eqn = S52L4;
S52_safe_q[2]_lut_out = S52_safe_q[2] $ (!S52_safe_q[2]_carry_eqn);
S52_safe_q[2] = DFFEAS(S52_safe_q[2]_lut_out, SW2, VCC, , J1L5, , , J1L11, );

--S52L6 is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S52L6 = CARRY(S52_safe_q[2] & !S52L4);


--S21_safe_q[2] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S21_safe_q[2]_carry_eqn = S21L4;
S21_safe_q[2]_lut_out = S21_safe_q[2] $ (!S21_safe_q[2]_carry_eqn);
S21_safe_q[2] = DFFEAS(S21_safe_q[2]_lut_out, SW2, VCC, , M1L6, , , M1L11, );

--S21L6 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S21L6 = CARRY(S21_safe_q[2] & !S21L4);


--S6_safe_q[2] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S6_safe_q[2]_carry_eqn = S6L4;
S6_safe_q[2]_lut_out = S6_safe_q[2] $ (!S6_safe_q[2]_carry_eqn);
S6_safe_q[2] = DFFEAS(S6_safe_q[2]_lut_out, C1L1, VCC, , Q1L4, , , Q1L3, );

--S6L6 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S6L6 = CARRY(S6_safe_q[2] & !S6L4);


--L1L32 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_1[2]~36
--operation mode is normal

L1L32 = D1_TimeSet_EN & S21_safe_q[2] # !D1_TimeSet_EN & S6_safe_q[2];


--J1L32 is alarmclock:inst11|alarm~462
--operation mode is normal

J1L32 = S32_safe_q[2] & S52_safe_q[2] $ L1L32 # !L1L51 # !S32_safe_q[2] & L1L51 # S52_safe_q[2] $ L1L32;


--J1L42 is alarmclock:inst11|alarm~463
--operation mode is normal

J1L42 = J1L02 # J1L12 # J1L22 # J1L32;


--S12_safe_q[2] is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S12_safe_q[2]_carry_eqn = S12L4;
S12_safe_q[2]_lut_out = S12_safe_q[2] $ (!S12_safe_q[2]_carry_eqn);
S12_safe_q[2] = DFFEAS(S12_safe_q[2]_lut_out, SW2, VCC, , J1L1, , , J1L9, );

--S12L6 is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S12L6 = CARRY(S12_safe_q[2] & !S12L4);


--S8_safe_q[2] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S8_safe_q[2]_carry_eqn = S8L4;
S8_safe_q[2]_lut_out = S8_safe_q[2] $ (!S8_safe_q[2]_carry_eqn);
S8_safe_q[2] = DFFEAS(S8_safe_q[2]_lut_out, SW2, VCC, , M1L1, , , M1L21, );

--S8L6 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S8L6 = CARRY(S8_safe_q[2] & !S8L4);


--S2_safe_q[2] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S2_safe_q[2]_carry_eqn = S2L4;
S2_safe_q[2]_lut_out = S2_safe_q[2] $ (!S2_safe_q[2]_carry_eqn);
S2_safe_q[2] = DFFEAS(S2_safe_q[2]_lut_out, P1_EO, VCC, , N1L4, , , N1L2, );

--S2L6 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S2L6 = CARRY(S2_safe_q[2] & !S2L4);


--L1L7 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_1[2]~36
--operation mode is normal

L1L7 = D1_TimeSet_EN & S8_safe_q[2] # !D1_TimeSet_EN & S2_safe_q[2];


--S22_safe_q[2] is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S22_safe_q[2]_carry_eqn = S22L4;
S22_safe_q[2]_lut_out = S22_safe_q[2] $ (!S22_safe_q[2]_carry_eqn);
S22_safe_q[2] = DFFEAS(S22_safe_q[2]_lut_out, SW2, VCC, , J1L4, , , J1L8, );

--S22L6 is alarmclock:inst11|lpm_counter:minute_set0_rtl_6|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S22L6 = CARRY(S22_safe_q[2] & !S22L4);


--S9_safe_q[2] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S9_safe_q[2]_carry_eqn = S9L4;
S9_safe_q[2]_lut_out = S9_safe_q[2] $ (!S9_safe_q[2]_carry_eqn);
S9_safe_q[2] = DFFEAS(S9_safe_q[2]_lut_out, SW2, VCC, , M1L5, , , M1L8, );

--S9L6 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set0_rtl_8|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S9L6 = CARRY(S9_safe_q[2] & !S9L4);


--S3_safe_q[2] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S3_safe_q[2]_carry_eqn = S3L4;
S3_safe_q[2]_lut_out = S3_safe_q[2] $ (!S3_safe_q[2]_carry_eqn);
S3_safe_q[2] = DFFEAS(S3_safe_q[2]_lut_out, Q1_EO, VCC, , D1_Timepiece_EN, , , P1L2, );

--S3L6 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data0_rtl_7|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S3L6 = CARRY(S3_safe_q[2] & !S3L4);


--L1L11 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_0[2]~39
--operation mode is normal

L1L11 = D1_TimeSet_EN & S9_safe_q[2] # !D1_TimeSet_EN & S3_safe_q[2];


--J1L52 is alarmclock:inst11|alarm~464
--operation mode is normal

J1L52 = S12_safe_q[2] & S22_safe_q[2] $ L1L11 # !L1L7 # !S12_safe_q[2] & L1L7 # S22_safe_q[2] $ L1L11;


--S02_safe_q[1] is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S02_safe_q[1]_carry_eqn = S02L2;
S02_safe_q[1]_lut_out = S02_safe_q[1] $ (S02_safe_q[1]_carry_eqn);
S02_safe_q[1] = DFFEAS(S02_safe_q[1]_lut_out, SW2, VCC, , J1L2, , , J1L14, );

--S02L4 is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S02L4 = CARRY(!S02L2 # !S02_safe_q[1]);


--S7_safe_q[1] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S7_safe_q[1]_carry_eqn = S7L2;
S7_safe_q[1]_lut_out = S7_safe_q[1] $ (S7_safe_q[1]_carry_eqn);
S7_safe_q[1] = DFFEAS(S7_safe_q[1]_lut_out, SW2, VCC, , M1L2, , , M1L9, );

--S7L4 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S7L4 = CARRY(!S7L2 # !S7_safe_q[1]);


--S1_safe_q[1] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S1_safe_q[1]_carry_eqn = S1L2;
S1_safe_q[1]_lut_out = S1_safe_q[1] $ (S1_safe_q[1]_carry_eqn);
S1_safe_q[1] = DFFEAS(S1_safe_q[1]_lut_out, P1_EO, VCC, , D1_Timepiece_EN, , , N1L6, );

--S1L4 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S1L4 = CARRY(!S1L2 # !S1_safe_q[1]);


--L1L2 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_0[1]~37
--operation mode is normal

L1L2 = D1_TimeSet_EN & S7_safe_q[1] # !D1_TimeSet_EN & S1_safe_q[1];


--S52_safe_q[3] is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S52_safe_q[3]_carry_eqn = S52L6;
S52_safe_q[3]_lut_out = S52_safe_q[3] $ (S52_safe_q[3]_carry_eqn);
S52_safe_q[3] = DFFEAS(S52_safe_q[3]_lut_out, SW2, VCC, , J1L5, , , J1L11, );


--S21_safe_q[3] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S21_safe_q[3]_carry_eqn = S21L6;
S21_safe_q[3]_lut_out = S21_safe_q[3] $ (S21_safe_q[3]_carry_eqn);
S21_safe_q[3] = DFFEAS(S21_safe_q[3]_lut_out, SW2, VCC, , M1L6, , , M1L11, );


--S6_safe_q[3] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S6_safe_q[3]_carry_eqn = S6L6;
S6_safe_q[3]_lut_out = S6_safe_q[3] $ (S6_safe_q[3]_carry_eqn);
S6_safe_q[3] = DFFEAS(S6_safe_q[3]_lut_out, C1L1, VCC, , Q1L4, , , Q1L3, );


--L1L42 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_1[3]~37
--operation mode is normal

L1L42 = D1_TimeSet_EN & S21_safe_q[3] # !D1_TimeSet_EN & S6_safe_q[3];


--J1L62 is alarmclock:inst11|alarm~465
--operation mode is normal

J1L62 = S02_safe_q[1] & S52_safe_q[3] $ L1L42 # !L1L2 # !S02_safe_q[1] & L1L2 # S52_safe_q[3] $ L1L42;


--S42_safe_q[2] is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S42_safe_q[2]_carry_eqn = S42L4;
S42_safe_q[2]_lut_out = S42_safe_q[2] $ (!S42_safe_q[2]_carry_eqn);
S42_safe_q[2] = DFFEAS(S42_safe_q[2]_lut_out, SW2, VCC, , J1L6, , , J1L7, );

--S42L6 is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S42L6 = CARRY(S42_safe_q[2] & !S42L4);


--S11_safe_q[2] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S11_safe_q[2]_carry_eqn = S11L4;
S11_safe_q[2]_lut_out = S11_safe_q[2] $ (!S11_safe_q[2]_carry_eqn);
S11_safe_q[2] = DFFEAS(S11_safe_q[2]_lut_out, SW2, VCC, , M1L4, , , M1L7, );

--S11L6 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S11L6 = CARRY(S11_safe_q[2] & !S11L4);


--S5_safe_q[2] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S5_safe_q[2]_carry_eqn = S5L4;
S5_safe_q[2]_lut_out = S5_safe_q[2] $ (!S5_safe_q[2]_carry_eqn);
S5_safe_q[2] = DFFEAS(S5_safe_q[2]_lut_out, C1L1, VCC, , D1_Timepiece_EN, , , Q1L2, );

--S5L6 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S5L6 = CARRY(S5_safe_q[2] & !S5L4);


--L1L91 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_0[2]~37
--operation mode is normal

L1L91 = D1_TimeSet_EN & S11_safe_q[2] # !D1_TimeSet_EN & S5_safe_q[2];


--S42_safe_q[0] is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S42_safe_q[0]_lut_out = !S42_safe_q[0];
S42_safe_q[0] = DFFEAS(S42_safe_q[0]_lut_out, SW2, VCC, , J1L6, , , J1L7, );

--S42L2 is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S42L2 = CARRY(S42_safe_q[0]);


--S11_safe_q[0] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S11_safe_q[0]_lut_out = !S11_safe_q[0];
S11_safe_q[0] = DFFEAS(S11_safe_q[0]_lut_out, SW2, VCC, , M1L4, , , M1L7, );

--S11L2 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S11L2 = CARRY(S11_safe_q[0]);


--S5_safe_q[0] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S5_safe_q[0]_lut_out = !S5_safe_q[0];
S5_safe_q[0] = DFFEAS(S5_safe_q[0]_lut_out, C1L1, VCC, , D1_Timepiece_EN, , , Q1L2, );

--S5L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S5L2 = CARRY(S5_safe_q[0]);


--L1L71 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_0[0]~38
--operation mode is normal

L1L71 = D1_TimeSet_EN & S11_safe_q[0] # !D1_TimeSet_EN & S5_safe_q[0];


--J1L72 is alarmclock:inst11|alarm~466
--operation mode is normal

J1L72 = S42_safe_q[2] & S42_safe_q[0] $ L1L71 # !L1L91 # !S42_safe_q[2] & L1L91 # S42_safe_q[0] $ L1L71;


--S52_safe_q[0] is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S52_safe_q[0]_lut_out = !S52_safe_q[0];
S52_safe_q[0] = DFFEAS(S52_safe_q[0]_lut_out, SW2, VCC, , J1L5, , , J1L11, );

--S52L2 is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S52L2 = CARRY(S52_safe_q[0]);


--S21_safe_q[0] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S21_safe_q[0]_lut_out = !S21_safe_q[0];
S21_safe_q[0] = DFFEAS(S21_safe_q[0]_lut_out, SW2, VCC, , M1L6, , , M1L11, );

--S21L2 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S21L2 = CARRY(S21_safe_q[0]);


--S6_safe_q[0] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S6_safe_q[0]_lut_out = !S6_safe_q[0];
S6_safe_q[0] = DFFEAS(S6_safe_q[0]_lut_out, C1L1, VCC, , Q1L4, , , Q1L3, );

--S6L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S6L2 = CARRY(S6_safe_q[0]);


--L1L12 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_1[0]~38
--operation mode is normal

L1L12 = D1_TimeSet_EN & S21_safe_q[0] # !D1_TimeSet_EN & S6_safe_q[0];


--S32_safe_q[3] is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S32_safe_q[3]_carry_eqn = S32L6;
S32_safe_q[3]_lut_out = S32_safe_q[3] $ (S32_safe_q[3]_carry_eqn);
S32_safe_q[3] = DFFEAS(S32_safe_q[3]_lut_out, SW2, VCC, , J1L3, , , J1L01, );


--S01_safe_q[3] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S01_safe_q[3]_carry_eqn = S01L6;
S01_safe_q[3]_lut_out = S01_safe_q[3] $ (S01_safe_q[3]_carry_eqn);
S01_safe_q[3] = DFFEAS(S01_safe_q[3]_lut_out, SW2, VCC, , M1L3, , , M1L01, );


--S4_safe_q[3] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S4_safe_q[3]_carry_eqn = S4L6;
S4_safe_q[3]_lut_out = S4_safe_q[3] $ (S4_safe_q[3]_carry_eqn);
S4_safe_q[3] = DFFEAS(S4_safe_q[3]_lut_out, Q1_EO, VCC, , P1L4, , , P1L3, );


--L1L61 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_1[3]~38
--operation mode is normal

L1L61 = D1_TimeSet_EN & S01_safe_q[3] # !D1_TimeSet_EN & S4_safe_q[3];


--J1L82 is alarmclock:inst11|alarm~467
--operation mode is normal

J1L82 = S52_safe_q[0] & S32_safe_q[3] $ L1L61 # !L1L12 # !S52_safe_q[0] & L1L12 # S32_safe_q[3] $ L1L61;


--J1L92 is alarmclock:inst11|alarm~468
--operation mode is normal

J1L92 = J1L52 # J1L62 # J1L72 # J1L82;


--S32_safe_q[1] is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S32_safe_q[1]_carry_eqn = S32L2;
S32_safe_q[1]_lut_out = S32_safe_q[1] $ (S32_safe_q[1]_carry_eqn);
S32_safe_q[1] = DFFEAS(S32_safe_q[1]_lut_out, SW2, VCC, , J1L3, , , J1L01, );

--S32L4 is alarmclock:inst11|lpm_counter:minute_set1_rtl_9|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S32L4 = CARRY(!S32L2 # !S32_safe_q[1]);


--S01_safe_q[1] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S01_safe_q[1]_carry_eqn = S01L2;
S01_safe_q[1]_lut_out = S01_safe_q[1] $ (S01_safe_q[1]_carry_eqn);
S01_safe_q[1] = DFFEAS(S01_safe_q[1]_lut_out, SW2, VCC, , M1L3, , , M1L01, );

--S01L4 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:minute_set1_rtl_11|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S01L4 = CARRY(!S01L2 # !S01_safe_q[1]);


--S4_safe_q[1] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S4_safe_q[1]_carry_eqn = S4L2;
S4_safe_q[1]_lut_out = S4_safe_q[1] $ (S4_safe_q[1]_carry_eqn);
S4_safe_q[1] = DFFEAS(S4_safe_q[1]_lut_out, Q1_EO, VCC, , P1L4, , , P1L3, );

--S4L4 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|lpm_counter:minute_data1_rtl_10|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S4L4 = CARRY(!S4L2 # !S4_safe_q[1]);


--L1L41 is time_auto_and_set:inst1|time_mux:b2v_inst2|minute_1[1]~39
--operation mode is normal

L1L41 = D1_TimeSet_EN & S01_safe_q[1] # !D1_TimeSet_EN & S4_safe_q[1];


--S12_safe_q[1] is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S12_safe_q[1]_carry_eqn = S12L2;
S12_safe_q[1]_lut_out = S12_safe_q[1] $ (S12_safe_q[1]_carry_eqn);
S12_safe_q[1] = DFFEAS(S12_safe_q[1]_lut_out, SW2, VCC, , J1L1, , , J1L9, );

--S12L4 is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S12L4 = CARRY(!S12L2 # !S12_safe_q[1]);


--S8_safe_q[1] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S8_safe_q[1]_carry_eqn = S8L2;
S8_safe_q[1]_lut_out = S8_safe_q[1] $ (S8_safe_q[1]_carry_eqn);
S8_safe_q[1] = DFFEAS(S8_safe_q[1]_lut_out, SW2, VCC, , M1L1, , , M1L21, );

--S8L4 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S8L4 = CARRY(!S8L2 # !S8_safe_q[1]);


--S2_safe_q[1] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S2_safe_q[1]_carry_eqn = S2L2;
S2_safe_q[1]_lut_out = S2_safe_q[1] $ (S2_safe_q[1]_carry_eqn);
S2_safe_q[1] = DFFEAS(S2_safe_q[1]_lut_out, P1_EO, VCC, , N1L4, , , N1L2, );

--S2L4 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S2L4 = CARRY(!S2L2 # !S2_safe_q[1]);


--L1L6 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_1[1]~37
--operation mode is normal

L1L6 = D1_TimeSet_EN & S8_safe_q[1] # !D1_TimeSet_EN & S2_safe_q[1];


--J1L03 is alarmclock:inst11|alarm~469
--operation mode is normal

J1L03 = S32_safe_q[1] & S12_safe_q[1] $ L1L6 # !L1L41 # !S32_safe_q[1] & L1L41 # S12_safe_q[1] $ L1L6;


--S12_safe_q[0] is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S12_safe_q[0]_lut_out = !S12_safe_q[0];
S12_safe_q[0] = DFFEAS(S12_safe_q[0]_lut_out, SW2, VCC, , J1L1, , , J1L9, );

--S12L2 is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S12L2 = CARRY(S12_safe_q[0]);


--S8_safe_q[0] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S8_safe_q[0]_lut_out = !S8_safe_q[0];
S8_safe_q[0] = DFFEAS(S8_safe_q[0]_lut_out, SW2, VCC, , M1L1, , , M1L21, );

--S8L2 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S8L2 = CARRY(S8_safe_q[0]);


--S2_safe_q[0] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S2_safe_q[0]_lut_out = !S2_safe_q[0];
S2_safe_q[0] = DFFEAS(S2_safe_q[0]_lut_out, P1_EO, VCC, , N1L4, , , N1L2, );

--S2L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S2L2 = CARRY(S2_safe_q[0]);


--L1L5 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_1[0]~38
--operation mode is normal

L1L5 = D1_TimeSet_EN & S8_safe_q[0] # !D1_TimeSet_EN & S2_safe_q[0];


--S02_safe_q[2] is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S02_safe_q[2]_carry_eqn = S02L4;
S02_safe_q[2]_lut_out = S02_safe_q[2] $ (!S02_safe_q[2]_carry_eqn);
S02_safe_q[2] = DFFEAS(S02_safe_q[2]_lut_out, SW2, VCC, , J1L2, , , J1L14, );

--S02L6 is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S02L6 = CARRY(S02_safe_q[2] & !S02L4);


--S7_safe_q[2] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S7_safe_q[2]_carry_eqn = S7L4;
S7_safe_q[2]_lut_out = S7_safe_q[2] $ (!S7_safe_q[2]_carry_eqn);
S7_safe_q[2] = DFFEAS(S7_safe_q[2]_lut_out, SW2, VCC, , M1L2, , , M1L9, );

--S7L6 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S7L6 = CARRY(S7_safe_q[2] & !S7L4);


--S1_safe_q[2] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S1_safe_q[2]_carry_eqn = S1L4;
S1_safe_q[2]_lut_out = S1_safe_q[2] $ (!S1_safe_q[2]_carry_eqn);
S1_safe_q[2] = DFFEAS(S1_safe_q[2]_lut_out, P1_EO, VCC, , D1_Timepiece_EN, , , N1L6, );

--S1L6 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S1L6 = CARRY(S1_safe_q[2] & !S1L4);


--L1L3 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_0[2]~38
--operation mode is normal

L1L3 = D1_TimeSet_EN & S7_safe_q[2] # !D1_TimeSet_EN & S1_safe_q[2];


--J1L13 is alarmclock:inst11|alarm~470
--operation mode is normal

J1L13 = S12_safe_q[0] & S02_safe_q[2] $ L1L3 # !L1L5 # !S12_safe_q[0] & L1L5 # S02_safe_q[2] $ L1L3;


--S52_safe_q[1] is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S52_safe_q[1]_carry_eqn = S52L2;
S52_safe_q[1]_lut_out = S52_safe_q[1] $ (S52_safe_q[1]_carry_eqn);
S52_safe_q[1] = DFFEAS(S52_safe_q[1]_lut_out, SW2, VCC, , J1L5, , , J1L11, );

--S52L4 is alarmclock:inst11|lpm_counter:second_set1_rtl_3|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S52L4 = CARRY(!S52L2 # !S52_safe_q[1]);


--S21_safe_q[1] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S21_safe_q[1]_carry_eqn = S21L2;
S21_safe_q[1]_lut_out = S21_safe_q[1] $ (S21_safe_q[1]_carry_eqn);
S21_safe_q[1] = DFFEAS(S21_safe_q[1]_lut_out, SW2, VCC, , M1L6, , , M1L11, );

--S21L4 is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set1_rtl_5|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S21L4 = CARRY(!S21L2 # !S21_safe_q[1]);


--S6_safe_q[1] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S6_safe_q[1]_carry_eqn = S6L2;
S6_safe_q[1]_lut_out = S6_safe_q[1] $ (S6_safe_q[1]_carry_eqn);
S6_safe_q[1] = DFFEAS(S6_safe_q[1]_lut_out, C1L1, VCC, , Q1L4, , , Q1L3, );

--S6L4 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data1_rtl_4|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S6L4 = CARRY(!S6L2 # !S6_safe_q[1]);


--L1L22 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_1[1]~39
--operation mode is normal

L1L22 = D1_TimeSet_EN & S21_safe_q[1] # !D1_TimeSet_EN & S6_safe_q[1];


--S02_safe_q[3] is alarmclock:inst11|lpm_counter:hour_set0_rtl_12|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S02_safe_q[3]_carry_eqn = S02L6;
S02_safe_q[3]_lut_out = S02_safe_q[3] $ (S02_safe_q[3]_carry_eqn);
S02_safe_q[3] = DFFEAS(S02_safe_q[3]_lut_out, SW2, VCC, , J1L2, , , J1L14, );


--S7_safe_q[3] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set0_rtl_14|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S7_safe_q[3]_carry_eqn = S7L6;
S7_safe_q[3]_lut_out = S7_safe_q[3] $ (S7_safe_q[3]_carry_eqn);
S7_safe_q[3] = DFFEAS(S7_safe_q[3]_lut_out, SW2, VCC, , M1L2, , , M1L9, );


--S1_safe_q[3] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data0_rtl_13|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S1_safe_q[3]_carry_eqn = S1L6;
S1_safe_q[3]_lut_out = S1_safe_q[3] $ (S1_safe_q[3]_carry_eqn);
S1_safe_q[3] = DFFEAS(S1_safe_q[3]_lut_out, P1_EO, VCC, , D1_Timepiece_EN, , , N1L6, );


--L1L4 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_0[3]~39
--operation mode is normal

L1L4 = D1_TimeSet_EN & S7_safe_q[3] # !D1_TimeSet_EN & S1_safe_q[3];


--J1L23 is alarmclock:inst11|alarm~471
--operation mode is normal

J1L23 = S52_safe_q[1] & S02_safe_q[3] $ L1L4 # !L1L22 # !S52_safe_q[1] & L1L22 # S02_safe_q[3] $ L1L4;


--S12_safe_q[3] is alarmclock:inst11|lpm_counter:hour_set1_rtl_15|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S12_safe_q[3]_carry_eqn = S12L6;
S12_safe_q[3]_lut_out = S12_safe_q[3] $ (S12_safe_q[3]_carry_eqn);
S12_safe_q[3] = DFFEAS(S12_safe_q[3]_lut_out, SW2, VCC, , J1L1, , , J1L9, );


--S8_safe_q[3] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:hour_set1_rtl_17|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S8_safe_q[3]_carry_eqn = S8L6;
S8_safe_q[3]_lut_out = S8_safe_q[3] $ (S8_safe_q[3]_carry_eqn);
S8_safe_q[3] = DFFEAS(S8_safe_q[3]_lut_out, SW2, VCC, , M1L1, , , M1L21, );


--S2_safe_q[3] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|lpm_counter:hour_data1_rtl_16|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S2_safe_q[3]_carry_eqn = S2L6;
S2_safe_q[3]_lut_out = S2_safe_q[3] $ (S2_safe_q[3]_carry_eqn);
S2_safe_q[3] = DFFEAS(S2_safe_q[3]_lut_out, P1_EO, VCC, , N1L4, , , N1L2, );


--L1L8 is time_auto_and_set:inst1|time_mux:b2v_inst2|hour_1[3]~39
--operation mode is normal

L1L8 = D1_TimeSet_EN & S8_safe_q[3] # !D1_TimeSet_EN & S2_safe_q[3];


--S42_safe_q[3] is alarmclock:inst11|lpm_counter:second_set0_rtl_0|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S42_safe_q[3]_carry_eqn = S42L6;
S42_safe_q[3]_lut_out = S42_safe_q[3] $ (S42_safe_q[3]_carry_eqn);
S42_safe_q[3] = DFFEAS(S42_safe_q[3]_lut_out, SW2, VCC, , J1L6, , , J1L7, );


--S11_safe_q[3] is time_auto_and_set:inst1|timeset:b2v_inst3|lpm_counter:second_set0_rtl_2|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S11_safe_q[3]_carry_eqn = S11L6;
S11_safe_q[3]_lut_out = S11_safe_q[3] $ (S11_safe_q[3]_carry_eqn);
S11_safe_q[3] = DFFEAS(S11_safe_q[3]_lut_out, SW2, VCC, , M1L4, , , M1L7, );


--S5_safe_q[3] is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|lpm_counter:second_data0_rtl_1|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S5_safe_q[3]_carry_eqn = S5L6;
S5_safe_q[3]_lut_out = S5_safe_q[3] $ (S5_safe_q[3]_carry_eqn);
S5_safe_q[3] = DFFEAS(S5_safe_q[3]_lut_out, C1L1, VCC, , D1_Timepiece_EN, , , Q1L2, );


--L1L02 is time_auto_and_set:inst1|time_mux:b2v_inst2|second_0[3]~39
--operation mode is normal

L1L02 = D1_TimeSet_EN & S11_safe_q[3] # !D1_TimeSet_EN & S5_safe_q[3];


--J1L33 is alarmclock:inst11|alarm~472
--operation mode is normal

J1L33 = S12_safe_q[3] & S42_safe_q[3] $ L1L02 # !L1L8 # !S12_safe_q[3] & L1L8 # S42_safe_q[3] $ L1L02;


--J1L43 is alarmclock:inst11|alarm~473
--operation mode is normal

J1L43 = J1L03 # J1L13 # J1L23 # J1L33;


--J1_alarm is alarmclock:inst11|alarm
--operation mode is normal

J1_alarm = J1L42 # J1L92 # J1L43;


--H1L68 is disp_data_mux:inst8|reduce_or~38
--operation mode is normal

H1L68 = H1_Data[1] & H1_Data[3] # !H1_Data[1] & H1_Data[2] $ (H1_Data[0] & !H1_Data[3]);


--H1L78 is disp_data_mux:inst8|reduce_or~40
--operation mode is normal

H1L78 = H1_Data[2] & H1_Data[3] # H1_Data[0] $ H1_Data[1] # !H1_Data[2] & H1_Data[1] & H1_Data[3];


--H1L88 is disp_data_mux:inst8|reduce_or~42
--operation mode is normal

H1L88 = H1_Data[2] & H1_Data[3] # !H1_Data[2] & H1_Data[1] & H1_Data[3] # !H1_Data[0];


--H1L66 is disp_data_mux:inst8|disp_data[3]~32
--operation mode is normal

H1L66 = H1_Data[1] & H1_Data[3] # H1_Data[0] & H1_Data[2] # !H1_Data[1] & H1_Data[2] $ (H1_Data[0] & !H1_Data[3]);


--H1L56 is disp_data_mux:inst8|disp_data[2]~34
--operation mode is normal

H1L56 = H1_Data[0] # H1_Data[1] & H1_Data[3] # !H1_Data[1] & H1_Data[2];


--H1L46 is disp_data_mux:inst8|disp_data[1]~36
--operation mode is normal

H1L46 = H1_Data[0] & H1_Data[1] # H1_Data[2] $ !H1_Data[3] # !H1_Data[0] & H1_Data[2] & H1_Data[3] # !H1_Data[2] & H1_Data[1];


--H1L36 is disp_data_mux:inst8|disp_data[0]~38
--operation mode is normal

H1L36 = H1_Data[1] & !H1_Data[3] & !H1_Data[2] # !H1_Data[0] # !H1_Data[1] & H1_Data[2] $ H1_Data[3];


--J1L8 is alarmclock:inst11|LessThan~164
--operation mode is normal

J1L8 = S22_safe_q[3] & S22_safe_q[0] # S22_safe_q[1] # S22_safe_q[2];


--J1_disp_drive[1] is alarmclock:inst11|disp_drive[1]
--operation mode is normal

J1_disp_drive[1]_lut_out = J1_disp_drive[1] & !J1_disp_drive[0] # !J1_disp_drive[1] & !J1_disp_drive[2] & J1_disp_drive[0];
J1_disp_drive[1] = DFFEAS(J1_disp_drive[1]_lut_out, SW1, VCC, , D1_Alarmclock_EN, , , , );


--J1_disp_drive[0] is alarmclock:inst11|disp_drive[0]
--operation mode is normal

J1_disp_drive[0]_lut_out = !J1_disp_drive[0];
J1_disp_drive[0] = DFFEAS(J1_disp_drive[0]_lut_out, SW1, VCC, , D1_Alarmclock_EN, , , , );


--J1_disp_drive[2] is alarmclock:inst11|disp_drive[2]
--operation mode is normal

J1_disp_drive[2]_lut_out = J1_disp_drive[2] & !J1_disp_drive[0] # !J1_disp_drive[2] & J1_disp_drive[1] & J1_disp_drive[0];
J1_disp_drive[2] = DFFEAS(J1_disp_drive[2]_lut_out, SW1, VCC, , D1_Alarmclock_EN, , , , );


--J1L4 is alarmclock:inst11|Decoder~20
--operation mode is normal

J1L4 = J1_disp_drive[1] & J1_disp_drive[0] & !J1_disp_drive[2];


--M1L8 is time_auto_and_set:inst1|timeset:b2v_inst3|LessThan~160
--operation mode is normal

M1L8 = S9_safe_q[3] & S9_safe_q[0] # S9_safe_q[1] # S9_safe_q[2];


--M1_disp_drive[1] is time_auto_and_set:inst1|timeset:b2v_inst3|disp_drive[1]
--operation mode is normal

M1_disp_drive[1]_lut_out = !M1_disp_drive[2] & M1_disp_drive[1] $ M1_disp_drive[0];
M1_disp_drive[1] = DFFEAS(M1_disp_drive[1]_lut_out, SW1, VCC, , D1_TimeSet_EN, , , , );


--M1_disp_drive[0] is time_auto_and_set:inst1|timeset:b2v_inst3|disp_drive[0]
--operation mode is normal

M1_disp_drive[0]_lut_out = !M1_disp_drive[0] & !M1_disp_drive[1] # !M1_disp_drive[2];
M1_disp_drive[0] = DFFEAS(M1_disp_drive[0]_lut_out, SW1, VCC, , D1_TimeSet_EN, , , , );


--M1_disp_drive[2] is time_auto_and_set:inst1|timeset:b2v_inst3|disp_drive[2]
--operation mode is normal

M1_disp_drive[2]_lut_out = M1_disp_drive[2] & !M1_disp_drive[1] & !M1_disp_drive[0] # !M1_disp_drive[2] & M1_disp_drive[1] & M1_disp_drive[0];
M1_disp_drive[2] = DFFEAS(M1_disp_drive[2]_lut_out, SW1, VCC, , D1_TimeSet_EN, , , , );


--M1L5 is time_auto_and_set:inst1|timeset:b2v_inst3|Decoder~95
--operation mode is normal

M1L5 = M1_disp_drive[1] & M1_disp_drive[0] & !M1_disp_drive[2];


--Q1_EO is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|EO
--operation mode is normal

Q1_EO_lut_out = Q1L3;
Q1_EO = DFFEAS(Q1_EO_lut_out, C1L1, VCC, , Q1L4, , , , );


--P1L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|LessThan~47
--operation mode is normal

P1L2 = S3_safe_q[3] & S3_safe_q[0] # S3_safe_q[1] # S3_safe_q[2];


--D1_Timepiece_EN is maincontrol:inst3|Timepiece_EN
--operation mode is normal

D1_Timepiece_EN_lut_out = !D1_Function[2] & !D1_Function[1] & !D1_Function[0];
D1_Timepiece_EN = DFFEAS(D1_Timepiece_EN_lut_out, SW3, VCC, , , , , , );


--D1_Function[0] is maincontrol:inst3|Function[0]
--operation mode is normal

D1_Function[0]_lut_out = !D1_Function[0] & !D1_Function[1] # !D1_Function[2];
D1_Function[0] = DFFEAS(D1_Function[0]_lut_out, SW3, VCC, , , , , , );


--D1_Function[2] is maincontrol:inst3|Function[2]
--operation mode is normal

D1_Function[2]_lut_out = D1_Function[2] & !D1_Function[1] & !D1_Function[0] # !D1_Function[2] & D1_Function[1] & D1_Function[0];
D1_Function[2] = DFFEAS(D1_Function[2]_lut_out, SW3, VCC, , , , , , );


--D1_Function[1] is maincontrol:inst3|Function[1]
--operation mode is normal

D1_Function[1]_lut_out = !D1_Function[2] & D1_Function[1] $ D1_Function[0];
D1_Function[1] = DFFEAS(D1_Function[1]_lut_out, SW3, VCC, , , , , , );


--J1L53 is alarmclock:inst11|always2~26
--operation mode is normal

J1L53 = S12_safe_q[1] & !S12_safe_q[2] & !S12_safe_q[0] & !S12_safe_q[3];


--J1L9 is alarmclock:inst11|LessThan~214
--operation mode is normal

J1L9 = S12_safe_q[2] # S12_safe_q[1] # S12_safe_q[3];


--J1L04 is alarmclock:inst11|hour_set0[2]~117
--operation mode is normal

J1L04 = S02_safe_q[2] # S02_safe_q[3] & S02_safe_q[0] # S02_safe_q[1];


--J1L14 is alarmclock:inst11|hour_set0[2]~118
--operation mode is normal

J1L14 = J1L9 & S02_safe_q[3] # J1L04 # !J1L53 # !J1L9 & S02_safe_q[3] & J1L04;


--J1L2 is alarmclock:inst11|Decoder~18
--operation mode is normal

J1L2 = J1_disp_drive[0] & !J1_disp_drive[1] & !J1_disp_drive[2];


--M1L9 is time_auto_and_set:inst1|timeset:b2v_inst3|LessThan~192
--operation mode is normal

M1L9 = S7_safe_q[3] & S7_safe_q[0] # S7_safe_q[1] # S7_safe_q[2];


--M1L2 is time_auto_and_set:inst1|timeset:b2v_inst3|Decoder~18
--operation mode is normal

M1L2 = M1_disp_drive[0] & !M1_disp_drive[2] & !M1_disp_drive[1];


--P1_EO is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|EO
--operation mode is normal

P1_EO_lut_out = P1L3;
P1_EO = DFFEAS(P1_EO_lut_out, Q1_EO, VCC, , P1L4, , , , );


--N1L3 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|always0~86
--operation mode is normal

N1L3 = S2_safe_q[1] & !S2_safe_q[2] & !S2_safe_q[0] & !S2_safe_q[3];


--N1L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|LessThan~82
--operation mode is normal

N1L2 = S2_safe_q[2] # S2_safe_q[1] # S2_safe_q[3];


--N1L5 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|hour_data1[0]~71
--operation mode is normal

N1L5 = S1_safe_q[2] # S1_safe_q[3] & S1_safe_q[0] # S1_safe_q[1];


--N1L6 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|hour_data1[0]~72
--operation mode is normal

N1L6 = N1L2 & S1_safe_q[3] # N1L5 # !N1L3 # !N1L2 & S1_safe_q[3] & N1L5;


--J1L01 is alarmclock:inst11|LessThan~290
--operation mode is normal

J1L01 = S32_safe_q[3] # S32_safe_q[2] & S32_safe_q[0] # S32_safe_q[1];


--J1L3 is alarmclock:inst11|Decoder~19
--operation mode is normal

J1L3 = J1_disp_drive[1] & !J1_disp_drive[2] & !J1_disp_drive[0];


--M1L01 is time_auto_and_set:inst1|timeset:b2v_inst3|LessThan~312
--operation mode is normal

M1L01 = S01_safe_q[3] # S01_safe_q[2] & S01_safe_q[0] # S01_safe_q[1];


--M1L3 is time_auto_and_set:inst1|timeset:b2v_inst3|Decoder~19
--operation mode is normal

M1L3 = M1_disp_drive[1] & !M1_disp_drive[2] & !M1_disp_drive[0];


--P1L3 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|LessThan~92
--operation mode is normal

P1L3 = S4_safe_q[3] # S4_safe_q[2] & S4_safe_q[0] # S4_safe_q[1];


--P1L4 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|minute_counter:b2v_inst1|minute_data1[0]~11
--operation mode is normal

P1L4 = D1_Timepiece_EN & P1L2;


--J1L7 is alarmclock:inst11|LessThan~132
--operation mode is normal

J1L7 = S42_safe_q[3] & S42_safe_q[1] # S42_safe_q[2] # S42_safe_q[0];


--J1L6 is alarmclock:inst11|Decoder~22
--operation mode is normal

J1L6 = J1_disp_drive[2] & J1_disp_drive[0] & !J1_disp_drive[1];


--M1L7 is time_auto_and_set:inst1|timeset:b2v_inst3|LessThan~128
--operation mode is normal

M1L7 = S11_safe_q[3] & S11_safe_q[1] # S11_safe_q[2] # S11_safe_q[0];


--M1L4 is time_auto_and_set:inst1|timeset:b2v_inst3|Decoder~22
--operation mode is normal

M1L4 = M1_disp_drive[2] & M1_disp_drive[0] & !M1_disp_drive[1];


--F1_f60hz is fdiv:inst5|f60hz
--operation mode is normal

F1_f60hz_lut_out = F1L5;
F1_f60hz = DFFEAS(F1_f60hz_lut_out, F1_f200hz, VCC, , , , , , );


--F1_f1hz is fdiv:inst5|f1hz
--operation mode is normal

F1_f1hz_lut_out = F1L1;
F1_f1hz = DFFEAS(F1_f1hz_lut_out, F1_f200hz, VCC, , , , , , );


--D1_Stopwatch_EN is maincontrol:inst3|Stopwatch_EN
--operation mode is normal

D1_Stopwatch_EN_lut_out = D1_Function[1] & !D1_Function[2] & !D1_Function[0];
D1_Stopwatch_EN = DFFEAS(D1_Stopwatch_EN_lut_out, SW3, VCC, , , , , , );


--C1L1 is stopwatch:inst2|F_out~8
--operation mode is normal

C1L1 = D1_Stopwatch_EN & F1_f60hz # !D1_Stopwatch_EN & F1_f1hz;


--Q1L2 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|LessThan~47
--operation mode is normal

Q1L2 = S5_safe_q[3] & S5_safe_q[1] # S5_safe_q[2] # S5_safe_q[0];


--J1L11 is alarmclock:inst11|LessThan~291
--operation mode is normal

J1L11 = S52_safe_q[3] # S52_safe_q[2] & S52_safe_q[0] # S52_safe_q[1];


--J1L5 is alarmclock:inst11|Decoder~21
--operation mode is normal

J1L5 = J1_disp_drive[2] & !J1_disp_drive[1] & !J1_disp_drive[0];


--M1L11 is time_auto_and_set:inst1|timeset:b2v_inst3|LessThan~313
--operation mode is normal

M1L11 = S21_safe_q[3] # S21_safe_q[2] & S21_safe_q[0] # S21_safe_q[1];


--M1L6 is time_auto_and_set:inst1|timeset:b2v_inst3|Decoder~96
--operation mode is normal

M1L6 = M1_disp_drive[2] & !M1_disp_drive[1] & !M1_disp_drive[0];


--Q1L3 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|LessThan~92
--operation mode is normal

Q1L3 = S6_safe_q[3] # S6_safe_q[2] & S6_safe_q[0] # S6_safe_q[1];


--Q1L4 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|second_counter:b2v_inst2|second_data1[0]~11
--operation mode is normal

Q1L4 = D1_Timepiece_EN & Q1L2;


--J1L1 is alarmclock:inst11|Decoder~17
--operation mode is normal

J1L1 = !J1_disp_drive[1] & !J1_disp_drive[2] & !J1_disp_drive[0];


--M1L21 is time_auto_and_set:inst1|timeset:b2v_inst3|LessThan~314
--operation mode is normal

M1L21 = S8_safe_q[2] # S8_safe_q[1] # S8_safe_q[3];


--M1L1 is time_auto_and_set:inst1|timeset:b2v_inst3|Decoder~17
--operation mode is normal

M1L1 = !M1_disp_drive[2] & !M1_disp_drive[1] & !M1_disp_drive[0];


--N1L4 is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|hour_data1[0]~11
--operation mode is normal

N1L4 = D1_Timepiece_EN & N1L6;


--D1_Alarmclock_EN is maincontrol:inst3|Alarmclock_EN
--operation mode is normal

D1_Alarmclock_EN_lut_out = D1_Function[1] & D1_Function[0] & !D1_Function[2];
D1_Alarmclock_EN = DFFEAS(D1_Alarmclock_EN_lut_out, SW3, VCC, , , , , , );


--J1_alarmclock_disp_select[5] is alarmclock:inst11|alarmclock_disp_select[5]
--operation mode is normal

J1_alarmclock_disp_select[5]_lut_out = J1L1;
J1_alarmclock_disp_select[5] = DFFEAS(J1_alarmclock_disp_select[5]_lut_out, F1_f200hz, VCC, , , , , , );


--J1_alarmclock_disp_select[4] is alarmclock:inst11|alarmclock_disp_select[4]
--operation mode is normal

J1_alarmclock_disp_select[4]_lut_out = J1L2;
J1_alarmclock_disp_select[4] = DFFEAS(J1_alarmclock_disp_select[4]_lut_out, F1_f200hz, VCC, , , , , , );


--H1L23 is disp_data_mux:inst8|Data~1512
--operation mode is normal

H1L23 = !J1_alarmclock_disp_select[5] & !J1_alarmclock_disp_select[4];


--H1L16 is disp_data_mux:inst8|always0~1
--operation mode is normal

H1L16 = D1_TimeSet_EN # D1_Timepiece_EN # D1_Stopwatch_EN;


--J1_alarmclock_disp_select[1] is alarmclock:inst11|alarmclock_disp_select[1]
--operation mode is normal

J1_alarmclock_disp_select[1]_lut_out = J1L5;
J1_alarmclock_disp_select[1] = DFFEAS(J1_alarmclock_disp_select[1]_lut_out, F1_f200hz, VCC, , , , , , );


--H1L33 is disp_data_mux:inst8|Data~1513
--operation mode is normal

H1L33 = D1_Alarmclock_EN & H1L23 & !H1L16 & !J1_alarmclock_disp_select[1];


--J1_alarmclock_disp_select[0] is alarmclock:inst11|alarmclock_disp_select[0]
--operation mode is normal

J1_alarmclock_disp_select[0]_lut_out = J1L6;
J1_alarmclock_disp_select[0] = DFFEAS(J1_alarmclock_disp_select[0]_lut_out, F1_f200hz, VCC, , , , , , );


--J1_alarmclock_disp_select[3] is alarmclock:inst11|alarmclock_disp_select[3]
--operation mode is normal

J1_alarmclock_disp_select[3]_lut_out = J1L3;
J1_alarmclock_disp_select[3] = DFFEAS(J1_alarmclock_disp_select[3]_lut_out, F1_f200hz, VCC, , , , , , );


--J1_alarmclock_disp_select[2] is alarmclock:inst11|alarmclock_disp_select[2]
--operation mode is normal

J1_alarmclock_disp_select[2]_lut_out = J1L4;
J1_alarmclock_disp_select[2] = DFFEAS(J1_alarmclock_disp_select[2]_lut_out, F1_f200hz, VCC, , , , , , );


--H1L43 is disp_data_mux:inst8|Data~1514
--operation mode is normal

H1L43 = H1L33 & J1_alarmclock_disp_select[0] & !J1_alarmclock_disp_select[3] & !J1_alarmclock_disp_select[2];


--G1_time_disp_select[5] is time_disp_select:inst6|time_disp_select[5]
--operation mode is normal

G1_time_disp_select[5]_lut_out = !G1_disp_drive[0] & !G1_disp_drive[2] & !G1_disp_drive[1];
G1_time_disp_select[5] = DFFEAS(G1_time_disp_select[5]_lut_out, G1_clk, VCC, , , , , , );


--G1_time_disp_select[3] is time_disp_select:inst6|time_disp_select[3]
--operation mode is normal

G1_time_disp_select[3]_lut_out = G1_disp_drive[1] & !G1_disp_drive[0] & !G1_disp_drive[2];
G1_time_disp_select[3] = DFFEAS(G1_time_disp_select[3]_lut_out, G1_clk, VCC, , , , , , );


--G1_time_disp_select[2] is time_disp_select:inst6|time_disp_select[2]
--operation mode is normal

G1_time_disp_select[2]_lut_out = G1_disp_drive[0] & G1_disp_drive[1] & !G1_disp_drive[2];
G1_time_disp_select[2] = DFFEAS(G1_time_disp_select[2]_lut_out, G1_clk, VCC, , , , , , );


--H1L53 is disp_data_mux:inst8|Data~1515
--operation mode is normal

H1L53 = H1L16 & !G1_time_disp_select[5] & !G1_time_disp_select[3] & !G1_time_disp_select[2];


--G1_time_disp_select[0] is time_disp_select:inst6|time_disp_select[0]
--operation mode is normal

G1_time_disp_select[0]_lut_out = G1_disp_drive[0] & G1_disp_drive[2] & !G1_disp_drive[1];
G1_time_disp_select[0] = DFFEAS(G1_time_disp_select[0]_lut_out, G1_clk, VCC, , , , , , );


--G1_time_disp_select[4] is time_disp_select:inst6|time_disp_select[4]
--operation mode is normal

G1_time_disp_select[4]_lut_out = G1_disp_drive[0] & !G1_disp_drive[2] & !G1_disp_drive[1];
G1_time_disp_select[4] = DFFEAS(G1_time_disp_select[4]_lut_out, G1_clk, VCC, , , , , , );


--H1L63 is disp_data_mux:inst8|Data~1516
--operation mode is normal

H1L63 = G1_time_disp_select[0] & !G1_time_disp_select[4];


--G1_time_disp_select[1] is time_disp_select:inst6|time_disp_select[1]
--operation mode is normal

G1_time_disp_select[1]_lut_out = G1_disp_drive[2] & !G1_disp_drive[0] & !G1_disp_drive[1];
G1_time_disp_select[1] = DFFEAS(G1_time_disp_select[1]_lut_out, G1_clk, VCC, , , , , , );


--H1L73 is disp_data_mux:inst8|Data~1517
--operation mode is normal

H1L73 = H1L43 # H1L53 & H1L63 & !G1_time_disp_select[1];


--H1L83 is disp_data_mux:inst8|Data~1518
--operation mode is normal

H1L83 = G1_time_disp_select[1] & H1L53 & !G1_time_disp_select[4] & !G1_time_disp_select[0];


--H1L93 is disp_data_mux:inst8|Data~1519
--operation mode is normal

H1L93 = D1_Alarmclock_EN & !H1L16 & !J1_alarmclock_disp_select[5] & !J1_alarmclock_disp_select[4];


--H1L04 is disp_data_mux:inst8|Data~1520
--operation mode is normal

H1L04 = !J1_alarmclock_disp_select[3] & !J1_alarmclock_disp_select[2] & !J1_alarmclock_disp_select[0];


--H1L14 is disp_data_mux:inst8|Data~1521
--operation mode is normal

H1L14 = H1L83 # J1_alarmclock_disp_select[1] & H1L93 & H1L04;


--H1L41 is disp_data_mux:inst8|Data~386
--operation mode is normal

H1L41 = H1L73 # H1L14;


--H1L24 is disp_data_mux:inst8|Data~1522
--operation mode is normal

H1L24 = H1L16 & !G1_time_disp_select[5] & !G1_time_disp_select[4] & !G1_time_disp_select[0];


--H1L34 is disp_data_mux:inst8|Data~1523
--operation mode is normal

H1L34 = G1_time_disp_select[2] & H1L24 & !G1_time_disp_select[1] & !G1_time_disp_select[3];


--H1L44 is disp_data_mux:inst8|Data~1524
--operation mode is normal

H1L44 = H1L33 & J1_alarmclock_disp_select[2] & !J1_alarmclock_disp_select[3] & !J1_alarmclock_disp_select[0];


--H1L54 is disp_data_mux:inst8|Data~1525
--operation mode is normal

H1L54 = H1L73 # !H1L14 & H1L34 # H1L44;


--U1_day0[0] is date_main:inst4|datecontrol:b2v_inst1|day0[0]
--operation mode is normal

U1_day0[0]_lut_out = D1_Date_EN & T1_EO1 & S31_safe_q[0] # !T1_EO1 & S61_safe_q[0] # !D1_Date_EN & S61_safe_q[0];
U1_day0[0] = DFFEAS(U1_day0[0]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--U1_disp_select[4] is date_main:inst4|datecontrol:b2v_inst1|disp_select[4]
--operation mode is normal

U1_disp_select[4]_lut_out = V1_disp_drive[0] & !V1_disp_drive[1] & !T1_EO1 # !D1_Date_EN;
U1_disp_select[4] = DFFEAS(U1_disp_select[4]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--U1_disp_select[2] is date_main:inst4|datecontrol:b2v_inst1|disp_select[2]
--operation mode is normal

U1_disp_select[2]_lut_out = D1_Date_EN & T1_EO1 # V1_disp_drive[1] & V1_disp_drive[0] # !D1_Date_EN & V1_disp_drive[1] & V1_disp_drive[0];
U1_disp_select[2] = DFFEAS(U1_disp_select[2]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--U1_disp_select[5] is date_main:inst4|datecontrol:b2v_inst1|disp_select[5]
--operation mode is normal

U1_disp_select[5]_lut_out = !V1_disp_drive[1] & !V1_disp_drive[0] & !T1_EO1 # !D1_Date_EN;
U1_disp_select[5] = DFFEAS(U1_disp_select[5]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--U1_disp_select[3] is date_main:inst4|datecontrol:b2v_inst1|disp_select[3]
--operation mode is normal

U1_disp_select[3]_lut_out = V1_disp_drive[1] & !V1_disp_drive[0] & !T1_EO1 # !D1_Date_EN;
U1_disp_select[3] = DFFEAS(U1_disp_select[3]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--H1L64 is disp_data_mux:inst8|Data~1526
--operation mode is normal

H1L64 = !U1_disp_select[5] & !U1_disp_select[3] & U1_disp_select[4] $ U1_disp_select[2];


--U1_month1[0] is date_main:inst4|datecontrol:b2v_inst1|month1[0]
--operation mode is normal

U1_month1[0]_lut_out = D1_Date_EN & T1_EO1 & T1_month1[0] # !T1_EO1 & S91_safe_q[0] # !D1_Date_EN & S91_safe_q[0];
U1_month1[0] = DFFEAS(U1_month1[0]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--H1L74 is disp_data_mux:inst8|Data~1527
--operation mode is normal

H1L74 = U1_disp_select[5] # U1_disp_select[4] # U1_disp_select[3] $ !U1_disp_select[2];


--U1_day1[0] is date_main:inst4|datecontrol:b2v_inst1|day1[0]
--operation mode is normal

U1_day1[0]_lut_out = D1_Date_EN & T1_EO1 & S41_safe_q[0] # !T1_EO1 & S71_safe_q[0] # !D1_Date_EN & S71_safe_q[0];
U1_day1[0] = DFFEAS(U1_day1[0]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--H1L61 is disp_data_mux:inst8|Data~403
--operation mode is normal

H1L61 = H1L64 & H1L74 # !H1L64 & H1L74 & U1_month1[0] # !H1L74 & U1_day1[0];


--U1_month0[0] is date_main:inst4|datecontrol:b2v_inst1|month0[0]
--operation mode is normal

U1_month0[0]_lut_out = D1_Date_EN & T1_EO1 & S51_safe_q[0] # !T1_EO1 & S81_safe_q[0] # !D1_Date_EN & S81_safe_q[0];
U1_month0[0] = DFFEAS(U1_month0[0]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--H1L71 is disp_data_mux:inst8|Data~404
--operation mode is normal

H1L71 = H1L64 & H1L61 & U1_month0[0] # !H1L61 & U1_day0[0] # !H1L64 & H1L61;


--H1L84 is disp_data_mux:inst8|Data~1528
--operation mode is normal

H1L84 = H1L16 & !G1_time_disp_select[4] & !G1_time_disp_select[0];


--H1L94 is disp_data_mux:inst8|Data~1529
--operation mode is normal

H1L94 = !G1_time_disp_select[1] & !G1_time_disp_select[2];


--H1L05 is disp_data_mux:inst8|Data~1530
--operation mode is normal

H1L05 = G1_time_disp_select[5] & H1L84 & H1L94 & !G1_time_disp_select[3];


--H1L15 is disp_data_mux:inst8|Data~1531
--operation mode is normal

H1L15 = D1_Alarmclock_EN & H1L04 & !H1L16 & !J1_alarmclock_disp_select[1];


--H1L25 is disp_data_mux:inst8|Data~1532
--operation mode is normal

H1L25 = H1L05 # J1_alarmclock_disp_select[5] & H1L15 & !J1_alarmclock_disp_select[4];


--H1L35 is disp_data_mux:inst8|Data~1533
--operation mode is normal

H1L35 = U1_disp_select[5] & !U1_disp_select[4] & !U1_disp_select[3] & !U1_disp_select[2] # !U1_disp_select[5] & U1_disp_select[4] & !U1_disp_select[3] & !U1_disp_select[2] # !U1_disp_select[4] & U1_disp_select[3] $ U1_disp_select[2];


--H1L45 is disp_data_mux:inst8|Data~1534
--operation mode is normal

H1L45 = H1L35 & !H1L16 & !D1_Alarmclock_EN;


--H1L55 is disp_data_mux:inst8|Data~1535
--operation mode is normal

H1L55 = J1_alarmclock_disp_select[3] & H1L33 & !J1_alarmclock_disp_select[2] & !J1_alarmclock_disp_select[0];


--H1L65 is disp_data_mux:inst8|Data~1536
--operation mode is normal

H1L65 = H1L55 # G1_time_disp_select[3] & H1L24 & H1L94;


--H1L75 is disp_data_mux:inst8|Data~1537
--operation mode is normal

H1L75 = H1L53 & G1_time_disp_select[4] & !G1_time_disp_select[1] & !G1_time_disp_select[0];


--H1L85 is disp_data_mux:inst8|Data~1538
--operation mode is normal

H1L85 = H1L75 # J1_alarmclock_disp_select[4] & H1L15 & !J1_alarmclock_disp_select[5];


--H1L95 is disp_data_mux:inst8|Data~1539
--operation mode is normal

H1L95 = !H1L65 & !H1L85 & H1L25 # H1L45;


--H1L51 is disp_data_mux:inst8|Data~390
--operation mode is normal

H1L51 = H1L65 # H1L85;


--H1L06 is disp_data_mux:inst8|Data~1540
--operation mode is normal

H1L06 = H1L65 # H1L25 & !H1L85;


--H1L21 is disp_data_mux:inst8|Data~7adv_mux_opt_ptn_431
--operation mode is normal

H1L21 = H1L51 & H1L06 & L1L31 # !H1L06 & L1L1 # !H1L51 & H1L06;


--H1L31 is disp_data_mux:inst8|Data~7adv_mux_opt_ptn_432
--operation mode is normal

H1L31 = H1L95 & H1L21 & L1L5 # !H1L21 & H1L71 # !H1L95 & H1L21;


--H1L81 is disp_data_mux:inst8|Data~405
--operation mode is normal

H1L81 = H1L41 & H1L54 # !H1L41 & H1L54 & L1L9 # !H1L54 & H1L31;


--H1L91 is disp_data_mux:inst8|Data~406
--operation mode is normal

H1L91 = H1L41 & H1L81 & L1L71 # !H1L81 & L1L12 # !H1L41 & H1L81;


--D1_DateSet_EN is maincontrol:inst3|DateSet_EN
--operation mode is normal

D1_DateSet_EN_lut_out = D1_Function[2] & D1_Function[0] & !D1_Function[1];
D1_DateSet_EN = DFFEAS(D1_DateSet_EN_lut_out, SW3, VCC, , , , , , );


--D1_Date_EN is maincontrol:inst3|Date_EN
--operation mode is normal

D1_Date_EN_lut_out = D1_Function[2] & !D1_Function[1] & !D1_Function[0];
D1_Date_EN = DFFEAS(D1_Date_EN_lut_out, SW3, VCC, , , , , , );


--H1L26 is disp_data_mux:inst8|always0~4
--operation mode is normal

H1L26 = H1L16 # D1_Alarmclock_EN # D1_DateSet_EN # D1_Date_EN;


--H1_Data[0] is disp_data_mux:inst8|Data[0]
--operation mode is normal

H1_Data[0] = H1L26 & H1L91 # !H1L26 & H1_Data[0];


--U1_month1[1] is date_main:inst4|datecontrol:b2v_inst1|month1[1]
--operation mode is normal

U1_month1[1]_lut_out = S91_safe_q[1] & !T1_EO1 # !D1_Date_EN;
U1_month1[1] = DFFEAS(U1_month1[1]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--U1_day0[1] is date_main:inst4|datecontrol:b2v_inst1|day0[1]
--operation mode is normal

U1_day0[1]_lut_out = D1_Date_EN & T1_EO1 & S31_safe_q[1] # !T1_EO1 & S61_safe_q[1] # !D1_Date_EN & S61_safe_q[1];
U1_day0[1] = DFFEAS(U1_day0[1]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--U1_day1[1] is date_main:inst4|datecontrol:b2v_inst1|day1[1]
--operation mode is normal

U1_day1[1]_lut_out = D1_Date_EN & T1_EO1 & S41_safe_q[1] # !T1_EO1 & S71_safe_q[1] # !D1_Date_EN & S71_safe_q[1];
U1_day1[1] = DFFEAS(U1_day1[1]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--H1L02 is disp_data_mux:inst8|Data~407
--operation mode is normal

H1L02 = H1L74 & H1L64 # !H1L74 & H1L64 & U1_day0[1] # !H1L64 & U1_day1[1];


--U1_month0[1] is date_main:inst4|datecontrol:b2v_inst1|month0[1]
--operation mode is normal

U1_month0[1]_lut_out = D1_Date_EN & T1_EO1 & S51_safe_q[1] # !T1_EO1 & S81_safe_q[1] # !D1_Date_EN & S81_safe_q[1];
U1_month0[1] = DFFEAS(U1_month0[1]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--H1L12 is disp_data_mux:inst8|Data~408
--operation mode is normal

H1L12 = H1L74 & H1L02 & U1_month0[1] # !H1L02 & U1_month1[1] # !H1L74 & H1L02;


--H1L01 is disp_data_mux:inst8|Data~6adv_mux_opt_ptn_435
--operation mode is normal

H1L01 = H1L51 & H1L06 & L1L41 # !H1L06 & L1L2 # !H1L51 & H1L06;


--H1L11 is disp_data_mux:inst8|Data~6adv_mux_opt_ptn_436
--operation mode is normal

H1L11 = H1L95 & H1L01 & L1L6 # !H1L01 & H1L12 # !H1L95 & H1L01;


--H1L22 is disp_data_mux:inst8|Data~409
--operation mode is normal

H1L22 = H1L54 & H1L41 # !H1L54 & H1L41 & L1L22 # !H1L41 & H1L11;


--H1L32 is disp_data_mux:inst8|Data~410
--operation mode is normal

H1L32 = H1L54 & H1L22 & L1L81 # !H1L22 & L1L01 # !H1L54 & H1L22;


--H1_Data[1] is disp_data_mux:inst8|Data[1]
--operation mode is normal

H1_Data[1] = H1L26 & H1L32 # !H1L26 & H1_Data[1];


--U1_day0[2] is date_main:inst4|datecontrol:b2v_inst1|day0[2]
--operation mode is normal

U1_day0[2]_lut_out = D1_Date_EN & T1_EO1 & S31_safe_q[2] # !T1_EO1 & S61_safe_q[2] # !D1_Date_EN & S61_safe_q[2];
U1_day0[2] = DFFEAS(U1_day0[2]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--U1_month1[2] is date_main:inst4|datecontrol:b2v_inst1|month1[2]
--operation mode is normal

U1_month1[2]_lut_out = S91_safe_q[2] & !T1_EO1 # !D1_Date_EN;
U1_month1[2] = DFFEAS(U1_month1[2]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--U1_day1[2] is date_main:inst4|datecontrol:b2v_inst1|day1[2]
--operation mode is normal

U1_day1[2]_lut_out = D1_Date_EN & T1_EO1 & S41_safe_q[2] # !T1_EO1 & S71_safe_q[2] # !D1_Date_EN & S71_safe_q[2];
U1_day1[2] = DFFEAS(U1_day1[2]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--H1L42 is disp_data_mux:inst8|Data~411
--operation mode is normal

H1L42 = H1L64 & H1L74 # !H1L64 & H1L74 & U1_month1[2] # !H1L74 & U1_day1[2];


--U1_month0[2] is date_main:inst4|datecontrol:b2v_inst1|month0[2]
--operation mode is normal

U1_month0[2]_lut_out = D1_Date_EN & T1_EO1 & S51_safe_q[2] # !T1_EO1 & S81_safe_q[2] # !D1_Date_EN & S81_safe_q[2];
U1_month0[2] = DFFEAS(U1_month0[2]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--H1L52 is disp_data_mux:inst8|Data~412
--operation mode is normal

H1L52 = H1L64 & H1L42 & U1_month0[2] # !H1L42 & U1_day0[2] # !H1L64 & H1L42;


--H1L8 is disp_data_mux:inst8|Data~5adv_mux_opt_ptn_439
--operation mode is normal

H1L8 = H1L51 & H1L06 & L1L51 # !H1L06 & L1L3 # !H1L51 & H1L06;


--H1L9 is disp_data_mux:inst8|Data~5adv_mux_opt_ptn_440
--operation mode is normal

H1L9 = H1L95 & H1L8 & L1L7 # !H1L8 & H1L52 # !H1L95 & H1L8;


--H1L62 is disp_data_mux:inst8|Data~413
--operation mode is normal

H1L62 = H1L41 & H1L54 # !H1L41 & H1L54 & L1L11 # !H1L54 & H1L9;


--H1L72 is disp_data_mux:inst8|Data~414
--operation mode is normal

H1L72 = H1L41 & H1L62 & L1L91 # !H1L62 & L1L32 # !H1L41 & H1L62;


--H1_Data[2] is disp_data_mux:inst8|Data[2]
--operation mode is normal

H1_Data[2] = H1L26 & H1L72 # !H1L26 & H1_Data[2];


--U1_month1[3] is date_main:inst4|datecontrol:b2v_inst1|month1[3]
--operation mode is normal

U1_month1[3]_lut_out = S91_safe_q[3] & !T1_EO1 # !D1_Date_EN;
U1_month1[3] = DFFEAS(U1_month1[3]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--U1_day0[3] is date_main:inst4|datecontrol:b2v_inst1|day0[3]
--operation mode is normal

U1_day0[3]_lut_out = D1_Date_EN & T1_EO1 & S31_safe_q[3] # !T1_EO1 & S61_safe_q[3] # !D1_Date_EN & S61_safe_q[3];
U1_day0[3] = DFFEAS(U1_day0[3]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--U1_day1[3] is date_main:inst4|datecontrol:b2v_inst1|day1[3]
--operation mode is normal

U1_day1[3]_lut_out = D1_Date_EN & T1_EO1 & S41_safe_q[3] # !T1_EO1 & S71_safe_q[3] # !D1_Date_EN & S71_safe_q[3];
U1_day1[3] = DFFEAS(U1_day1[3]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--H1L82 is disp_data_mux:inst8|Data~415
--operation mode is normal

H1L82 = H1L74 & H1L64 # !H1L74 & H1L64 & U1_day0[3] # !H1L64 & U1_day1[3];


--U1_month0[3] is date_main:inst4|datecontrol:b2v_inst1|month0[3]
--operation mode is normal

U1_month0[3]_lut_out = D1_Date_EN & T1_EO1 & S51_safe_q[3] # !T1_EO1 & S81_safe_q[3] # !D1_Date_EN & S81_safe_q[3];
U1_month0[3] = DFFEAS(U1_month0[3]_lut_out, F1_f200hz, VCC, , U1L81, , , , );


--H1L92 is disp_data_mux:inst8|Data~416
--operation mode is normal

H1L92 = H1L74 & H1L82 & U1_month0[3] # !H1L82 & U1_month1[3] # !H1L74 & H1L82;


--H1L6 is disp_data_mux:inst8|Data~4adv_mux_opt_ptn_443
--operation mode is normal

H1L6 = H1L51 & H1L06 & L1L61 # !H1L06 & L1L4 # !H1L51 & H1L06;


--H1L7 is disp_data_mux:inst8|Data~4adv_mux_opt_ptn_444
--operation mode is normal

H1L7 = H1L95 & H1L6 & L1L8 # !H1L6 & H1L92 # !H1L95 & H1L6;


--H1L03 is disp_data_mux:inst8|Data~417
--operation mode is normal

H1L03 = H1L54 & H1L41 # !H1L54 & H1L41 & L1L42 # !H1L41 & H1L7;


--H1L13 is disp_data_mux:inst8|Data~418
--operation mode is normal

H1L13 = H1L54 & H1L03 & L1L02 # !H1L03 & L1L21 # !H1L54 & H1L03;


--H1_Data[3] is disp_data_mux:inst8|Data[3]
--operation mode is normal

H1_Data[3] = H1L26 & H1L13 # !H1L26 & H1_Data[3];


--H1L47 is disp_data_mux:inst8|disp_select~588
--operation mode is normal

H1L47 = G1_time_disp_select[5] & D1_TimeSet_EN # D1_Timepiece_EN # D1_Stopwatch_EN;


--H1L57 is disp_data_mux:inst8|disp_select~589
--operation mode is normal

H1L57 = !H1L16 & D1_Alarmclock_EN & J1_alarmclock_disp_select[5] # !D1_Alarmclock_EN & U1_disp_select[5];


--H1_disp_select[5] is disp_data_mux:inst8|disp_select[5]
--operation mode is normal

H1_disp_select[5] = H1L26 & H1L47 # H1L57 # !H1L26 & H1_disp_select[5];


--H1L67 is disp_data_mux:inst8|disp_select~590
--operation mode is normal

H1L67 = G1_time_disp_select[4] & D1_TimeSet_EN # D1_Timepiece_EN # D1_Stopwatch_EN;


--H1L77 is disp_data_mux:inst8|disp_select~591
--operation mode is normal

H1L77 = !H1L16 & D1_Alarmclock_EN & J1_alarmclock_disp_select[4] # !D1_Alarmclock_EN & U1_disp_select[4];


--H1_disp_select[4] is disp_data_mux:inst8|disp_select[4]
--operation mode is normal

H1_disp_select[4] = H1L26 & H1L67 # H1L77 # !H1L26 & H1_disp_select[4];


--H1L87 is disp_data_mux:inst8|disp_select~592
--operation mode is normal

H1L87 = G1_time_disp_select[3] & D1_TimeSet_EN # D1_Timepiece_EN # D1_Stopwatch_EN;


--H1L97 is disp_data_mux:inst8|disp_select~593
--operation mode is normal

H1L97 = !H1L16 & D1_Alarmclock_EN & J1_alarmclock_disp_select[3] # !D1_Alarmclock_EN & U1_disp_select[3];


--H1_disp_select[3] is disp_data_mux:inst8|disp_select[3]
--operation mode is normal

H1_disp_select[3] = H1L26 & H1L87 # H1L97 # !H1L26 & H1_disp_select[3];


--H1L08 is disp_data_mux:inst8|disp_select~594
--operation mode is normal

H1L08 = G1_time_disp_select[2] & D1_TimeSet_EN # D1_Timepiece_EN # D1_Stopwatch_EN;


--H1L18 is disp_data_mux:inst8|disp_select~595
--operation mode is normal

H1L18 = !H1L16 & D1_Alarmclock_EN & J1_alarmclock_disp_select[2] # !D1_Alarmclock_EN & U1_disp_select[2];


--H1_disp_select[2] is disp_data_mux:inst8|disp_select[2]
--operation mode is normal

H1_disp_select[2] = H1L26 & H1L08 # H1L18 # !H1L26 & H1_disp_select[2];


--H1L28 is disp_data_mux:inst8|disp_select~596
--operation mode is normal

H1L28 = J1_alarmclock_disp_select[1] & D1_Alarmclock_EN & !H1L16;


--H1L38 is disp_data_mux:inst8|disp_select~597
--operation mode is normal

H1L38 = G1_time_disp_select[1] & D1_TimeSet_EN # D1_Timepiece_EN # D1_Stopwatch_EN;


--H1_disp_select[1] is disp_data_mux:inst8|disp_select[1]
--operation mode is normal

H1_disp_select[1] = H1L26 & H1L28 # H1L38 # !H1L26 & H1_disp_select[1];


--H1L48 is disp_data_mux:inst8|disp_select~598
--operation mode is normal

H1L48 = D1_Alarmclock_EN & J1_alarmclock_disp_select[0] & !H1L16;


--H1L58 is disp_data_mux:inst8|disp_select~599
--operation mode is normal

H1L58 = G1_time_disp_select[0] & D1_TimeSet_EN # D1_Timepiece_EN # D1_Stopwatch_EN;


--H1_disp_select[0] is disp_data_mux:inst8|disp_select[0]
--operation mode is normal

H1_disp_select[0] = H1L26 & H1L48 # H1L58 # !H1L26 & H1_disp_select[0];


--W2_safe_q[31] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[31]
--operation mode is normal

W2_safe_q[31]_carry_eqn = W2L26;
W2_safe_q[31]_lut_out = W2_safe_q[31] $ (W2_safe_q[31]_carry_eqn);
W2_safe_q[31] = DFFEAS(W2_safe_q[31]_lut_out, F1_f200hz, VCC, , , , , F1L5, );


--W2_safe_q[1] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[1]
--operation mode is arithmetic

W2_safe_q[1]_carry_eqn = W2L2;
W2_safe_q[1]_lut_out = W2_safe_q[1] $ (W2_safe_q[1]_carry_eqn);
W2_safe_q[1] = DFFEAS(W2_safe_q[1]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L4 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

W2L4 = CARRY(!W2L2 # !W2_safe_q[1]);


--W2_safe_q[2] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[2]
--operation mode is arithmetic

W2_safe_q[2]_carry_eqn = W2L4;
W2_safe_q[2]_lut_out = W2_safe_q[2] $ (!W2_safe_q[2]_carry_eqn);
W2_safe_q[2] = DFFEAS(W2_safe_q[2]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L6 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

W2L6 = CARRY(W2_safe_q[2] & !W2L4);


--W2_safe_q[3] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[3]
--operation mode is arithmetic

W2_safe_q[3]_carry_eqn = W2L6;
W2_safe_q[3]_lut_out = W2_safe_q[3] $ (W2_safe_q[3]_carry_eqn);
W2_safe_q[3] = DFFEAS(W2_safe_q[3]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L8 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella3~COUT
--operation mode is arithmetic

W2L8 = CARRY(!W2L6 # !W2_safe_q[3]);


--W2_safe_q[4] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[4]
--operation mode is arithmetic

W2_safe_q[4]_carry_eqn = W2L8;
W2_safe_q[4]_lut_out = W2_safe_q[4] $ (!W2_safe_q[4]_carry_eqn);
W2_safe_q[4] = DFFEAS(W2_safe_q[4]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L01 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella4~COUT
--operation mode is arithmetic

W2L01 = CARRY(W2_safe_q[4] & !W2L8);


--W2L69 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]~441
--operation mode is normal

W2L69 = !W2_safe_q[1] & !W2_safe_q[2] & !W2_safe_q[3] & !W2_safe_q[4];


--W2_safe_q[5] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[5]
--operation mode is arithmetic

W2_safe_q[5]_carry_eqn = W2L01;
W2_safe_q[5]_lut_out = W2_safe_q[5] $ (W2_safe_q[5]_carry_eqn);
W2_safe_q[5] = DFFEAS(W2_safe_q[5]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L21 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella5~COUT
--operation mode is arithmetic

W2L21 = CARRY(!W2L01 # !W2_safe_q[5]);


--W2_safe_q[6] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[6]
--operation mode is arithmetic

W2_safe_q[6]_carry_eqn = W2L21;
W2_safe_q[6]_lut_out = W2_safe_q[6] $ (!W2_safe_q[6]_carry_eqn);
W2_safe_q[6] = DFFEAS(W2_safe_q[6]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L41 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella6~COUT
--operation mode is arithmetic

W2L41 = CARRY(W2_safe_q[6] & !W2L21);


--W2_safe_q[7] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[7]
--operation mode is arithmetic

W2_safe_q[7]_carry_eqn = W2L41;
W2_safe_q[7]_lut_out = W2_safe_q[7] $ (W2_safe_q[7]_carry_eqn);
W2_safe_q[7] = DFFEAS(W2_safe_q[7]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L61 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella7~COUT
--operation mode is arithmetic

W2L61 = CARRY(!W2L41 # !W2_safe_q[7]);


--W2_safe_q[8] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[8]
--operation mode is arithmetic

W2_safe_q[8]_carry_eqn = W2L61;
W2_safe_q[8]_lut_out = W2_safe_q[8] $ (!W2_safe_q[8]_carry_eqn);
W2_safe_q[8] = DFFEAS(W2_safe_q[8]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L81 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella8~COUT
--operation mode is arithmetic

W2L81 = CARRY(W2_safe_q[8] & !W2L61);


--W2L79 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]~442
--operation mode is normal

W2L79 = !W2_safe_q[5] & !W2_safe_q[6] & !W2_safe_q[7] & !W2_safe_q[8];


--W2_safe_q[9] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[9]
--operation mode is arithmetic

W2_safe_q[9]_carry_eqn = W2L81;
W2_safe_q[9]_lut_out = W2_safe_q[9] $ (W2_safe_q[9]_carry_eqn);
W2_safe_q[9] = DFFEAS(W2_safe_q[9]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L02 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella9~COUT
--operation mode is arithmetic

W2L02 = CARRY(!W2L81 # !W2_safe_q[9]);


--W2_safe_q[10] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[10]
--operation mode is arithmetic

W2_safe_q[10]_carry_eqn = W2L02;
W2_safe_q[10]_lut_out = W2_safe_q[10] $ (!W2_safe_q[10]_carry_eqn);
W2_safe_q[10] = DFFEAS(W2_safe_q[10]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L22 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella10~COUT
--operation mode is arithmetic

W2L22 = CARRY(W2_safe_q[10] & !W2L02);


--W2_safe_q[11] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[11]
--operation mode is arithmetic

W2_safe_q[11]_carry_eqn = W2L22;
W2_safe_q[11]_lut_out = W2_safe_q[11] $ (W2_safe_q[11]_carry_eqn);
W2_safe_q[11] = DFFEAS(W2_safe_q[11]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L42 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella11~COUT
--operation mode is arithmetic

W2L42 = CARRY(!W2L22 # !W2_safe_q[11]);


--W2_safe_q[12] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[12]
--operation mode is arithmetic

W2_safe_q[12]_carry_eqn = W2L42;
W2_safe_q[12]_lut_out = W2_safe_q[12] $ (!W2_safe_q[12]_carry_eqn);
W2_safe_q[12] = DFFEAS(W2_safe_q[12]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L62 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella12~COUT
--operation mode is arithmetic

W2L62 = CARRY(W2_safe_q[12] & !W2L42);


--W2L89 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]~443
--operation mode is normal

W2L89 = !W2_safe_q[9] & !W2_safe_q[10] & !W2_safe_q[11] & !W2_safe_q[12];


--W2_safe_q[13] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[13]
--operation mode is arithmetic

W2_safe_q[13]_carry_eqn = W2L62;
W2_safe_q[13]_lut_out = W2_safe_q[13] $ (W2_safe_q[13]_carry_eqn);
W2_safe_q[13] = DFFEAS(W2_safe_q[13]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L82 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella13~COUT
--operation mode is arithmetic

W2L82 = CARRY(!W2L62 # !W2_safe_q[13]);


--W2_safe_q[14] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[14]
--operation mode is arithmetic

W2_safe_q[14]_carry_eqn = W2L82;
W2_safe_q[14]_lut_out = W2_safe_q[14] $ (!W2_safe_q[14]_carry_eqn);
W2_safe_q[14] = DFFEAS(W2_safe_q[14]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L03 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella14~COUT
--operation mode is arithmetic

W2L03 = CARRY(W2_safe_q[14] & !W2L82);


--W2_safe_q[15] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[15]
--operation mode is arithmetic

W2_safe_q[15]_carry_eqn = W2L03;
W2_safe_q[15]_lut_out = W2_safe_q[15] $ (W2_safe_q[15]_carry_eqn);
W2_safe_q[15] = DFFEAS(W2_safe_q[15]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L23 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella15~COUT
--operation mode is arithmetic

W2L23 = CARRY(!W2L03 # !W2_safe_q[15]);


--W2_safe_q[16] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[16]
--operation mode is arithmetic

W2_safe_q[16]_carry_eqn = W2L23;
W2_safe_q[16]_lut_out = W2_safe_q[16] $ (!W2_safe_q[16]_carry_eqn);
W2_safe_q[16] = DFFEAS(W2_safe_q[16]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L43 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella16~COUT
--operation mode is arithmetic

W2L43 = CARRY(W2_safe_q[16] & !W2L23);


--W2L99 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]~444
--operation mode is normal

W2L99 = !W2_safe_q[13] & !W2_safe_q[14] & !W2_safe_q[15] & !W2_safe_q[16];


--W2L001 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]~445
--operation mode is normal

W2L001 = W2L69 & W2L79 & W2L89 & W2L99;


--W2_safe_q[18] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[18]
--operation mode is arithmetic

W2_safe_q[18]_carry_eqn = W2L63;
W2_safe_q[18]_lut_out = W2_safe_q[18] $ (!W2_safe_q[18]_carry_eqn);
W2_safe_q[18] = DFFEAS(W2_safe_q[18]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L83 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella18~COUT
--operation mode is arithmetic

W2L83 = CARRY(W2_safe_q[18] & !W2L63);


--W2_safe_q[19] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[19]
--operation mode is arithmetic

W2_safe_q[19]_carry_eqn = W2L83;
W2_safe_q[19]_lut_out = W2_safe_q[19] $ (W2_safe_q[19]_carry_eqn);
W2_safe_q[19] = DFFEAS(W2_safe_q[19]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L04 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella19~COUT
--operation mode is arithmetic

W2L04 = CARRY(!W2L83 # !W2_safe_q[19]);


--W2_safe_q[29] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[29]
--operation mode is arithmetic

W2_safe_q[29]_carry_eqn = W2L85;
W2_safe_q[29]_lut_out = W2_safe_q[29] $ (W2_safe_q[29]_carry_eqn);
W2_safe_q[29] = DFFEAS(W2_safe_q[29]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L06 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella29~COUT
--operation mode is arithmetic

W2L06 = CARRY(!W2L85 # !W2_safe_q[29]);


--W2_safe_q[30] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]
--operation mode is arithmetic

W2_safe_q[30]_carry_eqn = W2L06;
W2_safe_q[30]_lut_out = W2_safe_q[30] $ (!W2_safe_q[30]_carry_eqn);
W2_safe_q[30] = DFFEAS(W2_safe_q[30]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L26 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella30~COUT
--operation mode is arithmetic

W2L26 = CARRY(W2_safe_q[30] & !W2L06);


--F1L3 is fdiv:inst5|LessThan~1040
--operation mode is normal

F1L3 = W2_safe_q[18] # W2_safe_q[19] # W2_safe_q[29] # W2_safe_q[30];


--W2_safe_q[17] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[17]
--operation mode is arithmetic

W2_safe_q[17]_carry_eqn = W2L43;
W2_safe_q[17]_lut_out = W2_safe_q[17] $ (W2_safe_q[17]_carry_eqn);
W2_safe_q[17] = DFFEAS(W2_safe_q[17]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L63 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella17~COUT
--operation mode is arithmetic

W2L63 = CARRY(!W2L43 # !W2_safe_q[17]);


--W2_safe_q[21] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[21]
--operation mode is arithmetic

W2_safe_q[21]_carry_eqn = W2L24;
W2_safe_q[21]_lut_out = W2_safe_q[21] $ (W2_safe_q[21]_carry_eqn);
W2_safe_q[21] = DFFEAS(W2_safe_q[21]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L44 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella21~COUT
--operation mode is arithmetic

W2L44 = CARRY(!W2L24 # !W2_safe_q[21]);


--W2_safe_q[22] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[22]
--operation mode is arithmetic

W2_safe_q[22]_carry_eqn = W2L44;
W2_safe_q[22]_lut_out = W2_safe_q[22] $ (!W2_safe_q[22]_carry_eqn);
W2_safe_q[22] = DFFEAS(W2_safe_q[22]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L64 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella22~COUT
--operation mode is arithmetic

W2L64 = CARRY(W2_safe_q[22] & !W2L44);


--W2_safe_q[23] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[23]
--operation mode is arithmetic

W2_safe_q[23]_carry_eqn = W2L64;
W2_safe_q[23]_lut_out = W2_safe_q[23] $ (W2_safe_q[23]_carry_eqn);
W2_safe_q[23] = DFFEAS(W2_safe_q[23]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L84 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella23~COUT
--operation mode is arithmetic

W2L84 = CARRY(!W2L64 # !W2_safe_q[23]);


--W2_safe_q[24] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[24]
--operation mode is arithmetic

W2_safe_q[24]_carry_eqn = W2L84;
W2_safe_q[24]_lut_out = W2_safe_q[24] $ (!W2_safe_q[24]_carry_eqn);
W2_safe_q[24] = DFFEAS(W2_safe_q[24]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L05 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella24~COUT
--operation mode is arithmetic

W2L05 = CARRY(W2_safe_q[24] & !W2L84);


--W2L101 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]~446
--operation mode is normal

W2L101 = !W2_safe_q[21] & !W2_safe_q[22] & !W2_safe_q[23] & !W2_safe_q[24];


--W2_safe_q[20] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[20]
--operation mode is arithmetic

W2_safe_q[20]_carry_eqn = W2L04;
W2_safe_q[20]_lut_out = W2_safe_q[20] $ (!W2_safe_q[20]_carry_eqn);
W2_safe_q[20] = DFFEAS(W2_safe_q[20]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L24 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella20~COUT
--operation mode is arithmetic

W2L24 = CARRY(W2_safe_q[20] & !W2L04);


--W2_safe_q[25] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[25]
--operation mode is arithmetic

W2_safe_q[25]_carry_eqn = W2L05;
W2_safe_q[25]_lut_out = W2_safe_q[25] $ (W2_safe_q[25]_carry_eqn);
W2_safe_q[25] = DFFEAS(W2_safe_q[25]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L25 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella25~COUT
--operation mode is arithmetic

W2L25 = CARRY(!W2L05 # !W2_safe_q[25]);


--W2_safe_q[26] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[26]
--operation mode is arithmetic

W2_safe_q[26]_carry_eqn = W2L25;
W2_safe_q[26]_lut_out = W2_safe_q[26] $ (!W2_safe_q[26]_carry_eqn);
W2_safe_q[26] = DFFEAS(W2_safe_q[26]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L45 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella26~COUT
--operation mode is arithmetic

W2L45 = CARRY(W2_safe_q[26] & !W2L25);


--W2_safe_q[27] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[27]
--operation mode is arithmetic

W2_safe_q[27]_carry_eqn = W2L45;
W2_safe_q[27]_lut_out = W2_safe_q[27] $ (W2_safe_q[27]_carry_eqn);
W2_safe_q[27] = DFFEAS(W2_safe_q[27]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L65 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella27~COUT
--operation mode is arithmetic

W2L65 = CARRY(!W2L45 # !W2_safe_q[27]);


--W2_safe_q[28] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[28]
--operation mode is arithmetic

W2_safe_q[28]_carry_eqn = W2L65;
W2_safe_q[28]_lut_out = W2_safe_q[28] $ (!W2_safe_q[28]_carry_eqn);
W2_safe_q[28] = DFFEAS(W2_safe_q[28]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L85 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella28~COUT
--operation mode is arithmetic

W2L85 = CARRY(W2_safe_q[28] & !W2L65);


--W2L201 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[30]~447
--operation mode is normal

W2L201 = !W2_safe_q[25] & !W2_safe_q[26] & !W2_safe_q[27] & !W2_safe_q[28];


--F1L4 is fdiv:inst5|LessThan~1046
--operation mode is normal

F1L4 = !W2_safe_q[17] & W2L101 & !W2_safe_q[20] & W2L201;


--F1L5 is fdiv:inst5|LessThan~1047
--operation mode is normal

F1L5 = !W2_safe_q[31] & F1L3 # !F1L4 # !W2L001;


--F1_f200hz is fdiv:inst5|f200hz
--operation mode is normal

F1_f200hz_lut_out = F1L2;
F1_f200hz = DFFEAS(F1_f200hz_lut_out, Clock, VCC, , , , , , );


--W3_safe_q[31] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[31]
--operation mode is normal

W3_safe_q[31]_carry_eqn = W3L26;
W3_safe_q[31]_lut_out = W3_safe_q[31] $ (W3_safe_q[31]_carry_eqn);
W3_safe_q[31] = DFFEAS(W3_safe_q[31]_lut_out, F1_f200hz, VCC, , , , , F1L1, );


--W3_safe_q[8] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[8]
--operation mode is arithmetic

W3_safe_q[8]_carry_eqn = W3L61;
W3_safe_q[8]_lut_out = W3_safe_q[8] $ (!W3_safe_q[8]_carry_eqn);
W3_safe_q[8] = DFFEAS(W3_safe_q[8]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L81 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella8~COUT
--operation mode is arithmetic

W3L81 = CARRY(W3_safe_q[8] & !W3L61);


--W3_safe_q[9] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[9]
--operation mode is arithmetic

W3_safe_q[9]_carry_eqn = W3L81;
W3_safe_q[9]_lut_out = W3_safe_q[9] $ (W3_safe_q[9]_carry_eqn);
W3_safe_q[9] = DFFEAS(W3_safe_q[9]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L02 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella9~COUT
--operation mode is arithmetic

W3L02 = CARRY(!W3L81 # !W3_safe_q[9]);


--W3_safe_q[10] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[10]
--operation mode is arithmetic

W3_safe_q[10]_carry_eqn = W3L02;
W3_safe_q[10]_lut_out = W3_safe_q[10] $ (!W3_safe_q[10]_carry_eqn);
W3_safe_q[10] = DFFEAS(W3_safe_q[10]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L22 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella10~COUT
--operation mode is arithmetic

W3L22 = CARRY(W3_safe_q[10] & !W3L02);


--W3_safe_q[11] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[11]
--operation mode is arithmetic

W3_safe_q[11]_carry_eqn = W3L22;
W3_safe_q[11]_lut_out = W3_safe_q[11] $ (W3_safe_q[11]_carry_eqn);
W3_safe_q[11] = DFFEAS(W3_safe_q[11]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L42 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella11~COUT
--operation mode is arithmetic

W3L42 = CARRY(!W3L22 # !W3_safe_q[11]);


--F1L6 is fdiv:inst5|LessThan~1048
--operation mode is normal

F1L6 = !W3_safe_q[8] & !W3_safe_q[9] & !W3_safe_q[10] & !W3_safe_q[11];


--W3_safe_q[0] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[0]
--operation mode is arithmetic

W3_safe_q[0]_lut_out = !W3_safe_q[0];
W3_safe_q[0] = DFFEAS(W3_safe_q[0]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L2 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

W3L2 = CARRY(W3_safe_q[0]);


--W3_safe_q[1] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[1]
--operation mode is arithmetic

W3_safe_q[1]_carry_eqn = W3L2;
W3_safe_q[1]_lut_out = W3_safe_q[1] $ (W3_safe_q[1]_carry_eqn);
W3_safe_q[1] = DFFEAS(W3_safe_q[1]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L4 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

W3L4 = CARRY(!W3L2 # !W3_safe_q[1]);


--W3_safe_q[2] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[2]
--operation mode is arithmetic

W3_safe_q[2]_carry_eqn = W3L4;
W3_safe_q[2]_lut_out = W3_safe_q[2] $ (!W3_safe_q[2]_carry_eqn);
W3_safe_q[2] = DFFEAS(W3_safe_q[2]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L6 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

W3L6 = CARRY(W3_safe_q[2] & !W3L4);


--F1L7 is fdiv:inst5|LessThan~1049
--operation mode is normal

F1L7 = !W3_safe_q[2] # !W3_safe_q[1] # !W3_safe_q[0];


--W3_safe_q[3] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[3]
--operation mode is arithmetic

W3_safe_q[3]_carry_eqn = W3L6;
W3_safe_q[3]_lut_out = W3_safe_q[3] $ (W3_safe_q[3]_carry_eqn);
W3_safe_q[3] = DFFEAS(W3_safe_q[3]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L8 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella3~COUT
--operation mode is arithmetic

W3L8 = CARRY(!W3L6 # !W3_safe_q[3]);


--W3_safe_q[4] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[4]
--operation mode is arithmetic

W3_safe_q[4]_carry_eqn = W3L8;
W3_safe_q[4]_lut_out = W3_safe_q[4] $ (!W3_safe_q[4]_carry_eqn);
W3_safe_q[4] = DFFEAS(W3_safe_q[4]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L01 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella4~COUT
--operation mode is arithmetic

W3L01 = CARRY(W3_safe_q[4] & !W3L8);


--W3_safe_q[5] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[5]
--operation mode is arithmetic

W3_safe_q[5]_carry_eqn = W3L01;
W3_safe_q[5]_lut_out = W3_safe_q[5] $ (W3_safe_q[5]_carry_eqn);
W3_safe_q[5] = DFFEAS(W3_safe_q[5]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L21 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella5~COUT
--operation mode is arithmetic

W3L21 = CARRY(!W3L01 # !W3_safe_q[5]);


--F1L8 is fdiv:inst5|LessThan~1050
--operation mode is normal

F1L8 = F1L7 & !W3_safe_q[3] & !W3_safe_q[4] & !W3_safe_q[5];


--W3_safe_q[6] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[6]
--operation mode is arithmetic

W3_safe_q[6]_carry_eqn = W3L21;
W3_safe_q[6]_lut_out = W3_safe_q[6] $ (!W3_safe_q[6]_carry_eqn);
W3_safe_q[6] = DFFEAS(W3_safe_q[6]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L41 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella6~COUT
--operation mode is arithmetic

W3L41 = CARRY(W3_safe_q[6] & !W3L21);


--W3_safe_q[7] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[7]
--operation mode is arithmetic

W3_safe_q[7]_carry_eqn = W3L41;
W3_safe_q[7]_lut_out = W3_safe_q[7] $ (W3_safe_q[7]_carry_eqn);
W3_safe_q[7] = DFFEAS(W3_safe_q[7]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L61 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella7~COUT
--operation mode is arithmetic

W3L61 = CARRY(!W3L41 # !W3_safe_q[7]);


--F1L9 is fdiv:inst5|LessThan~1051
--operation mode is normal

F1L9 = F1L6 & F1L8 # !W3_safe_q[7] # !W3_safe_q[6];


--W3_safe_q[12] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[12]
--operation mode is arithmetic

W3_safe_q[12]_carry_eqn = W3L42;
W3_safe_q[12]_lut_out = W3_safe_q[12] $ (!W3_safe_q[12]_carry_eqn);
W3_safe_q[12] = DFFEAS(W3_safe_q[12]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L62 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella12~COUT
--operation mode is arithmetic

W3L62 = CARRY(W3_safe_q[12] & !W3L42);


--W3_safe_q[13] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[13]
--operation mode is arithmetic

W3_safe_q[13]_carry_eqn = W3L62;
W3_safe_q[13]_lut_out = W3_safe_q[13] $ (W3_safe_q[13]_carry_eqn);
W3_safe_q[13] = DFFEAS(W3_safe_q[13]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L82 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella13~COUT
--operation mode is arithmetic

W3L82 = CARRY(!W3L62 # !W3_safe_q[13]);


--W3_safe_q[14] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[14]
--operation mode is arithmetic

W3_safe_q[14]_carry_eqn = W3L82;
W3_safe_q[14]_lut_out = W3_safe_q[14] $ (!W3_safe_q[14]_carry_eqn);
W3_safe_q[14] = DFFEAS(W3_safe_q[14]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L03 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella14~COUT
--operation mode is arithmetic

W3L03 = CARRY(W3_safe_q[14] & !W3L82);


--W3_safe_q[15] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[15]
--operation mode is arithmetic

W3_safe_q[15]_carry_eqn = W3L03;
W3_safe_q[15]_lut_out = W3_safe_q[15] $ (W3_safe_q[15]_carry_eqn);
W3_safe_q[15] = DFFEAS(W3_safe_q[15]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L23 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella15~COUT
--operation mode is arithmetic

W3L23 = CARRY(!W3L03 # !W3_safe_q[15]);


--F1L01 is fdiv:inst5|LessThan~1052
--operation mode is normal

F1L01 = !W3_safe_q[12] & !W3_safe_q[13] & !W3_safe_q[14] & !W3_safe_q[15];


--W3_safe_q[16] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[16]
--operation mode is arithmetic

W3_safe_q[16]_carry_eqn = W3L23;
W3_safe_q[16]_lut_out = W3_safe_q[16] $ (!W3_safe_q[16]_carry_eqn);
W3_safe_q[16] = DFFEAS(W3_safe_q[16]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L43 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella16~COUT
--operation mode is arithmetic

W3L43 = CARRY(W3_safe_q[16] & !W3L23);


--W3_safe_q[17] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[17]
--operation mode is arithmetic

W3_safe_q[17]_carry_eqn = W3L43;
W3_safe_q[17]_lut_out = W3_safe_q[17] $ (W3_safe_q[17]_carry_eqn);
W3_safe_q[17] = DFFEAS(W3_safe_q[17]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L63 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella17~COUT
--operation mode is arithmetic

W3L63 = CARRY(!W3L43 # !W3_safe_q[17]);


--W3_safe_q[18] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[18]
--operation mode is arithmetic

W3_safe_q[18]_carry_eqn = W3L63;
W3_safe_q[18]_lut_out = W3_safe_q[18] $ (!W3_safe_q[18]_carry_eqn);
W3_safe_q[18] = DFFEAS(W3_safe_q[18]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L83 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella18~COUT
--operation mode is arithmetic

W3L83 = CARRY(W3_safe_q[18] & !W3L63);


--W3_safe_q[19] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[19]
--operation mode is arithmetic

W3_safe_q[19]_carry_eqn = W3L83;
W3_safe_q[19]_lut_out = W3_safe_q[19] $ (W3_safe_q[19]_carry_eqn);
W3_safe_q[19] = DFFEAS(W3_safe_q[19]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L04 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella19~COUT
--operation mode is arithmetic

W3L04 = CARRY(!W3L83 # !W3_safe_q[19]);


--F1L11 is fdiv:inst5|LessThan~1053
--operation mode is normal

F1L11 = !W3_safe_q[16] & !W3_safe_q[17] & !W3_safe_q[18] & !W3_safe_q[19];


--W3_safe_q[20] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[20]
--operation mode is arithmetic

W3_safe_q[20]_carry_eqn = W3L04;
W3_safe_q[20]_lut_out = W3_safe_q[20] $ (!W3_safe_q[20]_carry_eqn);
W3_safe_q[20] = DFFEAS(W3_safe_q[20]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L24 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella20~COUT
--operation mode is arithmetic

W3L24 = CARRY(W3_safe_q[20] & !W3L04);


--W3_safe_q[21] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[21]
--operation mode is arithmetic

W3_safe_q[21]_carry_eqn = W3L24;
W3_safe_q[21]_lut_out = W3_safe_q[21] $ (W3_safe_q[21]_carry_eqn);
W3_safe_q[21] = DFFEAS(W3_safe_q[21]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L44 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella21~COUT
--operation mode is arithmetic

W3L44 = CARRY(!W3L24 # !W3_safe_q[21]);


--W3_safe_q[22] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[22]
--operation mode is arithmetic

W3_safe_q[22]_carry_eqn = W3L44;
W3_safe_q[22]_lut_out = W3_safe_q[22] $ (!W3_safe_q[22]_carry_eqn);
W3_safe_q[22] = DFFEAS(W3_safe_q[22]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L64 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella22~COUT
--operation mode is arithmetic

W3L64 = CARRY(W3_safe_q[22] & !W3L44);


--W3_safe_q[23] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[23]
--operation mode is arithmetic

W3_safe_q[23]_carry_eqn = W3L64;
W3_safe_q[23]_lut_out = W3_safe_q[23] $ (W3_safe_q[23]_carry_eqn);
W3_safe_q[23] = DFFEAS(W3_safe_q[23]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L84 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella23~COUT
--operation mode is arithmetic

W3L84 = CARRY(!W3L64 # !W3_safe_q[23]);


--F1L21 is fdiv:inst5|LessThan~1054
--operation mode is normal

F1L21 = !W3_safe_q[20] & !W3_safe_q[21] & !W3_safe_q[22] & !W3_safe_q[23];


--W3_safe_q[24] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[24]
--operation mode is arithmetic

W3_safe_q[24]_carry_eqn = W3L84;
W3_safe_q[24]_lut_out = W3_safe_q[24] $ (!W3_safe_q[24]_carry_eqn);
W3_safe_q[24] = DFFEAS(W3_safe_q[24]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L05 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella24~COUT
--operation mode is arithmetic

W3L05 = CARRY(W3_safe_q[24] & !W3L84);


--W3_safe_q[25] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[25]
--operation mode is arithmetic

W3_safe_q[25]_carry_eqn = W3L05;
W3_safe_q[25]_lut_out = W3_safe_q[25] $ (W3_safe_q[25]_carry_eqn);
W3_safe_q[25] = DFFEAS(W3_safe_q[25]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L25 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella25~COUT
--operation mode is arithmetic

W3L25 = CARRY(!W3L05 # !W3_safe_q[25]);


--W3_safe_q[26] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[26]
--operation mode is arithmetic

W3_safe_q[26]_carry_eqn = W3L25;
W3_safe_q[26]_lut_out = W3_safe_q[26] $ (!W3_safe_q[26]_carry_eqn);
W3_safe_q[26] = DFFEAS(W3_safe_q[26]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L45 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella26~COUT
--operation mode is arithmetic

W3L45 = CARRY(W3_safe_q[26] & !W3L25);


--W3_safe_q[27] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[27]
--operation mode is arithmetic

W3_safe_q[27]_carry_eqn = W3L45;
W3_safe_q[27]_lut_out = W3_safe_q[27] $ (W3_safe_q[27]_carry_eqn);
W3_safe_q[27] = DFFEAS(W3_safe_q[27]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L65 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella27~COUT
--operation mode is arithmetic

W3L65 = CARRY(!W3L45 # !W3_safe_q[27]);


--F1L31 is fdiv:inst5|LessThan~1055
--operation mode is normal

F1L31 = !W3_safe_q[24] & !W3_safe_q[25] & !W3_safe_q[26] & !W3_safe_q[27];


--F1L41 is fdiv:inst5|LessThan~1056
--operation mode is normal

F1L41 = F1L01 & F1L11 & F1L21 & F1L31;


--W3_safe_q[28] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[28]
--operation mode is arithmetic

W3_safe_q[28]_carry_eqn = W3L65;
W3_safe_q[28]_lut_out = W3_safe_q[28] $ (!W3_safe_q[28]_carry_eqn);
W3_safe_q[28] = DFFEAS(W3_safe_q[28]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L85 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella28~COUT
--operation mode is arithmetic

W3L85 = CARRY(W3_safe_q[28] & !W3L65);


--W3_safe_q[29] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[29]
--operation mode is arithmetic

W3_safe_q[29]_carry_eqn = W3L85;
W3_safe_q[29]_lut_out = W3_safe_q[29] $ (W3_safe_q[29]_carry_eqn);
W3_safe_q[29] = DFFEAS(W3_safe_q[29]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L06 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella29~COUT
--operation mode is arithmetic

W3L06 = CARRY(!W3L85 # !W3_safe_q[29]);


--W3_safe_q[30] is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|safe_q[30]
--operation mode is arithmetic

W3_safe_q[30]_carry_eqn = W3L06;
W3_safe_q[30]_lut_out = W3_safe_q[30] $ (!W3_safe_q[30]_carry_eqn);
W3_safe_q[30] = DFFEAS(W3_safe_q[30]_lut_out, F1_f200hz, VCC, , , , , F1L1, );

--W3L26 is fdiv:inst5|lpm_counter:CNT3_rtl_18|cntr_jd7:auto_generated|counter_cella30~COUT
--operation mode is arithmetic

W3L26 = CARRY(W3_safe_q[30] & !W3L06);


--F1L51 is fdiv:inst5|LessThan~1057
--operation mode is normal

F1L51 = !W3_safe_q[28] & !W3_safe_q[29] & !W3_safe_q[30];


--F1L1 is fdiv:inst5|LessThan~518
--operation mode is normal

F1L1 = !W3_safe_q[31] & !F1L51 # !F1L41 # !F1L9;


--S31_safe_q[0] is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S31_safe_q[0]_lut_out = !S31_safe_q[0];
S31_safe_q[0] = DFFEAS(S31_safe_q[0]_lut_out, N1_EO, VCC, , T1L51, , , T1L81, );

--S31L2 is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S31L2 = CARRY(S31_safe_q[0]);


--S61_safe_q[0] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S61_safe_q[0]_lut_out = !S61_safe_q[0];
S61_safe_q[0] = DFFEAS(S61_safe_q[0]_lut_out, SW2, VCC, , U1L4, , , V1L2, );

--S61L2 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S61L2 = CARRY(S61_safe_q[0]);


--T1_EO1 is date_main:inst4|autodate:b2v_inst|EO1
--operation mode is normal

T1_EO1_lut_out = !D1_DateSet_EN;
T1_EO1 = DFFEAS(T1_EO1_lut_out, N1_EO, VCC, , , , , , );


--U1L81 is date_main:inst4|datecontrol:b2v_inst1|disp_select[3]~43
--operation mode is normal

U1L81 = D1_DateSet_EN # D1_Date_EN & T1_EO1;


--V1_disp_drive[0] is date_main:inst4|setdate:b2v_inst2|disp_drive[0]
--operation mode is normal

V1_disp_drive[0]_lut_out = !V1_disp_drive[0];
V1_disp_drive[0] = DFFEAS(V1_disp_drive[0]_lut_out, SW1, VCC, , D1_DateSet_EN, , , , );


--V1_disp_drive[1] is date_main:inst4|setdate:b2v_inst2|disp_drive[1]
--operation mode is normal

V1_disp_drive[1]_lut_out = V1_disp_drive[1] $ V1_disp_drive[0];
V1_disp_drive[1] = DFFEAS(V1_disp_drive[1]_lut_out, SW1, VCC, , D1_DateSet_EN, , , , );


--T1_month1[0] is date_main:inst4|autodate:b2v_inst|month1[0]
--operation mode is normal

T1_month1[0]_lut_out = !T1_month1[0];
T1_month1[0] = DFFEAS(T1_month1[0]_lut_out, N1_EO, VCC, , T1L03, , , , );


--S91_safe_q[0] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S91_safe_q[0]_lut_out = !S91_safe_q[0];
S91_safe_q[0] = DFFEAS(S91_safe_q[0]_lut_out, SW2, VCC, , U1L1, , , V1L3, );

--S91L2 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S91L2 = CARRY(S91_safe_q[0]);


--S41_safe_q[0] is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S41_safe_q[0]_lut_out = !S41_safe_q[0];
S41_safe_q[0] = DFFEAS(S41_safe_q[0]_lut_out, N1_EO, VCC, , T1L12, , , T1L22, );

--S41L2 is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S41L2 = CARRY(S41_safe_q[0]);


--S71_safe_q[0] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S71_safe_q[0]_lut_out = !S71_safe_q[0];
S71_safe_q[0] = DFFEAS(S71_safe_q[0]_lut_out, SW2, VCC, , U1L3, , , V1L4, );

--S71L2 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S71L2 = CARRY(S71_safe_q[0]);


--S51_safe_q[0] is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S51_safe_q[0]_lut_out = !S51_safe_q[0];
S51_safe_q[0] = DFFEAS(S51_safe_q[0]_lut_out, N1_EO, VCC, , T1L42, , , T1L62, );

--S51L2 is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S51L2 = CARRY(S51_safe_q[0]);


--S81_safe_q[0] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|safe_q[0]
--operation mode is arithmetic

S81_safe_q[0]_lut_out = !S81_safe_q[0];
S81_safe_q[0] = DFFEAS(S81_safe_q[0]_lut_out, SW2, VCC, , U1L2, , , V1L1, );

--S81L2 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

S81L2 = CARRY(S81_safe_q[0]);


--S91_safe_q[1] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S91_safe_q[1]_carry_eqn = S91L2;
S91_safe_q[1]_lut_out = S91_safe_q[1] $ (S91_safe_q[1]_carry_eqn);
S91_safe_q[1] = DFFEAS(S91_safe_q[1]_lut_out, SW2, VCC, , U1L1, , , V1L3, );

--S91L4 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S91L4 = CARRY(!S91L2 # !S91_safe_q[1]);


--S31_safe_q[1] is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S31_safe_q[1]_carry_eqn = S31L2;
S31_safe_q[1]_lut_out = S31_safe_q[1] $ (S31_safe_q[1]_carry_eqn);
S31_safe_q[1] = DFFEAS(S31_safe_q[1]_lut_out, N1_EO, VCC, , T1L51, , , T1L81, );

--S31L4 is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S31L4 = CARRY(!S31L2 # !S31_safe_q[1]);


--S61_safe_q[1] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S61_safe_q[1]_carry_eqn = S61L2;
S61_safe_q[1]_lut_out = S61_safe_q[1] $ (S61_safe_q[1]_carry_eqn);
S61_safe_q[1] = DFFEAS(S61_safe_q[1]_lut_out, SW2, VCC, , U1L4, , , V1L2, );

--S61L4 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S61L4 = CARRY(!S61L2 # !S61_safe_q[1]);


--S41_safe_q[1] is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S41_safe_q[1]_carry_eqn = S41L2;
S41_safe_q[1]_lut_out = S41_safe_q[1] $ (S41_safe_q[1]_carry_eqn);
S41_safe_q[1] = DFFEAS(S41_safe_q[1]_lut_out, N1_EO, VCC, , T1L12, , , T1L22, );

--S41L4 is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S41L4 = CARRY(!S41L2 # !S41_safe_q[1]);


--S71_safe_q[1] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S71_safe_q[1]_carry_eqn = S71L2;
S71_safe_q[1]_lut_out = S71_safe_q[1] $ (S71_safe_q[1]_carry_eqn);
S71_safe_q[1] = DFFEAS(S71_safe_q[1]_lut_out, SW2, VCC, , U1L3, , , V1L4, );

--S71L4 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S71L4 = CARRY(!S71L2 # !S71_safe_q[1]);


--S51_safe_q[1] is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S51_safe_q[1]_carry_eqn = S51L2;
S51_safe_q[1]_lut_out = S51_safe_q[1] $ (S51_safe_q[1]_carry_eqn);
S51_safe_q[1] = DFFEAS(S51_safe_q[1]_lut_out, N1_EO, VCC, , T1L42, , , T1L62, );

--S51L4 is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S51L4 = CARRY(!S51L2 # !S51_safe_q[1]);


--S81_safe_q[1] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|safe_q[1]
--operation mode is arithmetic

S81_safe_q[1]_carry_eqn = S81L2;
S81_safe_q[1]_lut_out = S81_safe_q[1] $ (S81_safe_q[1]_carry_eqn);
S81_safe_q[1] = DFFEAS(S81_safe_q[1]_lut_out, SW2, VCC, , U1L2, , , V1L1, );

--S81L4 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

S81L4 = CARRY(!S81L2 # !S81_safe_q[1]);


--S31_safe_q[2] is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S31_safe_q[2]_carry_eqn = S31L4;
S31_safe_q[2]_lut_out = S31_safe_q[2] $ (!S31_safe_q[2]_carry_eqn);
S31_safe_q[2] = DFFEAS(S31_safe_q[2]_lut_out, N1_EO, VCC, , T1L51, , , T1L81, );

--S31L6 is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S31L6 = CARRY(S31_safe_q[2] & !S31L4);


--S61_safe_q[2] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S61_safe_q[2]_carry_eqn = S61L4;
S61_safe_q[2]_lut_out = S61_safe_q[2] $ (!S61_safe_q[2]_carry_eqn);
S61_safe_q[2] = DFFEAS(S61_safe_q[2]_lut_out, SW2, VCC, , U1L4, , , V1L2, );

--S61L6 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S61L6 = CARRY(S61_safe_q[2] & !S61L4);


--S91_safe_q[2] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S91_safe_q[2]_carry_eqn = S91L4;
S91_safe_q[2]_lut_out = S91_safe_q[2] $ (!S91_safe_q[2]_carry_eqn);
S91_safe_q[2] = DFFEAS(S91_safe_q[2]_lut_out, SW2, VCC, , U1L1, , , V1L3, );

--S91L6 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S91L6 = CARRY(S91_safe_q[2] & !S91L4);


--S41_safe_q[2] is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S41_safe_q[2]_carry_eqn = S41L4;
S41_safe_q[2]_lut_out = S41_safe_q[2] $ (!S41_safe_q[2]_carry_eqn);
S41_safe_q[2] = DFFEAS(S41_safe_q[2]_lut_out, N1_EO, VCC, , T1L12, , , T1L22, );

--S41L6 is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S41L6 = CARRY(S41_safe_q[2] & !S41L4);


--S71_safe_q[2] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S71_safe_q[2]_carry_eqn = S71L4;
S71_safe_q[2]_lut_out = S71_safe_q[2] $ (!S71_safe_q[2]_carry_eqn);
S71_safe_q[2] = DFFEAS(S71_safe_q[2]_lut_out, SW2, VCC, , U1L3, , , V1L4, );

--S71L6 is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S71L6 = CARRY(S71_safe_q[2] & !S71L4);


--S51_safe_q[2] is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S51_safe_q[2]_carry_eqn = S51L4;
S51_safe_q[2]_lut_out = S51_safe_q[2] $ (!S51_safe_q[2]_carry_eqn);
S51_safe_q[2] = DFFEAS(S51_safe_q[2]_lut_out, N1_EO, VCC, , T1L42, , , T1L62, );

--S51L6 is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S51L6 = CARRY(S51_safe_q[2] & !S51L4);


--S81_safe_q[2] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|safe_q[2]
--operation mode is arithmetic

S81_safe_q[2]_carry_eqn = S81L4;
S81_safe_q[2]_lut_out = S81_safe_q[2] $ (!S81_safe_q[2]_carry_eqn);
S81_safe_q[2] = DFFEAS(S81_safe_q[2]_lut_out, SW2, VCC, , U1L2, , , V1L1, );

--S81L6 is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

S81L6 = CARRY(S81_safe_q[2] & !S81L4);


--S91_safe_q[3] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set1_rtl_24|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S91_safe_q[3]_carry_eqn = S91L6;
S91_safe_q[3]_lut_out = S91_safe_q[3] $ (S91_safe_q[3]_carry_eqn);
S91_safe_q[3] = DFFEAS(S91_safe_q[3]_lut_out, SW2, VCC, , U1L1, , , V1L3, );


--S31_safe_q[3] is date_main:inst4|autodate:b2v_inst|lpm_counter:day0_rtl_23|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S31_safe_q[3]_carry_eqn = S31L6;
S31_safe_q[3]_lut_out = S31_safe_q[3] $ (S31_safe_q[3]_carry_eqn);
S31_safe_q[3] = DFFEAS(S31_safe_q[3]_lut_out, N1_EO, VCC, , T1L51, , , T1L81, );


--S61_safe_q[3] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set0_rtl_22|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S61_safe_q[3]_carry_eqn = S61L6;
S61_safe_q[3]_lut_out = S61_safe_q[3] $ (S61_safe_q[3]_carry_eqn);
S61_safe_q[3] = DFFEAS(S61_safe_q[3]_lut_out, SW2, VCC, , U1L4, , , V1L2, );


--S41_safe_q[3] is date_main:inst4|autodate:b2v_inst|lpm_counter:day1_rtl_21|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S41_safe_q[3]_carry_eqn = S41L6;
S41_safe_q[3]_lut_out = S41_safe_q[3] $ (S41_safe_q[3]_carry_eqn);
S41_safe_q[3] = DFFEAS(S41_safe_q[3]_lut_out, N1_EO, VCC, , T1L12, , , T1L22, );


--S71_safe_q[3] is date_main:inst4|setdate:b2v_inst2|lpm_counter:day_set1_rtl_20|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S71_safe_q[3]_carry_eqn = S71L6;
S71_safe_q[3]_lut_out = S71_safe_q[3] $ (S71_safe_q[3]_carry_eqn);
S71_safe_q[3] = DFFEAS(S71_safe_q[3]_lut_out, SW2, VCC, , U1L3, , , V1L4, );


--S51_safe_q[3] is date_main:inst4|autodate:b2v_inst|lpm_counter:month0_rtl_26|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S51_safe_q[3]_carry_eqn = S51L6;
S51_safe_q[3]_lut_out = S51_safe_q[3] $ (S51_safe_q[3]_carry_eqn);
S51_safe_q[3] = DFFEAS(S51_safe_q[3]_lut_out, N1_EO, VCC, , T1L42, , , T1L62, );


--S81_safe_q[3] is date_main:inst4|setdate:b2v_inst2|lpm_counter:month_set0_rtl_25|cntr_e08:auto_generated|safe_q[3]
--operation mode is normal

S81_safe_q[3]_carry_eqn = S81L6;
S81_safe_q[3]_lut_out = S81_safe_q[3] $ (S81_safe_q[3]_carry_eqn);
S81_safe_q[3] = DFFEAS(S81_safe_q[3]_lut_out, SW2, VCC, , U1L2, , , V1L1, );


--W2_safe_q[0] is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|safe_q[0]
--operation mode is arithmetic

W2_safe_q[0]_lut_out = !W2_safe_q[0];
W2_safe_q[0] = DFFEAS(W2_safe_q[0]_lut_out, F1_f200hz, VCC, , , , , F1L5, );

--W2L2 is fdiv:inst5|lpm_counter:CNT2_rtl_19|cntr_jd7:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

W2L2 = CARRY(W2_safe_q[0]);


--W1_safe_q[31] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[31]
--operation mode is normal

W1_safe_q[31]_carry_eqn = W1L26;
W1_safe_q[31]_lut_out = W1_safe_q[31] $ (W1_safe_q[31]_carry_eqn);
W1_safe_q[31] = DFFEAS(W1_safe_q[31]_lut_out, Clock, VCC, , , , , F1L2, );


--W1_safe_q[2] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[2]
--operation mode is arithmetic

W1_safe_q[2]_carry_eqn = W1L4;
W1_safe_q[2]_lut_out = W1_safe_q[2] $ (!W1_safe_q[2]_carry_eqn);
W1_safe_q[2] = DFFEAS(W1_safe_q[2]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L6 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

W1L6 = CARRY(W1_safe_q[2] & !W1L4);


--W1_safe_q[3] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[3]
--operation mode is arithmetic

W1_safe_q[3]_carry_eqn = W1L6;
W1_safe_q[3]_lut_out = W1_safe_q[3] $ (W1_safe_q[3]_carry_eqn);
W1_safe_q[3] = DFFEAS(W1_safe_q[3]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L8 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella3~COUT
--operation mode is arithmetic

W1L8 = CARRY(!W1L6 # !W1_safe_q[3]);


--W1_safe_q[4] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[4]
--operation mode is arithmetic

W1_safe_q[4]_carry_eqn = W1L8;
W1_safe_q[4]_lut_out = W1_safe_q[4] $ (!W1_safe_q[4]_carry_eqn);
W1_safe_q[4] = DFFEAS(W1_safe_q[4]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L01 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella4~COUT
--operation mode is arithmetic

W1L01 = CARRY(W1_safe_q[4] & !W1L8);


--W1_safe_q[5] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[5]
--operation mode is arithmetic

W1_safe_q[5]_carry_eqn = W1L01;
W1_safe_q[5]_lut_out = W1_safe_q[5] $ (W1_safe_q[5]_carry_eqn);
W1_safe_q[5] = DFFEAS(W1_safe_q[5]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L21 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella5~COUT
--operation mode is arithmetic

W1L21 = CARRY(!W1L01 # !W1_safe_q[5]);


--W1L69 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~424
--operation mode is normal

W1L69 = !W1_safe_q[2] & !W1_safe_q[3] & !W1_safe_q[4] & !W1_safe_q[5];


--W1_safe_q[6] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[6]
--operation mode is arithmetic

W1_safe_q[6]_carry_eqn = W1L21;
W1_safe_q[6]_lut_out = W1_safe_q[6] $ (!W1_safe_q[6]_carry_eqn);
W1_safe_q[6] = DFFEAS(W1_safe_q[6]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L41 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella6~COUT
--operation mode is arithmetic

W1L41 = CARRY(W1_safe_q[6] & !W1L21);


--W1_safe_q[7] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[7]
--operation mode is arithmetic

W1_safe_q[7]_carry_eqn = W1L41;
W1_safe_q[7]_lut_out = W1_safe_q[7] $ (W1_safe_q[7]_carry_eqn);
W1_safe_q[7] = DFFEAS(W1_safe_q[7]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L61 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella7~COUT
--operation mode is arithmetic

W1L61 = CARRY(!W1L41 # !W1_safe_q[7]);


--W1_safe_q[8] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[8]
--operation mode is arithmetic

W1_safe_q[8]_carry_eqn = W1L61;
W1_safe_q[8]_lut_out = W1_safe_q[8] $ (!W1_safe_q[8]_carry_eqn);
W1_safe_q[8] = DFFEAS(W1_safe_q[8]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L81 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella8~COUT
--operation mode is arithmetic

W1L81 = CARRY(W1_safe_q[8] & !W1L61);


--W1_safe_q[9] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[9]
--operation mode is arithmetic

W1_safe_q[9]_carry_eqn = W1L81;
W1_safe_q[9]_lut_out = W1_safe_q[9] $ (W1_safe_q[9]_carry_eqn);
W1_safe_q[9] = DFFEAS(W1_safe_q[9]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L02 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella9~COUT
--operation mode is arithmetic

W1L02 = CARRY(!W1L81 # !W1_safe_q[9]);


--W1L79 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~425
--operation mode is normal

W1L79 = !W1_safe_q[6] & !W1_safe_q[7] & !W1_safe_q[8] & !W1_safe_q[9];


--W1_safe_q[10] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[10]
--operation mode is arithmetic

W1_safe_q[10]_carry_eqn = W1L02;
W1_safe_q[10]_lut_out = W1_safe_q[10] $ (!W1_safe_q[10]_carry_eqn);
W1_safe_q[10] = DFFEAS(W1_safe_q[10]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L22 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella10~COUT
--operation mode is arithmetic

W1L22 = CARRY(W1_safe_q[10] & !W1L02);


--W1_safe_q[11] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[11]
--operation mode is arithmetic

W1_safe_q[11]_carry_eqn = W1L22;
W1_safe_q[11]_lut_out = W1_safe_q[11] $ (W1_safe_q[11]_carry_eqn);
W1_safe_q[11] = DFFEAS(W1_safe_q[11]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L42 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella11~COUT
--operation mode is arithmetic

W1L42 = CARRY(!W1L22 # !W1_safe_q[11]);


--W1_safe_q[12] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[12]
--operation mode is arithmetic

W1_safe_q[12]_carry_eqn = W1L42;
W1_safe_q[12]_lut_out = W1_safe_q[12] $ (!W1_safe_q[12]_carry_eqn);
W1_safe_q[12] = DFFEAS(W1_safe_q[12]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L62 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella12~COUT
--operation mode is arithmetic

W1L62 = CARRY(W1_safe_q[12] & !W1L42);


--W1_safe_q[13] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[13]
--operation mode is arithmetic

W1_safe_q[13]_carry_eqn = W1L62;
W1_safe_q[13]_lut_out = W1_safe_q[13] $ (W1_safe_q[13]_carry_eqn);
W1_safe_q[13] = DFFEAS(W1_safe_q[13]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L82 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella13~COUT
--operation mode is arithmetic

W1L82 = CARRY(!W1L62 # !W1_safe_q[13]);


--W1L89 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~426
--operation mode is normal

W1L89 = !W1_safe_q[10] & !W1_safe_q[11] & !W1_safe_q[12] & !W1_safe_q[13];


--W1_safe_q[14] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[14]
--operation mode is arithmetic

W1_safe_q[14]_carry_eqn = W1L82;
W1_safe_q[14]_lut_out = W1_safe_q[14] $ (!W1_safe_q[14]_carry_eqn);
W1_safe_q[14] = DFFEAS(W1_safe_q[14]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L03 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella14~COUT
--operation mode is arithmetic

W1L03 = CARRY(W1_safe_q[14] & !W1L82);


--W1_safe_q[15] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[15]
--operation mode is arithmetic

W1_safe_q[15]_carry_eqn = W1L03;
W1_safe_q[15]_lut_out = W1_safe_q[15] $ (W1_safe_q[15]_carry_eqn);
W1_safe_q[15] = DFFEAS(W1_safe_q[15]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L23 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella15~COUT
--operation mode is arithmetic

W1L23 = CARRY(!W1L03 # !W1_safe_q[15]);


--W1_safe_q[16] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[16]
--operation mode is arithmetic

W1_safe_q[16]_carry_eqn = W1L23;
W1_safe_q[16]_lut_out = W1_safe_q[16] $ (!W1_safe_q[16]_carry_eqn);
W1_safe_q[16] = DFFEAS(W1_safe_q[16]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L43 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella16~COUT
--operation mode is arithmetic

W1L43 = CARRY(W1_safe_q[16] & !W1L23);


--W1_safe_q[17] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[17]
--operation mode is arithmetic

W1_safe_q[17]_carry_eqn = W1L43;
W1_safe_q[17]_lut_out = W1_safe_q[17] $ (W1_safe_q[17]_carry_eqn);
W1_safe_q[17] = DFFEAS(W1_safe_q[17]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L63 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella17~COUT
--operation mode is arithmetic

W1L63 = CARRY(!W1L43 # !W1_safe_q[17]);


--W1L99 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~427
--operation mode is normal

W1L99 = !W1_safe_q[14] & !W1_safe_q[15] & !W1_safe_q[16] & !W1_safe_q[17];


--W1L001 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~428
--operation mode is normal

W1L001 = W1L69 & W1L79 & W1L89 & W1L99;


--W1_safe_q[18] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[18]
--operation mode is arithmetic

W1_safe_q[18]_carry_eqn = W1L63;
W1_safe_q[18]_lut_out = W1_safe_q[18] $ (!W1_safe_q[18]_carry_eqn);
W1_safe_q[18] = DFFEAS(W1_safe_q[18]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L83 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella18~COUT
--operation mode is arithmetic

W1L83 = CARRY(W1_safe_q[18] & !W1L63);


--W1_safe_q[19] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[19]
--operation mode is arithmetic

W1_safe_q[19]_carry_eqn = W1L83;
W1_safe_q[19]_lut_out = W1_safe_q[19] $ (W1_safe_q[19]_carry_eqn);
W1_safe_q[19] = DFFEAS(W1_safe_q[19]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L04 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella19~COUT
--operation mode is arithmetic

W1L04 = CARRY(!W1L83 # !W1_safe_q[19]);


--W1_safe_q[20] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[20]
--operation mode is arithmetic

W1_safe_q[20]_carry_eqn = W1L04;
W1_safe_q[20]_lut_out = W1_safe_q[20] $ (!W1_safe_q[20]_carry_eqn);
W1_safe_q[20] = DFFEAS(W1_safe_q[20]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L24 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella20~COUT
--operation mode is arithmetic

W1L24 = CARRY(W1_safe_q[20] & !W1L04);


--W1_safe_q[21] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[21]
--operation mode is arithmetic

W1_safe_q[21]_carry_eqn = W1L24;
W1_safe_q[21]_lut_out = W1_safe_q[21] $ (W1_safe_q[21]_carry_eqn);
W1_safe_q[21] = DFFEAS(W1_safe_q[21]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L44 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella21~COUT
--operation mode is arithmetic

W1L44 = CARRY(!W1L24 # !W1_safe_q[21]);


--W1L101 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~429
--operation mode is normal

W1L101 = !W1_safe_q[18] & !W1_safe_q[19] & !W1_safe_q[20] & !W1_safe_q[21];


--W1_safe_q[22] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[22]
--operation mode is arithmetic

W1_safe_q[22]_carry_eqn = W1L44;
W1_safe_q[22]_lut_out = W1_safe_q[22] $ (!W1_safe_q[22]_carry_eqn);
W1_safe_q[22] = DFFEAS(W1_safe_q[22]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L64 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella22~COUT
--operation mode is arithmetic

W1L64 = CARRY(W1_safe_q[22] & !W1L44);


--W1_safe_q[23] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[23]
--operation mode is arithmetic

W1_safe_q[23]_carry_eqn = W1L64;
W1_safe_q[23]_lut_out = W1_safe_q[23] $ (W1_safe_q[23]_carry_eqn);
W1_safe_q[23] = DFFEAS(W1_safe_q[23]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L84 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella23~COUT
--operation mode is arithmetic

W1L84 = CARRY(!W1L64 # !W1_safe_q[23]);


--W1_safe_q[24] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[24]
--operation mode is arithmetic

W1_safe_q[24]_carry_eqn = W1L84;
W1_safe_q[24]_lut_out = W1_safe_q[24] $ (!W1_safe_q[24]_carry_eqn);
W1_safe_q[24] = DFFEAS(W1_safe_q[24]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L05 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella24~COUT
--operation mode is arithmetic

W1L05 = CARRY(W1_safe_q[24] & !W1L84);


--W1_safe_q[25] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[25]
--operation mode is arithmetic

W1_safe_q[25]_carry_eqn = W1L05;
W1_safe_q[25]_lut_out = W1_safe_q[25] $ (W1_safe_q[25]_carry_eqn);
W1_safe_q[25] = DFFEAS(W1_safe_q[25]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L25 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella25~COUT
--operation mode is arithmetic

W1L25 = CARRY(!W1L05 # !W1_safe_q[25]);


--W1L201 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~430
--operation mode is normal

W1L201 = !W1_safe_q[22] & !W1_safe_q[23] & !W1_safe_q[24] & !W1_safe_q[25];


--W1_safe_q[26] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[26]
--operation mode is arithmetic

W1_safe_q[26]_carry_eqn = W1L25;
W1_safe_q[26]_lut_out = W1_safe_q[26] $ (!W1_safe_q[26]_carry_eqn);
W1_safe_q[26] = DFFEAS(W1_safe_q[26]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L45 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella26~COUT
--operation mode is arithmetic

W1L45 = CARRY(W1_safe_q[26] & !W1L25);


--W1_safe_q[27] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[27]
--operation mode is arithmetic

W1_safe_q[27]_carry_eqn = W1L45;
W1_safe_q[27]_lut_out = W1_safe_q[27] $ (W1_safe_q[27]_carry_eqn);
W1_safe_q[27] = DFFEAS(W1_safe_q[27]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L65 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella27~COUT
--operation mode is arithmetic

W1L65 = CARRY(!W1L45 # !W1_safe_q[27]);


--W1_safe_q[28] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[28]
--operation mode is arithmetic

W1_safe_q[28]_carry_eqn = W1L65;
W1_safe_q[28]_lut_out = W1_safe_q[28] $ (!W1_safe_q[28]_carry_eqn);
W1_safe_q[28] = DFFEAS(W1_safe_q[28]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L85 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella28~COUT
--operation mode is arithmetic

W1L85 = CARRY(W1_safe_q[28] & !W1L65);


--W1_safe_q[29] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[29]
--operation mode is arithmetic

W1_safe_q[29]_carry_eqn = W1L85;
W1_safe_q[29]_lut_out = W1_safe_q[29] $ (W1_safe_q[29]_carry_eqn);
W1_safe_q[29] = DFFEAS(W1_safe_q[29]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L06 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella29~COUT
--operation mode is arithmetic

W1L06 = CARRY(!W1L85 # !W1_safe_q[29]);


--W1L301 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~431
--operation mode is normal

W1L301 = !W1_safe_q[26] & !W1_safe_q[27] & !W1_safe_q[28] & !W1_safe_q[29];


--W1_safe_q[30] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]
--operation mode is arithmetic

W1_safe_q[30]_carry_eqn = W1L06;
W1_safe_q[30]_lut_out = W1_safe_q[30] $ (!W1_safe_q[30]_carry_eqn);
W1_safe_q[30] = DFFEAS(W1_safe_q[30]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L26 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella30~COUT
--operation mode is arithmetic

W1L26 = CARRY(W1_safe_q[30] & !W1L06);


--W1L401 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[30]~432
--operation mode is normal

W1L401 = W1L101 & W1L201 & W1L301 & !W1_safe_q[30];


--F1L2 is fdiv:inst5|LessThan~774
--operation mode is normal

F1L2 = !W1_safe_q[31] & !W1L401 # !W1L001;


--G1L31 is time_disp_select:inst6|disp_drive~63
--operation mode is normal

G1L31 = M1_disp_drive[0] & !D1_Timepiece_EN;


--G1_auto_disp_drive[0] is time_disp_select:inst6|auto_disp_drive[0]
--operation mode is normal

G1_auto_disp_drive[0]_lut_out = !G1_auto_disp_drive[0] & !G1_auto_disp_drive[1] # !G1_auto_disp_drive[2];
G1_auto_disp_drive[0] = DFFEAS(G1_auto_disp_drive[0]_lut_out, Clock, VCC, , , , , , );


--G1L41 is time_disp_select:inst6|disp_drive~64
--operation mode is normal

G1L41 = D1_Timepiece_EN & G1_auto_disp_drive[0];


--G1L1 is time_disp_select:inst6|always1~2
--operation mode is normal

G1L1 = !D1_TimeSet_EN & !D1_Timepiece_EN;


--G1_disp_drive[0] is time_disp_select:inst6|disp_drive[0]
--operation mode is normal

G1_disp_drive[0] = G1L1 & G1_disp_drive[0] # !G1L1 & G1L31 # G1L41;


--G1L51 is time_disp_select:inst6|disp_drive~65
--operation mode is normal

G1L51 = M1_disp_drive[2] & !D1_Timepiece_EN;


--G1_auto_disp_drive[2] is time_disp_select:inst6|auto_disp_drive[2]
--operation mode is normal

G1_auto_disp_drive[2]_lut_out = G1_auto_disp_drive[2] & !G1_auto_disp_drive[0] & !G1_auto_disp_drive[1] # !G1_auto_disp_drive[2] & G1_auto_disp_drive[0] & G1_auto_disp_drive[1];
G1_auto_disp_drive[2] = DFFEAS(G1_auto_disp_drive[2]_lut_out, Clock, VCC, , , , , , );


--G1L61 is time_disp_select:inst6|disp_drive~66
--operation mode is normal

G1L61 = D1_Timepiece_EN & G1_auto_disp_drive[2];


--G1_disp_drive[2] is time_disp_select:inst6|disp_drive[2]
--operation mode is normal

G1_disp_drive[2] = G1L1 & G1_disp_drive[2] # !G1L1 & G1L51 # G1L61;


--G1L71 is time_disp_select:inst6|disp_drive~67
--operation mode is normal

G1L71 = M1_disp_drive[1] & !D1_Timepiece_EN;


--G1_auto_disp_drive[1] is time_disp_select:inst6|auto_disp_drive[1]
--operation mode is normal

G1_auto_disp_drive[1]_lut_out = !G1_auto_disp_drive[2] & G1_auto_disp_drive[0] $ G1_auto_disp_drive[1];
G1_auto_disp_drive[1] = DFFEAS(G1_auto_disp_drive[1]_lut_out, Clock, VCC, , , , , , );


--G1L81 is time_disp_select:inst6|disp_drive~68
--operation mode is normal

G1L81 = D1_Timepiece_EN & G1_auto_disp_drive[1];


--G1_disp_drive[1] is time_disp_select:inst6|disp_drive[1]
--operation mode is normal

G1_disp_drive[1] = G1L1 & G1_disp_drive[1] # !G1L1 & G1L71 # G1L81;


--G1L7 is time_disp_select:inst6|clk~21
--operation mode is normal

G1L7 = F1_f200hz & !D1_Timepiece_EN;


--G1L8 is time_disp_select:inst6|clk~22
--operation mode is normal

G1L8 = D1_Timepiece_EN & Clock;


--G1_clk is time_disp_select:inst6|clk
--operation mode is normal

G1_clk = G1L1 & G1_clk # !G1L1 & G1L7 # G1L8;


--N1_EO is time_auto_and_set:inst1|timepiece_main:b2v_inst1|hour_counter:b2v_inst|EO
--operation mode is normal

N1_EO_lut_out = N1L2;
N1_EO = DFFEAS(N1_EO_lut_out, P1_EO, VCC, , N1L4, , , , );


--T1L5 is date_main:inst4|autodate:b2v_inst|always0~575
--operation mode is normal

T1L5 = !S41_safe_q[2] & !S41_safe_q[3];


--T1L6 is date_main:inst4|autodate:b2v_inst|always0~576
--operation mode is normal

T1L6 = !S31_safe_q[0] & !S31_safe_q[1] & !S31_safe_q[2] & !S31_safe_q[3];


--T1L7 is date_main:inst4|autodate:b2v_inst|always0~577
--operation mode is normal

T1L7 = S41_safe_q[0] & S41_safe_q[1] & T1L5 & T1L6;


--T1L8 is date_main:inst4|autodate:b2v_inst|always0~578
--operation mode is normal

T1L8 = S51_safe_q[2] # S51_safe_q[1] & !T1_month1[0];


--T1L9 is date_main:inst4|autodate:b2v_inst|always0~579
--operation mode is normal

T1L9 = S51_safe_q[0] & S51_safe_q[3] # T1_month1[0] # !S51_safe_q[0] & T1L8 # S51_safe_q[3] & T1_month1[0];


--T1L61 is date_main:inst4|autodate:b2v_inst|day0[2]~462
--operation mode is normal

T1L61 = T1L7 & !T1L9;


--T1L01 is date_main:inst4|autodate:b2v_inst|always0~580
--operation mode is normal

T1L01 = !S41_safe_q[1] & !S41_safe_q[2] & !S41_safe_q[3];


--T1L11 is date_main:inst4|autodate:b2v_inst|always0~581
--operation mode is normal

T1L11 = !S31_safe_q[0] & !S31_safe_q[1] & !S31_safe_q[2];


--T1L2 is date_main:inst4|autodate:b2v_inst|LessThan~216
--operation mode is normal

T1L2 = S41_safe_q[2] # S41_safe_q[3] # S41_safe_q[0] & S41_safe_q[1];


--T1L21 is date_main:inst4|autodate:b2v_inst|always0~582
--operation mode is normal

T1L21 = T1L01 & T1L11 # !S31_safe_q[3] # !T1L01 & !T1L2 & !S31_safe_q[3];


--T1L31 is date_main:inst4|autodate:b2v_inst|always0~583
--operation mode is normal

T1L31 = !S51_safe_q[1] & !S51_safe_q[2] & S51_safe_q[3] $ T1_month1[0];


--T1L13 is date_main:inst4|autodate:b2v_inst|month1[2]~198
--operation mode is normal

T1L13 = !S51_safe_q[3] & !T1_month1[0];


--T1L4 is date_main:inst4|autodate:b2v_inst|always0~118
--operation mode is normal

T1L4 = S51_safe_q[0] & T1L31 # !S51_safe_q[0] & S51_safe_q[2] & T1L13;


--T1L71 is date_main:inst4|autodate:b2v_inst|day0[2]~463
--operation mode is normal

T1L71 = T1L9 & !T1L4;


--T1L41 is date_main:inst4|autodate:b2v_inst|always0~584
--operation mode is normal

T1L41 = T1L2 # S31_safe_q[3] & !T1L11;


--T1L81 is date_main:inst4|autodate:b2v_inst|day0[2]~464
--operation mode is normal

T1L81 = !T1L61 & T1L71 & !T1L21 # !T1L71 & T1L41;


--T1L3 is date_main:inst4|autodate:b2v_inst|always0~24
--operation mode is normal

T1L3 = S51_safe_q[0] # S51_safe_q[2] # !T1L13 # !S51_safe_q[1];


--T1L51 is date_main:inst4|autodate:b2v_inst|day0[0]~adv_mux_opt_ce_267
--operation mode is normal

T1L51 = !D1_DateSet_EN & T1L4 # !T1L3 # !T1L9;


--V1L2 is date_main:inst4|setdate:b2v_inst2|LessThan~146
--operation mode is normal

V1L2 = S61_safe_q[3] & S61_safe_q[0] # S61_safe_q[1] # S61_safe_q[2];


--U1L4 is date_main:inst4|datecontrol:b2v_inst1|Decoder~17
--operation mode is normal

U1L4 = V1_disp_drive[1] & V1_disp_drive[0];


--T1L52 is date_main:inst4|autodate:b2v_inst|month0[3]~522
--operation mode is normal

T1L52 = S51_safe_q[1] # S51_safe_q[3] & S51_safe_q[0] # T1_month1[0];


--T1L62 is date_main:inst4|autodate:b2v_inst|month0[3]~523
--operation mode is normal

T1L62 = !T1L13 & !T1L71 & S51_safe_q[2] # T1L52;


--T1L92 is date_main:inst4|autodate:b2v_inst|month1[0]~199
--operation mode is normal

T1L92 = !D1_DateSet_EN & T1L9 # !T1L7;


--T1L03 is date_main:inst4|autodate:b2v_inst|month1[0]~adv_mux_opt_ce_287
--operation mode is normal

T1L03 = T1L2 & T1L62 & T1L92;


--V1L3 is date_main:inst4|setdate:b2v_inst2|LessThan~199
--operation mode is normal

V1L3 = S91_safe_q[1] # S91_safe_q[2] # S91_safe_q[3];


--U1L1 is date_main:inst4|datecontrol:b2v_inst1|Decoder~14
--operation mode is normal

U1L1 = !V1_disp_drive[1] & !V1_disp_drive[0];


--T1L22 is date_main:inst4|autodate:b2v_inst|day1[1]~703
--operation mode is normal

T1L22 = S41_safe_q[1] & S41_safe_q[0] # T1L71 # !T1L5;


--T1L91 is date_main:inst4|autodate:b2v_inst|day1[0]~704
--operation mode is normal

T1L91 = T1L9 & T1L4 & !T1L41 # !T1L9 & T1L7 # !T1L41;


--T1L02 is date_main:inst4|autodate:b2v_inst|day1[0]~705
--operation mode is normal

T1L02 = T1L21 # T1L3;


--T1L12 is date_main:inst4|autodate:b2v_inst|day1[0]~706
--operation mode is normal

T1L12 = !D1_DateSet_EN & !T1L91 & !T1L02 # !T1L71;


--V1L4 is date_main:inst4|setdate:b2v_inst2|LessThan~200
--operation mode is normal

V1L4 = S71_safe_q[2] # S71_safe_q[3] # S71_safe_q[0] & S71_safe_q[1];


--U1L3 is date_main:inst4|datecontrol:b2v_inst1|Decoder~16
--operation mode is normal

U1L3 = V1_disp_drive[1] & !V1_disp_drive[0];


--T1L32 is date_main:inst4|autodate:b2v_inst|month0[0]~524
--operation mode is normal

T1L32 = T1L71 & T1L01 # T1L3 # !T1L92;


--T1L42 is date_main:inst4|autodate:b2v_inst|month0[0]~525
--operation mode is normal

T1L42 = !T1L32 & T1L2 # S31_safe_q[3] & T1L71;


--V1L1 is date_main:inst4|setdate:b2v_inst2|LessThan~114
--operation mode is normal

V1L1 = S81_safe_q[3] & S81_safe_q[0] # S81_safe_q[1] # S81_safe_q[2];


--U1L2 is date_main:inst4|datecontrol:b2v_inst1|Decoder~15
--operation mode is normal

U1L2 = V1_disp_drive[0] & !V1_disp_drive[1];


--W1_safe_q[1] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[1]
--operation mode is arithmetic

W1_safe_q[1]_carry_eqn = W1L2;
W1_safe_q[1]_lut_out = W1_safe_q[1] $ (W1_safe_q[1]_carry_eqn);
W1_safe_q[1] = DFFEAS(W1_safe_q[1]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L4 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

W1L4 = CARRY(!W1L2 # !W1_safe_q[1]);


--W1_safe_q[0] is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|safe_q[0]
--operation mode is arithmetic

W1_safe_q[0]_lut_out = !W1_safe_q[0];
W1_safe_q[0] = DFFEAS(W1_safe_q[0]_lut_out, Clock, VCC, , , , , F1L2, );

--W1L2 is fdiv:inst5|lpm_counter:CNT1_rtl_27|cntr_jd7:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

W1L2 = CARRY(W1_safe_q[0]);


--SW2 is SW2
--operation mode is input

SW2 = INPUT();


--SW3 is SW3
--operation mode is input

SW3 = INPUT();


--SW1 is SW1
--operation mode is input

SW1 = INPUT();


--Clock is Clock
--operation mode is input

Clock = INPUT();


--alarm is alarm
--operation mode is output

alarm = OUTPUT(!J1_alarm);


--disp_data[6] is disp_data[6]
--operation mode is output

disp_data[6] = OUTPUT(!H1L68);


--disp_data[5] is disp_data[5]
--operation mode is output

disp_data[5] = OUTPUT(!H1L78);


--disp_data[4] is disp_data[4]
--operation mode is output

disp_data[4] = OUTPUT(!H1L88);


--disp_data[3] is disp_data[3]
--operation mode is output

disp_data[3] = OUTPUT(!H1L66);


--disp_data[2] is disp_data[2]
--operation mode is output

disp_data[2] = OUTPUT(!H1L56);


--disp_data[1] is disp_data[1]
--operation mode is output

disp_data[1] = OUTPUT(!H1L46);


--disp_data[0] is disp_data[0]
--operation mode is output

disp_data[0] = OUTPUT(H1L36);


--disp_select[5] is disp_select[5]
--operation mode is output

disp_select[5] = OUTPUT(H1_disp_select[5]);


--disp_select[4] is disp_select[4]
--operation mode is output

disp_select[4] = OUTPUT(H1_disp_select[4]);


--disp_select[3] is disp_select[3]
--operation mode is output

disp_select[3] = OUTPUT(H1_disp_select[3]);


--disp_select[2] is disp_select[2]
--operation mode is output

disp_select[2] = OUTPUT(H1_disp_select[2]);


--disp_select[1] is disp_select[1]
--operation mode is output

disp_select[1] = OUTPUT(H1_disp_select[1]);


--disp_select[0] is disp_select[0]
--operation mode is output

disp_select[0] = OUTPUT(H1_disp_select[0]);


