--lpm_counter DEVICE_FAMILY="Stratix" lpm_direction="UP" lpm_width=32 clock q sclr
--VERSION_BEGIN 4.2 cbx_cycloneii 2004:08:25:19:39:42:SJ cbx_lpm_add_sub 2004:10:25:10:56:48:SJ cbx_lpm_compare 2004:10:18:11:29:46:SJ cbx_lpm_counter 2004:10:25:23:03:40:SJ cbx_lpm_decode 2004:08:15:21:16:20:SJ cbx_mgl 2004:10:26:10:32:18:SJ cbx_stratix 2004:09:23:18:28:34:SJ cbx_stratixii 2004:08:10:15:01:36:SJ  VERSION_END


--  Copyright (C) 1988-2002 Altera Corporation
--  Any  megafunction  design,  and related netlist (encrypted  or  decrypted),
--  support information,  device programming or simulation file,  and any other
--  associated  documentation or information  provided by  Altera  or a partner
--  under  Altera's   Megafunction   Partnership   Program  may  be  used  only
--  to program  PLD  devices (but not masked  PLD  devices) from  Altera.   Any
--  other  use  of such  megafunction  design,  netlist,  support  information,
--  device programming or simulation file,  or any other  related documentation
--  or information  is prohibited  for  any  other purpose,  including, but not
--  limited to  modification,  reverse engineering,  de-compiling, or use  with
--  any other  silicon devices,  unless such use is  explicitly  licensed under
--  a separate agreement with  Altera  or a megafunction partner.  Title to the
--  intellectual property,  including patents,  copyrights,  trademarks,  trade
--  secrets,  or maskworks,  embodied in any such megafunction design, netlist,
--  support  information,  device programming or simulation file,  or any other
--  related documentation or information provided by  Altera  or a megafunction
--  partner, remains with Altera, the megafunction partner, or their respective
--  licensors. No other licenses, including any licenses needed under any third
--  party's intellectual property, are provided herein.


FUNCTION stratix_lcell (aclr, aload, cin, clk, dataa, datab, datac, datad, ena, inverta, regcascin, sclr, sload)
WITH ( 	cin_used,	lut_mask,	operation_mode,	output_mode,	register_cascade_mode,	sum_lutc_input,	synch_mode) 
RETURNS ( combout, cout, regout);

--synthesis_resources = lut 32 
SUBDESIGN cntr_jd7
( 
	clock	:	input;
	cout	:	output;
	q[31..0]	:	output;
	sclr	:	input;
) 
VARIABLE 
	counter_cella0 : stratix_lcell
		WITH (
			cin_used = "false",
			lut_mask = "11AA",
			operation_mode = "arithmetic",
			synch_mode = "on"
		);
	counter_cella1 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella2 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella3 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella4 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella5 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella6 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella7 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella8 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella9 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella10 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella11 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella12 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella13 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella14 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella15 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella16 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella17 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella18 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella19 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella20 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella21 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella22 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella23 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella24 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella25 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella26 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella27 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella28 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella29 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella30 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	counter_cella31 : stratix_lcell
		WITH (
			cin_used = "true",
			lut_mask = "12A0",
			operation_mode = "arithmetic",
			sum_lutc_input = "cin",
			synch_mode = "on"
		);
	a_val[31..0]	: WIRE;
	aclr	: NODE;
	aclr_actual	: WIRE;
	aset_node	: WIRE;
	clk_en	: NODE;
	data[31..0]	: NODE;
	s_val[31..0]	: WIRE;
	safe_q[31..0]	: WIRE;
	sload	: NODE;
	sset_node	: WIRE;
	time_to_clear	: WIRE;
	updownDir	: WIRE;

BEGIN 
	counter_cella[31..0].aclr = aclr_actual;
	counter_cella[31..0].aload = B"00000000000000000000000000000000";
	counter_cella[1].cin = counter_cella[0].cout;
	counter_cella[2].cin = counter_cella[1].cout;
	counter_cella[3].cin = counter_cella[2].cout;
	counter_cella[4].cin = counter_cella[3].cout;
	counter_cella[5].cin = counter_cella[4].cout;
	counter_cella[6].cin = counter_cella[5].cout;
	counter_cella[7].cin = counter_cella[6].cout;
	counter_cella[8].cin = counter_cella[7].cout;
	counter_cella[9].cin = counter_cella[8].cout;
	counter_cella[10].cin = counter_cella[9].cout;
	counter_cella[11].cin = counter_cella[10].cout;
	counter_cella[12].cin = counter_cella[11].cout;
	counter_cella[13].cin = counter_cella[12].cout;
	counter_cella[14].cin = counter_cella[13].cout;
	counter_cella[15].cin = counter_cella[14].cout;
	counter_cella[16].cin = counter_cella[15].cout;
	counter_cella[17].cin = counter_cella[16].cout;
	counter_cella[18].cin = counter_cella[17].cout;
	counter_cella[19].cin = counter_cella[18].cout;
	counter_cella[20].cin = counter_cella[19].cout;
	counter_cella[21].cin = counter_cella[20].cout;
	counter_cella[22].cin = counter_cella[21].cout;
	counter_cella[23].cin = counter_cella[22].cout;
	counter_cella[24].cin = counter_cella[23].cout;
	counter_cella[25].cin = counter_cella[24].cout;
	counter_cella[26].cin = counter_cella[25].cout;
	counter_cella[27].cin = counter_cella[26].cout;
	counter_cella[28].cin = counter_cella[27].cout;
	counter_cella[29].cin = counter_cella[28].cout;
	counter_cella[30].cin = counter_cella[29].cout;
	counter_cella[31].cin = counter_cella[30].cout;
	counter_cella[31..0].clk = clock;
	counter_cella[31..0].dataa = safe_q[];
	counter_cella[31..0].datab = B"00000000000000000000000000000000";
	counter_cella[31..0].datac = data[];
	counter_cella[31..0].ena = clk_en;
	counter_cella[31..0].sclr = sclr;
	counter_cella[31..0].sload = sload;
	a_val[] = B"11111111111111111111111111111111";
	aclr = GND;
	aclr_actual = aclr;
	aset_node = B"0";
	clk_en = VCC;
	cout = counter_cella[31].cout;
	data[] = GND;
	q[] = safe_q[];
	s_val[] = B"11111111111111111111111111111111";
	safe_q[] = counter_cella[31..0].regout;
	sload = GND;
	sset_node = B"0";
	time_to_clear = B"0";
	updownDir = B"1";
END;
--VALID FILE
