--disp_drive[0] is disp_drive[0] at LC18
disp_drive[0]_or_out = EN;
disp_drive[0]_reg_input = disp_drive[0]_or_out;
disp_drive[0] = TFFE(disp_drive[0]_reg_input, SW1, , , );


--disp_drive[1] is disp_drive[1] at LC19
disp_drive[1]_p1_out = !disp_drive[2] & disp_drive[0] & EN;
disp_drive[1]_p2_out = disp_drive[0] & EN & disp_drive[1];
disp_drive[1]_or_out = disp_drive[1]_p1_out # disp_drive[1]_p2_out;
disp_drive[1]_reg_input = disp_drive[1]_or_out;
disp_drive[1] = TFFE(disp_drive[1]_reg_input, SW1, , , );


--disp_drive[2] is disp_drive[2] at LC20
disp_drive[2]_p1_out = disp_drive[1] & disp_drive[0] & EN;
disp_drive[2]_p2_out = disp_drive[0] & EN & disp_drive[2];
disp_drive[2]_or_out = disp_drive[2]_p1_out # disp_drive[2]_p2_out;
disp_drive[2]_reg_input = disp_drive[2]_or_out;
disp_drive[2] = TFFE(disp_drive[2]_reg_input, SW1, , , );


--A1L91Q is alarmclock_disp_select[4]~reg0 at LC6
A1L91Q_p1_out = disp_drive[0] & !disp_drive[2] & !disp_drive[1];
A1L91Q_or_out = A1L91Q_p1_out;
A1L91Q_reg_input = A1L91Q_or_out;
A1L91Q = DFFE(A1L91Q_reg_input, GLOBAL(clk_200hz), , , );


--A1L51Q is alarmclock_disp_select[2]~reg0 at LC5
A1L51Q_p1_out = !disp_drive[2] & disp_drive[0] & disp_drive[1];
A1L51Q_or_out = A1L51Q_p1_out;
A1L51Q_reg_input = A1L51Q_or_out;
A1L51Q = DFFE(A1L51Q_reg_input, GLOBAL(clk_200hz), , , );


--B3_dffs[1] is lpm_counter:minute_set0_rtl_2|dffs[1] at LC37
B3_dffs[1]_p1_out = !B3_dffs[3] & B3_dffs[0] & !B3_dffs[1];
B3_dffs[1]_p2_out = !B3_dffs[3] & !B3_dffs[0] & B3_dffs[1];
B3_dffs[1]_or_out = B3_dffs[1]_p1_out # B3_dffs[1]_p2_out;
B3_dffs[1]_reg_input = B3_dffs[1]_or_out;
B3_dffs[1]_p3_out = !disp_drive[2] & disp_drive[0] & disp_drive[1];
B3_dffs[1] = DFFE(B3_dffs[1]_reg_input, GLOBAL(SW2), , , B3_dffs[1]_p3_out);


--B1_dffs[1] is lpm_counter:hour_set0_rtl_4|dffs[1] at LC23
B1_dffs[1]_p0_out = !B1_dffs[3] & !B1_dffs[0] & B1_dffs[1] & !B1_dffs[2] & !B2_dffs[0];
B1_dffs[1]_p1_out = !B2_dffs[1] & !B1_dffs[3] & B1_dffs[0] & !B1_dffs[1];
B1_dffs[1]_p2_out = !B2_dffs[1] & !B1_dffs[3] & !B1_dffs[0] & B1_dffs[1];
B1_dffs[1]_p4_out = !B1_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & !B2_dffs[0];
B1_dffs[1]_or_out = B1_dffs[1]_p0_out # B1_dffs[1]_p1_out # B1_dffs[1]_p2_out # B1_dffs[1]_p4_out;
B1_dffs[1]_reg_input = B1_dffs[1]_or_out;
B1_dffs[1]_p3_out = disp_drive[0] & !disp_drive[2] & !disp_drive[1];
B1_dffs[1] = DFFE(B1_dffs[1]_reg_input, GLOBAL(SW2), , , B1_dffs[1]_p3_out);


--A1L12Q is alarmclock_disp_select[5]~reg0 at LC4
A1L12Q_p1_out = !disp_drive[1] & !disp_drive[0] & !disp_drive[2];
A1L12Q_or_out = A1L12Q_p1_out;
A1L12Q_reg_input = A1L12Q_or_out;
A1L12Q = DFFE(A1L12Q_reg_input, GLOBAL(clk_200hz), , , );


--A1L71Q is alarmclock_disp_select[3]~reg0 at LC3
A1L71Q_p1_out = disp_drive[1] & !disp_drive[0] & !disp_drive[2];
A1L71Q_or_out = A1L71Q_p1_out;
A1L71Q_reg_input = A1L71Q_or_out;
A1L71Q = DFFE(A1L71Q_reg_input, GLOBAL(clk_200hz), , , );


--A1L31Q is alarmclock_disp_select[1]~reg0 at LC2
A1L31Q_p1_out = !disp_drive[0] & disp_drive[2] & !disp_drive[1];
A1L31Q_or_out = A1L31Q_p1_out;
A1L31Q_reg_input = A1L31Q_or_out;
A1L31Q = DFFE(A1L31Q_reg_input, GLOBAL(clk_200hz), , , );


--A1L11Q is alarmclock_disp_select[0]~reg0 at LC1
A1L11Q_p1_out = disp_drive[0] & disp_drive[2] & !disp_drive[1];
A1L11Q_or_out = A1L11Q_p1_out;
A1L11Q_reg_input = A1L11Q_or_out;
A1L11Q = DFFE(A1L11Q_reg_input, GLOBAL(clk_200hz), , , );


--B5_dffs[1] is lpm_counter:second_set0_rtl_0|dffs[1] at LC8
B5_dffs[1]_p1_out = !B5_dffs[3] & B5_dffs[0] & !B5_dffs[1];
B5_dffs[1]_p2_out = !B5_dffs[3] & !B5_dffs[0] & B5_dffs[1];
B5_dffs[1]_or_out = B5_dffs[1]_p1_out # B5_dffs[1]_p2_out;
B5_dffs[1]_reg_input = B5_dffs[1]_or_out;
B5_dffs[1]_p3_out = disp_drive[0] & disp_drive[2] & !disp_drive[1];
B5_dffs[1] = DFFE(B5_dffs[1]_reg_input, GLOBAL(SW2), , , B5_dffs[1]_p3_out);


--B6_dffs[1] is lpm_counter:second_set1_rtl_1|dffs[1] at LC11
B6_dffs[1]_p1_out = !B6_dffs[2] & B6_dffs[0] & !B6_dffs[1];
B6_dffs[1]_p2_out = !B6_dffs[2] & !B6_dffs[0] & B6_dffs[1];
B6_dffs[1]_or_out = B6_dffs[1]_p1_out # B6_dffs[1]_p2_out;
B6_dffs[1]_reg_input = B6_dffs[1]_or_out;
B6_dffs[1]_p3_out = !disp_drive[0] & disp_drive[2] & !disp_drive[1];
B6_dffs[1] = DFFE(B6_dffs[1]_reg_input, GLOBAL(SW2), , , B6_dffs[1]_p3_out);


--B4_dffs[1] is lpm_counter:minute_set1_rtl_3|dffs[1] at LC42
B4_dffs[1]_p1_out = !B4_dffs[2] & B4_dffs[0] & !B4_dffs[1];
B4_dffs[1]_p2_out = !B4_dffs[2] & !B4_dffs[0] & B4_dffs[1];
B4_dffs[1]_or_out = B4_dffs[1]_p1_out # B4_dffs[1]_p2_out;
B4_dffs[1]_reg_input = B4_dffs[1]_or_out;
B4_dffs[1]_p3_out = disp_drive[1] & !disp_drive[0] & !disp_drive[2];
B4_dffs[1] = DFFE(B4_dffs[1]_reg_input, GLOBAL(SW2), , , B4_dffs[1]_p3_out);


--B2_dffs[0] is lpm_counter:hour_set1_rtl_5|dffs[0] at LC26
B2_dffs[0]_p1_out = !B2_dffs[0] & !B2_dffs[1];
B2_dffs[0]_or_out = B2_dffs[0]_p1_out;
B2_dffs[0]_reg_input = B2_dffs[0]_or_out;
B2_dffs[0]_p3_out = !disp_drive[1] & !disp_drive[0] & !disp_drive[2];
B2_dffs[0] = DFFE(B2_dffs[0]_reg_input, GLOBAL(SW2), , , B2_dffs[0]_p3_out);


--B2_dffs[1] is lpm_counter:hour_set1_rtl_5|dffs[1] at LC27
B2_dffs[1]_p1_out = B2_dffs[0] & !B2_dffs[1];
B2_dffs[1]_or_out = B2_dffs[1]_p1_out;
B2_dffs[1]_reg_input = B2_dffs[1]_or_out;
B2_dffs[1]_p3_out = !disp_drive[1] & !disp_drive[0] & !disp_drive[2];
B2_dffs[1] = DFFE(B2_dffs[1]_reg_input, GLOBAL(SW2), , , B2_dffs[1]_p3_out);


--B3_dffs[2] is lpm_counter:minute_set0_rtl_2|dffs[2] at LC44
B3_dffs[2]_p1_out = !B3_dffs[3] & B3_dffs[0] & B3_dffs[1];
B3_dffs[2]_p2_out = B3_dffs[3] & B3_dffs[2];
B3_dffs[2]_or_out = B3_dffs[2]_p1_out # B3_dffs[2]_p2_out;
B3_dffs[2]_reg_input = B3_dffs[2]_or_out;
B3_dffs[2]_p3_out = !disp_drive[2] & disp_drive[0] & disp_drive[1];
B3_dffs[2] = TFFE(B3_dffs[2]_reg_input, GLOBAL(SW2), , , B3_dffs[2]_p3_out);


--B1_dffs[2] is lpm_counter:hour_set0_rtl_4|dffs[2] at LC29
B1_dffs[2]_p0_out = !B1_dffs[3] & !B1_dffs[2] & B1_dffs[0] & B1_dffs[1] & !B2_dffs[0];
B1_dffs[2]_p1_out = !B2_dffs[1] & !B1_dffs[3] & B1_dffs[2] & !B1_dffs[0];
B1_dffs[2]_p2_out = !B2_dffs[1] & !B1_dffs[3] & B1_dffs[2] & !B1_dffs[1];
B1_dffs[2]_p4_out = !B2_dffs[1] & !B1_dffs[3] & !B1_dffs[2] & B1_dffs[0] & B1_dffs[1];
B1_dffs[2]_or_out = B1_dffs[2]_p0_out # B1_dffs[2]_p1_out # B1_dffs[2]_p2_out # B1_dffs[2]_p4_out;
B1_dffs[2]_reg_input = B1_dffs[2]_or_out;
B1_dffs[2]_p3_out = disp_drive[0] & !disp_drive[2] & !disp_drive[1];
B1_dffs[2] = DFFE(B1_dffs[2]_reg_input, GLOBAL(SW2), , , B1_dffs[2]_p3_out);


--B5_dffs[2] is lpm_counter:second_set0_rtl_0|dffs[2] at LC14
B5_dffs[2]_p1_out = !B5_dffs[3] & B5_dffs[0] & B5_dffs[1];
B5_dffs[2]_p2_out = B5_dffs[3] & B5_dffs[2];
B5_dffs[2]_or_out = B5_dffs[2]_p1_out # B5_dffs[2]_p2_out;
B5_dffs[2]_reg_input = B5_dffs[2]_or_out;
B5_dffs[2]_p3_out = disp_drive[0] & disp_drive[2] & !disp_drive[1];
B5_dffs[2] = TFFE(B5_dffs[2]_reg_input, GLOBAL(SW2), , , B5_dffs[2]_p3_out);


--B6_dffs[2] is lpm_counter:second_set1_rtl_1|dffs[2] at LC15
B6_dffs[2]_p1_out = B6_dffs[0] & B6_dffs[1] & !B6_dffs[2];
B6_dffs[2]_p2_out = !B6_dffs[0] & !B6_dffs[1] & B6_dffs[2];
B6_dffs[2]_or_out = B6_dffs[2]_p1_out # B6_dffs[2]_p2_out;
B6_dffs[2]_reg_input = B6_dffs[2]_or_out;
B6_dffs[2]_p3_out = !disp_drive[0] & disp_drive[2] & !disp_drive[1];
B6_dffs[2] = DFFE(B6_dffs[2]_reg_input, GLOBAL(SW2), , , B6_dffs[2]_p3_out);


--B4_dffs[2] is lpm_counter:minute_set1_rtl_3|dffs[2] at LC34
B4_dffs[2]_p1_out = B4_dffs[0] & B4_dffs[1] & !B4_dffs[2];
B4_dffs[2]_p2_out = !B4_dffs[0] & !B4_dffs[1] & B4_dffs[2];
B4_dffs[2]_or_out = B4_dffs[2]_p1_out # B4_dffs[2]_p2_out;
B4_dffs[2]_reg_input = B4_dffs[2]_or_out;
B4_dffs[2]_p3_out = disp_drive[1] & !disp_drive[0] & !disp_drive[2];
B4_dffs[2] = DFFE(B4_dffs[2]_reg_input, GLOBAL(SW2), , , B4_dffs[2]_p3_out);


--B6_dffs[0] is lpm_counter:second_set1_rtl_1|dffs[0] at LC13
B6_dffs[0]_p1_out = B6_dffs[2] & B6_dffs[1] & !B6_dffs[0];
B6_dffs[0]_or_out = B6_dffs[0]_p1_out;
B6_dffs[0]_reg_input = !B6_dffs[0]_or_out;
B6_dffs[0]_p3_out = !disp_drive[0] & disp_drive[2] & !disp_drive[1];
B6_dffs[0] = TFFE(B6_dffs[0]_reg_input, GLOBAL(SW2), , , B6_dffs[0]_p3_out);


--B3_dffs[3] is lpm_counter:minute_set0_rtl_2|dffs[3] at LC35
B3_dffs[3]_p1_out = B3_dffs[0] & B3_dffs[1] & B3_dffs[2] & !B3_dffs[3];
B3_dffs[3]_p2_out = !B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2] & B3_dffs[3];
B3_dffs[3]_or_out = B3_dffs[3]_p1_out # B3_dffs[3]_p2_out;
B3_dffs[3]_reg_input = B3_dffs[3]_or_out;
B3_dffs[3]_p3_out = !disp_drive[2] & disp_drive[0] & disp_drive[1];
B3_dffs[3] = DFFE(B3_dffs[3]_reg_input, GLOBAL(SW2), , , B3_dffs[3]_p3_out);


--B4_dffs[0] is lpm_counter:minute_set1_rtl_3|dffs[0] at LC41
B4_dffs[0]_p1_out = B4_dffs[2] & B4_dffs[1] & !B4_dffs[0];
B4_dffs[0]_or_out = B4_dffs[0]_p1_out;
B4_dffs[0]_reg_input = !B4_dffs[0]_or_out;
B4_dffs[0]_p3_out = disp_drive[1] & !disp_drive[0] & !disp_drive[2];
B4_dffs[0] = TFFE(B4_dffs[0]_reg_input, GLOBAL(SW2), , , B4_dffs[0]_p3_out);


--B1_dffs[3] is lpm_counter:hour_set0_rtl_4|dffs[3] at LC25
B1_dffs[3]_p1_out = !B2_dffs[1] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[0] & !B1_dffs[1];
B1_dffs[3]_p2_out = !B2_dffs[1] & !B1_dffs[3] & B1_dffs[2] & B1_dffs[0] & B1_dffs[1];
B1_dffs[3]_or_out = B1_dffs[3]_p1_out # B1_dffs[3]_p2_out;
B1_dffs[3]_reg_input = B1_dffs[3]_or_out;
B1_dffs[3]_p3_out = disp_drive[0] & !disp_drive[2] & !disp_drive[1];
B1_dffs[3] = DFFE(B1_dffs[3]_reg_input, GLOBAL(SW2), , , B1_dffs[3]_p3_out);


--B5_dffs[3] is lpm_counter:second_set0_rtl_0|dffs[3] at LC16
B5_dffs[3]_p1_out = B5_dffs[0] & B5_dffs[1] & B5_dffs[2] & !B5_dffs[3];
B5_dffs[3]_p2_out = !B5_dffs[0] & !B5_dffs[1] & !B5_dffs[2] & B5_dffs[3];
B5_dffs[3]_or_out = B5_dffs[3]_p1_out # B5_dffs[3]_p2_out;
B5_dffs[3]_reg_input = B5_dffs[3]_or_out;
B5_dffs[3]_p3_out = disp_drive[0] & disp_drive[2] & !disp_drive[1];
B5_dffs[3] = DFFE(B5_dffs[3]_reg_input, GLOBAL(SW2), , , B5_dffs[3]_p3_out);


--B3_dffs[0] is lpm_counter:minute_set0_rtl_2|dffs[0] at LC33
B3_dffs[0]_p1_out = !B3_dffs[0] & !B3_dffs[3];
B3_dffs[0]_p2_out = !B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2];
B3_dffs[0]_or_out = B3_dffs[0]_p1_out # B3_dffs[0]_p2_out;
B3_dffs[0]_reg_input = B3_dffs[0]_or_out;
B3_dffs[0]_p3_out = !disp_drive[2] & disp_drive[0] & disp_drive[1];
B3_dffs[0] = DFFE(B3_dffs[0]_reg_input, GLOBAL(SW2), , , B3_dffs[0]_p3_out);


--B5_dffs[0] is lpm_counter:second_set0_rtl_0|dffs[0] at LC7
B5_dffs[0]_p1_out = !B5_dffs[0] & !B5_dffs[3];
B5_dffs[0]_p2_out = !B5_dffs[0] & !B5_dffs[1] & !B5_dffs[2];
B5_dffs[0]_or_out = B5_dffs[0]_p1_out # B5_dffs[0]_p2_out;
B5_dffs[0]_reg_input = B5_dffs[0]_or_out;
B5_dffs[0]_p3_out = disp_drive[0] & disp_drive[2] & !disp_drive[1];
B5_dffs[0] = DFFE(B5_dffs[0]_reg_input, GLOBAL(SW2), , , B5_dffs[0]_p3_out);


--B1_dffs[0] is lpm_counter:hour_set0_rtl_4|dffs[0] at LC17
B1_dffs[0]_p1_out = !B1_dffs[1] & !B2_dffs[1] & !B1_dffs[0] & !B1_dffs[2];
B1_dffs[0]_p2_out = !B2_dffs[1] & !B1_dffs[0] & !B1_dffs[3];
B1_dffs[0]_p4_out = !B1_dffs[0] & !B1_dffs[2] & !B1_dffs[3] & !B2_dffs[0];
B1_dffs[0]_or_out = B1_dffs[0]_p1_out # B1_dffs[0]_p2_out # B1_dffs[0]_p4_out;
B1_dffs[0]_reg_input = B1_dffs[0]_or_out;
B1_dffs[0]_p3_out = disp_drive[0] & !disp_drive[2] & !disp_drive[1];
B1_dffs[0] = DFFE(B1_dffs[0]_reg_input, GLOBAL(SW2), , , B1_dffs[0]_p3_out);


--A1L03 is always0~68 at LC38
A1L03_or_out = minute0[1];
A1L03 = B3_dffs[1] $ A1L03_or_out;


--A1L13 is always0~72 at LC39
A1L13_or_out = minute0[2];
A1L13 = B3_dffs[2] $ A1L13_or_out;


--A1L23 is always0~76 at LC40
A1L23_or_out = minute0[3];
A1L23 = B3_dffs[3] $ A1L23_or_out;


--A1L33 is always0~80 at LC43
A1L33_or_out = minute1[0];
A1L33 = B4_dffs[0] $ A1L33_or_out;


--A1L43 is always0~84 at LC36
A1L43_or_out = minute1[1];
A1L43 = B4_dffs[1] $ A1L43_or_out;


--A1L53 is always0~88 at LC48
A1L53_or_out = minute1[2];
A1L53 = B4_dffs[2] $ A1L53_or_out;


--A1L63 is always0~92 at LC21
A1L63_or_out = hour0[0];
A1L63 = B1_dffs[0] $ A1L63_or_out;


--A1L73 is always0~96 at LC28
A1L73_or_out = hour0[1];
A1L73 = B1_dffs[1] $ A1L73_or_out;


--A1L83 is always0~100 at LC24
A1L83_or_out = hour0[2];
A1L83 = B1_dffs[2] $ A1L83_or_out;


--A1L93 is always0~104 at LC32
A1L93_or_out = hour0[3];
A1L93 = B1_dffs[3] $ A1L93_or_out;


--A1L04 is always0~108 at LC31
A1L04_or_out = hour1[0];
A1L04 = B2_dffs[0] $ A1L04_or_out;


--A1L14 is always0~112 at LC30
A1L14_or_out = hour1[1];
A1L14 = B2_dffs[1] $ A1L14_or_out;


--A1L24 is always0~117 at LC49
A1L24_p1_out = !second1[3] & !A1L03 & !A1L13 & !A1L23 & !A1L33 & !A1L43 & !A1L53 & !minute1[3] & !A1L63 & !A1L73 & !A1L83 & !A1L93 & !A1L04 & !A1L14 & !hour1[2] & !hour1[3] & A1L22 & A1L15 & A1L32 & A1L25 & A1L42 & A1L35 & A1L52 & A1L45 & A1L62 & A1L55 & A1L72 & A1L65 & A1L82 & A1L75 & A1L92 & A1L85;
A1L24_or_out = A1L24_p1_out;
A1L24 = A1L24_or_out;


--A1L22 is always0~36sexp at SEXP57
A1L22 = EXP(B5_dffs[0] & !second0[0]);


--A1L15 is always0~126 at SEXP58
A1L15 = EXP(!B5_dffs[0] & second0[0]);


--A1L32 is always0~40sexp at SEXP59
A1L32 = EXP(B5_dffs[1] & !second0[1]);


--A1L25 is always0~127 at SEXP60
A1L25 = EXP(!B5_dffs[1] & second0[1]);


--A1L42 is always0~44sexp at SEXP61
A1L42 = EXP(B5_dffs[2] & !second0[2]);


--A1L35 is always0~128 at SEXP62
A1L35 = EXP(!B5_dffs[2] & second0[2]);


--A1L52 is always0~48sexp at SEXP63
A1L52 = EXP(B5_dffs[3] & !second0[3]);


--A1L45 is always0~129 at SEXP64
A1L45 = EXP(!B5_dffs[3] & second0[3]);


--A1L62 is always0~52sexp at SEXP56
A1L62 = EXP(B6_dffs[0] & !second1[0]);


--A1L55 is always0~130 at SEXP55
A1L55 = EXP(!B6_dffs[0] & second1[0]);


--A1L72 is always0~56sexp at SEXP54
A1L72 = EXP(B6_dffs[1] & !second1[1]);


--A1L65 is always0~131 at SEXP53
A1L65 = EXP(!B6_dffs[1] & second1[1]);


--A1L82 is always0~60sexp at SEXP52
A1L82 = EXP(B6_dffs[2] & !second1[2]);


--A1L75 is always0~132 at SEXP51
A1L75 = EXP(!B6_dffs[2] & second1[2]);


--A1L92 is always0~64sexp at SEXP50
A1L92 = EXP(B3_dffs[0] & !minute0[0]);


--A1L85 is always0~133 at SEXP49
A1L85 = EXP(!B3_dffs[0] & minute0[0]);


--clk_200hz is clk_200hz at PIN_87
--operation mode is input

clk_200hz = INPUT();


--EN is EN at PIN_46
--operation mode is input

EN = INPUT();


--SW1 is SW1 at PIN_47
--operation mode is input

SW1 = INPUT();


--SW2 is SW2 at PIN_90
--operation mode is input

SW2 = INPUT();


--hour1[3] is hour1[3] at PIN_25
--operation mode is input

hour1[3] = INPUT();


--hour1[2] is hour1[2] at PIN_97
--operation mode is input

hour1[2] = INPUT();


--hour1[1] is hour1[1] at PIN_19
--operation mode is input

hour1[1] = INPUT();


--hour1[0] is hour1[0] at PIN_17
--operation mode is input

hour1[0] = INPUT();


--hour0[3] is hour0[3] at PIN_93
--operation mode is input

hour0[3] = INPUT();


--hour0[2] is hour0[2] at PIN_92
--operation mode is input

hour0[2] = INPUT();


--hour0[1] is hour0[1] at PIN_42
--operation mode is input

hour0[1] = INPUT();


--hour0[0] is hour0[0] at PIN_44
--operation mode is input

hour0[0] = INPUT();


--minute1[3] is minute1[3] at PIN_96
--operation mode is input

minute1[3] = INPUT();


--minute1[2] is minute1[2] at PIN_6
--operation mode is input

minute1[2] = INPUT();


--minute1[1] is minute1[1] at PIN_29
--operation mode is input

minute1[1] = INPUT();


--minute1[0] is minute1[0] at PIN_60
--operation mode is input

minute1[0] = INPUT();


--minute0[3] is minute0[3] at PIN_94
--operation mode is input

minute0[3] = INPUT();


--minute0[2] is minute0[2] at PIN_84
--operation mode is input

minute0[2] = INPUT();


--minute0[1] is minute0[1] at PIN_16
--operation mode is input

minute0[1] = INPUT();


--minute0[0] is minute0[0] at PIN_61
--operation mode is input

minute0[0] = INPUT();


--second1[3] is second1[3] at PIN_85
--operation mode is input

second1[3] = INPUT();


--second1[2] is second1[2] at PIN_58
--operation mode is input

second1[2] = INPUT();


--second1[1] is second1[1] at PIN_83
--operation mode is input

second1[1] = INPUT();


--second1[0] is second1[0] at PIN_45
--operation mode is input

second1[0] = INPUT();


--second0[3] is second0[3] at PIN_32
--operation mode is input

second0[3] = INPUT();


--second0[2] is second0[2] at PIN_31
--operation mode is input

second0[2] = INPUT();


--second0[1] is second0[1] at PIN_81
--operation mode is input

second0[1] = INPUT();


--second0[0] is second0[0] at PIN_48
--operation mode is input

second0[0] = INPUT();


--alarmclock_disp_select[4] is alarmclock_disp_select[4] at PIN_8
--operation mode is output

alarmclock_disp_select[4] = OUTPUT(A1L91Q);


--alarmclock_disp_select[2] is alarmclock_disp_select[2] at PIN_9
--operation mode is output

alarmclock_disp_select[2] = OUTPUT(A1L51Q);


--alarmclock_disp_select[5] is alarmclock_disp_select[5] at PIN_10
--operation mode is output

alarmclock_disp_select[5] = OUTPUT(A1L12Q);


--alarmclock_disp_select[3] is alarmclock_disp_select[3] at PIN_12
--operation mode is output

alarmclock_disp_select[3] = OUTPUT(A1L71Q);


--alarmclock_disp_select[1] is alarmclock_disp_select[1] at PIN_13
--operation mode is output

alarmclock_disp_select[1] = OUTPUT(A1L31Q);


--alarmclock_disp_select[0] is alarmclock_disp_select[0] at PIN_14
--operation mode is output

alarmclock_disp_select[0] = OUTPUT(A1L11Q);


--alarm is alarm at PIN_63
--operation mode is output

alarm = OUTPUT(A1L24);






