--A1L22 is always0~3 at LC3
A1L22_p1_out = !Reset & !En;
A1L22_or_out = A1L22_p1_out;
A1L22 = !(A1L22_or_out);


--A1L51 is Now_Floor_Disp_Data~119 at LC5
A1L51_p1_out = !Now_Floor[1] & !Reset & !En & Now_Floor[3] & !Now_Floor[2];
A1L51_p2_out = !Reset & !En & !Now_Floor[3] & Now_Floor[0];
A1L51_p3_out = !Reset & !En & !Now_Floor[3] & Now_Floor[2];
A1L51_or_out = A1L51_p1_out # A1L51_p2_out # A1L51_p3_out;
A1L51 = A1L51_or_out;


--A1L32 is reduce_or~1077 at LC6
A1L32_p1_out = !Now_Floor[0] & !Now_Floor[2] & Now_Floor[3] & !Now_Floor[1] & !Reset & !En;
A1L32_p2_out = !Now_Floor[0] & !Now_Floor[3] & Now_Floor[1] & !Reset & !En;
A1L32_or_out = A1L32_p1_out # A1L32_p2_out;
A1L32 = A1L32_or_out;


--A1L42 is reduce_or~1083 at LC7
A1L42_p0_out = !Reset & !En & Now_Floor[2] & !Now_Floor[3] & !Now_Floor[1] & !Now_Floor[0];
A1L42_p1_out = !Reset & !En & !Now_Floor[2] & !Now_Floor[3] & Now_Floor[1];
A1L42_p2_out = !Reset & !En & !Now_Floor[2] & !Now_Floor[3] & Now_Floor[0];
A1L42_p3_out = !Reset & !En & !Now_Floor[3] & Now_Floor[1] & Now_Floor[0];
A1L42_p4_out = !Reset & !En & !Now_Floor[2] & Now_Floor[3] & !Now_Floor[1];
A1L42_or_out = A1L42_p0_out # A1L42_p1_out # A1L42_p2_out # A1L42_p3_out # A1L42_p4_out;
A1L42 = A1L42_or_out;


--A1L52 is reduce_or~1088 at LC8
A1L52_p1_out = Now_Floor[2] & Now_Floor[0] & !Now_Floor[3] & !Now_Floor[1] & !Reset & !En;
A1L52_p2_out = !Now_Floor[2] & !Now_Floor[3] & Now_Floor[1] & !Reset & !En;
A1L52_p3_out = !Now_Floor[2] & !Now_Floor[0] & Now_Floor[3] & !Now_Floor[1] & !Reset & !En;
A1L52_p4_out = !Now_Floor[0] & !Now_Floor[3] & Now_Floor[1] & !Reset & !En;
A1L52_or_out = A1L52_p1_out # A1L52_p2_out # A1L52_p3_out # A1L52_p4_out;
A1L52 = A1L52_or_out;


--A1L62 is reduce_or~1092 at LC10
A1L62_p1_out = !Now_Floor[0] & !Reset & !En & Now_Floor[2] & !Now_Floor[3];
A1L62_p2_out = !Reset & !En & !Now_Floor[2] & Now_Floor[3] & !Now_Floor[1];
A1L62_p3_out = !Reset & !En & Now_Floor[2] & !Now_Floor[3] & !Now_Floor[1];
A1L62_or_out = A1L62_p1_out # A1L62_p2_out # A1L62_p3_out;
A1L62 = A1L62_or_out;


--A1L72 is reduce_or~1096 at LC2
A1L72_p1_out = !Now_Floor[3] & !Reset & !En & Now_Floor[1];
A1L72_p2_out = !Now_Floor[3] & !Reset & !En & Now_Floor[2] & Now_Floor[0];
A1L72_p3_out = Now_Floor[3] & !Reset & !En & !Now_Floor[1] & !Now_Floor[2];
A1L72_or_out = A1L72_p1_out # A1L72_p2_out # A1L72_p3_out;
A1L72 = A1L72_or_out;


--A1L82 is reduce_or~1101 at LC1
A1L82_p1_out = !Reset & !En & !Now_Floor[2] & !Now_Floor[3] & Now_Floor[1];
A1L82_p2_out = !Reset & !En & !Now_Floor[2] & Now_Floor[3] & !Now_Floor[1];
A1L82_p3_out = !Reset & !En & !Now_Floor[3] & Now_Floor[1] & !Now_Floor[0];
A1L82_p4_out = !Reset & !En & Now_Floor[2] & !Now_Floor[3] & !Now_Floor[1];
A1L82_or_out = A1L82_p1_out # A1L82_p2_out # A1L82_p3_out # A1L82_p4_out;
A1L82 = A1L82_or_out;


--Reset is Reset at PIN_24
--operation mode is input

Reset = INPUT();


--En is En at PIN_40
--operation mode is input

En = INPUT();


--Now_Floor[3] is Now_Floor[3] at PIN_21
--operation mode is input

Now_Floor[3] = INPUT();


--Now_Floor[2] is Now_Floor[2] at PIN_16
--operation mode is input

Now_Floor[2] = INPUT();


--Now_Floor[1] is Now_Floor[1] at PIN_33
--operation mode is input

Now_Floor[1] = INPUT();


--Now_Floor[0] is Now_Floor[0] at PIN_36
--operation mode is input

Now_Floor[0] = INPUT();


--Now_Floor_Disp_Select is Now_Floor_Disp_Select at PIN_6
--operation mode is output

Now_Floor_Disp_Select = OUTPUT(A1L22);


--Now_Floor_Disp_Data[4] is Now_Floor_Disp_Data[4] at PIN_8
--operation mode is output

Now_Floor_Disp_Data[4] = OUTPUT(A1L51);


--Now_Floor_Disp_Data[2] is Now_Floor_Disp_Data[2] at PIN_9
--operation mode is output

Now_Floor_Disp_Data[2] = OUTPUT(A1L32);


--Now_Floor_Disp_Data[5] is Now_Floor_Disp_Data[5] at PIN_11
--operation mode is output

Now_Floor_Disp_Data[5] = OUTPUT(A1L42);


--Now_Floor_Disp_Data[3] is Now_Floor_Disp_Data[3] at PIN_12
--operation mode is output

Now_Floor_Disp_Data[3] = OUTPUT(A1L52);


--Now_Floor_Disp_Data[1] is Now_Floor_Disp_Data[1] at PIN_14
--operation mode is output

Now_Floor_Disp_Data[1] = OUTPUT(A1L62);


--Now_Floor_Disp_Data[6] is Now_Floor_Disp_Data[6] at PIN_5
--operation mode is output

Now_Floor_Disp_Data[6] = OUTPUT(A1L72);


--Now_Floor_Disp_Data[0] is Now_Floor_Disp_Data[0] at PIN_4
--operation mode is output

Now_Floor_Disp_Data[0] = OUTPUT(A1L82);






