--A1L71Q is disp_select[0]~reg0
A1L71Q_p1_out = A1L91Q & A1L12Q & !A1L71Q;
A1L71Q_or_out = A1L71Q_p1_out;
A1L71Q_reg_input = !A1L71Q_or_out;
A1L71Q = TFFE(A1L71Q_reg_input, GLOBAL(clk), , , );


--A1L91Q is disp_select[1]~reg0
A1L91Q_p1_out = !A1L12Q & A1L91Q & !A1L71Q;
A1L91Q_p2_out = !A1L12Q & !A1L91Q & A1L71Q;
A1L91Q_or_out = A1L91Q_p1_out # A1L91Q_p2_out;
A1L91Q_reg_input = A1L91Q_or_out;
A1L91Q = DFFE(A1L91Q_reg_input, GLOBAL(clk), , , );


--A1L12Q is disp_select[2]~reg0
A1L12Q_p1_out = !A1L91Q & !A1L12Q;
A1L12Q_p2_out = !A1L12Q & !A1L71Q;
A1L12Q_p3_out = !A1L91Q & !A1L71Q;
A1L12Q_or_out = A1L12Q_p1_out # A1L12Q_p2_out # A1L12Q_p3_out;
A1L12Q_reg_input = !A1L12Q_or_out;
A1L12Q = TFFE(A1L12Q_reg_input, GLOBAL(clk), , , );


--A1L31Q is Q[5]~reg0
A1L31Q_p1_out = !A1L12Q & !A1L91Q & !A1L71Q;
A1L31Q_or_out = A1L31Q_p1_out;
A1L31Q_reg_input = A1L31Q_or_out;
A1L31Q = DFFE(A1L31Q_reg_input, GLOBAL(clk), , , );


--A1L11Q is Q[4]~reg0
A1L11Q_p1_out = !A1L12Q & !A1L91Q & A1L71Q;
A1L11Q_or_out = A1L11Q_p1_out;
A1L11Q_reg_input = A1L11Q_or_out;
A1L11Q = DFFE(A1L11Q_reg_input, GLOBAL(clk), , , );


--A1L9Q is Q[3]~reg0
A1L9Q_p1_out = !A1L12Q & A1L91Q & !A1L71Q;
A1L9Q_or_out = A1L9Q_p1_out;
A1L9Q_reg_input = A1L9Q_or_out;
A1L9Q = DFFE(A1L9Q_reg_input, GLOBAL(clk), , , );


--A1L7Q is Q[2]~reg0
A1L7Q_p1_out = !A1L12Q & A1L91Q & A1L71Q;
A1L7Q_or_out = A1L7Q_p1_out;
A1L7Q_reg_input = A1L7Q_or_out;
A1L7Q = DFFE(A1L7Q_reg_input, GLOBAL(clk), , , );


--A1L5Q is Q[1]~reg0
A1L5Q_p1_out = A1L12Q & !A1L91Q & !A1L71Q;
A1L5Q_or_out = A1L5Q_p1_out;
A1L5Q_reg_input = A1L5Q_or_out;
A1L5Q = DFFE(A1L5Q_reg_input, GLOBAL(clk), , , );


--A1L3Q is Q[0]~reg0
A1L3Q_p1_out = A1L12Q & !A1L91Q & A1L71Q;
A1L3Q_or_out = A1L3Q_p1_out;
A1L3Q_reg_input = A1L3Q_or_out;
A1L3Q = DFFE(A1L3Q_reg_input, GLOBAL(clk), , , );


--clk is clk
--operation mode is input

clk = INPUT();


--disp_select[0] is disp_select[0]
--operation mode is output

disp_select[0] = OUTPUT(A1L71Q);


--disp_select[1] is disp_select[1]
--operation mode is output

disp_select[1] = OUTPUT(A1L91Q);


--disp_select[2] is disp_select[2]
--operation mode is output

disp_select[2] = OUTPUT(A1L12Q);


--Q[5] is Q[5]
--operation mode is output

Q[5] = OUTPUT(A1L31Q);


--Q[4] is Q[4]
--operation mode is output

Q[4] = OUTPUT(A1L11Q);


--Q[3] is Q[3]
--operation mode is output

Q[3] = OUTPUT(A1L9Q);


--Q[2] is Q[2]
--operation mode is output

Q[2] = OUTPUT(A1L7Q);


--Q[1] is Q[1]
--operation mode is output

Q[1] = OUTPUT(A1L5Q);


--Q[0] is Q[0]
--operation mode is output

Q[0] = OUTPUT(A1L3Q);


