 -- Copyright (C) 1991-2004 Altera Corporation
 -- Any  megafunction  design,  and related netlist (encrypted  or  decrypted),
 -- support information,  device programming or simulation file,  and any other
 -- associated  documentation or information  provided by  Altera  or a partner
 -- under  Altera's   Megafunction   Partnership   Program  may  be  used  only
 -- to program  PLD  devices (but not masked  PLD  devices) from  Altera.   Any
 -- other  use  of such  megafunction  design,  netlist,  support  information,
 -- device programming or simulation file,  or any other  related documentation
 -- or information  is prohibited  for  any  other purpose,  including, but not
 -- limited to  modification,  reverse engineering,  de-compiling, or use  with
 -- any other  silicon devices,  unless such use is  explicitly  licensed under
 -- a separate agreement with  Altera  or a megafunction partner.  Title to the
 -- intellectual property,  including patents,  copyrights,  trademarks,  trade
 -- secrets,  or maskworks,  embodied in any such megafunction design, netlist,
 -- support  information,  device programming or simulation file,  or any other
 -- related documentation or information provided by  Altera  or a megafunction
 -- partner, remains with Altera, the megafunction partner, or their respective
 -- licensors. No other licenses, including any licenses needed under any third
 -- party's intellectual property, are provided herein.
 -- 
 -- This is a Quartus II output file. It is for reporting purposes only, and is
 -- not intended for use as a Quartus II input file. This file cannot be used
 -- to make Quartus II pin assignments - for instructions on how to make pin
 -- assignments, please see Quartus II help.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- NC            : No Connect. This pin has no internal connection to the device.
 -- VCC           : Dedicated power pin, which MUST be connected to VCC.
 -- VCCIO         : Dedicated power pin, which MUST be connected to VCC
 --                 of its bank.
 -- GND           : Dedicated ground pin. Dedicated GND pins MUST be connected to GND.
 --					It can also be used to report unused dedicated pins. The connection
 --					on the board for unused dedicated pins depends on whether this will
 --					be used in a future design. One example is device migration. When
 --					using device migration, refer to the device pin-tables. If it is a
 --					GND pin in the pin table or if it will not be used in a future design
 --					for another purpose the it MUST be connected to GND. If it is an unused
 --					dedicated pin, then it can be connected to a valid signal on the board
 --					(low, high, or toggling) if that signal is required for a different
 --					revision of the design.
 -- GND+          : Unused input pin. It can also be used to report unused dual-purpose pins.
 --					This pin should be connected to GND. It may also be connected  to a
 --					valid signal  on the board  (low, high, or toggling)  if that signal
 --					is required for a different revision of the design.
 -- GND*          : Unused  I/O  pin.   This pin can either be left unconnected or
 --           	    connected to GND.  Connecting this pin to GND will improve the
 --           	    device's immunity to noise.
 -- RESERVED      : Unused I/O pin, which MUST be left unconnected.
 -- RESERVED_INPUT    : Pin is tri-stated and should be connected to the board.
 -- NON_MIGRATABLE: This pin cannot be migrated.
 ---------------------------------------------------------------------------------

Quartus II Version 4.2 Build 157 12/07/2004 SJ Full Version
CHIP  "Data_Mux"  ASSIGNED TO AN: EPM7032SLC44-5

Pin Name/Usage               : Location  : Dir.   : I/O Standard      : Voltage : I/O Bank  : User Assignment
-------------------------------------------------------------------------------------------------------------
GND+                         : 1         :        :                   :         :           :                
GND+                         : 2         :        :                   :         :           :                
VCC                          : 3         : power  :                   :         :           :                
Y_1                          : 4         : output : TTL               :         :           : N              
Y_2                          : 5         : output : TTL               :         :           : N              
RESERVED                     : 6         :        :                   :         :           :                
TDI                          : 7         : input  : TTL               :         :           : N              
RESERVED                     : 8         :        :                   :         :           :                
RESERVED                     : 9         :        :                   :         :           :                
GND                          : 10        : gnd    :                   :         :           :                
G1_L                         : 11        : input  : TTL               :         :           : N              
B                            : 12        : input  : TTL               :         :           : N              
TMS                          : 13        : input  : TTL               :         :           : N              
RESERVED                     : 14        :        :                   :         :           :                
VCC                          : 15        : power  :                   :         :           :                
C1_0                         : 16        : input  : TTL               :         :           : N              
RESERVED                     : 17        :        :                   :         :           :                
C1_2                         : 18        : input  : TTL               :         :           : N              
C1_3                         : 19        : input  : TTL               :         :           : N              
C2_0                         : 20        : input  : TTL               :         :           : N              
C2_2                         : 21        : input  : TTL               :         :           : N              
GND                          : 22        : gnd    :                   :         :           :                
VCC                          : 23        : power  :                   :         :           :                
C2_3                         : 24        : input  : TTL               :         :           : N              
C2_1                         : 25        : input  : TTL               :         :           : N              
RESERVED                     : 26        :        :                   :         :           :                
RESERVED                     : 27        :        :                   :         :           :                
C1_1                         : 28        : input  : TTL               :         :           : N              
RESERVED                     : 29        :        :                   :         :           :                
GND                          : 30        : gnd    :                   :         :           :                
RESERVED                     : 31        :        :                   :         :           :                
TCK                          : 32        : input  : TTL               :         :           : N              
A                            : 33        : input  : TTL               :         :           : N              
G2_L                         : 34        : input  : TTL               :         :           : N              
VCC                          : 35        : power  :                   :         :           :                
RESERVED                     : 36        :        :                   :         :           :                
RESERVED                     : 37        :        :                   :         :           :                
TDO                          : 38        : output : TTL               :         :           : N              
RESERVED                     : 39        :        :                   :         :           :                
RESERVED                     : 40        :        :                   :         :           :                
RESERVED                     : 41        :        :                   :         :           :                
GND                          : 42        : gnd    :                   :         :           :                
GND+                         : 43        :        :                   :         :           :                
GND+                         : 44        :        :                   :         :           :                
