--A1L9 is EO~28 at LC1
A1L9_p1_out = !EN & I6 & I5 & I7 & I1 & I2 & I4 & I3 & I0;
A1L9_or_out = A1L9_p1_out;
A1L9 = !(A1L9_or_out);


--A1L6 is A2~31 at LC2
A1L6_p1_out = I4 & I6 & I7 & I5;
A1L6_or_out = A1L6_p1_out # EN;
A1L6 = A1L6_or_out;


--A1L2 is A0~96 at LC3
A1L2_p1_out = !I4 & I5 & I7;
A1L2_p2_out = I5 & I7 & I1 & I3;
A1L2_p3_out = I5 & I7 & I3 & !I2;
A1L2_p4_out = I7 & !I6;
A1L2_or_out = EN # A1L2_p1_out # A1L2_p2_out # A1L2_p3_out # A1L2_p4_out;
A1L2 = A1L2_or_out;


--A1L11 is GS~24 at LC5
A1L11_p1_out = I5 & I6 & I7 & I1 & I2 & I4 & I3 & I0;
A1L11_or_out = A1L11_p1_out # EN;
A1L11 = A1L11_or_out;


--A1L4 is A1~98 at LC6
A1L4_p1_out = !I5 & I7 & I6;
A1L4_p2_out = I7 & I6 & I2 & I3;
A1L4_p3_out = I7 & I6 & !I4;
A1L4_or_out = A1L4_p1_out # A1L4_p2_out # A1L4_p3_out # EN;
A1L4 = A1L4_or_out;


--EN is EN at PIN_36
--operation mode is input

EN = INPUT();


--I0 is I0 at PIN_11
--operation mode is input

I0 = INPUT();


--I1 is I1 at PIN_33
--operation mode is input

I1 = INPUT();


--I2 is I2 at PIN_24
--operation mode is input

I2 = INPUT();


--I3 is I3 at PIN_21
--operation mode is input

I3 = INPUT();


--I4 is I4 at PIN_20
--operation mode is input

I4 = INPUT();


--I5 is I5 at PIN_28
--operation mode is input

I5 = INPUT();


--I6 is I6 at PIN_16
--operation mode is input

I6 = INPUT();


--I7 is I7 at PIN_12
--operation mode is input

I7 = INPUT();


--EO is EO at PIN_4
--operation mode is output

EO = OUTPUT(A1L9);


--A2 is A2 at PIN_5
--operation mode is output

A2 = OUTPUT(A1L6);


--A0 is A0 at PIN_6
--operation mode is output

A0 = OUTPUT(A1L2);


--GS is GS at PIN_8
--operation mode is output

GS = OUTPUT(A1L11);


--A1 is A1 at PIN_9
--operation mode is output

A1 = OUTPUT(A1L4);






