--A1L5 is Sample_Ctrl_out~15 at LC2_A17
--operation mode is normal

A1L5 = Adc_Busy # Reset # En;


--Adc_Busy is Adc_Busy at PIN_91
--operation mode is input

Adc_Busy = INPUT();


--Reset is Reset at PIN_89
--operation mode is input

Reset = INPUT();


--En is En at PIN_38
--operation mode is input

En = INPUT();


--Sample_Ctrl_out is Sample_Ctrl_out at PIN_6
--operation mode is output

Sample_Ctrl_out = OUTPUT(!A1L5);


