--B1_dffs[0] is lpm_counter:CNT_rtl_0|dffs[0] at LC2
B1_dffs[0]_p1_out = !B1_dffs[0] & !B1_dffs[3];
B1_dffs[0]_p2_out = !B1_dffs[0] & !B1_dffs[2] & !B1_dffs[1];
B1_dffs[0]_or_out = B1_dffs[0]_p1_out # B1_dffs[0]_p2_out;
B1_dffs[0]_reg_input = B1_dffs[0]_or_out;
B1_dffs[0] = DFFE(B1_dffs[0]_reg_input, GLOBAL(Clock_In), , , );


--B1_dffs[1] is lpm_counter:CNT_rtl_0|dffs[1] at LC3
B1_dffs[1]_p1_out = !B1_dffs[3] & B1_dffs[1] & !B1_dffs[0];
B1_dffs[1]_p2_out = !B1_dffs[3] & !B1_dffs[1] & B1_dffs[0];
B1_dffs[1]_or_out = B1_dffs[1]_p1_out # B1_dffs[1]_p2_out;
B1_dffs[1]_reg_input = B1_dffs[1]_or_out;
B1_dffs[1] = DFFE(B1_dffs[1]_reg_input, GLOBAL(Clock_In), , , );


--B1_dffs[2] is lpm_counter:CNT_rtl_0|dffs[2] at LC4
B1_dffs[2]_p1_out = !B1_dffs[3] & B1_dffs[1] & B1_dffs[0];
B1_dffs[2]_p2_out = B1_dffs[3] & B1_dffs[2];
B1_dffs[2]_or_out = B1_dffs[2]_p1_out # B1_dffs[2]_p2_out;
B1_dffs[2]_reg_input = B1_dffs[2]_or_out;
B1_dffs[2] = TFFE(B1_dffs[2]_reg_input, GLOBAL(Clock_In), , , );


--B1_dffs[3] is lpm_counter:CNT_rtl_0|dffs[3] at LC5
B1_dffs[3]_p1_out = B1_dffs[2] & B1_dffs[1] & B1_dffs[0] & !B1_dffs[3];
B1_dffs[3]_p2_out = !B1_dffs[2] & !B1_dffs[1] & !B1_dffs[0] & B1_dffs[3];
B1_dffs[3]_or_out = B1_dffs[3]_p1_out # B1_dffs[3]_p2_out;
B1_dffs[3]_reg_input = B1_dffs[3]_or_out;
B1_dffs[3] = DFFE(B1_dffs[3]_reg_input, GLOBAL(Clock_In), , , );


--A1L3Q is Clock_Out~reg0 at LC1
A1L3Q_p1_out = !B1_dffs[2] & !B1_dffs[1] & !B1_dffs[0];
A1L3Q_or_out = A1L3Q_p1_out # !B1_dffs[3];
A1L3Q_reg_input = !(A1L3Q_or_out);
A1L3Q = DFFE(A1L3Q_reg_input, GLOBAL(Clock_In), , , );


--Clock_In is Clock_In at PIN_43
--operation mode is input

Clock_In = INPUT();


--Clock_Out is Clock_Out at PIN_4
--operation mode is output

Clock_Out = OUTPUT(A1L3Q);






