--A1L6Q is Serial_Out[1]~reg0 at LC10
A1L6Q_p1_out = A1L4Q & !A1L6Q & !A1L8Q & !A1L41Q & !A1L21Q & !A1L01Q;
A1L6Q_or_out = A1L6Q_p1_out;
A1L6Q_reg_input = A1L6Q_or_out;
A1L6Q = DFFE(A1L6Q_reg_input, GLOBAL(Clock), , , );


--A1L01Q is Serial_Out[3]~reg0 at LC8
A1L01Q_p1_out = A1L4Q & A1L6Q & !A1L8Q & !A1L41Q & !A1L21Q & !A1L01Q;
A1L01Q_or_out = A1L01Q_p1_out;
A1L01Q_reg_input = A1L01Q_or_out;
A1L01Q = DFFE(A1L01Q_reg_input, GLOBAL(Clock), , , );


--A1L8Q is Serial_Out[2]~reg0 at LC7
A1L8Q_p1_out = !A1L4Q & A1L6Q & !A1L8Q & !A1L41Q & !A1L21Q & !A1L01Q;
A1L8Q_or_out = A1L8Q_p1_out;
A1L8Q_reg_input = A1L8Q_or_out;
A1L8Q = DFFE(A1L8Q_reg_input, GLOBAL(Clock), , , );


--A1L41Q is Serial_Out[5]~reg0 at LC6
A1L41Q_p1_out = A1L4Q & !A1L6Q & A1L8Q & !A1L41Q & !A1L21Q & !A1L01Q;
A1L41Q_or_out = A1L41Q_p1_out;
A1L41Q_reg_input = A1L41Q_or_out;
A1L41Q = DFFE(A1L41Q_reg_input, GLOBAL(Clock), , , );


--A1L21Q is Serial_Out[4]~reg0 at LC5
A1L21Q_p1_out = !A1L4Q & !A1L6Q & A1L8Q & !A1L41Q & !A1L21Q & !A1L01Q;
A1L21Q_or_out = A1L21Q_p1_out;
A1L21Q_reg_input = A1L21Q_or_out;
A1L21Q = DFFE(A1L21Q_reg_input, GLOBAL(Clock), , , );


--A1L4Q is Serial_Out[0]~reg0 at LC3
A1L4Q_p1_out = !A1L4Q & !A1L6Q & !A1L8Q & !A1L41Q & !A1L21Q & !A1L01Q & !A1L81Q;
A1L4Q_p2_out = !A1L4Q & !A1L6Q & !A1L8Q & !A1L41Q & !A1L21Q & !A1L01Q & A1L61Q;
A1L4Q_or_out = A1L4Q_p1_out # A1L4Q_p2_out;
A1L4Q_reg_input = A1L4Q_or_out;
A1L4Q = DFFE(A1L4Q_reg_input, GLOBAL(Clock), , , );


--A1L61Q is Serial_Out[6]~reg0 at LC2
A1L61Q_p1_out = !A1L4Q & A1L6Q & A1L8Q & !A1L41Q & !A1L21Q & !A1L01Q;
A1L61Q_or_out = A1L61Q_p1_out;
A1L61Q_reg_input = A1L61Q_or_out;
A1L61Q = DFFE(A1L61Q_reg_input, GLOBAL(Clock), , , );


--A1L81Q is Serial_Out[7]~reg0 at LC1
A1L81Q_p1_out = A1L81Q & !A1L61Q & !A1L4Q & !A1L6Q & !A1L8Q & !A1L41Q & !A1L21Q & !A1L01Q;
A1L81Q_p2_out = A1L4Q & A1L6Q & A1L8Q & !A1L41Q & !A1L21Q & !A1L01Q;
A1L81Q_or_out = A1L81Q_p2_out;
A1L81Q_reg_input = A1L81Q_p1_out $ A1L81Q_or_out;
A1L81Q = DFFE(A1L81Q_reg_input, GLOBAL(Clock), , , );


--Clock is Clock at PIN_43
--operation mode is input

Clock = INPUT();


--Serial_Out[1] is Serial_Out[1] at PIN_14
--operation mode is output

Serial_Out[1] = OUTPUT(A1L6Q);


--Serial_Out[3] is Serial_Out[3] at PIN_12
--operation mode is output

Serial_Out[3] = OUTPUT(A1L01Q);


--Serial_Out[2] is Serial_Out[2] at PIN_11
--operation mode is output

Serial_Out[2] = OUTPUT(A1L8Q);


--Serial_Out[5] is Serial_Out[5] at PIN_9
--operation mode is output

Serial_Out[5] = OUTPUT(A1L41Q);


--Serial_Out[4] is Serial_Out[4] at PIN_8
--operation mode is output

Serial_Out[4] = OUTPUT(A1L21Q);


--Serial_Out[0] is Serial_Out[0] at PIN_6
--operation mode is output

Serial_Out[0] = OUTPUT(A1L4Q);


--Serial_Out[6] is Serial_Out[6] at PIN_5
--operation mode is output

Serial_Out[6] = OUTPUT(A1L61Q);


--Serial_Out[7] is Serial_Out[7] at PIN_4
--operation mode is output

Serial_Out[7] = OUTPUT(A1L81Q);






