--disp_drive[0] is disp_drive[0]
disp_drive[0]_or_out = EN;
disp_drive[0]_reg_input = disp_drive[0]_or_out;
disp_drive[0] = TFFE(disp_drive[0]_reg_input, SW1, , , );


--disp_drive[1] is disp_drive[1]
disp_drive[1]_p1_out = !disp_drive[2] & disp_drive[0] & EN;
disp_drive[1]_p2_out = disp_drive[0] & EN & disp_drive[1];
disp_drive[1]_or_out = disp_drive[1]_p1_out # disp_drive[1]_p2_out;
disp_drive[1]_reg_input = disp_drive[1]_or_out;
disp_drive[1] = TFFE(disp_drive[1]_reg_input, SW1, , , );


--disp_drive[2] is disp_drive[2]
disp_drive[2]_p1_out = disp_drive[1] & disp_drive[0] & EN;
disp_drive[2]_p2_out = disp_drive[0] & EN & disp_drive[2];
disp_drive[2]_or_out = disp_drive[2]_p1_out # disp_drive[2]_p2_out;
disp_drive[2]_reg_input = disp_drive[2]_or_out;
disp_drive[2] = TFFE(disp_drive[2]_reg_input, SW1, , , );


--A1L51Q is alarmclock_disp_select[4]~reg0
A1L51Q_p1_out = disp_drive[0] & !disp_drive[2] & !disp_drive[1];
A1L51Q_or_out = A1L51Q_p1_out;
A1L51Q_reg_input = A1L51Q_or_out;
A1L51Q = DFFE(A1L51Q_reg_input, GLOBAL(clk_200hz), , , );


--A1L11Q is alarmclock_disp_select[2]~reg0
A1L11Q_p1_out = !disp_drive[2] & disp_drive[0] & disp_drive[1];
A1L11Q_or_out = A1L11Q_p1_out;
A1L11Q_reg_input = A1L11Q_or_out;
A1L11Q = DFFE(A1L11Q_reg_input, GLOBAL(clk_200hz), , , );


--B3_dffs[1] is lpm_counter:minute_set0_rtl_2|dffs[1]
B3_dffs[1]_p1_out = !B3_dffs[3] & B3_dffs[0] & !B3_dffs[1];
B3_dffs[1]_p2_out = !B3_dffs[3] & !B3_dffs[0] & B3_dffs[1];
B3_dffs[1]_or_out = B3_dffs[1]_p1_out # B3_dffs[1]_p2_out;
B3_dffs[1]_reg_input = B3_dffs[1]_or_out;
B3_dffs[1]_p3_out = !disp_drive[2] & disp_drive[0] & disp_drive[1];
B3_dffs[1] = DFFE(B3_dffs[1]_reg_input, GLOBAL(SW2), , , B3_dffs[1]_p3_out);


--B1_dffs[1] is lpm_counter:hour_set0_rtl_4|dffs[1]
B1_dffs[1]_p0_out = !B1_dffs[3] & !B1_dffs[0] & B1_dffs[1] & !B1_dffs[2] & !B2_dffs[0];
B1_dffs[1]_p1_out = !B2_dffs[1] & !B1_dffs[3] & B1_dffs[0] & !B1_dffs[1];
B1_dffs[1]_p2_out = !B2_dffs[1] & !B1_dffs[3] & !B1_dffs[0] & B1_dffs[1];
B1_dffs[1]_p4_out = !B1_dffs[3] & B1_dffs[0] & !B1_dffs[1] & !B1_dffs[2] & !B2_dffs[0];
B1_dffs[1]_or_out = B1_dffs[1]_p0_out # B1_dffs[1]_p1_out # B1_dffs[1]_p2_out # B1_dffs[1]_p4_out;
B1_dffs[1]_reg_input = B1_dffs[1]_or_out;
B1_dffs[1]_p3_out = disp_drive[0] & !disp_drive[2] & !disp_drive[1];
B1_dffs[1] = DFFE(B1_dffs[1]_reg_input, GLOBAL(SW2), , , B1_dffs[1]_p3_out);


--A1L71Q is alarmclock_disp_select[5]~reg0
A1L71Q_p1_out = !disp_drive[1] & !disp_drive[0] & !disp_drive[2];
A1L71Q_or_out = A1L71Q_p1_out;
A1L71Q_reg_input = A1L71Q_or_out;
A1L71Q = DFFE(A1L71Q_reg_input, GLOBAL(clk_200hz), , , );


--A1L31Q is alarmclock_disp_select[3]~reg0
A1L31Q_p1_out = disp_drive[1] & !disp_drive[0] & !disp_drive[2];
A1L31Q_or_out = A1L31Q_p1_out;
A1L31Q_reg_input = A1L31Q_or_out;
A1L31Q = DFFE(A1L31Q_reg_input, GLOBAL(clk_200hz), , , );


--A1L9Q is alarmclock_disp_select[1]~reg0
A1L9Q_p1_out = !disp_drive[0] & disp_drive[2] & !disp_drive[1];
A1L9Q_or_out = A1L9Q_p1_out;
A1L9Q_reg_input = A1L9Q_or_out;
A1L9Q = DFFE(A1L9Q_reg_input, GLOBAL(clk_200hz), , , );


--A1L7Q is alarmclock_disp_select[0]~reg0
A1L7Q_p1_out = disp_drive[0] & disp_drive[2] & !disp_drive[1];
A1L7Q_or_out = A1L7Q_p1_out;
A1L7Q_reg_input = A1L7Q_or_out;
A1L7Q = DFFE(A1L7Q_reg_input, GLOBAL(clk_200hz), , , );


--B5_dffs[1] is lpm_counter:second_set0_rtl_0|dffs[1]
B5_dffs[1]_p1_out = !B5_dffs[3] & B5_dffs[0] & !B5_dffs[1];
B5_dffs[1]_p2_out = !B5_dffs[3] & !B5_dffs[0] & B5_dffs[1];
B5_dffs[1]_or_out = B5_dffs[1]_p1_out # B5_dffs[1]_p2_out;
B5_dffs[1]_reg_input = B5_dffs[1]_or_out;
B5_dffs[1]_p3_out = disp_drive[0] & disp_drive[2] & !disp_drive[1];
B5_dffs[1] = DFFE(B5_dffs[1]_reg_input, GLOBAL(SW2), , , B5_dffs[1]_p3_out);


--B6_dffs[1] is lpm_counter:second_set1_rtl_1|dffs[1]
B6_dffs[1]_p1_out = !B6_dffs[2] & B6_dffs[0] & !B6_dffs[1];
B6_dffs[1]_p2_out = !B6_dffs[2] & !B6_dffs[0] & B6_dffs[1];
B6_dffs[1]_or_out = B6_dffs[1]_p1_out # B6_dffs[1]_p2_out;
B6_dffs[1]_reg_input = B6_dffs[1]_or_out;
B6_dffs[1]_p3_out = !disp_drive[0] & disp_drive[2] & !disp_drive[1];
B6_dffs[1] = DFFE(B6_dffs[1]_reg_input, GLOBAL(SW2), , , B6_dffs[1]_p3_out);


--B4_dffs[1] is lpm_counter:minute_set1_rtl_3|dffs[1]
B4_dffs[1]_p1_out = !B4_dffs[2] & B4_dffs[0] & !B4_dffs[1];
B4_dffs[1]_p2_out = !B4_dffs[2] & !B4_dffs[0] & B4_dffs[1];
B4_dffs[1]_or_out = B4_dffs[1]_p1_out # B4_dffs[1]_p2_out;
B4_dffs[1]_reg_input = B4_dffs[1]_or_out;
B4_dffs[1]_p3_out = disp_drive[1] & !disp_drive[0] & !disp_drive[2];
B4_dffs[1] = DFFE(B4_dffs[1]_reg_input, GLOBAL(SW2), , , B4_dffs[1]_p3_out);


--B2_dffs[0] is lpm_counter:hour_set1_rtl_5|dffs[0]
B2_dffs[0]_p1_out = !B2_dffs[0] & !B2_dffs[1];
B2_dffs[0]_or_out = B2_dffs[0]_p1_out;
B2_dffs[0]_reg_input = B2_dffs[0]_or_out;
B2_dffs[0]_p3_out = !disp_drive[1] & !disp_drive[0] & !disp_drive[2];
B2_dffs[0] = DFFE(B2_dffs[0]_reg_input, GLOBAL(SW2), , , B2_dffs[0]_p3_out);


--B2_dffs[1] is lpm_counter:hour_set1_rtl_5|dffs[1]
B2_dffs[1]_p1_out = B2_dffs[0] & !B2_dffs[1];
B2_dffs[1]_or_out = B2_dffs[1]_p1_out;
B2_dffs[1]_reg_input = B2_dffs[1]_or_out;
B2_dffs[1]_p3_out = !disp_drive[1] & !disp_drive[0] & !disp_drive[2];
B2_dffs[1] = DFFE(B2_dffs[1]_reg_input, GLOBAL(SW2), , , B2_dffs[1]_p3_out);


--B3_dffs[2] is lpm_counter:minute_set0_rtl_2|dffs[2]
B3_dffs[2]_p1_out = !B3_dffs[3] & B3_dffs[0] & B3_dffs[1];
B3_dffs[2]_p2_out = B3_dffs[3] & B3_dffs[2];
B3_dffs[2]_or_out = B3_dffs[2]_p1_out # B3_dffs[2]_p2_out;
B3_dffs[2]_reg_input = B3_dffs[2]_or_out;
B3_dffs[2]_p3_out = !disp_drive[2] & disp_drive[0] & disp_drive[1];
B3_dffs[2] = TFFE(B3_dffs[2]_reg_input, GLOBAL(SW2), , , B3_dffs[2]_p3_out);


--B1_dffs[2] is lpm_counter:hour_set0_rtl_4|dffs[2]
B1_dffs[2]_p0_out = !B1_dffs[3] & !B1_dffs[2] & B1_dffs[0] & B1_dffs[1] & !B2_dffs[0];
B1_dffs[2]_p1_out = !B2_dffs[1] & !B1_dffs[3] & B1_dffs[2] & !B1_dffs[0];
B1_dffs[2]_p2_out = !B2_dffs[1] & !B1_dffs[3] & B1_dffs[2] & !B1_dffs[1];
B1_dffs[2]_p4_out = !B2_dffs[1] & !B1_dffs[3] & !B1_dffs[2] & B1_dffs[0] & B1_dffs[1];
B1_dffs[2]_or_out = B1_dffs[2]_p0_out # B1_dffs[2]_p1_out # B1_dffs[2]_p2_out # B1_dffs[2]_p4_out;
B1_dffs[2]_reg_input = B1_dffs[2]_or_out;
B1_dffs[2]_p3_out = disp_drive[0] & !disp_drive[2] & !disp_drive[1];
B1_dffs[2] = DFFE(B1_dffs[2]_reg_input, GLOBAL(SW2), , , B1_dffs[2]_p3_out);


--B5_dffs[2] is lpm_counter:second_set0_rtl_0|dffs[2]
B5_dffs[2]_p1_out = !B5_dffs[3] & B5_dffs[0] & B5_dffs[1];
B5_dffs[2]_p2_out = B5_dffs[3] & B5_dffs[2];
B5_dffs[2]_or_out = B5_dffs[2]_p1_out # B5_dffs[2]_p2_out;
B5_dffs[2]_reg_input = B5_dffs[2]_or_out;
B5_dffs[2]_p3_out = disp_drive[0] & disp_drive[2] & !disp_drive[1];
B5_dffs[2] = TFFE(B5_dffs[2]_reg_input, GLOBAL(SW2), , , B5_dffs[2]_p3_out);


--B6_dffs[2] is lpm_counter:second_set1_rtl_1|dffs[2]
B6_dffs[2]_p1_out = B6_dffs[0] & B6_dffs[1] & !B6_dffs[2];
B6_dffs[2]_p2_out = !B6_dffs[0] & !B6_dffs[1] & B6_dffs[2];
B6_dffs[2]_or_out = B6_dffs[2]_p1_out # B6_dffs[2]_p2_out;
B6_dffs[2]_reg_input = B6_dffs[2]_or_out;
B6_dffs[2]_p3_out = !disp_drive[0] & disp_drive[2] & !disp_drive[1];
B6_dffs[2] = DFFE(B6_dffs[2]_reg_input, GLOBAL(SW2), , , B6_dffs[2]_p3_out);


--B4_dffs[2] is lpm_counter:minute_set1_rtl_3|dffs[2]
B4_dffs[2]_p1_out = B4_dffs[0] & B4_dffs[1] & !B4_dffs[2];
B4_dffs[2]_p2_out = !B4_dffs[0] & !B4_dffs[1] & B4_dffs[2];
B4_dffs[2]_or_out = B4_dffs[2]_p1_out # B4_dffs[2]_p2_out;
B4_dffs[2]_reg_input = B4_dffs[2]_or_out;
B4_dffs[2]_p3_out = disp_drive[1] & !disp_drive[0] & !disp_drive[2];
B4_dffs[2] = DFFE(B4_dffs[2]_reg_input, GLOBAL(SW2), , , B4_dffs[2]_p3_out);


--B6_dffs[0] is lpm_counter:second_set1_rtl_1|dffs[0]
B6_dffs[0]_p1_out = B6_dffs[2] & B6_dffs[1] & !B6_dffs[0];
B6_dffs[0]_or_out = B6_dffs[0]_p1_out;
B6_dffs[0]_reg_input = !B6_dffs[0]_or_out;
B6_dffs[0]_p3_out = !disp_drive[0] & disp_drive[2] & !disp_drive[1];
B6_dffs[0] = TFFE(B6_dffs[0]_reg_input, GLOBAL(SW2), , , B6_dffs[0]_p3_out);


--B3_dffs[3] is lpm_counter:minute_set0_rtl_2|dffs[3]
B3_dffs[3]_p1_out = B3_dffs[0] & B3_dffs[1] & B3_dffs[2] & !B3_dffs[3];
B3_dffs[3]_p2_out = !B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2] & B3_dffs[3];
B3_dffs[3]_or_out = B3_dffs[3]_p1_out # B3_dffs[3]_p2_out;
B3_dffs[3]_reg_input = B3_dffs[3]_or_out;
B3_dffs[3]_p3_out = !disp_drive[2] & disp_drive[0] & disp_drive[1];
B3_dffs[3] = DFFE(B3_dffs[3]_reg_input, GLOBAL(SW2), , , B3_dffs[3]_p3_out);


--B4_dffs[0] is lpm_counter:minute_set1_rtl_3|dffs[0]
B4_dffs[0]_p1_out = B4_dffs[2] & B4_dffs[1] & !B4_dffs[0];
B4_dffs[0]_or_out = B4_dffs[0]_p1_out;
B4_dffs[0]_reg_input = !B4_dffs[0]_or_out;
B4_dffs[0]_p3_out = disp_drive[1] & !disp_drive[0] & !disp_drive[2];
B4_dffs[0] = TFFE(B4_dffs[0]_reg_input, GLOBAL(SW2), , , B4_dffs[0]_p3_out);


--B1_dffs[3] is lpm_counter:hour_set0_rtl_4|dffs[3]
B1_dffs[3]_p1_out = !B2_dffs[1] & B1_dffs[3] & !B1_dffs[2] & !B1_dffs[0] & !B1_dffs[1];
B1_dffs[3]_p2_out = !B2_dffs[1] & !B1_dffs[3] & B1_dffs[2] & B1_dffs[0] & B1_dffs[1];
B1_dffs[3]_or_out = B1_dffs[3]_p1_out # B1_dffs[3]_p2_out;
B1_dffs[3]_reg_input = B1_dffs[3]_or_out;
B1_dffs[3]_p3_out = disp_drive[0] & !disp_drive[2] & !disp_drive[1];
B1_dffs[3] = DFFE(B1_dffs[3]_reg_input, GLOBAL(SW2), , , B1_dffs[3]_p3_out);


--B5_dffs[3] is lpm_counter:second_set0_rtl_0|dffs[3]
B5_dffs[3]_p1_out = B5_dffs[0] & B5_dffs[1] & B5_dffs[2] & !B5_dffs[3];
B5_dffs[3]_p2_out = !B5_dffs[0] & !B5_dffs[1] & !B5_dffs[2] & B5_dffs[3];
B5_dffs[3]_or_out = B5_dffs[3]_p1_out # B5_dffs[3]_p2_out;
B5_dffs[3]_reg_input = B5_dffs[3]_or_out;
B5_dffs[3]_p3_out = disp_drive[0] & disp_drive[2] & !disp_drive[1];
B5_dffs[3] = DFFE(B5_dffs[3]_reg_input, GLOBAL(SW2), , , B5_dffs[3]_p3_out);


--B3_dffs[0] is lpm_counter:minute_set0_rtl_2|dffs[0]
B3_dffs[0]_p1_out = !B3_dffs[0] & !B3_dffs[3];
B3_dffs[0]_p2_out = !B3_dffs[0] & !B3_dffs[1] & !B3_dffs[2];
B3_dffs[0]_or_out = B3_dffs[0]_p1_out # B3_dffs[0]_p2_out;
B3_dffs[0]_reg_input = B3_dffs[0]_or_out;
B3_dffs[0]_p3_out = !disp_drive[2] & disp_drive[0] & disp_drive[1];
B3_dffs[0] = DFFE(B3_dffs[0]_reg_input, GLOBAL(SW2), , , B3_dffs[0]_p3_out);


--B5_dffs[0] is lpm_counter:second_set0_rtl_0|dffs[0]
B5_dffs[0]_p1_out = !B5_dffs[0] & !B5_dffs[3];
B5_dffs[0]_p2_out = !B5_dffs[0] & !B5_dffs[1] & !B5_dffs[2];
B5_dffs[0]_or_out = B5_dffs[0]_p1_out # B5_dffs[0]_p2_out;
B5_dffs[0]_reg_input = B5_dffs[0]_or_out;
B5_dffs[0]_p3_out = disp_drive[0] & disp_drive[2] & !disp_drive[1];
B5_dffs[0] = DFFE(B5_dffs[0]_reg_input, GLOBAL(SW2), , , B5_dffs[0]_p3_out);


--B1_dffs[0] is lpm_counter:hour_set0_rtl_4|dffs[0]
B1_dffs[0]_p1_out = !B1_dffs[1] & !B2_dffs[1] & !B1_dffs[0] & !B1_dffs[2];
B1_dffs[0]_p2_out = !B2_dffs[1] & !B1_dffs[0] & !B1_dffs[3];
B1_dffs[0]_p4_out = !B1_dffs[0] & !B1_dffs[2] & !B1_dffs[3] & !B2_dffs[0];
B1_dffs[0]_or_out = B1_dffs[0]_p1_out # B1_dffs[0]_p2_out # B1_dffs[0]_p4_out;
B1_dffs[0]_reg_input = B1_dffs[0]_or_out;
B1_dffs[0]_p3_out = disp_drive[0] & !disp_drive[2] & !disp_drive[1];
B1_dffs[0] = DFFE(B1_dffs[0]_reg_input, GLOBAL(SW2), , , B1_dffs[0]_p3_out);


--A1L62 is always0~68
A1L62_or_out = minute0[1];
A1L62 = B3_dffs[1] $ A1L62_or_out;


--A1L72 is always0~72
A1L72_or_out = minute0[2];
A1L72 = B3_dffs[2] $ A1L72_or_out;


--A1L82 is always0~76
A1L82_or_out = minute0[3];
A1L82 = B3_dffs[3] $ A1L82_or_out;


--A1L92 is always0~80
A1L92_or_out = minute1[0];
A1L92 = B4_dffs[0] $ A1L92_or_out;


--A1L03 is always0~84
A1L03_or_out = minute1[1];
A1L03 = B4_dffs[1] $ A1L03_or_out;


--A1L13 is always0~88
A1L13_or_out = minute1[2];
A1L13 = B4_dffs[2] $ A1L13_or_out;


--A1L23 is always0~92
A1L23_or_out = hour0[0];
A1L23 = B1_dffs[0] $ A1L23_or_out;


--A1L33 is always0~96
A1L33_or_out = hour0[1];
A1L33 = B1_dffs[1] $ A1L33_or_out;


--A1L43 is always0~100
A1L43_or_out = hour0[2];
A1L43 = B1_dffs[2] $ A1L43_or_out;


--A1L53 is always0~104
A1L53_or_out = hour0[3];
A1L53 = B1_dffs[3] $ A1L53_or_out;


--A1L63 is always0~108
A1L63_or_out = hour1[0];
A1L63 = B2_dffs[0] $ A1L63_or_out;


--A1L73 is always0~112
A1L73_or_out = hour1[1];
A1L73 = B2_dffs[1] $ A1L73_or_out;


--A1L83 is always0~117
A1L83_p1_out = !second1[3] & !A1L62 & !A1L72 & !A1L82 & !A1L92 & !A1L03 & !A1L13 & !minute1[3] & !A1L23 & !A1L33 & !A1L43 & !A1L53 & !A1L63 & !A1L73 & !hour1[2] & !hour1[3] & A1L81 & A1L74 & A1L91 & A1L84 & A1L02 & A1L94 & A1L12 & A1L05 & A1L22 & A1L15 & A1L32 & A1L25 & A1L42 & A1L35 & A1L52 & A1L45;
A1L83_or_out = A1L83_p1_out;
A1L83 = A1L83_or_out;


--A1L81 is always0~36sexp
A1L81 = EXP(B5_dffs[0] & !second0[0]);


--A1L74 is always0~126
A1L74 = EXP(!B5_dffs[0] & second0[0]);


--A1L91 is always0~40sexp
A1L91 = EXP(B5_dffs[1] & !second0[1]);


--A1L84 is always0~127
A1L84 = EXP(!B5_dffs[1] & second0[1]);


--A1L02 is always0~44sexp
A1L02 = EXP(B5_dffs[2] & !second0[2]);


--A1L94 is always0~128
A1L94 = EXP(!B5_dffs[2] & second0[2]);


--A1L12 is always0~48sexp
A1L12 = EXP(B5_dffs[3] & !second0[3]);


--A1L05 is always0~129
A1L05 = EXP(!B5_dffs[3] & second0[3]);


--A1L22 is always0~52sexp
A1L22 = EXP(B6_dffs[0] & !second1[0]);


--A1L15 is always0~130
A1L15 = EXP(!B6_dffs[0] & second1[0]);


--A1L32 is always0~56sexp
A1L32 = EXP(B6_dffs[1] & !second1[1]);


--A1L25 is always0~131
A1L25 = EXP(!B6_dffs[1] & second1[1]);


--A1L42 is always0~60sexp
A1L42 = EXP(B6_dffs[2] & !second1[2]);


--A1L35 is always0~132
A1L35 = EXP(!B6_dffs[2] & second1[2]);


--A1L52 is always0~64sexp
A1L52 = EXP(B3_dffs[0] & !minute0[0]);


--A1L45 is always0~133
A1L45 = EXP(!B3_dffs[0] & minute0[0]);


--clk_200hz is clk_200hz
--operation mode is input

clk_200hz = INPUT();


--EN is EN
--operation mode is input

EN = INPUT();


--SW1 is SW1
--operation mode is input

SW1 = INPUT();


--SW2 is SW2
--operation mode is input

SW2 = INPUT();


--hour1[3] is hour1[3]
--operation mode is input

hour1[3] = INPUT();


--hour1[2] is hour1[2]
--operation mode is input

hour1[2] = INPUT();


--hour1[1] is hour1[1]
--operation mode is input

hour1[1] = INPUT();


--hour1[0] is hour1[0]
--operation mode is input

hour1[0] = INPUT();


--hour0[3] is hour0[3]
--operation mode is input

hour0[3] = INPUT();


--hour0[2] is hour0[2]
--operation mode is input

hour0[2] = INPUT();


--hour0[1] is hour0[1]
--operation mode is input

hour0[1] = INPUT();


--hour0[0] is hour0[0]
--operation mode is input

hour0[0] = INPUT();


--minute1[3] is minute1[3]
--operation mode is input

minute1[3] = INPUT();


--minute1[2] is minute1[2]
--operation mode is input

minute1[2] = INPUT();


--minute1[1] is minute1[1]
--operation mode is input

minute1[1] = INPUT();


--minute1[0] is minute1[0]
--operation mode is input

minute1[0] = INPUT();


--minute0[3] is minute0[3]
--operation mode is input

minute0[3] = INPUT();


--minute0[2] is minute0[2]
--operation mode is input

minute0[2] = INPUT();


--minute0[1] is minute0[1]
--operation mode is input

minute0[1] = INPUT();


--minute0[0] is minute0[0]
--operation mode is input

minute0[0] = INPUT();


--second1[3] is second1[3]
--operation mode is input

second1[3] = INPUT();


--second1[2] is second1[2]
--operation mode is input

second1[2] = INPUT();


--second1[1] is second1[1]
--operation mode is input

second1[1] = INPUT();


--second1[0] is second1[0]
--operation mode is input

second1[0] = INPUT();


--second0[3] is second0[3]
--operation mode is input

second0[3] = INPUT();


--second0[2] is second0[2]
--operation mode is input

second0[2] = INPUT();


--second0[1] is second0[1]
--operation mode is input

second0[1] = INPUT();


--second0[0] is second0[0]
--operation mode is input

second0[0] = INPUT();


--alarmclock_disp_select[4] is alarmclock_disp_select[4]
--operation mode is output

alarmclock_disp_select[4] = OUTPUT(A1L51Q);


--alarmclock_disp_select[2] is alarmclock_disp_select[2]
--operation mode is output

alarmclock_disp_select[2] = OUTPUT(A1L11Q);


--alarmclock_disp_select[5] is alarmclock_disp_select[5]
--operation mode is output

alarmclock_disp_select[5] = OUTPUT(A1L71Q);


--alarmclock_disp_select[3] is alarmclock_disp_select[3]
--operation mode is output

alarmclock_disp_select[3] = OUTPUT(A1L31Q);


--alarmclock_disp_select[1] is alarmclock_disp_select[1]
--operation mode is output

alarmclock_disp_select[1] = OUTPUT(A1L9Q);


--alarmclock_disp_select[0] is alarmclock_disp_select[0]
--operation mode is output

alarmclock_disp_select[0] = OUTPUT(A1L7Q);


--alarm is alarm
--operation mode is output

alarm = OUTPUT(A1L83);


