 -- Copyright (C) 1991-2004 Altera Corporation
 -- Any  megafunction  design,  and related netlist (encrypted  or  decrypted),
 -- support information,  device programming or simulation file,  and any other
 -- associated  documentation or information  provided by  Altera  or a partner
 -- under  Altera's   Megafunction   Partnership   Program  may  be  used  only
 -- to program  PLD  devices (but not masked  PLD  devices) from  Altera.   Any
 -- other  use  of such  megafunction  design,  netlist,  support  information,
 -- device programming or simulation file,  or any other  related documentation
 -- or information  is prohibited  for  any  other purpose,  including, but not
 -- limited to  modification,  reverse engineering,  de-compiling, or use  with
 -- any other  silicon devices,  unless such use is  explicitly  licensed under
 -- a separate agreement with  Altera  or a megafunction partner.  Title to the
 -- intellectual property,  including patents,  copyrights,  trademarks,  trade
 -- secrets,  or maskworks,  embodied in any such megafunction design, netlist,
 -- support  information,  device programming or simulation file,  or any other
 -- related documentation or information provided by  Altera  or a megafunction
 -- partner, remains with Altera, the megafunction partner, or their respective
 -- licensors. No other licenses, including any licenses needed under any third
 -- party's intellectual property, are provided herein.
 -- 
 -- This is a Quartus II output file. It is for reporting purposes only, and is
 -- not intended for use as a Quartus II input file. This file cannot be used
 -- to make Quartus II pin assignments - for instructions on how to make pin
 -- assignments, please see Quartus II help.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- NC            : No Connect. This pin has no internal connection to the device.
 -- VCC           : Dedicated power pin, which MUST be connected to VCC.
 -- VCCIO         : Dedicated power pin, which MUST be connected to VCC
 --                 of its bank.
 -- GND           : Dedicated ground pin. Dedicated GND pins MUST be connected to GND.
 --					It can also be used to report unused dedicated pins. The connection
 --					on the board for unused dedicated pins depends on whether this will
 --					be used in a future design. One example is device migration. When
 --					using device migration, refer to the device pin-tables. If it is a
 --					GND pin in the pin table or if it will not be used in a future design
 --					for another purpose the it MUST be connected to GND. If it is an unused
 --					dedicated pin, then it can be connected to a valid signal on the board
 --					(low, high, or toggling) if that signal is required for a different
 --					revision of the design.
 -- GND+          : Unused input pin. It can also be used to report unused dual-purpose pins.
 --					This pin should be connected to GND. It may also be connected  to a
 --					valid signal  on the board  (low, high, or toggling)  if that signal
 --					is required for a different revision of the design.
 -- GND*          : Unused  I/O  pin.   This pin can either be left unconnected or
 --           	    connected to GND.  Connecting this pin to GND will improve the
 --           	    device's immunity to noise.
 -- RESERVED      : Unused I/O pin, which MUST be left unconnected.
 -- RESERVED_INPUT    : Pin is tri-stated and should be connected to the board.
 -- NON_MIGRATABLE: This pin cannot be migrated.
 ---------------------------------------------------------------------------------

Quartus II Version 4.2 Build 157 12/07/2004 SJ Full Version
CHIP  "Master_Control_Main"  ASSIGNED TO AN: EPM7128STC100-6

Pin Name/Usage               : Location  : Dir.   : I/O Standard      : Voltage : I/O Bank  : User Assignment
-------------------------------------------------------------------------------------------------------------
Motor_Data[0]                : 1         : output : TTL               :         :           : N              
Now_Floor[3]                 : 2         : output : TTL               :         :           : N              
VCCIO                        : 3         : power  :                   : 5.0V    :           :                
TDI                          : 4         : input  : TTL               :         :           : N              
Master_Floor8                : 5         : input  : TTL               :         :           : N              
Door_On_Off                  : 6         : output : TTL               :         :           : N              
Slave_Floor6[4]              : 7         : input  : TTL               :         :           : N              
RESERVED                     : 8         :        :                   :         :           :                
Ahead_Request                : 9         : input  : TTL               :         :           : N              
Slave_Floor7[2]              : 10        : input  : TTL               :         :           : N              
GND                          : 11        : gnd    :                   :         :           :                
Slave_Floor8[4]              : 12        : input  : TTL               :         :           : N              
Delay_Request                : 13        : input  : TTL               :         :           : N              
RESERVED                     : 14        :        :                   :         :           :                
TMS                          : 15        : input  : TTL               :         :           : N              
Master_Floor7                : 16        : input  : TTL               :         :           : N              
Slave_Floor3[3]              : 17        : input  : TTL               :         :           : N              
VCCIO                        : 18        : power  :                   : 5.0V    :           :                
Slave_Floor3[2]              : 19        : input  : TTL               :         :           : N              
Slave_Floor9[1]              : 20        : input  : TTL               :         :           : N              
Slave_Floor5[2]              : 21        : input  : TTL               :         :           : N              
Slave_Floor6[2]              : 22        : input  : TTL               :         :           : N              
Now_Floor[0]                 : 23        : output : TTL               :         :           : N              
Now_Floor[1]                 : 24        : output : TTL               :         :           : N              
Now_Floor[2]                 : 25        : output : TTL               :         :           : N              
GND                          : 26        : gnd    :                   :         :           :                
Slave_Floor3[4]              : 27        : input  : TTL               :         :           : N              
Master_Floor6                : 28        : input  : TTL               :         :           : N              
Master_Floor1                : 29        : input  : TTL               :         :           : N              
Slave_Floor2[0]              : 30        : input  : TTL               :         :           : N              
Slave_Floor7[4]              : 31        : input  : TTL               :         :           : N              
Slave_Floor5[1]              : 32        : input  : TTL               :         :           : N              
Slave_Floor6[0]              : 33        : input  : TTL               :         :           : N              
VCCIO                        : 34        : power  :                   : 5.0V    :           :                
Slave_Floor7[0]              : 35        : input  : TTL               :         :           : N              
Master_Floor9                : 36        : input  : TTL               :         :           : N              
RESERVED                     : 37        :        :                   :         :           :                
GND                          : 38        : gnd    :                   :         :           :                
VCCINT                       : 39        : power  :                   : 5.0V    :           :                
RESERVED                     : 40        :        :                   :         :           :                
Slave_Floor9[3]              : 41        : input  : TTL               :         :           : N              
Slave_Floor8[3]              : 42        : input  : TTL               :         :           : N              
GND                          : 43        : gnd    :                   :         :           :                
Slave_Floor9[2]              : 44        : input  : TTL               :         :           : N              
Slave_Floor3[0]              : 45        : input  : TTL               :         :           : N              
RESERVED                     : 46        :        :                   :         :           :                
Slave_Floor9[0]              : 47        : input  : TTL               :         :           : N              
Slave_Floor4[3]              : 48        : input  : TTL               :         :           : N              
Master_Floor5                : 49        : input  : TTL               :         :           : N              
Master_Floor3                : 50        : input  : TTL               :         :           : N              
VCCIO                        : 51        : power  :                   : 5.0V    :           :                
Slave_Floor1[1]              : 52        : input  : TTL               :         :           : N              
Slave_Floor8[0]              : 53        : input  : TTL               :         :           : N              
Slave_Floor8[1]              : 54        : input  : TTL               :         :           : N              
Slave_Floor7[3]              : 55        : input  : TTL               :         :           : N              
Slave_Floor5[3]              : 56        : input  : TTL               :         :           : N              
RESERVED                     : 57        :        :                   :         :           :                
Slave_Floor1[2]              : 58        : input  : TTL               :         :           : N              
GND                          : 59        : gnd    :                   :         :           :                
Master_Floor2                : 60        : input  : TTL               :         :           : N              
Slave_Floor2[4]              : 61        : input  : TTL               :         :           : N              
TCK                          : 62        : input  : TTL               :         :           : N              
RESERVED                     : 63        :        :                   :         :           :                
Slave_Floor9[4]              : 64        : input  : TTL               :         :           : N              
Slave_Floor7[1]              : 65        : input  : TTL               :         :           : N              
VCCIO                        : 66        : power  :                   : 5.0V    :           :                
Slave_Floor6[3]              : 67        : input  : TTL               :         :           : N              
Slave_Request_Arrive         : 68        : input  : TTL               :         :           : N              
RESERVED                     : 69        :        :                   :         :           :                
Slave_Floor2[2]              : 70        : input  : TTL               :         :           : N              
Slave_Floor2[3]              : 71        : input  : TTL               :         :           : N              
Master_Floor4                : 72        : input  : TTL               :         :           : N              
TDO                          : 73        : output : TTL               :         :           : N              
GND                          : 74        : gnd    :                   :         :           :                
Slave_Floor1[0]              : 75        : input  : TTL               :         :           : N              
Slave_Floor3[1]              : 76        : input  : TTL               :         :           : N              
Slave_Floor8[2]              : 77        : input  : TTL               :         :           : N              
Slave_Floor6[1]              : 78        : input  : TTL               :         :           : N              
Slave_Floor5[0]              : 79        : input  : TTL               :         :           : N              
Slave_Floor4[0]              : 80        : input  : TTL               :         :           : N              
Slave_Floor1[3]              : 81        : input  : TTL               :         :           : N              
VCCIO                        : 82        : power  :                   : 5.0V    :           :                
Slave_Floor4[2]              : 83        : input  : TTL               :         :           : N              
Slave_Floor4[4]              : 84        : input  : TTL               :         :           : N              
En                           : 85        : input  : TTL               :         :           : N              
GND                          : 86        : gnd    :                   :         :           :                
Clock_1Hz                    : 87        : input  : TTL               :         :           : N              
Slave_Floor1[4]              : 88        : input  : TTL               :         :           : N              
GND+                         : 89        :        :                   :         :           :                
Floor_Time                   : 90        : input  : TTL               :         :           : N              
VCCINT                       : 91        : power  :                   : 5.0V    :           :                
Reset                        : 92        : input  : TTL               :         :           : N              
Slave_Floor5[4]              : 93        : input  : TTL               :         :           : N              
Slave_Floor4[1]              : 94        : input  : TTL               :         :           : N              
GND                          : 95        : gnd    :                   :         :           :                
Slave_Floor2[1]              : 96        : input  : TTL               :         :           : N              
RESERVED                     : 97        :        :                   :         :           :                
Now_Direction[1]             : 98        : output : TTL               :         :           : N              
Now_Direction[0]             : 99        : output : TTL               :         :           : N              
Motor_Data[1]                : 100       : output : TTL               :         :           : N              
