 -- Copyright (C) 1991-2004 Altera Corporation
 -- Any  megafunction  design,  and related netlist (encrypted  or  decrypted),
 -- support information,  device programming or simulation file,  and any other
 -- associated  documentation or information  provided by  Altera  or a partner
 -- under  Altera's   Megafunction   Partnership   Program  may  be  used  only
 -- to program  PLD  devices (but not masked  PLD  devices) from  Altera.   Any
 -- other  use  of such  megafunction  design,  netlist,  support  information,
 -- device programming or simulation file,  or any other  related documentation
 -- or information  is prohibited  for  any  other purpose,  including, but not
 -- limited to  modification,  reverse engineering,  de-compiling, or use  with
 -- any other  silicon devices,  unless such use is  explicitly  licensed under
 -- a separate agreement with  Altera  or a megafunction partner.  Title to the
 -- intellectual property,  including patents,  copyrights,  trademarks,  trade
 -- secrets,  or maskworks,  embodied in any such megafunction design, netlist,
 -- support  information,  device programming or simulation file,  or any other
 -- related documentation or information provided by  Altera  or a megafunction
 -- partner, remains with Altera, the megafunction partner, or their respective
 -- licensors. No other licenses, including any licenses needed under any third
 -- party's intellectual property, are provided herein.
 -- 
 -- This is a Quartus II output file. It is for reporting purposes only, and is
 -- not intended for use as a Quartus II input file. This file cannot be used
 -- to make Quartus II pin assignments - for instructions on how to make pin
 -- assignments, please see Quartus II help.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- NC            : No Connect. This pin has no internal connection to the device.
 -- VCC           : Dedicated power pin, which MUST be connected to VCC.
 -- VCCIO         : Dedicated power pin, which MUST be connected to VCC
 --                 of its bank.
 -- GND           : Dedicated ground pin. Dedicated GND pins MUST be connected to GND.
 --					It can also be used to report unused dedicated pins. The connection
 --					on the board for unused dedicated pins depends on whether this will
 --					be used in a future design. One example is device migration. When
 --					using device migration, refer to the device pin-tables. If it is a
 --					GND pin in the pin table or if it will not be used in a future design
 --					for another purpose the it MUST be connected to GND. If it is an unused
 --					dedicated pin, then it can be connected to a valid signal on the board
 --					(low, high, or toggling) if that signal is required for a different
 --					revision of the design.
 -- GND+          : Unused input pin. It can also be used to report unused dual-purpose pins.
 --					This pin should be connected to GND. It may also be connected  to a
 --					valid signal  on the board  (low, high, or toggling)  if that signal
 --					is required for a different revision of the design.
 -- GND*          : Unused  I/O  pin.   This pin can either be left unconnected or
 --           	    connected to GND.  Connecting this pin to GND will improve the
 --           	    device's immunity to noise.
 -- RESERVED      : Unused I/O pin, which MUST be left unconnected.
 -- RESERVED_INPUT    : Pin is tri-stated and should be connected to the board.
 -- NON_MIGRATABLE: This pin cannot be migrated.
 ---------------------------------------------------------------------------------

Quartus II Version 4.2 Build 157 12/07/2004 SJ Full Version
CHIP  "DC_Motor_Main"  ASSIGNED TO AN: EPM7128STC100-6

Pin Name/Usage               : Location  : Dir.   : I/O Standard      : Voltage : I/O Bank  : User Assignment
-------------------------------------------------------------------------------------------------------------
RESERVED                     : 1         :        :                   :         :           :                
Rate_Over                    : 2         : output : TTL               :         :           : N              
VCCIO                        : 3         : power  :                   : 5.0V    :           :                
TDI                          : 4         : input  : TTL               :         :           : N              
AD7895_Data                  : 5         : input  : TTL               :         :           : N              
Rate_Set[10]                 : 6         : input  : TTL               :         :           : N              
Rate_Set[6]                  : 7         : input  : TTL               :         :           : N              
RESERVED                     : 8         :        :                   :         :           :                
Rate_Set[14]                 : 9         : input  : TTL               :         :           : N              
AD7492_Conv                  : 10        : output : TTL               :         :           : N              
GND                          : 11        : gnd    :                   :         :           :                
AD7492_RD                    : 12        : output : TTL               :         :           : N              
AD7492_Mode                  : 13        : output : TTL               :         :           : N              
AD7492_CS                    : 14        : output : TTL               :         :           : N              
TMS                          : 15        : input  : TTL               :         :           : N              
AD7895_Busy                  : 16        : input  : TTL               :         :           : N              
Rate_Set[15]                 : 17        : input  : TTL               :         :           : N              
VCCIO                        : 18        : power  :                   : 5.0V    :           :                
Current_Set[7]               : 19        : input  : TTL               :         :           : N              
Position_Set[6]              : 20        : input  : TTL               :         :           : N              
AD7492_Data[1]               : 21        : input  : TTL               :         :           : N              
Rate_Set[2]                  : 22        : input  : TTL               :         :           : N              
AD7492_Data[8]               : 23        : input  : TTL               :         :           : N              
Position_Set[1]              : 24        : input  : TTL               :         :           : N              
Position_Set[5]              : 25        : input  : TTL               :         :           : N              
GND                          : 26        : gnd    :                   :         :           :                
Reset                        : 27        : input  : TTL               :         :           : N              
Rate_Set[11]                 : 28        : input  : TTL               :         :           : N              
Current_Set[8]               : 29        : input  : TTL               :         :           : N              
Current_Set[4]               : 30        : input  : TTL               :         :           : N              
Position_Set[9]              : 31        : input  : TTL               :         :           : N              
Current_Set[9]               : 32        : input  : TTL               :         :           : N              
AD7492_Data[4]               : 33        : input  : TTL               :         :           : N              
VCCIO                        : 34        : power  :                   : 5.0V    :           :                
Rate_Set[0]                  : 35        : input  : TTL               :         :           : N              
RESERVED                     : 36        :        :                   :         :           :                
AD7895_Conv                  : 37        : output : TTL               :         :           : N              
GND                          : 38        : gnd    :                   :         :           :                
VCCINT                       : 39        : power  :                   : 5.0V    :           :                
AD7895_SCL                   : 40        : output : TTL               :         :           : N              
RESERVED                     : 41        :        :                   :         :           :                
AD7492_Data[10]              : 42        : input  : TTL               :         :           : N              
GND                          : 43        : gnd    :                   :         :           :                
Rate_Set[3]                  : 44        : input  : TTL               :         :           : N              
AD7492_Data[3]               : 45        : input  : TTL               :         :           : N              
Current_Set[11]              : 46        : input  : TTL               :         :           : N              
Rate_Set[5]                  : 47        : input  : TTL               :         :           : N              
Rate_Set[7]                  : 48        : input  : TTL               :         :           : N              
Current_Set[3]               : 49        : input  : TTL               :         :           : N              
Rate_SW                      : 50        : input  : TTL               :         :           : N              
VCCIO                        : 51        : power  :                   : 5.0V    :           :                
Current_Adjust_Drive         : 52        : output : TTL               :         :           : N              
RESERVED                     : 53        :        :                   :         :           :                
AD7492_Data[9]               : 54        : input  : TTL               :         :           : N              
AD7492_Data[6]               : 55        : input  : TTL               :         :           : N              
AD7492_Data[2]               : 56        : input  : TTL               :         :           : N              
RESERVED                     : 57        :        :                   :         :           :                
Current_Set[6]               : 58        : input  : TTL               :         :           : N              
GND                          : 59        : gnd    :                   :         :           :                
Rate_Pulse                   : 60        : input  : TTL               :         :           : N              
Rate_Set[8]                  : 61        : input  : TTL               :         :           : N              
TCK                          : 62        : input  : TTL               :         :           : N              
Position_Adjust_Drive        : 63        : output : TTL               :         :           : N              
Current_Set[5]               : 64        : input  : TTL               :         :           : N              
Position_Set[3]              : 65        : input  : TTL               :         :           : N              
VCCIO                        : 66        : power  :                   : 5.0V    :           :                
AD7492_Data[5]               : 67        : input  : TTL               :         :           : N              
Rate_Measure_Ctrl            : 68        : input  : TTL               :         :           : N              
Position_Set[7]              : 69        : input  : TTL               :         :           : N              
Rate_Set[4]                  : 70        : input  : TTL               :         :           : N              
Current_Set[1]               : 71        : input  : TTL               :         :           : N              
Current_Set[2]               : 72        : input  : TTL               :         :           : N              
TDO                          : 73        : output : TTL               :         :           : N              
GND                          : 74        : gnd    :                   :         :           :                
Rate_Adjust_Drive            : 75        : output : TTL               :         :           : N              
RESERVED                     : 76        :        :                   :         :           :                
AD7492_Data[7]               : 77        : input  : TTL               :         :           : N              
Rate_Set[1]                  : 78        : input  : TTL               :         :           : N              
Current_Set[10]              : 79        : input  : TTL               :         :           : N              
Position_Set[8]              : 80        : input  : TTL               :         :           : N              
AD7492_Busy                  : 81        : input  : TTL               :         :           : N              
VCCIO                        : 82        : power  :                   : 5.0V    :           :                
Current_Set[0]               : 83        : input  : TTL               :         :           : N              
Rate_Set[12]                 : 84        : input  : TTL               :         :           : N              
Current_SW                   : 85        : input  : TTL               :         :           : N              
GND                          : 86        : gnd    :                   :         :           :                
Clk_SCL                      : 87        : input  : TTL               :         :           : N              
Position_Set[0]              : 88        : input  : TTL               :         :           : N              
Position_Set[2]              : 89        : input  : TTL               :         :           : N              
Clock                        : 90        : input  : TTL               :         :           : N              
VCCINT                       : 91        : power  :                   : 5.0V    :           :                
Position_SW                  : 92        : input  : TTL               :         :           : N              
Rate_Set[13]                 : 93        : input  : TTL               :         :           : N              
Rate_Set[9]                  : 94        : input  : TTL               :         :           : N              
GND                          : 95        : gnd    :                   :         :           :                
Position_Set[4]              : 96        : input  : TTL               :         :           : N              
Position_Set[10]             : 97        : input  : TTL               :         :           : N              
AD7492_Data[0]               : 98        : input  : TTL               :         :           : N              
Position_Set[11]             : 99        : input  : TTL               :         :           : N              
AD7492_Data[11]              : 100       : input  : TTL               :         :           : N              
