--B1_sdata[1] is scan:inst|sdata[1]
--operation mode is normal

B1_sdata[1]_lut_out = !B1_sdata[1];
B1_sdata[1] = DFFEAS(B1_sdata[1]_lut_out, B1_EN_in, VCC, , B1_sdata[0], , , , );


--M1L3 is control:inst14|Red1~14
--operation mode is normal

M1L3 = B1_sdata[1] & Reset & SW;


--M1L4 is control:inst14|Yellow1~11
--operation mode is normal

M1L4 = Reset & SW & !B1_sdata[1];


--B1_sdata[0] is scan:inst|sdata[0]
--operation mode is normal

B1_sdata[0]_lut_out = !B1_sdata[0];
B1_sdata[0] = DFFEAS(B1_sdata[0]_lut_out, B1_EN_in, VCC, , , , , , );


--M1L5 is control:inst14|Yellow1~12
--operation mode is normal

M1L5 = Reset & SW & B1_sdata[0] & !B1_sdata[1];


--M1L6 is control:inst14|Yellow2~10
--operation mode is normal

M1L6 = B1_sdata[1] & Reset & SW & B1_sdata[0];


--M1L1 is control:inst14|Green1~1
--operation mode is normal

M1L1 = B1_sdata[1] # B1_sdata[0] # !SW # !Reset;


--M1L2 is control:inst14|Green2~10
--operation mode is normal

M1L2 = B1_sdata[1] & Reset & SW & !B1_sdata[0];


--J1_D_OUT[0] is dispselect:inst9|D_OUT[0]
--operation mode is normal

J1_D_OUT[0]_lut_out = !J1_D_OUT[0];
J1_D_OUT[0] = DFFEAS(J1_D_OUT[0]_lut_out, L1_clk_out, VCC, , , , , , );


--P2_safe_q[0] is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|safe_q[0]
--operation mode is arithmetic

P2_safe_q[0]_lut_out = !P2_safe_q[0];
P2_safe_q[0] = DFFEAS(P2_safe_q[0]_lut_out, K1_clk_out, VCC, , , , , D1L1, );

--P2L2 is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

P2L2 = CARRY(P2_safe_q[0]);


--P1_safe_q[0] is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|safe_q[0]
--operation mode is arithmetic

P1_safe_q[0]_lut_out = !P1_safe_q[0];
P1_safe_q[0] = DFFEAS(P1_safe_q[0]_lut_out, K1_clk_out, VCC, , , , , C1L1, );

--P1L2 is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

P1L2 = CARRY(P1_safe_q[0]);


--P1_safe_q[3] is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|safe_q[3]
--operation mode is normal

P1_safe_q[3]_carry_eqn = P1L6;
P1_safe_q[3]_lut_out = P1_safe_q[3] $ (P1_safe_q[3]_carry_eqn);
P1_safe_q[3] = DFFEAS(P1_safe_q[3]_lut_out, K1_clk_out, VCC, , , , , C1L1, );


--P1_safe_q[1] is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|safe_q[1]
--operation mode is arithmetic

P1_safe_q[1]_carry_eqn = P1L2;
P1_safe_q[1]_lut_out = P1_safe_q[1] $ (P1_safe_q[1]_carry_eqn);
P1_safe_q[1] = DFFEAS(P1_safe_q[1]_lut_out, K1_clk_out, VCC, , , , , C1L1, );

--P1L4 is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

P1L4 = CARRY(!P1L2 # !P1_safe_q[1]);


--P1_safe_q[2] is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|safe_q[2]
--operation mode is arithmetic

P1_safe_q[2]_carry_eqn = P1L4;
P1_safe_q[2]_lut_out = P1_safe_q[2] $ (!P1_safe_q[2]_carry_eqn);
P1_safe_q[2] = DFFEAS(P1_safe_q[2]_lut_out, K1_clk_out, VCC, , , , , C1L1, );

--P1L6 is counter05:inst1|lpm_counter:CData0_rtl_1|cntr_0b7:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

P1L6 = CARRY(P1_safe_q[2] & !P1L4);


--F1L1 is datamux:inst6|D_OUT0[0]~112
--operation mode is normal

F1L1 = P1_safe_q[0] # P1_safe_q[3] # P1_safe_q[1] & P1_safe_q[2];


--H1L1 is dispmux:inst8|D_OUT[0]~737
--operation mode is normal

H1L1 = J1_D_OUT[0] & B1_sdata[0] & !F1L1 # !B1_sdata[0] & !P2_safe_q[0];


--D1L21 is counter55:inst2|add~161
--operation mode is arithmetic

D1L21_carry_eqn = D1L11;
D1L21 = Q1_safe_q[0] $ (D1L21_carry_eqn);

--D1L31 is counter55:inst2|add~161COUT
--operation mode is arithmetic

D1L31 = CARRY(Q1_safe_q[0] & !D1L11);


--D1L81 is counter55:inst2|add~164
--operation mode is normal

D1L81_carry_eqn = D1L71;
D1L81 = Q1_safe_q[3] $ (D1L81_carry_eqn);


--H1L5 is dispmux:inst8|D_OUT[1]~738
--operation mode is normal

H1L5 = !D1L81 & !B1_sdata[0] & !J1_D_OUT[0];


--D1L41 is counter55:inst2|add~162
--operation mode is arithmetic

D1L41_carry_eqn = D1L31;
D1L41 = Q1_safe_q[1] $ (D1L41_carry_eqn);

--D1L51 is counter55:inst2|add~162COUT
--operation mode is arithmetic

D1L51 = CARRY(!Q1_safe_q[1] & !D1L31);


--D1L61 is counter55:inst2|add~163
--operation mode is arithmetic

D1L61_carry_eqn = D1L51;
D1L61 = Q1_safe_q[2] $ (D1L61_carry_eqn);

--D1L71 is counter55:inst2|add~163COUT
--operation mode is arithmetic

D1L71 = CARRY(Q1_safe_q[2] & !D1L51);


--H1L7 is dispmux:inst8|D_OUT[2]~739
--operation mode is normal

H1L7 = H1L5 & !D1L61 # !D1L41;


--H1L2 is dispmux:inst8|D_OUT[0]~740
--operation mode is normal

H1L2 = H1L1 # D1L21 & H1L7;


--H1L6 is dispmux:inst8|D_OUT[1]~741
--operation mode is normal

H1L6 = D1L41 & H1L5 & !D1L61;


--D1L01 is counter55:inst2|add~160
--operation mode is arithmetic

D1L01_carry_eqn = D1L9;
D1L01 = P2_safe_q[3] $ (D1L01_carry_eqn);

--D1L11 is counter55:inst2|add~160COUT
--operation mode is arithmetic

D1L11 = CARRY(!P2_safe_q[3] & !D1L9);


--D1L8 is counter55:inst2|add~159
--operation mode is arithmetic

D1L8_carry_eqn = D1L6;
D1L8 = P2_safe_q[2] $ (D1L8_carry_eqn);

--D1L9 is counter55:inst2|add~159COUT
--operation mode is arithmetic

D1L9 = CARRY(P2_safe_q[2] & !D1L6);


--P2_safe_q[1] is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|safe_q[1]
--operation mode is arithmetic

P2_safe_q[1]_carry_eqn = P2L2;
P2_safe_q[1]_lut_out = P2_safe_q[1] $ (P2_safe_q[1]_carry_eqn);
P2_safe_q[1] = DFFEAS(P2_safe_q[1]_lut_out, K1_clk_out, VCC, , , , , D1L1, );

--P2L4 is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

P2L4 = CARRY(!P2L2 # !P2_safe_q[1]);


--D1L5 is counter55:inst2|LessThan~93
--operation mode is normal

D1L5 = D1L8 # P2_safe_q[1];


--H1L51 is dispmux:inst8|D_OUT[3]~742
--operation mode is normal

H1L51 = J1_D_OUT[0] & B1_sdata[0] # D1L01 & D1L5;


--H1L21 is dispmux:inst8|D_OUT[3]~65
--operation mode is normal

H1L21 = P1_safe_q[3] # P1_safe_q[1] & P1_safe_q[2] # !J1_D_OUT[0];


--H1L8 is dispmux:inst8|D_OUT[2]~743
--operation mode is normal

H1L8 = J1_D_OUT[0] & !B1_sdata[0];


--H1L4 is dispmux:inst8|D_OUT[1]~23adv_mux_opt_ptn_119
--operation mode is normal

H1L4 = H1L61 & H1L51 & P1_safe_q[1] # !H1L51 & H1L6 # !H1L61 & !H1L51;


--H1L3 is dispmux:inst8|D_OUT[1]~23
--operation mode is normal

H1L3 = H1L4 $ (J1_D_OUT[0] & !B1_sdata[0] & !P2_safe_q[1]);


--H1L9 is dispmux:inst8|D_OUT[2]~744
--operation mode is normal

H1L9 = B1_sdata[0] & J1_D_OUT[0] & P1_safe_q[1] $ !P1_safe_q[2];


--H1L01 is dispmux:inst8|D_OUT[2]~745
--operation mode is normal

H1L01 = H1L8 & D1L8 $ (D1L01 & P2_safe_q[1]);


--H1L11 is dispmux:inst8|D_OUT[2]~746
--operation mode is normal

H1L11 = H1L9 # H1L01 # D1L61 & H1L7;


--H1L31 is dispmux:inst8|D_OUT[3]~729
--operation mode is normal

H1L31 = H1L51 & !H1L8 # !P2_safe_q[1] # !D1L8;


--G1L5 is dispdecoder:inst7|reduce_or~38
--operation mode is normal

G1L5 = H1L3 & H1L41 # !H1L3 & H1L11 $ (H1L2 & !H1L41);


--G1L6 is dispdecoder:inst7|reduce_or~40
--operation mode is normal

G1L6 = H1L11 & H1L41 # H1L2 $ H1L3 # !H1L11 & H1L3 & H1L41;


--G1L7 is dispdecoder:inst7|reduce_or~42
--operation mode is normal

G1L7 = H1L11 & H1L41 # !H1L11 & H1L3 & H1L41 # !H1L2;


--G1L4 is dispdecoder:inst7|data_out[4]~31
--operation mode is normal

G1L4 = H1L2 & H1L41 # H1L3 $ !H1L11 # !H1L2 & H1L3 & H1L41 # !H1L3 & H1L11;


--G1L3 is dispdecoder:inst7|data_out[3]~33
--operation mode is normal

G1L3 = H1L2 # H1L3 & H1L41 # !H1L3 & H1L11;


--G1L2 is dispdecoder:inst7|data_out[2]~35
--operation mode is normal

G1L2 = H1L2 & H1L3 # H1L11 $ !H1L41 # !H1L2 & H1L11 & H1L41 # !H1L11 & H1L3;


--G1L1 is dispdecoder:inst7|data_out[1]~37
--operation mode is normal

G1L1 = H1L3 & !H1L41 & !H1L11 # !H1L2 # !H1L3 & H1L11 $ H1L41;


--C1_C_out is counter05:inst1|C_out
--operation mode is normal

C1_C_out_lut_out = Reset & B1_sdata[0] & C1L3;
C1_C_out = DFFEAS(C1_C_out_lut_out, K1_clk_out, VCC, , , , , , );


--D1_C_out is counter55:inst2|C_out
--operation mode is normal

D1_C_out_lut_out = D1L2 & D1L91 $ (!Q1L21 # !D1L22);
D1_C_out = DFFEAS(D1_C_out_lut_out, K1_clk_out, VCC, , , , , , );


--B1_EN_in is scan:inst|EN_in
--operation mode is normal

B1_EN_in = C1_C_out # D1_C_out;


--L1_clk_out is fdiv1khz:inst12|clk_out
--operation mode is normal

L1_clk_out_lut_out = L1L1;
L1_clk_out = DFFEAS(L1_clk_out_lut_out, CLK, VCC, , , , , , );


--K1_clk_out is fdiv1hz:inst11|clk_out
--operation mode is normal

K1_clk_out_lut_out = K1L1;
K1_clk_out = DFFEAS(K1_clk_out_lut_out, L1_clk_out, VCC, , , , , , );


--Q1_safe_q[3] is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|safe_q[3]
--operation mode is normal

Q1_safe_q[3]_carry_eqn = Q1L6;
Q1_safe_q[3]_lut_out = Q1_safe_q[3] $ (Q1_safe_q[3]_carry_eqn);
Q1_safe_q[3] = DFFEAS(Q1_safe_q[3]_lut_out, K1_clk_out, VCC, , D1L1, , , D1L3, );


--Q1_safe_q[1] is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|safe_q[1]
--operation mode is arithmetic

Q1_safe_q[1]_carry_eqn = Q1L2;
Q1_safe_q[1]_lut_out = Q1_safe_q[1] $ (Q1_safe_q[1]_carry_eqn);
Q1_safe_q[1] = DFFEAS(Q1_safe_q[1]_lut_out, K1_clk_out, VCC, , D1L1, , , D1L3, );

--Q1L4 is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

Q1L4 = CARRY(!Q1L2 # !Q1_safe_q[1]);


--P2_safe_q[3] is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|safe_q[3]
--operation mode is normal

P2_safe_q[3]_carry_eqn = P2L6;
P2_safe_q[3]_lut_out = P2_safe_q[3] $ (P2_safe_q[3]_carry_eqn);
P2_safe_q[3] = DFFEAS(P2_safe_q[3]_lut_out, K1_clk_out, VCC, , , , , D1L1, );


--Q1_safe_q[0] is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|safe_q[0]
--operation mode is arithmetic

Q1_safe_q[0]_lut_out = !Q1_safe_q[0];
Q1_safe_q[0] = DFFEAS(Q1_safe_q[0]_lut_out, K1_clk_out, VCC, , D1L1, , , D1L3, );

--Q1L2 is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

Q1L2 = CARRY(Q1_safe_q[0]);


--P2_safe_q[2] is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|safe_q[2]
--operation mode is arithmetic

P2_safe_q[2]_carry_eqn = P2L4;
P2_safe_q[2]_lut_out = P2_safe_q[2] $ (!P2_safe_q[2]_carry_eqn);
P2_safe_q[2] = DFFEAS(P2_safe_q[2]_lut_out, K1_clk_out, VCC, , , , , D1L1, );

--P2L6 is counter55:inst2|lpm_counter:CData0_rtl_0|cntr_0b7:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

P2L6 = CARRY(P2_safe_q[2] & !P2L4);


--D1L02 is counter55:inst2|always0~42
--operation mode is normal

D1L02 = Q1_safe_q[1] # P2_safe_q[3] # !P2_safe_q[2] # !Q1_safe_q[0];


--Q1_safe_q[2] is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|safe_q[2]
--operation mode is arithmetic

Q1_safe_q[2]_carry_eqn = Q1L4;
Q1_safe_q[2]_lut_out = Q1_safe_q[2] $ (!Q1_safe_q[2]_carry_eqn);
Q1_safe_q[2] = DFFEAS(Q1_safe_q[2]_lut_out, K1_clk_out, VCC, , D1L1, , , D1L3, );

--Q1L6 is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

Q1L6 = CARRY(Q1_safe_q[2] & !Q1L4);


--D1L12 is counter55:inst2|always0~43
--operation mode is normal

D1L12 = P2_safe_q[0] & !P2_safe_q[1];


--D1L91 is counter55:inst2|always0~1
--operation mode is normal

D1L91 = Q1_safe_q[3] # D1L02 # !D1L12 # !Q1_safe_q[2];


--D1L22 is counter55:inst2|reduce_or~31
--operation mode is normal

D1L22 = P2_safe_q[0] & P2_safe_q[3] & !P2_safe_q[1] & !P2_safe_q[2];


--D1L2 is counter55:inst2|CData0[0]~64
--operation mode is normal

D1L2 = Reset & !B1_sdata[0];


--C1L3 is counter05:inst1|reduce_or~28
--operation mode is normal

C1L3 = P1_safe_q[0] & P1_safe_q[2] & !P1_safe_q[3] & !P1_safe_q[1];


--C1L1 is counter05:inst1|CData0[0]~16
--operation mode is normal

C1L1 = C1L3 # !B1_sdata[0] # !Reset;


--D1L6 is counter55:inst2|add~158
--operation mode is arithmetic

D1L6 = CARRY(!P2_safe_q[1]);


--Q1L21 is counter55:inst2|lpm_counter:CData1_rtl_2|cntr_cv7:auto_generated|safe_q[2]~88
--operation mode is normal

Q1L21 = Q1_safe_q[1] & Q1_safe_q[2] & !Q1_safe_q[0] & !Q1_safe_q[3];


--R2_safe_q[31] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[31]
--operation mode is normal

R2_safe_q[31]_carry_eqn = R2L26;
R2_safe_q[31]_lut_out = R2_safe_q[31] $ (R2_safe_q[31]_carry_eqn);
R2_safe_q[31] = DFFEAS(R2_safe_q[31]_lut_out, CLK, VCC, , , , , L1L1, );


--R2_safe_q[9] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[9]
--operation mode is arithmetic

R2_safe_q[9]_carry_eqn = R2L81;
R2_safe_q[9]_lut_out = R2_safe_q[9] $ (R2_safe_q[9]_carry_eqn);
R2_safe_q[9] = DFFEAS(R2_safe_q[9]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L02 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella9~COUT
--operation mode is arithmetic

R2L02 = CARRY(!R2L81 # !R2_safe_q[9]);


--R2_safe_q[10] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[10]
--operation mode is arithmetic

R2_safe_q[10]_carry_eqn = R2L02;
R2_safe_q[10]_lut_out = R2_safe_q[10] $ (!R2_safe_q[10]_carry_eqn);
R2_safe_q[10] = DFFEAS(R2_safe_q[10]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L22 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella10~COUT
--operation mode is arithmetic

R2L22 = CARRY(R2_safe_q[10] & !R2L02);


--L1L2 is fdiv1khz:inst12|LessThan~471
--operation mode is normal

L1L2 = !R2_safe_q[10] # !R2_safe_q[9];


--R2_safe_q[0] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[0]
--operation mode is arithmetic

R2_safe_q[0]_lut_out = !R2_safe_q[0];
R2_safe_q[0] = DFFEAS(R2_safe_q[0]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L2 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

R2L2 = CARRY(R2_safe_q[0]);


--R2_safe_q[1] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[1]
--operation mode is arithmetic

R2_safe_q[1]_carry_eqn = R2L2;
R2_safe_q[1]_lut_out = R2_safe_q[1] $ (R2_safe_q[1]_carry_eqn);
R2_safe_q[1] = DFFEAS(R2_safe_q[1]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L4 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

R2L4 = CARRY(!R2L2 # !R2_safe_q[1]);


--R2_safe_q[2] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[2]
--operation mode is arithmetic

R2_safe_q[2]_carry_eqn = R2L4;
R2_safe_q[2]_lut_out = R2_safe_q[2] $ (!R2_safe_q[2]_carry_eqn);
R2_safe_q[2] = DFFEAS(R2_safe_q[2]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L6 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

R2L6 = CARRY(R2_safe_q[2] & !R2L4);


--R2_safe_q[3] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[3]
--operation mode is arithmetic

R2_safe_q[3]_carry_eqn = R2L6;
R2_safe_q[3]_lut_out = R2_safe_q[3] $ (R2_safe_q[3]_carry_eqn);
R2_safe_q[3] = DFFEAS(R2_safe_q[3]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L8 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella3~COUT
--operation mode is arithmetic

R2L8 = CARRY(!R2L6 # !R2_safe_q[3]);


--L1L3 is fdiv1khz:inst12|LessThan~472
--operation mode is normal

L1L3 = !R2_safe_q[3] # !R2_safe_q[2] # !R2_safe_q[1] # !R2_safe_q[0];


--R2_safe_q[4] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[4]
--operation mode is arithmetic

R2_safe_q[4]_carry_eqn = R2L8;
R2_safe_q[4]_lut_out = R2_safe_q[4] $ (!R2_safe_q[4]_carry_eqn);
R2_safe_q[4] = DFFEAS(R2_safe_q[4]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L01 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella4~COUT
--operation mode is arithmetic

R2L01 = CARRY(R2_safe_q[4] & !R2L8);


--R2_safe_q[5] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[5]
--operation mode is arithmetic

R2_safe_q[5]_carry_eqn = R2L01;
R2_safe_q[5]_lut_out = R2_safe_q[5] $ (R2_safe_q[5]_carry_eqn);
R2_safe_q[5] = DFFEAS(R2_safe_q[5]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L21 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella5~COUT
--operation mode is arithmetic

R2L21 = CARRY(!R2L01 # !R2_safe_q[5]);


--R2_safe_q[6] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[6]
--operation mode is arithmetic

R2_safe_q[6]_carry_eqn = R2L21;
R2_safe_q[6]_lut_out = R2_safe_q[6] $ (!R2_safe_q[6]_carry_eqn);
R2_safe_q[6] = DFFEAS(R2_safe_q[6]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L41 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella6~COUT
--operation mode is arithmetic

R2L41 = CARRY(R2_safe_q[6] & !R2L21);


--R2_safe_q[7] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[7]
--operation mode is arithmetic

R2_safe_q[7]_carry_eqn = R2L41;
R2_safe_q[7]_lut_out = R2_safe_q[7] $ (R2_safe_q[7]_carry_eqn);
R2_safe_q[7] = DFFEAS(R2_safe_q[7]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L61 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella7~COUT
--operation mode is arithmetic

R2L61 = CARRY(!R2L41 # !R2_safe_q[7]);


--L1L4 is fdiv1khz:inst12|LessThan~473
--operation mode is normal

L1L4 = !R2_safe_q[4] & !R2_safe_q[5] & !R2_safe_q[6] & !R2_safe_q[7];


--R2_safe_q[8] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[8]
--operation mode is arithmetic

R2_safe_q[8]_carry_eqn = R2L61;
R2_safe_q[8]_lut_out = R2_safe_q[8] $ (!R2_safe_q[8]_carry_eqn);
R2_safe_q[8] = DFFEAS(R2_safe_q[8]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L81 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella8~COUT
--operation mode is arithmetic

R2L81 = CARRY(R2_safe_q[8] & !R2L61);


--L1L5 is fdiv1khz:inst12|LessThan~474
--operation mode is normal

L1L5 = L1L2 # L1L3 & L1L4 # !R2_safe_q[8];


--R2_safe_q[11] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[11]
--operation mode is arithmetic

R2_safe_q[11]_carry_eqn = R2L22;
R2_safe_q[11]_lut_out = R2_safe_q[11] $ (R2_safe_q[11]_carry_eqn);
R2_safe_q[11] = DFFEAS(R2_safe_q[11]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L42 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella11~COUT
--operation mode is arithmetic

R2L42 = CARRY(!R2L22 # !R2_safe_q[11]);


--R2_safe_q[12] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[12]
--operation mode is arithmetic

R2_safe_q[12]_carry_eqn = R2L42;
R2_safe_q[12]_lut_out = R2_safe_q[12] $ (!R2_safe_q[12]_carry_eqn);
R2_safe_q[12] = DFFEAS(R2_safe_q[12]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L62 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella12~COUT
--operation mode is arithmetic

R2L62 = CARRY(R2_safe_q[12] & !R2L42);


--R2_safe_q[13] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[13]
--operation mode is arithmetic

R2_safe_q[13]_carry_eqn = R2L62;
R2_safe_q[13]_lut_out = R2_safe_q[13] $ (R2_safe_q[13]_carry_eqn);
R2_safe_q[13] = DFFEAS(R2_safe_q[13]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L82 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella13~COUT
--operation mode is arithmetic

R2L82 = CARRY(!R2L62 # !R2_safe_q[13]);


--L1L6 is fdiv1khz:inst12|LessThan~475
--operation mode is normal

L1L6 = L1L5 & !R2_safe_q[11] & !R2_safe_q[12] # !R2_safe_q[13];


--R2_safe_q[14] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[14]
--operation mode is arithmetic

R2_safe_q[14]_carry_eqn = R2L82;
R2_safe_q[14]_lut_out = R2_safe_q[14] $ (!R2_safe_q[14]_carry_eqn);
R2_safe_q[14] = DFFEAS(R2_safe_q[14]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L03 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella14~COUT
--operation mode is arithmetic

R2L03 = CARRY(R2_safe_q[14] & !R2L82);


--R2_safe_q[15] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[15]
--operation mode is arithmetic

R2_safe_q[15]_carry_eqn = R2L03;
R2_safe_q[15]_lut_out = R2_safe_q[15] $ (R2_safe_q[15]_carry_eqn);
R2_safe_q[15] = DFFEAS(R2_safe_q[15]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L23 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella15~COUT
--operation mode is arithmetic

R2L23 = CARRY(!R2L03 # !R2_safe_q[15]);


--R2_safe_q[16] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[16]
--operation mode is arithmetic

R2_safe_q[16]_carry_eqn = R2L23;
R2_safe_q[16]_lut_out = R2_safe_q[16] $ (!R2_safe_q[16]_carry_eqn);
R2_safe_q[16] = DFFEAS(R2_safe_q[16]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L43 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella16~COUT
--operation mode is arithmetic

R2L43 = CARRY(R2_safe_q[16] & !R2L23);


--R2_safe_q[17] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[17]
--operation mode is arithmetic

R2_safe_q[17]_carry_eqn = R2L43;
R2_safe_q[17]_lut_out = R2_safe_q[17] $ (R2_safe_q[17]_carry_eqn);
R2_safe_q[17] = DFFEAS(R2_safe_q[17]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L63 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella17~COUT
--operation mode is arithmetic

R2L63 = CARRY(!R2L43 # !R2_safe_q[17]);


--L1L7 is fdiv1khz:inst12|LessThan~476
--operation mode is normal

L1L7 = !R2_safe_q[14] & !R2_safe_q[15] & !R2_safe_q[16] & !R2_safe_q[17];


--R2_safe_q[18] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[18]
--operation mode is arithmetic

R2_safe_q[18]_carry_eqn = R2L63;
R2_safe_q[18]_lut_out = R2_safe_q[18] $ (!R2_safe_q[18]_carry_eqn);
R2_safe_q[18] = DFFEAS(R2_safe_q[18]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L83 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella18~COUT
--operation mode is arithmetic

R2L83 = CARRY(R2_safe_q[18] & !R2L63);


--R2_safe_q[19] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[19]
--operation mode is arithmetic

R2_safe_q[19]_carry_eqn = R2L83;
R2_safe_q[19]_lut_out = R2_safe_q[19] $ (R2_safe_q[19]_carry_eqn);
R2_safe_q[19] = DFFEAS(R2_safe_q[19]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L04 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella19~COUT
--operation mode is arithmetic

R2L04 = CARRY(!R2L83 # !R2_safe_q[19]);


--R2_safe_q[20] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[20]
--operation mode is arithmetic

R2_safe_q[20]_carry_eqn = R2L04;
R2_safe_q[20]_lut_out = R2_safe_q[20] $ (!R2_safe_q[20]_carry_eqn);
R2_safe_q[20] = DFFEAS(R2_safe_q[20]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L24 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella20~COUT
--operation mode is arithmetic

R2L24 = CARRY(R2_safe_q[20] & !R2L04);


--R2_safe_q[21] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[21]
--operation mode is arithmetic

R2_safe_q[21]_carry_eqn = R2L24;
R2_safe_q[21]_lut_out = R2_safe_q[21] $ (R2_safe_q[21]_carry_eqn);
R2_safe_q[21] = DFFEAS(R2_safe_q[21]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L44 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella21~COUT
--operation mode is arithmetic

R2L44 = CARRY(!R2L24 # !R2_safe_q[21]);


--L1L8 is fdiv1khz:inst12|LessThan~477
--operation mode is normal

L1L8 = !R2_safe_q[18] & !R2_safe_q[19] & !R2_safe_q[20] & !R2_safe_q[21];


--R2_safe_q[22] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[22]
--operation mode is arithmetic

R2_safe_q[22]_carry_eqn = R2L44;
R2_safe_q[22]_lut_out = R2_safe_q[22] $ (!R2_safe_q[22]_carry_eqn);
R2_safe_q[22] = DFFEAS(R2_safe_q[22]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L64 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella22~COUT
--operation mode is arithmetic

R2L64 = CARRY(R2_safe_q[22] & !R2L44);


--R2_safe_q[23] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[23]
--operation mode is arithmetic

R2_safe_q[23]_carry_eqn = R2L64;
R2_safe_q[23]_lut_out = R2_safe_q[23] $ (R2_safe_q[23]_carry_eqn);
R2_safe_q[23] = DFFEAS(R2_safe_q[23]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L84 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella23~COUT
--operation mode is arithmetic

R2L84 = CARRY(!R2L64 # !R2_safe_q[23]);


--R2_safe_q[24] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[24]
--operation mode is arithmetic

R2_safe_q[24]_carry_eqn = R2L84;
R2_safe_q[24]_lut_out = R2_safe_q[24] $ (!R2_safe_q[24]_carry_eqn);
R2_safe_q[24] = DFFEAS(R2_safe_q[24]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L05 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella24~COUT
--operation mode is arithmetic

R2L05 = CARRY(R2_safe_q[24] & !R2L84);


--R2_safe_q[25] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[25]
--operation mode is arithmetic

R2_safe_q[25]_carry_eqn = R2L05;
R2_safe_q[25]_lut_out = R2_safe_q[25] $ (R2_safe_q[25]_carry_eqn);
R2_safe_q[25] = DFFEAS(R2_safe_q[25]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L25 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella25~COUT
--operation mode is arithmetic

R2L25 = CARRY(!R2L05 # !R2_safe_q[25]);


--L1L9 is fdiv1khz:inst12|LessThan~478
--operation mode is normal

L1L9 = !R2_safe_q[22] & !R2_safe_q[23] & !R2_safe_q[24] & !R2_safe_q[25];


--R2_safe_q[26] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[26]
--operation mode is arithmetic

R2_safe_q[26]_carry_eqn = R2L25;
R2_safe_q[26]_lut_out = R2_safe_q[26] $ (!R2_safe_q[26]_carry_eqn);
R2_safe_q[26] = DFFEAS(R2_safe_q[26]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L45 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella26~COUT
--operation mode is arithmetic

R2L45 = CARRY(R2_safe_q[26] & !R2L25);


--R2_safe_q[27] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[27]
--operation mode is arithmetic

R2_safe_q[27]_carry_eqn = R2L45;
R2_safe_q[27]_lut_out = R2_safe_q[27] $ (R2_safe_q[27]_carry_eqn);
R2_safe_q[27] = DFFEAS(R2_safe_q[27]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L65 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella27~COUT
--operation mode is arithmetic

R2L65 = CARRY(!R2L45 # !R2_safe_q[27]);


--R2_safe_q[28] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[28]
--operation mode is arithmetic

R2_safe_q[28]_carry_eqn = R2L65;
R2_safe_q[28]_lut_out = R2_safe_q[28] $ (!R2_safe_q[28]_carry_eqn);
R2_safe_q[28] = DFFEAS(R2_safe_q[28]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L85 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella28~COUT
--operation mode is arithmetic

R2L85 = CARRY(R2_safe_q[28] & !R2L65);


--R2_safe_q[29] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[29]
--operation mode is arithmetic

R2_safe_q[29]_carry_eqn = R2L85;
R2_safe_q[29]_lut_out = R2_safe_q[29] $ (R2_safe_q[29]_carry_eqn);
R2_safe_q[29] = DFFEAS(R2_safe_q[29]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L06 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella29~COUT
--operation mode is arithmetic

R2L06 = CARRY(!R2L85 # !R2_safe_q[29]);


--L1L01 is fdiv1khz:inst12|LessThan~479
--operation mode is normal

L1L01 = !R2_safe_q[26] & !R2_safe_q[27] & !R2_safe_q[28] & !R2_safe_q[29];


--L1L11 is fdiv1khz:inst12|LessThan~480
--operation mode is normal

L1L11 = L1L7 & L1L8 & L1L9 & L1L01;


--R2_safe_q[30] is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|safe_q[30]
--operation mode is arithmetic

R2_safe_q[30]_carry_eqn = R2L06;
R2_safe_q[30]_lut_out = R2_safe_q[30] $ (!R2_safe_q[30]_carry_eqn);
R2_safe_q[30] = DFFEAS(R2_safe_q[30]_lut_out, CLK, VCC, , , , , L1L1, );

--R2L26 is fdiv1khz:inst12|lpm_counter:cnt_rtl_3|cntr_hc7:auto_generated|counter_cella30~COUT
--operation mode is arithmetic

R2L26 = CARRY(R2_safe_q[30] & !R2L06);


--L1L1 is fdiv1khz:inst12|LessThan~256
--operation mode is normal

L1L1 = !R2_safe_q[31] & R2_safe_q[30] # !L1L11 # !L1L6;


--R1_safe_q[31] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[31]
--operation mode is normal

R1_safe_q[31]_carry_eqn = R1L26;
R1_safe_q[31]_lut_out = R1_safe_q[31] $ (R1_safe_q[31]_carry_eqn);
R1_safe_q[31] = DFFEAS(R1_safe_q[31]_lut_out, L1_clk_out, VCC, , , , , K1L1, );


--R1_safe_q[5] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[5]
--operation mode is arithmetic

R1_safe_q[5]_carry_eqn = R1L01;
R1_safe_q[5]_lut_out = R1_safe_q[5] $ (R1_safe_q[5]_carry_eqn);
R1_safe_q[5] = DFFEAS(R1_safe_q[5]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L21 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella5~COUT
--operation mode is arithmetic

R1L21 = CARRY(!R1L01 # !R1_safe_q[5]);


--R1_safe_q[6] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[6]
--operation mode is arithmetic

R1_safe_q[6]_carry_eqn = R1L21;
R1_safe_q[6]_lut_out = R1_safe_q[6] $ (!R1_safe_q[6]_carry_eqn);
R1_safe_q[6] = DFFEAS(R1_safe_q[6]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L41 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella6~COUT
--operation mode is arithmetic

R1L41 = CARRY(R1_safe_q[6] & !R1L21);


--R1_safe_q[7] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[7]
--operation mode is arithmetic

R1_safe_q[7]_carry_eqn = R1L41;
R1_safe_q[7]_lut_out = R1_safe_q[7] $ (R1_safe_q[7]_carry_eqn);
R1_safe_q[7] = DFFEAS(R1_safe_q[7]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L61 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella7~COUT
--operation mode is arithmetic

R1L61 = CARRY(!R1L41 # !R1_safe_q[7]);


--R1_safe_q[8] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[8]
--operation mode is arithmetic

R1_safe_q[8]_carry_eqn = R1L61;
R1_safe_q[8]_lut_out = R1_safe_q[8] $ (!R1_safe_q[8]_carry_eqn);
R1_safe_q[8] = DFFEAS(R1_safe_q[8]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L81 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella8~COUT
--operation mode is arithmetic

R1L81 = CARRY(R1_safe_q[8] & !R1L61);


--K1L2 is fdiv1hz:inst11|LessThan~500
--operation mode is normal

K1L2 = !R1_safe_q[8] # !R1_safe_q[7] # !R1_safe_q[6] # !R1_safe_q[5];


--R1_safe_q[0] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[0]
--operation mode is arithmetic

R1_safe_q[0]_lut_out = !R1_safe_q[0];
R1_safe_q[0] = DFFEAS(R1_safe_q[0]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L2 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella0~COUT
--operation mode is arithmetic

R1L2 = CARRY(R1_safe_q[0]);


--R1_safe_q[1] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[1]
--operation mode is arithmetic

R1_safe_q[1]_carry_eqn = R1L2;
R1_safe_q[1]_lut_out = R1_safe_q[1] $ (R1_safe_q[1]_carry_eqn);
R1_safe_q[1] = DFFEAS(R1_safe_q[1]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L4 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella1~COUT
--operation mode is arithmetic

R1L4 = CARRY(!R1L2 # !R1_safe_q[1]);


--R1_safe_q[2] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[2]
--operation mode is arithmetic

R1_safe_q[2]_carry_eqn = R1L4;
R1_safe_q[2]_lut_out = R1_safe_q[2] $ (!R1_safe_q[2]_carry_eqn);
R1_safe_q[2] = DFFEAS(R1_safe_q[2]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L6 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella2~COUT
--operation mode is arithmetic

R1L6 = CARRY(R1_safe_q[2] & !R1L4);


--R1_safe_q[3] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[3]
--operation mode is arithmetic

R1_safe_q[3]_carry_eqn = R1L6;
R1_safe_q[3]_lut_out = R1_safe_q[3] $ (R1_safe_q[3]_carry_eqn);
R1_safe_q[3] = DFFEAS(R1_safe_q[3]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L8 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella3~COUT
--operation mode is arithmetic

R1L8 = CARRY(!R1L6 # !R1_safe_q[3]);


--K1L3 is fdiv1hz:inst11|LessThan~501
--operation mode is normal

K1L3 = !R1_safe_q[3] & !R1_safe_q[2] # !R1_safe_q[1] # !R1_safe_q[0];


--R1_safe_q[4] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[4]
--operation mode is arithmetic

R1_safe_q[4]_carry_eqn = R1L8;
R1_safe_q[4]_lut_out = R1_safe_q[4] $ (!R1_safe_q[4]_carry_eqn);
R1_safe_q[4] = DFFEAS(R1_safe_q[4]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L01 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella4~COUT
--operation mode is arithmetic

R1L01 = CARRY(R1_safe_q[4] & !R1L8);


--R1_safe_q[9] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[9]
--operation mode is arithmetic

R1_safe_q[9]_carry_eqn = R1L81;
R1_safe_q[9]_lut_out = R1_safe_q[9] $ (R1_safe_q[9]_carry_eqn);
R1_safe_q[9] = DFFEAS(R1_safe_q[9]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L02 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella9~COUT
--operation mode is arithmetic

R1L02 = CARRY(!R1L81 # !R1_safe_q[9]);


--K1L4 is fdiv1hz:inst11|LessThan~502
--operation mode is normal

K1L4 = K1L2 # K1L3 & !R1_safe_q[4] # !R1_safe_q[9];


--R1_safe_q[10] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[10]
--operation mode is arithmetic

R1_safe_q[10]_carry_eqn = R1L02;
R1_safe_q[10]_lut_out = R1_safe_q[10] $ (!R1_safe_q[10]_carry_eqn);
R1_safe_q[10] = DFFEAS(R1_safe_q[10]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L22 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella10~COUT
--operation mode is arithmetic

R1L22 = CARRY(R1_safe_q[10] & !R1L02);


--R1_safe_q[11] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[11]
--operation mode is arithmetic

R1_safe_q[11]_carry_eqn = R1L22;
R1_safe_q[11]_lut_out = R1_safe_q[11] $ (R1_safe_q[11]_carry_eqn);
R1_safe_q[11] = DFFEAS(R1_safe_q[11]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L42 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella11~COUT
--operation mode is arithmetic

R1L42 = CARRY(!R1L22 # !R1_safe_q[11]);


--R1_safe_q[12] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[12]
--operation mode is arithmetic

R1_safe_q[12]_carry_eqn = R1L42;
R1_safe_q[12]_lut_out = R1_safe_q[12] $ (!R1_safe_q[12]_carry_eqn);
R1_safe_q[12] = DFFEAS(R1_safe_q[12]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L62 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella12~COUT
--operation mode is arithmetic

R1L62 = CARRY(R1_safe_q[12] & !R1L42);


--R1_safe_q[13] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[13]
--operation mode is arithmetic

R1_safe_q[13]_carry_eqn = R1L62;
R1_safe_q[13]_lut_out = R1_safe_q[13] $ (R1_safe_q[13]_carry_eqn);
R1_safe_q[13] = DFFEAS(R1_safe_q[13]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L82 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella13~COUT
--operation mode is arithmetic

R1L82 = CARRY(!R1L62 # !R1_safe_q[13]);


--K1L5 is fdiv1hz:inst11|LessThan~503
--operation mode is normal

K1L5 = !R1_safe_q[10] & !R1_safe_q[11] & !R1_safe_q[12] & !R1_safe_q[13];


--R1_safe_q[14] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[14]
--operation mode is arithmetic

R1_safe_q[14]_carry_eqn = R1L82;
R1_safe_q[14]_lut_out = R1_safe_q[14] $ (!R1_safe_q[14]_carry_eqn);
R1_safe_q[14] = DFFEAS(R1_safe_q[14]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L03 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella14~COUT
--operation mode is arithmetic

R1L03 = CARRY(R1_safe_q[14] & !R1L82);


--R1_safe_q[15] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[15]
--operation mode is arithmetic

R1_safe_q[15]_carry_eqn = R1L03;
R1_safe_q[15]_lut_out = R1_safe_q[15] $ (R1_safe_q[15]_carry_eqn);
R1_safe_q[15] = DFFEAS(R1_safe_q[15]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L23 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella15~COUT
--operation mode is arithmetic

R1L23 = CARRY(!R1L03 # !R1_safe_q[15]);


--R1_safe_q[16] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[16]
--operation mode is arithmetic

R1_safe_q[16]_carry_eqn = R1L23;
R1_safe_q[16]_lut_out = R1_safe_q[16] $ (!R1_safe_q[16]_carry_eqn);
R1_safe_q[16] = DFFEAS(R1_safe_q[16]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L43 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella16~COUT
--operation mode is arithmetic

R1L43 = CARRY(R1_safe_q[16] & !R1L23);


--R1_safe_q[17] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[17]
--operation mode is arithmetic

R1_safe_q[17]_carry_eqn = R1L43;
R1_safe_q[17]_lut_out = R1_safe_q[17] $ (R1_safe_q[17]_carry_eqn);
R1_safe_q[17] = DFFEAS(R1_safe_q[17]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L63 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella17~COUT
--operation mode is arithmetic

R1L63 = CARRY(!R1L43 # !R1_safe_q[17]);


--K1L6 is fdiv1hz:inst11|LessThan~504
--operation mode is normal

K1L6 = !R1_safe_q[14] & !R1_safe_q[15] & !R1_safe_q[16] & !R1_safe_q[17];


--R1_safe_q[18] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[18]
--operation mode is arithmetic

R1_safe_q[18]_carry_eqn = R1L63;
R1_safe_q[18]_lut_out = R1_safe_q[18] $ (!R1_safe_q[18]_carry_eqn);
R1_safe_q[18] = DFFEAS(R1_safe_q[18]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L83 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella18~COUT
--operation mode is arithmetic

R1L83 = CARRY(R1_safe_q[18] & !R1L63);


--R1_safe_q[19] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[19]
--operation mode is arithmetic

R1_safe_q[19]_carry_eqn = R1L83;
R1_safe_q[19]_lut_out = R1_safe_q[19] $ (R1_safe_q[19]_carry_eqn);
R1_safe_q[19] = DFFEAS(R1_safe_q[19]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L04 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella19~COUT
--operation mode is arithmetic

R1L04 = CARRY(!R1L83 # !R1_safe_q[19]);


--R1_safe_q[20] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[20]
--operation mode is arithmetic

R1_safe_q[20]_carry_eqn = R1L04;
R1_safe_q[20]_lut_out = R1_safe_q[20] $ (!R1_safe_q[20]_carry_eqn);
R1_safe_q[20] = DFFEAS(R1_safe_q[20]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L24 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella20~COUT
--operation mode is arithmetic

R1L24 = CARRY(R1_safe_q[20] & !R1L04);


--R1_safe_q[21] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[21]
--operation mode is arithmetic

R1_safe_q[21]_carry_eqn = R1L24;
R1_safe_q[21]_lut_out = R1_safe_q[21] $ (R1_safe_q[21]_carry_eqn);
R1_safe_q[21] = DFFEAS(R1_safe_q[21]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L44 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella21~COUT
--operation mode is arithmetic

R1L44 = CARRY(!R1L24 # !R1_safe_q[21]);


--K1L7 is fdiv1hz:inst11|LessThan~505
--operation mode is normal

K1L7 = !R1_safe_q[18] & !R1_safe_q[19] & !R1_safe_q[20] & !R1_safe_q[21];


--R1_safe_q[22] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[22]
--operation mode is arithmetic

R1_safe_q[22]_carry_eqn = R1L44;
R1_safe_q[22]_lut_out = R1_safe_q[22] $ (!R1_safe_q[22]_carry_eqn);
R1_safe_q[22] = DFFEAS(R1_safe_q[22]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L64 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella22~COUT
--operation mode is arithmetic

R1L64 = CARRY(R1_safe_q[22] & !R1L44);


--R1_safe_q[23] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[23]
--operation mode is arithmetic

R1_safe_q[23]_carry_eqn = R1L64;
R1_safe_q[23]_lut_out = R1_safe_q[23] $ (R1_safe_q[23]_carry_eqn);
R1_safe_q[23] = DFFEAS(R1_safe_q[23]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L84 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella23~COUT
--operation mode is arithmetic

R1L84 = CARRY(!R1L64 # !R1_safe_q[23]);


--R1_safe_q[24] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[24]
--operation mode is arithmetic

R1_safe_q[24]_carry_eqn = R1L84;
R1_safe_q[24]_lut_out = R1_safe_q[24] $ (!R1_safe_q[24]_carry_eqn);
R1_safe_q[24] = DFFEAS(R1_safe_q[24]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L05 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella24~COUT
--operation mode is arithmetic

R1L05 = CARRY(R1_safe_q[24] & !R1L84);


--R1_safe_q[25] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[25]
--operation mode is arithmetic

R1_safe_q[25]_carry_eqn = R1L05;
R1_safe_q[25]_lut_out = R1_safe_q[25] $ (R1_safe_q[25]_carry_eqn);
R1_safe_q[25] = DFFEAS(R1_safe_q[25]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L25 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella25~COUT
--operation mode is arithmetic

R1L25 = CARRY(!R1L05 # !R1_safe_q[25]);


--K1L8 is fdiv1hz:inst11|LessThan~506
--operation mode is normal

K1L8 = !R1_safe_q[22] & !R1_safe_q[23] & !R1_safe_q[24] & !R1_safe_q[25];


--K1L9 is fdiv1hz:inst11|LessThan~507
--operation mode is normal

K1L9 = K1L5 & K1L6 & K1L7 & K1L8;


--R1_safe_q[26] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[26]
--operation mode is arithmetic

R1_safe_q[26]_carry_eqn = R1L25;
R1_safe_q[26]_lut_out = R1_safe_q[26] $ (!R1_safe_q[26]_carry_eqn);
R1_safe_q[26] = DFFEAS(R1_safe_q[26]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L45 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella26~COUT
--operation mode is arithmetic

R1L45 = CARRY(R1_safe_q[26] & !R1L25);


--R1_safe_q[27] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[27]
--operation mode is arithmetic

R1_safe_q[27]_carry_eqn = R1L45;
R1_safe_q[27]_lut_out = R1_safe_q[27] $ (R1_safe_q[27]_carry_eqn);
R1_safe_q[27] = DFFEAS(R1_safe_q[27]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L65 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella27~COUT
--operation mode is arithmetic

R1L65 = CARRY(!R1L45 # !R1_safe_q[27]);


--K1L01 is fdiv1hz:inst11|LessThan~508
--operation mode is normal

K1L01 = !R1_safe_q[26] & !R1_safe_q[27];


--R1_safe_q[30] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[30]
--operation mode is arithmetic

R1_safe_q[30]_carry_eqn = R1L06;
R1_safe_q[30]_lut_out = R1_safe_q[30] $ (!R1_safe_q[30]_carry_eqn);
R1_safe_q[30] = DFFEAS(R1_safe_q[30]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L26 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella30~COUT
--operation mode is arithmetic

R1L26 = CARRY(R1_safe_q[30] & !R1L06);


--R1_safe_q[28] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[28]
--operation mode is arithmetic

R1_safe_q[28]_carry_eqn = R1L65;
R1_safe_q[28]_lut_out = R1_safe_q[28] $ (!R1_safe_q[28]_carry_eqn);
R1_safe_q[28] = DFFEAS(R1_safe_q[28]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L85 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella28~COUT
--operation mode is arithmetic

R1L85 = CARRY(R1_safe_q[28] & !R1L65);


--R1_safe_q[29] is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|safe_q[29]
--operation mode is arithmetic

R1_safe_q[29]_carry_eqn = R1L85;
R1_safe_q[29]_lut_out = R1_safe_q[29] $ (R1_safe_q[29]_carry_eqn);
R1_safe_q[29] = DFFEAS(R1_safe_q[29]_lut_out, L1_clk_out, VCC, , , , , K1L1, );

--R1L06 is fdiv1hz:inst11|lpm_counter:cnt_rtl_4|cntr_hc7:auto_generated|counter_cella29~COUT
--operation mode is arithmetic

R1L06 = CARRY(!R1L85 # !R1_safe_q[29]);


--K1L11 is fdiv1hz:inst11|LessThan~509
--operation mode is normal

K1L11 = K1L01 & !R1_safe_q[30] & !R1_safe_q[28] & !R1_safe_q[29];


--K1L1 is fdiv1hz:inst11|LessThan~256
--operation mode is normal

K1L1 = !R1_safe_q[31] & !K1L11 # !K1L9 # !K1L4;


--H1L61 is dispmux:inst8|D_OUT[3]~747
--operation mode is normal

H1L61 = J1_D_OUT[0] & B1_sdata[0] & !H1L21 # !H1L51 # !J1_D_OUT[0] & !H1L21 # !H1L51;


--D1L1 is counter55:inst2|CData0[0]~21
--operation mode is normal

D1L1 = B1_sdata[0] # D1L91 $ !D1L22 # !Reset;


--D1L3 is counter55:inst2|CData1[0]~45
--operation mode is normal

D1L3 = B1_sdata[0] # Q1L21 # !D1L22 # !Reset;


--H1L41 is dispmux:inst8|D_OUT[3]~730
--operation mode is normal

H1L41 = J1_D_OUT[0] & !B1_sdata[0] & D1L01 $ H1L31;


--Reset is Reset
--operation mode is input

Reset = INPUT();


--SW is SW
--operation mode is input

SW = INPUT();


--CLK is CLK
--operation mode is input

CLK = INPUT();


--Red1 is Red1
--operation mode is output

Red1 = OUTPUT(M1L3);


--Red2 is Red2
--operation mode is output

Red2 = OUTPUT(M1L4);


--Yellow1 is Yellow1
--operation mode is output

Yellow1 = OUTPUT(M1L5);


--Yellow2 is Yellow2
--operation mode is output

Yellow2 = OUTPUT(M1L6);


--Green1 is Green1
--operation mode is output

Green1 = OUTPUT(!M1L1);


--Green2 is Green2
--operation mode is output

Green2 = OUTPUT(M1L2);


--SEG_Data[7] is SEG_Data[7]
--operation mode is output

SEG_Data[7] = OUTPUT(!G1L5);


--SEG_Data[6] is SEG_Data[6]
--operation mode is output

SEG_Data[6] = OUTPUT(!G1L6);


--SEG_Data[5] is SEG_Data[5]
--operation mode is output

SEG_Data[5] = OUTPUT(!G1L7);


--SEG_Data[4] is SEG_Data[4]
--operation mode is output

SEG_Data[4] = OUTPUT(!G1L4);


--SEG_Data[3] is SEG_Data[3]
--operation mode is output

SEG_Data[3] = OUTPUT(!G1L3);


--SEG_Data[2] is SEG_Data[2]
--operation mode is output

SEG_Data[2] = OUTPUT(!G1L2);


--SEG_Data[1] is SEG_Data[1]
--operation mode is output

SEG_Data[1] = OUTPUT(G1L1);


--SEG_Data[0] is SEG_Data[0]
--operation mode is output

SEG_Data[0] = OUTPUT(GND);


--SEG_Sel[1] is SEG_Sel[1]
--operation mode is output

SEG_Sel[1] = OUTPUT(!J1_D_OUT[0]);


--SEG_Sel[0] is SEG_Sel[0]
--operation mode is output

SEG_Sel[0] = OUTPUT(J1_D_OUT[0]);


