*Heading
 static
** Job name: link Model name: Model-1
*Preprint, echo=NO, model=NO, history=NO, contact=NO
**
** PARTS
**
*Part, name=link
*Node
      1,         400.,         300.
      2,           0.,         300.
      3,         400.,           0.
      4,           0.,           0.
*Element, type=T2D2
1, 1, 2
2, 1, 3
3, 3, 4
4, 4, 1
*Nset, nset=_PickedSet2, internal, generate
 1,  4,  1
*Elset, elset=_PickedSet2, internal, generate
 1,  4,  1
** Region: (Section-1:Picked)
*Elset, elset=_PickedSet2, internal, generate
 1,  4,  1
** Section: Section-1
*Solid Section, elset=_PickedSet2, material=mat01
100.,
*End Part
**  
**
** ASSEMBLY
**
*Assembly, name=Assembly
**  
*Instance, name=link-1, part=link
*End Instance
**  
*Nset, nset=_PickedSet4, internal, instance=link-1
 2,
*Nset, nset=_PickedSet5, internal, instance=link-1
 4,
*Nset, nset=_PickedSet6, internal, instance=link-1
 3,
*Nset, nset=_PickedSet7, internal, instance=link-1
 1,
*Nset, nset=_PickedSet8, internal, instance=link-1
 3,
*End Assembly
** 
** MATERIALS
** 
*Material, name=mat01
*Elastic
295000.,0.
** ----------------------------------------------------------------
** 
** STEP: Step-1
** 
*Step, name=Step-1
sdgfsdgfsdg
*Static
1., 1., 1e-05, 1.
** 
** BOUNDARY CONDITIONS
** 
** Name: BC-1 Type: Displacement/Rotation
*Boundary
_PickedSet4, 1, 1
_PickedSet4, 2, 2
** Name: BC-2 Type: Displacement/Rotation
*Boundary
_PickedSet5, 1, 1
_PickedSet5, 2, 2
** Name: BC-3 Type: Displacement/Rotation
*Boundary
_PickedSet6, 2, 2
** 
** LOADS
** 
** Name: Load-1   Type: Concentrated force
*Cload
_PickedSet7, 2, -25000.
** Name: Load-2   Type: Concentrated force
*Cload
_PickedSet8, 1, 20000.
** 
** OUTPUT REQUESTS
** 
*Restart, write, frequency=0
** 
** FIELD OUTPUT: F-Output-1
** 
*Output, field
*Node Output
CF, RF, RM, RT, U, UR, UT, V
VT
*Element Output, directions=YES
LE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
** 
** HISTORY OUTPUT: H-Output-1
** 
*Output, history
*Energy Output
ALLIE, ALLKE
*End Step
