*Heading
 My first analysis using Python script
** Job name: My-Beam Model name: My-Beam
*Preprint, echo=NO, model=NO, history=NO, contact=NO
**
** PARTS
**
*Part, name=My-Beam
*End Part
**  
**
** ASSEMBLY
**
*Assembly, name=Assembly
**  
*Instance, name=My-Beam-1, part=My-Beam
*Node
      1,           0.,           0.
      2,           0., 0.0199999996
      3,           0., 0.0399999991
      4,           0., 0.0599999987
      5,           0., 0.0799999982
      6,           0.,  0.100000001
      7,           0.,  0.119999997
      8,           0.,  0.140000001
      9,           0.,  0.159999996
     10,           0.,  0.180000007
     11,           0.,  0.200000003
*Element, type=B21
 1,  1,  2
 2,  2,  3
 3,  3,  4
 4,  4,  5
 5,  5,  6
 6,  6,  7
 7,  7,  8
 8,  8,  9
 9,  9, 10
10, 10, 11
*Nset, nset=_PickedSet2, internal, generate
  1,  11,   1
*Elset, elset=_PickedSet2, internal, generate
 1, 10,  1
*Nset, nset=_PickedSet3, internal, generate
  1,  11,   1
*Elset, elset=_PickedSet3, internal, generate
 1, 10,  1
** Region: (Sect-Beam:Picked), (Beam Orientation:Picked)
*Elset, elset=_PickedSet2, internal, generate
 1, 10,  1
** Section: Sect-Beam  Profile: Profile-Rect
*Beam General Section, elset=_PickedSet2, poisson = 0.33, density=7850., section=RECT
0.0005, 0.0005
0.,0.,-1.
 3e+12, 3e+12
*End Instance
**  
*Nset, nset=Beam-Bottom, instance=My-Beam-1
 1,
*Nset, nset=Beam-Top, instance=My-Beam-1
 11,
*Nset, nset=Beam_All, instance=My-Beam-1, generate
  1,  11,   1
*Elset, elset=Beam_All, instance=My-Beam-1, generate
 1, 10,  1
*End Assembly
** 
** BOUNDARY CONDITIONS
** 
** Name: Fixed-Bottom Type: Displacement/Rotation
*Boundary
Beam-Bottom, 1, 1
Beam-Bottom, 2, 2
Beam-Bottom, 6, 6
** ----------------------------------------------------------------
** 
** STEP: Step-1
** 
*Step, name=Step-1, nlgeom=YES, inc=10000
Apply force on the top of beam
*Static
0.1, 1., 1e-05, 1.
** 
** LOADS
** 
** Name: CForce   Type: Concentrated force
*Cload
Beam-Top, 1, 0.5
Beam-Top, 2, -50.
** 
** OUTPUT REQUESTS
** 
*Restart, write, frequency=0
** 
** FIELD OUTPUT: Reaction-force
** 
*Output, field
*Node Output
RF, RT
** 
** FIELD OUTPUT: F-Output-1
** 
*Output, field, variable=PRESELECT
** 
** HISTORY OUTPUT: H-Output-1
** 
*Output, history, variable=PRESELECT
*End Step
