--sld_ela_trigger_flow_sel CONDITION_WIDTH=1 POST_FILL_COUNT_WIDTH=7 RESOURCE_WIDTH=1 STATE_WIDTH=2 TRIGGER_FLOW_ENTITY_NAME="sld_reserved_FFT_auto_signaltap_0_flow_mgr_1f2a" acq_clk condition_met config_clk config_enable config_in config_out current_resource_value current_state final_trigger post_fill_count reset segment_trigger start_acq use_post_fill_count
--VERSION_BEGIN 7.2 cbx_mgl 2007:08:03:15:48:12:SJ cbx_sld_ela_trigger_flow_sel 2007:08:30:11:07:14:SJ  VERSION_END


-- Copyright (C) 1991-2007 Altera Corporation
--  Your use of Altera Corporation's design tools, logic functions 
--  and other software and tools, and its AMPP partner logic 
--  functions, and any output files from any of the foregoing 
--  (including device programming or simulation files), and any 
--  associated documentation or information are expressly subject 
--  to the terms and conditions of the Altera Program License 
--  Subscription Agreement, Altera MegaCore Function License 
--  Agreement, or other applicable license agreement, including, 
--  without limitation, that your use is for the sole purpose of 
--  programming logic devices manufactured by Altera and sold by 
--  Altera or its authorized distributors.  Please refer to the 
--  applicable agreement for further details.


FUNCTION sld_reserved_FFT_auto_signaltap_0_flow_mgr_1f2a (acq_clk, condition_met[0..0], config_clk, config_enable, config_in, reset, start_acq)
RETURNS ( config_out, current_resource_value[0..0], current_state[1..0], final_trigger, post_fill_count[6..0], segment_trigger, use_post_fill_count);

--synthesis_resources = sld_reserved_FFT_auto_signaltap_0_flow_mgr_1f2a 1 
SUBDESIGN sld_ela_trigger_flow_sel_q631
( 
	acq_clk	:	input;
	condition_met[0..0]	:	input;
	config_clk	:	input;
	config_enable	:	input;
	config_in	:	input;
	config_out	:	output;
	current_resource_value[0..0]	:	output;
	current_state[1..0]	:	output;
	final_trigger	:	output;
	post_fill_count[6..0]	:	output;
	reset	:	input;
	segment_trigger	:	output;
	start_acq	:	input;
	use_post_fill_count	:	output;
) 
VARIABLE 
	mgl_prim1 : sld_reserved_FFT_auto_signaltap_0_flow_mgr_1f2a;

BEGIN 
	mgl_prim1.acq_clk = acq_clk;
	mgl_prim1.condition_met[] = condition_met[];
	mgl_prim1.config_clk = config_clk;
	mgl_prim1.config_enable = config_enable;
	mgl_prim1.config_in = config_in;
	mgl_prim1.reset = reset;
	mgl_prim1.start_acq = start_acq;
	config_out = mgl_prim1.config_out;
	current_resource_value[] = mgl_prim1.current_resource_value[];
	current_state[] = mgl_prim1.current_state[];
	final_trigger = mgl_prim1.final_trigger;
	post_fill_count[] = mgl_prim1.post_fill_count[];
	segment_trigger = mgl_prim1.segment_trigger;
	use_post_fill_count = mgl_prim1.use_post_fill_count;
END;
--VALID FILE
