# Copyright (C) 1991-2007 Altera Corporation
# Your use of Altera Corporation's design tools, logic functions 
# and other software and tools, and its AMPP partner logic 
# functions, and any output files from any of the foregoing 
# (including device programming or simulation files), and any 
# associated documentation or information are expressly subject 
# to the terms and conditions of the Altera Program License 
# Subscription Agreement, Altera MegaCore Function License 
# Agreement, or other applicable license agreement, including, 
# without limitation, that your use is for the sole purpose of 
# programming logic devices manufactured by Altera and sold by 
# Altera or its authorized distributors.  Please refer to the 
# applicable agreement for further details.


# The default values for assignments are stored in the file
#		FFT_assignment_defaults.qdf
# If this file doesn't exist, and for assignments not listed, see file
#		assignment_defaults.qdf

# Altera recommends that you do not modify this file. This
# file is updated automatically by the Quartus II software
# and any changes you make may be lost or overwritten.


set_global_assignment -name FAMILY "Cyclone II"
set_global_assignment -name DEVICE EP2C8Q208C8
set_global_assignment -name TOP_LEVEL_ENTITY block
set_global_assignment -name ORIGINAL_QUARTUS_VERSION 7.2
set_global_assignment -name PROJECT_CREATION_TIME_DATE "23:37:51  MAY 30, 2010"
set_global_assignment -name LAST_QUARTUS_VERSION 7.2
set_global_assignment -name USE_GENERATED_PHYSICAL_CONSTRAINTS OFF -section_id eda_palace
set_global_assignment -name VERILOG_FILE T_control.v
set_global_assignment -name BDF_FILE block.bdf
set_global_assignment -name VERILOG_FILE butterfly.v
set_global_assignment -name VERILOG_FILE s2p.v
set_global_assignment -name VECTOR_WAVEFORM_FILE Waveform1.vwf
set_global_assignment -name VERILOG_FILE p2s.v
set_global_assignment -name VERILOG_FILE block_new.v
set_global_assignment -name VERILOG_FILE makeup_sign.v
set_global_assignment -name PARTITION_NETLIST_TYPE SOURCE -section_id Top
set_global_assignment -name PARTITION_COLOR 2147039 -section_id Top
set_global_assignment -name LL_ROOT_REGION ON -section_id "Root Region"
set_global_assignment -name LL_MEMBER_STATE LOCKED -section_id "Root Region"
set_instance_assignment -name PARTITION_HIERARCHY no_file_for_top_partition -to | -section_id Top
set_global_assignment -name VHDL_FILE ctrl_fft.vhd
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to clk
set_location_assignment PIN_23 -to clk
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[0]
set_location_assignment PIN_33 -to Imagdata_out[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[1]
set_location_assignment PIN_34 -to Imagdata_out[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[10]
set_location_assignment PIN_35 -to Imagdata_out[10]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[11]
set_location_assignment PIN_39 -to Imagdata_out[11]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[12]
set_location_assignment PIN_40 -to Imagdata_out[12]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[13]
set_location_assignment PIN_41 -to Imagdata_out[13]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[14]
set_location_assignment PIN_43 -to Imagdata_out[14]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[15]
set_location_assignment PIN_44 -to Imagdata_out[15]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[2]
set_location_assignment PIN_45 -to Imagdata_out[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[3]
set_location_assignment PIN_46 -to Imagdata_out[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[4]
set_location_assignment PIN_47 -to Imagdata_out[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[5]
set_location_assignment PIN_48 -to Imagdata_out[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[6]
set_location_assignment PIN_56 -to Imagdata_out[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[7]
set_location_assignment PIN_57 -to Imagdata_out[7]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[8]
set_location_assignment PIN_58 -to Imagdata_out[8]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Imagdata_out[9]
set_location_assignment PIN_59 -to Imagdata_out[9]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[0]
set_location_assignment PIN_60 -to Realdata_out[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[1]
set_location_assignment PIN_61 -to Realdata_out[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[10]
set_location_assignment PIN_63 -to Realdata_out[10]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[11]
set_location_assignment PIN_64 -to Realdata_out[11]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[12]
set_location_assignment PIN_68 -to Realdata_out[12]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[13]
set_location_assignment PIN_69 -to Realdata_out[13]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[14]
set_location_assignment PIN_70 -to Realdata_out[14]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[15]
set_location_assignment PIN_72 -to Realdata_out[15]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[2]
set_location_assignment PIN_74 -to Realdata_out[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[3]
set_location_assignment PIN_75 -to Realdata_out[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[4]
set_location_assignment PIN_76 -to Realdata_out[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[5]
set_location_assignment PIN_77 -to Realdata_out[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[6]
set_location_assignment PIN_80 -to Realdata_out[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[7]
set_location_assignment PIN_81 -to Realdata_out[7]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[8]
set_location_assignment PIN_82 -to Realdata_out[8]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to Realdata_out[9]
set_location_assignment PIN_84 -to Realdata_out[9]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[0]
set_location_assignment PIN_86 -to sin[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[1]
set_location_assignment PIN_87 -to sin[1]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[2]
set_location_assignment PIN_88 -to sin[2]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[3]
set_location_assignment PIN_90 -to sin[3]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[4]
set_location_assignment PIN_92 -to sin[4]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[5]
set_location_assignment PIN_94 -to sin[5]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[6]
set_location_assignment PIN_96 -to sin[6]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[7]
set_location_assignment PIN_95 -to sin[7]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[8]
set_location_assignment PIN_97 -to sin[8]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[9]
set_location_assignment PIN_99 -to sin[9]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[10]
set_location_assignment PIN_101 -to sin[10]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[11]
set_location_assignment PIN_102 -to sin[11]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[12]
set_location_assignment PIN_103 -to sin[12]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[13]
set_location_assignment PIN_104 -to sin[13]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[14]
set_location_assignment PIN_105 -to sin[14]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[15]
set_location_assignment PIN_106 -to sin[15]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[16]
set_location_assignment PIN_107 -to sin[16]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to sin[17]
set_location_assignment PIN_151 -to sin[17]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to source_sop
set_location_assignment PIN_110 -to source_sop
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to source_eop
set_location_assignment PIN_112 -to source_eop
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to source_valid18
set_location_assignment PIN_113 -to source_valid18
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to state[0]
set_location_assignment PIN_114 -to state[0]
set_instance_assignment -name IO_STANDARD "3.3-V LVTTL" -to state[1]
set_location_assignment PIN_115 -to state[1]
set_global_assignment -name VHDL_FILE reset_ctrl.vhd
set_global_assignment -name SIGNALTAP_FILE stp1.stp
set_global_assignment -name ENABLE_SIGNALTAP ON
set_global_assignment -name USE_SIGNALTAP_FILE stp1.stp
set_global_assignment -name SLD_NODE_CREATOR_ID 110 -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_ENTITY_NAME sld_signaltap -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[0] -to Imagdata_out[0] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[1] -to Imagdata_out[10] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[2] -to Imagdata_out[11] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[3] -to Imagdata_out[12] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[4] -to Imagdata_out[13] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[5] -to Imagdata_out[14] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[6] -to Imagdata_out[15] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[7] -to Imagdata_out[1] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[8] -to Imagdata_out[2] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[9] -to Imagdata_out[3] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[10] -to Imagdata_out[4] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[11] -to Imagdata_out[5] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[12] -to Imagdata_out[6] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[13] -to Imagdata_out[7] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[14] -to Imagdata_out[8] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[15] -to Imagdata_out[9] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[16] -to Realdata_out[0] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[17] -to Realdata_out[10] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[18] -to Realdata_out[11] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[19] -to Realdata_out[12] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[20] -to Realdata_out[13] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[21] -to Realdata_out[14] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[22] -to Realdata_out[15] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[23] -to Realdata_out[1] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[24] -to Realdata_out[2] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[25] -to Realdata_out[3] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[26] -to Realdata_out[4] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[27] -to Realdata_out[5] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[28] -to Realdata_out[6] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[29] -to Realdata_out[7] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[30] -to Realdata_out[8] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[31] -to Realdata_out[9] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[0] -to Imagdata_out[0] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[1] -to Imagdata_out[10] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[2] -to Imagdata_out[11] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[3] -to Imagdata_out[12] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[4] -to Imagdata_out[13] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[5] -to Imagdata_out[14] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[6] -to Imagdata_out[15] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[7] -to Imagdata_out[1] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[8] -to Imagdata_out[2] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[9] -to Imagdata_out[3] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[10] -to Imagdata_out[4] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[11] -to Imagdata_out[5] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[12] -to Imagdata_out[6] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[13] -to Imagdata_out[7] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[14] -to Imagdata_out[8] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[15] -to Imagdata_out[9] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[16] -to Realdata_out[0] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[17] -to Realdata_out[10] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[18] -to Realdata_out[11] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[19] -to Realdata_out[12] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[20] -to Realdata_out[13] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[21] -to Realdata_out[14] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[22] -to Realdata_out[15] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[23] -to Realdata_out[1] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[24] -to Realdata_out[2] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[25] -to Realdata_out[3] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[26] -to Realdata_out[4] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[27] -to Realdata_out[5] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[28] -to Realdata_out[6] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[29] -to Realdata_out[7] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[30] -to Realdata_out[8] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[31] -to Realdata_out[9] -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_NODE_INFO=805334528" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_POWER_UP_TRIGGER=0" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_TRIGGER_LEVEL=1" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_TRIGGER_IN_ENABLED=1" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_ADVANCED_TRIGGER_ENTITY=basic,1," -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_TRIGGER_LEVEL_PIPELINE=1" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_ENABLE_ADVANCED_TRIGGER=0" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_STATE_FLOW_USE_GENERATED=0" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_STATE_BITS=11" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_BUFFER_FULL_STOP=1" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_CURRENT_RESOURCE_WIDTH=1" -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[33] -to sin[0] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[34] -to sin[10] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[35] -to sin[11] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[36] -to sin[12] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[37] -to sin[13] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[38] -to sin[14] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[39] -to sin[15] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[33] -to sin[0] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[34] -to sin[10] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[35] -to sin[11] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[36] -to sin[12] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[37] -to sin[13] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[38] -to sin[14] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[39] -to sin[15] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_clk -to clk -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_SEGMENT_SIZE=2048" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_SAMPLE_DEPTH=2048" -section_id auto_signaltap_0
set_location_assignment PIN_206 -to aclr
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[32] -to aclr -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[32] -to aclr -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT trigger_in -to aclr -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[40] -to sin[1] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[41] -to sin[2] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[42] -to sin[3] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[43] -to sin[4] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[44] -to sin[5] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[45] -to sin[6] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[46] -to sin[7] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[47] -to sin[8] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[48] -to sin[9] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[49] -to source_eop -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[50] -to source_sop -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[51] -to source_valid18 -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[52] -to state[0] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_trigger_in[53] -to state[1] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[40] -to sin[1] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[41] -to sin[2] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[42] -to sin[3] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[43] -to sin[4] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[44] -to sin[5] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[45] -to sin[6] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[46] -to sin[7] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[47] -to sin[8] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[48] -to sin[9] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[49] -to source_eop -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[50] -to source_sop -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[51] -to source_valid18 -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[52] -to state[0] -section_id auto_signaltap_0
set_instance_assignment -name CONNECT_TO_SLD_NODE_ENTITY_PORT acq_data_in[53] -to state[1] -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_DATA_BITS=54" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_TRIGGER_BITS=54" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_INVERSION_MASK=0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_INVERSION_MASK_LENGTH=187" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_NODE_CRC_LOWORD=3297" -section_id auto_signaltap_0
set_global_assignment -name SLD_NODE_PARAMETER_ASSIGNMENT "SLD_NODE_CRC_HIWORD=32016" -section_id auto_signaltap_0