///////////////////////////////////////////////////////////////////////////////
//                                                                            /
// IAR 8051 C/C++ Compiler V7.30B/W32                   12/Sep/2010  21:57:23 /
// Copyright 2004-2007 IAR Systems. All rights reserved.                      /
//                                                                            /
//    Core               =  plain                                             /
//    Code model         =  banked                                            /
//    Data model         =  large                                             /
//    Calling convention =  xdata reentrant                                   /
//    Constant location  =  data                                              /
//    Dptr setup         =  1,16                                              /
//    Source file        =  C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Compon /
//                          ents\hal\target\CC2430BB\hal_dma.c                /
//    Command line       =  -f "C:\Texas Instruments                          /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\Tools\CC2430DB\f8wRouter. /
//                          cfg" (-DCPU32MHZ -DFORCE_MAC_NEAR                 /
//                          -DROOT=__near_func -DMAC_CFG_APP_PENDING_QUEUE=TR /
//                          UE -DRTR_NWK -DBLINK_LEDS "-DCONST=const __code"  /
//                          -DGENERIC=__generic) -f "C:\Texas Instruments     /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\Tools\CC2430DB\f8wConfig. /
//                          cfg" (-DSECURE=1 -DDEFAULT_CHANLIST=0x04000000    /
//                          -DZDAPP_CONFIG_PAN_ID=0x00FF                      /
//                          -DNWK_START_DELAY=100 -DEXTENDED_JOINING_RANDOM_M /
//                          ASK=0x007F -DBEACON_REQUEST_DELAY=100             /
//                          -DBEACON_REQ_DELAY_MASK=0x00FF                    /
//                          -DROUTE_EXPIRY_TIME=30 -DAPSC_ACK_WAIT_DURATION_P /
//                          OLLED=3000 -DNWK_INDIRECT_MSG_TIMEOUT=7           /
//                          -DMAX_RREQ_ENTRIES=10 -DAPSC_MAX_FRAME_RETRIES=3  /
//                          -DNWK_MAX_DATA_RETRIES=2                          /
//                          -DMAX_POLL_FAILURE_RETRIES=2 -DMAX_BCAST=9        /
//                          -DAPS_MAX_GROUPS=16 -DMAX_RTG_ENTRIES=20          /
//                          -DNWK_MAX_BINDING_ENTRIES=10                      /
//                          -DMAX_BINDING_CLUSTER_IDS=5                       /
//                          "-DDEFAULT_KEY={0x02, 0x03, 0x05, 0x07, 0x09,     /
//                          0x0B, 0x0D, 0x0F, 0x00, 0x02, 0x04, 0x06, 0x08,   /
//                          0x0A, 0x0C, 0x0D}" -DRFD_RCVC_ALWAYS_ON=FALSE     /
//                          -DPOLL_RATE=1000 -DQUEUED_POLL_RATE=100           /
//                          -DRESPONSE_POLL_RATE=100) -DREJOIN_POLL_RATE=440  /
//                          "C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Compo /
//                          nents\hal\target\CC2430BB\hal_dma.c" -D CC2430EB  /
//                          -D LOCATION_REFNODE -D xNV_RESTORE -D ZTOOL_P1    /
//                          -D MT_TASK -D POWER_SAVING -D                     /
//                          HAL_UART_BIG_TX_BUF=1 -D                          /
//                          SPI_MGR_DEFAULT_MAX_TX_BUFF=1024 -D               /
//                          SPI_MGR_DEFAULT_OVERFLOW=1 -lC "C:\Texas          /
//                          Instruments 33\ZStack-1.4.3-1.2.1\Projects\zstack /
//                          \Project\Location\CC2430DB\RefNode\List\" -lA     /
//                          "C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Proje /
//                          cts\zstack\Project\Location\CC2430DB\RefNode\List /
//                          \" --diag_suppress Pe001,Pa010 --diag_remark      /
//                          pe550 -o "C:\Texas Instruments                    /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\RefNode\Obj\" -e                   /
//                          --require_prototypes -z9 --no_code_motion         /
//                          --debug --core=plain --dptr=16,1                  /
//                          --data_model=large --code_model=banked            /
//                          --calling_convention=xdata_reentrant              /
//                          --place_constants=data --nr_virtual_regs 8 -I     /
//                          "C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Proje /
//                          cts\zstack\Project\Location\CC2430DB\" -I         /
//                          "C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Proje /
//                          cts\zstack\Project\Location\CC2430DB\..\SOURCE\"  /
//                          -I "C:\Texas Instruments                          /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\ZMAIN\TI2430DB\" -I       /
//                          "C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Proje /
//                          cts\zstack\Project\Location\CC2430DB\..\..\..\..\ /
//                          ..\COMPONENTS\MT\" -I "C:\Texas Instruments       /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\HAL\INCL /
//                          UDE\" -I "C:\Texas Instruments                    /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\HAL\TARG /
//                          ET\CC2430BB\" -I "C:\Texas Instruments            /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\OSAL\MCU /
//                          \CCSOC\" -I "C:\Texas Instruments                 /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\OSAL\INC /
//                          LUDE\" -I "C:\Texas Instruments                   /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\STACK\AF /
//                          \" -I "C:\Texas Instruments                       /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\STACK\NW /
//                          K\" -I "C:\Texas Instruments                      /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\STACK\SE /
//                          C\" -I "C:\Texas Instruments                      /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\STACK\SY /
//                          S\" -I "C:\Texas Instruments                      /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\STACK\ZD /
//                          O\" -I "C:\Texas Instruments                      /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\ZMAC\F8W /
//                          \" -I "C:\Texas Instruments                       /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\ZMAC\"   /
//                          -I "C:\Texas Instruments                          /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\SERVICES /
//                          \SADDR\" -I "C:\Texas Instruments                 /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\SERVICES /
//                          \SDATA\" -I "C:\Texas Instruments                 /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\MAC\INCL /
//                          UDE\" -I "C:\Texas Instruments                    /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\MAC\HIGH /
//                          _LEVEL\" -I "C:\Texas Instruments                 /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\MAC\LOW_ /
//                          LEVEL\SRF03\" -I "C:\Texas Instruments            /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\MAC\LOW_ /
//                          LEVEL\SRF03\SINGLE_CHIP\" -I "C:\Program          /
//                          Files\IAR Systems\Embedded Workbench 4.0          /
//                          Evaluation version\8051\INC\" -I "C:\Program      /
//                          Files\IAR Systems\Embedded Workbench 4.0          /
//                          Evaluation version\8051\INC\CLIB\"                /
//    List file          =  C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Projec /
//                          ts\zstack\Project\Location\CC2430DB\RefNode\List\ /
//                          hal_dma.s51                                       /
//                                                                            /
//                                                                            /
///////////////////////////////////////////////////////////////////////////////

        NAME hal_dma

        RTMODEL "__calling_convention", "xdata_reentrant"
        RTMODEL "__code_model", "banked"
        RTMODEL "__core", "plain"
        RTMODEL "__data_model", "large"
        RTMODEL "__dptr_size", "16"
        RTMODEL "__extended_stack", "disabled"
        RTMODEL "__location_for_constants", "data"
        RTMODEL "__number_of_dptrs", "1"
        RTMODEL "__rt_version", "1"

        RSEG DOVERLAY:DATA:NOROOT(0)
        RSEG IOVERLAY:IDATA:NOROOT(0)
        RSEG ISTACK:IDATA:NOROOT(0)
        RSEG PSTACK:XDATA:NOROOT(0)
        RSEG XSTACK:XDATA:NOROOT(0)

        EXTERN ?BDISPATCH
        EXTERN ?BRET
        EXTERN __INIT_XDATA_Z

        PUBLIC ??HalDmaInit?relay
        FUNCTION ??HalDmaInit?relay,0203H
        PUBWEAK DMA0CFGH
        PUBWEAK DMA0CFGL
        PUBWEAK DMA1CFGH
        PUBWEAK DMA1CFGL
        PUBLIC HalDmaInit
        FUNCTION HalDmaInit,0203H
        ARGFRAME XSTACK, 0, STACK
        PUBLIC dmaCh0
        PUBLIC dmaCh1234
        
        CFI Names cfiNames0
        CFI StackFrame CFA_SP SP DATA
        CFI StackFrame CFA_PSP16 PSP16 XDATA
        CFI StackFrame CFA_XSP16 XSP16 XDATA
        CFI StaticOverlayFrame CFA_IOVERLAY IOVERLAY
        CFI StaticOverlayFrame CFA_DOVERLAY DOVERLAY
        CFI Resource `PSW.CY`:1, `B.BR0`:1, `B.BR1`:1, `B.BR2`:1, `B.BR3`:1
        CFI Resource `B.BR4`:1, `B.BR5`:1, `B.BR6`:1, `B.BR7`:1, `VB.BR8`:1
        CFI Resource `VB.BR9`:1, `VB.BR10`:1, `VB.BR11`:1, `VB.BR12`:1
        CFI Resource `VB.BR13`:1, `VB.BR14`:1, `VB.BR15`:1, VB:8, B:8, A:8
        CFI Resource PSW:8, DPL0:8, DPH0:8, R0:8, R1:8, R2:8, R3:8, R4:8, R5:8
        CFI Resource R6:8, R7:8, V0:8, V1:8, V2:8, V3:8, V4:8, V5:8, V6:8, V7:8
        CFI Resource SP:8, PSPH:8, PSPL:8, PSP16:16, XSPH:8, XSPL:8, XSP16:16
        CFI VirtualResource ?RET:24
        CFI Resource ?BRET_EXT:8
        CFI VirtualResource ?RET_HIGH:8, ?RET_LOW:8
        CFI ResourceParts PSP16 PSPH, PSPL
        CFI ResourceParts XSP16 XSPH, XSPL
        CFI ResourceParts ?RET ?BRET_EXT, ?RET_HIGH, ?RET_LOW
        CFI EndNames cfiNames0
        
        CFI Common cfiCommon0 Using cfiNames0
        CFI CodeAlign 1
        CFI DataAlign -1
        CFI ReturnAddress ?RET CODE
        CFI CFA_DOVERLAY Used
        CFI CFA_IOVERLAY Used
        CFI CFA_SP SP+-3
        CFI CFA_PSP16 PSP16+0
        CFI CFA_XSP16 XSP16+0
        CFI `PSW.CY` SameValue
        CFI `B.BR0` SameValue
        CFI `B.BR1` SameValue
        CFI `B.BR2` SameValue
        CFI `B.BR3` SameValue
        CFI `B.BR4` SameValue
        CFI `B.BR5` SameValue
        CFI `B.BR6` SameValue
        CFI `B.BR7` SameValue
        CFI `VB.BR8` SameValue
        CFI `VB.BR9` SameValue
        CFI `VB.BR10` SameValue
        CFI `VB.BR11` SameValue
        CFI `VB.BR12` SameValue
        CFI `VB.BR13` SameValue
        CFI `VB.BR14` SameValue
        CFI `VB.BR15` SameValue
        CFI VB SameValue
        CFI B Undefined
        CFI A Undefined
        CFI PSW SameValue
        CFI DPL0 SameValue
        CFI DPH0 SameValue
        CFI R0 Undefined
        CFI R1 Undefined
        CFI R2 Undefined
        CFI R3 Undefined
        CFI R4 Undefined
        CFI R5 Undefined
        CFI R6 SameValue
        CFI R7 SameValue
        CFI V0 SameValue
        CFI V1 SameValue
        CFI V2 SameValue
        CFI V3 SameValue
        CFI V4 SameValue
        CFI V5 SameValue
        CFI V6 SameValue
        CFI V7 SameValue
        CFI PSPH Undefined
        CFI PSPL Undefined
        CFI XSPH Undefined
        CFI XSPL Undefined
        CFI ?RET Concat
        CFI ?BRET_EXT Frame(CFA_SP, 3)
        CFI ?RET_HIGH Frame(CFA_SP, 2)
        CFI ?RET_LOW Frame(CFA_SP, 1)
        CFI EndCommon cfiCommon0
        
HalDmaInit          SYMBOL "HalDmaInit"
??HalDmaInit?relay  SYMBOL "?relay", HalDmaInit

// C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Components\hal\target\CC2430BB\hal_dma.c
//    1 /**************************************************************************************************
//    2   Filename:       hal_dma.c
//    3   Revised:        $Date: 2007-11-01 08:44:53 -0700 (Thu, 01 Nov 2007) $
//    4   Revision:       $Revision: 15821 $
//    5 
//    6   Description:    This file contains the interface to the DMA.
//    7 
//    8 
//    9   Copyright 2007 Texas Instruments Incorporated. All rights reserved.
//   10 
//   11   IMPORTANT: Your use of this Software is limited to those specific rights
//   12   granted under the terms of a software license agreement between the user
//   13   who downloaded the software, his/her employer (which must be your employer)
//   14   and Texas Instruments Incorporated (the "License").  You may not use this
//   15   Software unless you agree to abide by the terms of the License. The License
//   16   limits your use, and you acknowledge, that the Software may not be modified,
//   17   copied or distributed unless embedded on a Texas Instruments microcontroller
//   18   or used solely and exclusively in conjunction with a Texas Instruments radio
//   19   frequency transceiver, which is integrated into your product.  Other than for
//   20   the foregoing purpose, you may not use, reproduce, copy, prepare derivative
//   21   works of, modify, distribute, perform, display or sell this Software and/or
//   22   its documentation for any purpose.
//   23 
//   24   YOU FURTHER ACKNOWLEDGE AND AGREE THAT THE SOFTWARE AND DOCUMENTATION ARE
//   25   PROVIDED “AS IS” WITHOUT WARRANTY OF ANY KIND, EITHER EXPRESS OR IMPLIED, 
//   26   INCLUDING WITHOUT LIMITATION, ANY WARRANTY OF MERCHANTABILITY, TITLE, 
//   27   NON-INFRINGEMENT AND FITNESS FOR A PARTICULAR PURPOSE. IN NO EVENT SHALL
//   28   TEXAS INSTRUMENTS OR ITS LICENSORS BE LIABLE OR OBLIGATED UNDER CONTRACT,
//   29   NEGLIGENCE, STRICT LIABILITY, CONTRIBUTION, BREACH OF WARRANTY, OR OTHER
//   30   LEGAL EQUITABLE THEORY ANY DIRECT OR INDIRECT DAMAGES OR EXPENSES
//   31   INCLUDING BUT NOT LIMITED TO ANY INCIDENTAL, SPECIAL, INDIRECT, PUNITIVE
//   32   OR CONSEQUENTIAL DAMAGES, LOST PROFITS OR LOST DATA, COST OF PROCUREMENT
//   33   OF SUBSTITUTE GOODS, TECHNOLOGY, SERVICES, OR ANY CLAIMS BY THIRD PARTIES
//   34   (INCLUDING BUT NOT LIMITED TO ANY DEFENSE THEREOF), OR OTHER SIMILAR COSTS.
//   35 
//   36   Should you have any questions regarding your right to use this Software,
//   37   contact Texas Instruments Incorporated at www.TI.com. 
//   38 **************************************************************************************************/
//   39 
//   40 /*********************************************************************
//   41  * INCLUDES
//   42  */
//   43 
//   44 #include "hal_types.h"
//   45 #include "hal_defs.h"
//   46 #include "hal_dma.h"

        ASEGN SFR_AN:DATA:NOROOT,0d2H
// unsigned char volatile __sfr DMA1CFGL
DMA1CFGL:
        DS 1

        ASEGN SFR_AN:DATA:NOROOT,0d3H
// unsigned char volatile __sfr DMA1CFGH
DMA1CFGH:
        DS 1

        ASEGN SFR_AN:DATA:NOROOT,0d4H
// unsigned char volatile __sfr DMA0CFGL
DMA0CFGL:
        DS 1

        ASEGN SFR_AN:DATA:NOROOT,0d5H
// unsigned char volatile __sfr DMA0CFGH
DMA0CFGH:
        DS 1
//   47 #include "hal_mcu.h"
//   48 #include "hal_uart.h"
//   49 
//   50 #if ((defined HAL_DMA) && (HAL_DMA == TRUE))
//   51 
//   52 /*********************************************************************
//   53  * MACROS
//   54  */
//   55 
//   56 /*********************************************************************
//   57  * CONSTANTS
//   58  */
//   59 
//   60 /*********************************************************************
//   61  * TYPEDEFS
//   62  */
//   63 
//   64 /*********************************************************************
//   65  * GLOBAL VARIABLES
//   66  */
//   67 

        RSEG XDATA_Z:XDATA:NOROOT(0)
//   68 halDMADesc_t dmaCh0;
dmaCh0:
        DS 8
        REQUIRE __INIT_XDATA_Z

        RSEG XDATA_Z:XDATA:NOROOT(0)
//   69 halDMADesc_t dmaCh1234[4];
dmaCh1234:
        DS 32
        REQUIRE __INIT_XDATA_Z
//   70 
//   71 /*********************************************************************
//   72  * GLOBAL FUNCTIONS
//   73  */
//   74 
//   75 /*********************************************************************
//   76  * LOCAL VARIABLES
//   77  */
//   78 
//   79 /*********************************************************************
//   80  * LOCAL FUNCTIONS
//   81  */
//   82 
//   83 /******************************************************************************
//   84  * @fn      HalDMAInit
//   85  *
//   86  * @brief   DMA Interrupt Service Routine
//   87  *
//   88  * @param   None
//   89  *
//   90  * @return  None
//   91  *****************************************************************************/

        RSEG BANKED_CODE:CODE:NOROOT(0)
//   92 void HalDmaInit( void )
HalDmaInit:
        CFI Block cfiBlock0 Using cfiCommon0
        CFI Function HalDmaInit
//   93 {
        ; Saved register size: 0
        ; Auto size: 0
//   94   HAL_DMA_SET_ADDR_DESC0( &dmaCh0 );
        MOV     A,#((dmaCh0 >> 8) & 0xff)
        MOV     0xd5,A
        MOV     0xd4,#(dmaCh0 & 0xff)
//   95   HAL_DMA_SET_ADDR_DESC1234( dmaCh1234 );
        MOV     A,#((dmaCh1234 >> 8) & 0xff)
        MOV     0xd3,A
        MOV     0xd2,#(dmaCh1234 & 0xff)
//   96 }
        LJMP    ?BRET
        CFI EndBlock cfiBlock0
        REQUIRE DMA1CFGL
        REQUIRE DMA1CFGH
        REQUIRE DMA0CFGL
        REQUIRE DMA0CFGH

        RSEG BANK_RELAYS:CODE:REORDER:NOROOT(0)
??HalDmaInit?relay:
        LCALL   ?BDISPATCH
        DATA
        DC24    HalDmaInit

        END
//   97 
//   98 #endif  // #if ((defined HAL_DMA) && (HAL_DMA == TRUE))
//   99 /******************************************************************************
//  100 ******************************************************************************/
// 
// 17 bytes in segment BANKED_CODE
//  6 bytes in segment BANK_RELAYS
//  4 bytes in segment SFR_AN
// 40 bytes in segment XDATA_Z
// 
// 23 bytes of CODE  memory
//  0 bytes of DATA  memory (+ 4 bytes shared)
// 40 bytes of XDATA memory
//
//Errors: none
//Warnings: none
