--scfifo ADD_RAM_OUTPUT_REGISTER="OFF" DEVICE_FAMILY="Cyclone II" LPM_NUMWORDS=64 LPM_SHOWAHEAD="OFF" lpm_width=16 lpm_widthu=6 OPTIMIZE_FOR_SPEED=5 OVERFLOW_CHECKING="ON" UNDERFLOW_CHECKING="ON" USE_EAB="ON" clock data empty full q rdreq usedw wrreq CARRY_CHAIN="MANUAL" CARRY_CHAIN_LENGTH=48 CYCLONEII_M4K_COMPATIBILITY="ON" INTENDED_DEVICE_FAMILY="Stratix II" LOW_POWER_MODE="AUTO"
--VERSION_BEGIN 7.2 cbx_altdpram 2007:04:25:14:55:30:SJ cbx_altsyncram 2007:08:27:07:35:30:SJ cbx_cycloneii 2007:06:13:15:47:32:SJ cbx_fifo_common 2007:04:09:14:30:26:SJ cbx_lpm_add_sub 2007:08:06:16:01:34:SJ cbx_lpm_compare 2007:06:21:15:54:06:SJ cbx_lpm_counter 2007:08:07:01:40:08:SJ cbx_lpm_decode 2007:03:12:19:01:52:SJ cbx_lpm_mux 2007:05:11:14:07:38:SJ cbx_mgl 2007:08:03:15:48:12:SJ cbx_scfifo 2007:04:06:15:45:12:SJ cbx_stratix 2007:05:02:16:27:14:SJ cbx_stratixii 2007:06:28:17:26:26:SJ cbx_stratixiii 2007:06:28:17:15:56:SJ cbx_util_mgl 2007:06:01:06:37:30:SJ  VERSION_END


-- Copyright (C) 1991-2007 Altera Corporation
--  Your use of Altera Corporation's design tools, logic functions 
--  and other software and tools, and its AMPP partner logic 
--  functions, and any output files from any of the foregoing 
--  (including device programming or simulation files), and any 
--  associated documentation or information are expressly subject 
--  to the terms and conditions of the Altera Program License 
--  Subscription Agreement, Altera MegaCore Function License 
--  Agreement, or other applicable license agreement, including, 
--  without limitation, that your use is for the sole purpose of 
--  programming logic devices manufactured by Altera and sold by 
--  Altera or its authorized distributors.  Please refer to the 
--  applicable agreement for further details.


FUNCTION a_dpfifo_ck31 (clock, data[15..0], rreq, sclr, wreq)
RETURNS ( empty, full, q[15..0], usedw[5..0]);

--synthesis_resources = lut 12 M4K 1 reg 12 
SUBDESIGN scfifo_5e31
( 
	clock	:	input;
	data[15..0]	:	input;
	empty	:	output;
	full	:	output;
	q[15..0]	:	output;
	rdreq	:	input;
	usedw[5..0]	:	output;
	wrreq	:	input;
) 
VARIABLE 
	dpfifo : a_dpfifo_ck31;
	sclr	: NODE;

BEGIN 
	dpfifo.clock = clock;
	dpfifo.data[] = data[];
	dpfifo.rreq = rdreq;
	dpfifo.sclr = sclr;
	dpfifo.wreq = wrreq;
	empty = dpfifo.empty;
	full = dpfifo.full;
	q[] = dpfifo.q[];
	sclr = GND;
	usedw[] = dpfifo.usedw[];
END;
--VALID FILE
