///////////////////////////////////////////////////////////////////////////////
//                                                                            /
// IAR 8051 C/C++ Compiler V7.30B/W32                   12/Sep/2010  21:57:29 /
// Copyright 2004-2007 IAR Systems. All rights reserved.                      /
//                                                                            /
//    Core               =  plain                                             /
//    Code model         =  banked                                            /
//    Data model         =  large                                             /
//    Calling convention =  xdata reentrant                                   /
//    Constant location  =  data                                              /
//    Dptr setup         =  1,16                                              /
//    Source file        =  C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Compon /
//                          ents\mt\MT_NWK.c                                  /
//    Command line       =  -f "C:\Texas Instruments                          /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\Tools\CC2430DB\f8wRouter. /
//                          cfg" (-DCPU32MHZ -DFORCE_MAC_NEAR                 /
//                          -DROOT=__near_func -DMAC_CFG_APP_PENDING_QUEUE=TR /
//                          UE -DRTR_NWK -DBLINK_LEDS "-DCONST=const __code"  /
//                          -DGENERIC=__generic) -f "C:\Texas Instruments     /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\Tools\CC2430DB\f8wConfig. /
//                          cfg" (-DSECURE=1 -DDEFAULT_CHANLIST=0x04000000    /
//                          -DZDAPP_CONFIG_PAN_ID=0x00FF                      /
//                          -DNWK_START_DELAY=100 -DEXTENDED_JOINING_RANDOM_M /
//                          ASK=0x007F -DBEACON_REQUEST_DELAY=100             /
//                          -DBEACON_REQ_DELAY_MASK=0x00FF                    /
//                          -DROUTE_EXPIRY_TIME=30 -DAPSC_ACK_WAIT_DURATION_P /
//                          OLLED=3000 -DNWK_INDIRECT_MSG_TIMEOUT=7           /
//                          -DMAX_RREQ_ENTRIES=10 -DAPSC_MAX_FRAME_RETRIES=3  /
//                          -DNWK_MAX_DATA_RETRIES=2                          /
//                          -DMAX_POLL_FAILURE_RETRIES=2 -DMAX_BCAST=9        /
//                          -DAPS_MAX_GROUPS=16 -DMAX_RTG_ENTRIES=20          /
//                          -DNWK_MAX_BINDING_ENTRIES=10                      /
//                          -DMAX_BINDING_CLUSTER_IDS=5                       /
//                          "-DDEFAULT_KEY={0x02, 0x03, 0x05, 0x07, 0x09,     /
//                          0x0B, 0x0D, 0x0F, 0x00, 0x02, 0x04, 0x06, 0x08,   /
//                          0x0A, 0x0C, 0x0D}" -DRFD_RCVC_ALWAYS_ON=FALSE     /
//                          -DPOLL_RATE=1000 -DQUEUED_POLL_RATE=100           /
//                          -DRESPONSE_POLL_RATE=100) -DREJOIN_POLL_RATE=440  /
//                          "C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Compo /
//                          nents\mt\MT_NWK.c" -D CC2430EB -D                 /
//                          LOCATION_REFNODE -D xNV_RESTORE -D ZTOOL_P1 -D    /
//                          MT_TASK -D POWER_SAVING -D HAL_UART_BIG_TX_BUF=1  /
//                          -D SPI_MGR_DEFAULT_MAX_TX_BUFF=1024 -D            /
//                          SPI_MGR_DEFAULT_OVERFLOW=1 -lC "C:\Texas          /
//                          Instruments 33\ZStack-1.4.3-1.2.1\Projects\zstack /
//                          \Project\Location\CC2430DB\RefNode\List\" -lA     /
//                          "C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Proje /
//                          cts\zstack\Project\Location\CC2430DB\RefNode\List /
//                          \" --diag_suppress Pe001,Pa010 --diag_remark      /
//                          pe550 -o "C:\Texas Instruments                    /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\RefNode\Obj\" -e                   /
//                          --require_prototypes -z9 --no_code_motion         /
//                          --debug --core=plain --dptr=16,1                  /
//                          --data_model=large --code_model=banked            /
//                          --calling_convention=xdata_reentrant              /
//                          --place_constants=data --nr_virtual_regs 8 -I     /
//                          "C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Proje /
//                          cts\zstack\Project\Location\CC2430DB\" -I         /
//                          "C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Proje /
//                          cts\zstack\Project\Location\CC2430DB\..\SOURCE\"  /
//                          -I "C:\Texas Instruments                          /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\ZMAIN\TI2430DB\" -I       /
//                          "C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Proje /
//                          cts\zstack\Project\Location\CC2430DB\..\..\..\..\ /
//                          ..\COMPONENTS\MT\" -I "C:\Texas Instruments       /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\HAL\INCL /
//                          UDE\" -I "C:\Texas Instruments                    /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\HAL\TARG /
//                          ET\CC2430BB\" -I "C:\Texas Instruments            /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\OSAL\MCU /
//                          \CCSOC\" -I "C:\Texas Instruments                 /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\OSAL\INC /
//                          LUDE\" -I "C:\Texas Instruments                   /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\STACK\AF /
//                          \" -I "C:\Texas Instruments                       /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\STACK\NW /
//                          K\" -I "C:\Texas Instruments                      /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\STACK\SE /
//                          C\" -I "C:\Texas Instruments                      /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\STACK\SY /
//                          S\" -I "C:\Texas Instruments                      /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\STACK\ZD /
//                          O\" -I "C:\Texas Instruments                      /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\ZMAC\F8W /
//                          \" -I "C:\Texas Instruments                       /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\ZMAC\"   /
//                          -I "C:\Texas Instruments                          /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\SERVICES /
//                          \SADDR\" -I "C:\Texas Instruments                 /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\SERVICES /
//                          \SDATA\" -I "C:\Texas Instruments                 /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\MAC\INCL /
//                          UDE\" -I "C:\Texas Instruments                    /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\MAC\HIGH /
//                          _LEVEL\" -I "C:\Texas Instruments                 /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\MAC\LOW_ /
//                          LEVEL\SRF03\" -I "C:\Texas Instruments            /
//                          33\ZStack-1.4.3-1.2.1\Projects\zstack\Project\Loc /
//                          ation\CC2430DB\..\..\..\..\..\COMPONENTS\MAC\LOW_ /
//                          LEVEL\SRF03\SINGLE_CHIP\" -I "C:\Program          /
//                          Files\IAR Systems\Embedded Workbench 4.0          /
//                          Evaluation version\8051\INC\" -I "C:\Program      /
//                          Files\IAR Systems\Embedded Workbench 4.0          /
//                          Evaluation version\8051\INC\CLIB\"                /
//    List file          =  C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Projec /
//                          ts\zstack\Project\Location\CC2430DB\RefNode\List\ /
//                          MT_NWK.s51                                        /
//                                                                            /
//                                                                            /
///////////////////////////////////////////////////////////////////////////////

        NAME MT_NWK

        RTMODEL "__calling_convention", "xdata_reentrant"
        RTMODEL "__code_model", "banked"
        RTMODEL "__core", "plain"
        RTMODEL "__data_model", "large"
        RTMODEL "__dptr_size", "16"
        RTMODEL "__extended_stack", "disabled"
        RTMODEL "__location_for_constants", "data"
        RTMODEL "__number_of_dptrs", "1"
        RTMODEL "__rt_version", "1"

        RSEG DOVERLAY:DATA:NOROOT(0)
        RSEG IOVERLAY:IDATA:NOROOT(0)
        RSEG ISTACK:IDATA:NOROOT(0)
        RSEG PSTACK:XDATA:NOROOT(0)
        RSEG XSTACK:XDATA:NOROOT(0)

        EXTERN ?BANKED_ENTER_XDATA
        EXTERN ?BANKED_LEAVE_XDATA
        EXTERN ?BDISPATCH
        EXTERN ?US_SWITCH_DENSE
        EXTERN ?V0
        EXTERN __INIT_XDATA_Z

        PUBLIC ??MT_NwkCommandProcessing?relay
        FUNCTION ??MT_NwkCommandProcessing?relay,0203H
        PUBLIC MT_NwkCommandProcessing
        FUNCTION MT_NwkCommandProcessing,0a1203H
        ARGFRAME XSTACK, 0, STACK
        LOCFRAME XSTACK, 10, STACK
        PUBLIC _nwkCallbackSub
        
        CFI Names cfiNames0
        CFI StackFrame CFA_SP SP DATA
        CFI StackFrame CFA_PSP16 PSP16 XDATA
        CFI StackFrame CFA_XSP16 XSP16 XDATA
        CFI StaticOverlayFrame CFA_IOVERLAY IOVERLAY
        CFI StaticOverlayFrame CFA_DOVERLAY DOVERLAY
        CFI Resource `PSW.CY`:1, `B.BR0`:1, `B.BR1`:1, `B.BR2`:1, `B.BR3`:1
        CFI Resource `B.BR4`:1, `B.BR5`:1, `B.BR6`:1, `B.BR7`:1, `VB.BR8`:1
        CFI Resource `VB.BR9`:1, `VB.BR10`:1, `VB.BR11`:1, `VB.BR12`:1
        CFI Resource `VB.BR13`:1, `VB.BR14`:1, `VB.BR15`:1, VB:8, B:8, A:8
        CFI Resource PSW:8, DPL0:8, DPH0:8, R0:8, R1:8, R2:8, R3:8, R4:8, R5:8
        CFI Resource R6:8, R7:8, V0:8, V1:8, V2:8, V3:8, V4:8, V5:8, V6:8, V7:8
        CFI Resource SP:8, PSPH:8, PSPL:8, PSP16:16, XSPH:8, XSPL:8, XSP16:16
        CFI VirtualResource ?RET:24
        CFI Resource ?BRET_EXT:8
        CFI VirtualResource ?RET_HIGH:8, ?RET_LOW:8
        CFI ResourceParts PSP16 PSPH, PSPL
        CFI ResourceParts XSP16 XSPH, XSPL
        CFI ResourceParts ?RET ?BRET_EXT, ?RET_HIGH, ?RET_LOW
        CFI EndNames cfiNames0
        
        CFI Common cfiCommon0 Using cfiNames0
        CFI CodeAlign 1
        CFI DataAlign -1
        CFI ReturnAddress ?RET CODE
        CFI CFA_DOVERLAY Used
        CFI CFA_IOVERLAY Used
        CFI CFA_SP SP+-3
        CFI CFA_PSP16 PSP16+0
        CFI CFA_XSP16 XSP16+0
        CFI `PSW.CY` SameValue
        CFI `B.BR0` SameValue
        CFI `B.BR1` SameValue
        CFI `B.BR2` SameValue
        CFI `B.BR3` SameValue
        CFI `B.BR4` SameValue
        CFI `B.BR5` SameValue
        CFI `B.BR6` SameValue
        CFI `B.BR7` SameValue
        CFI `VB.BR8` SameValue
        CFI `VB.BR9` SameValue
        CFI `VB.BR10` SameValue
        CFI `VB.BR11` SameValue
        CFI `VB.BR12` SameValue
        CFI `VB.BR13` SameValue
        CFI `VB.BR14` SameValue
        CFI `VB.BR15` SameValue
        CFI VB SameValue
        CFI B Undefined
        CFI A Undefined
        CFI PSW SameValue
        CFI DPL0 SameValue
        CFI DPH0 SameValue
        CFI R0 Undefined
        CFI R1 Undefined
        CFI R2 Undefined
        CFI R3 Undefined
        CFI R4 Undefined
        CFI R5 Undefined
        CFI R6 SameValue
        CFI R7 SameValue
        CFI V0 SameValue
        CFI V1 SameValue
        CFI V2 SameValue
        CFI V3 SameValue
        CFI V4 SameValue
        CFI V5 SameValue
        CFI V6 SameValue
        CFI V7 SameValue
        CFI PSPH Undefined
        CFI PSPL Undefined
        CFI XSPH Undefined
        CFI XSPL Undefined
        CFI ?RET Concat
        CFI ?BRET_EXT Frame(CFA_SP, 3)
        CFI ?RET_HIGH Frame(CFA_SP, 2)
        CFI ?RET_LOW Frame(CFA_SP, 1)
        CFI EndCommon cfiCommon0
        
NLME_PermitJoiningRequest SYMBOL "NLME_PermitJoiningRequest"
??NLME_PermitJoiningRequest?relay SYMBOL "?relay", NLME_PermitJoiningRequest
MT_NwkCommandProcessing SYMBOL "MT_NwkCommandProcessing"
??MT_NwkCommandProcessing?relay SYMBOL "?relay", MT_NwkCommandProcessing

        EXTERN NLME_PermitJoiningRequest
        FUNCTION NLME_PermitJoiningRequest,0202H
        ARGFRAME ISTACK, 0, STACK
        ARGFRAME PSTACK, 0, STACK
        ARGFRAME XSTACK, 10, STACK
        ARGFRAME IOVERLAY, 0, STATIC
        ARGFRAME DOVERLAY, 0, STATIC
        EXTERN ??NLME_PermitJoiningRequest?relay
        FUNCTION ??NLME_PermitJoiningRequest?relay,00H

// C:\Texas Instruments 33\ZStack-1.4.3-1.2.1\Components\mt\MT_NWK.c
//    1 /**************************************************************************************************
//    2   Filename:       MT_NWK.c
//    3   Revised:        $Date: 2007-10-28 18:43:04 -0700 (Sun, 28 Oct 2007) $
//    4   Revision:       $Revision: 15800 $
//    5 
//    6   Description:    MonitorTest functions for the NWK layer.
//    7 
//    8 
//    9   Copyright 2004-2007 Texas Instruments Incorporated. All rights reserved.
//   10 
//   11   IMPORTANT: Your use of this Software is limited to those specific rights
//   12   granted under the terms of a software license agreement between the user
//   13   who downloaded the software, his/her employer (which must be your employer)
//   14   and Texas Instruments Incorporated (the "License").  You may not use this
//   15   Software unless you agree to abide by the terms of the License. The License
//   16   limits your use, and you acknowledge, that the Software may not be modified,
//   17   copied or distributed unless embedded on a Texas Instruments microcontroller
//   18   or used solely and exclusively in conjunction with a Texas Instruments radio
//   19   frequency transceiver, which is integrated into your product.  Other than for
//   20   the foregoing purpose, you may not use, reproduce, copy, prepare derivative
//   21   works of, modify, distribute, perform, display or sell this Software and/or
//   22   its documentation for any purpose.
//   23 
//   24   YOU FURTHER ACKNOWLEDGE AND AGREE THAT THE SOFTWARE AND DOCUMENTATION ARE
//   25   PROVIDED “AS IS” WITHOUT WARRANTY OF ANY KIND, EITHER EXPRESS OR IMPLIED, 
//   26   INCLUDING WITHOUT LIMITATION, ANY WARRANTY OF MERCHANTABILITY, TITLE, 
//   27   NON-INFRINGEMENT AND FITNESS FOR A PARTICULAR PURPOSE. IN NO EVENT SHALL
//   28   TEXAS INSTRUMENTS OR ITS LICENSORS BE LIABLE OR OBLIGATED UNDER CONTRACT,
//   29   NEGLIGENCE, STRICT LIABILITY, CONTRIBUTION, BREACH OF WARRANTY, OR OTHER
//   30   LEGAL EQUITABLE THEORY ANY DIRECT OR INDIRECT DAMAGES OR EXPENSES
//   31   INCLUDING BUT NOT LIMITED TO ANY INCIDENTAL, SPECIAL, INDIRECT, PUNITIVE
//   32   OR CONSEQUENTIAL DAMAGES, LOST PROFITS OR LOST DATA, COST OF PROCUREMENT
//   33   OF SUBSTITUTE GOODS, TECHNOLOGY, SERVICES, OR ANY CLAIMS BY THIRD PARTIES
//   34   (INCLUDING BUT NOT LIMITED TO ANY DEFENSE THEREOF), OR OTHER SIMILAR COSTS.
//   35 
//   36   Should you have any questions regarding your right to use this Software,
//   37   contact Texas Instruments Incorporated at www.TI.com. 
//   38 **************************************************************************************************/
//   39 
//   40 /*********************************************************************
//   41  * INCLUDES
//   42  */
//   43 #include "ZComDef.h"
//   44 #include "OSAL.h"
//   45 #include "MTEL.h"
//   46 #include "NLMEDE.h"
//   47 #include "nwk.h"
//   48 #include "ZDApp.h"
//   49 #include "nwk_globals.h"
//   50 #include "MT_NWK.h"
//   51 
//   52 #if !defined( WIN32 )
//   53   #include "OnBoard.h"
//   54 #endif
//   55 
//   56 /*********************************************************************
//   57  * MACROS
//   58  */
//   59 
//   60 /*********************************************************************
//   61  * CONSTANTS
//   62  */
//   63 
//   64 /*********************************************************************
//   65  * TYPEDEFS
//   66  */
//   67 
//   68 /*********************************************************************
//   69  * GLOBAL VARIABLES
//   70  */

        RSEG XDATA_Z:XDATA:NOROOT(0)
//   71 uint16 _nwkCallbackSub;
_nwkCallbackSub:
        DS 2
        REQUIRE __INIT_XDATA_Z
//   72 
//   73 /*********************************************************************
//   74  * EXTERNAL VARIABLES
//   75  */
//   76 
//   77 /*********************************************************************
//   78  * EXTERNAL FUNCTIONS
//   79  */
//   80 
//   81 /*********************************************************************
//   82  * LOCAL VARIABLES
//   83  */
//   84 
//   85 /*********************************************************************
//   86  * LOCAL FUNCTIONS
//   87  */
//   88 #if defined ( MT_NWK_FUNC )  //NWK commands
//   89 uint8 MT_Nwk_DataRequest( uint16 dstAddr, uint8 nsduLen, uint8* nsdu,
//   90                          uint8 nsduHandle, uint16 nsduHandleOptions,
//   91                          uint8 secure, uint8 discoverRoute,
//   92                          uint8 radius);
//   93 
//   94 uint8 MT_Nwk_DataRequest( uint16 dstAddr, uint8 nsduLen, uint8* nsdu,
//   95                          uint8 nsduHandle, uint16 nsduHandleOptions,
//   96                          uint8 secure, uint8 discoverRoute,
//   97                          uint8 radius)
//   98 {
//   99     uint8               status;
//  100     NLDE_DataReqAlloc_t dra;
//  101     NLDE_DataReq_t*     req;
//  102 
//  103 
//  104     dra.overhead = sizeof(NLDE_DataReq_t);
//  105     dra.nsduLen  = nsduLen;
//  106     dra.secure   = secure;
//  107 
//  108     req = NLDE_DataReqAlloc(&dra);
//  109 
//  110     if ( req != NULL )
//  111     {
//  112       osal_memcpy(req->nfd.nsdu, nsdu, nsduLen);
//  113 
//  114       req->nfd.dstAddr           = dstAddr;
//  115       req->nfd.nsduHandleOptions = nsduHandleOptions;
//  116       req->nfd.discoverRoute     = discoverRoute;
//  117       req->nfd.radius            = radius;
//  118 
//  119       status = NLDE_DataReq( req );
//  120     }
//  121     else
//  122     {
//  123       status = ZMemError;
//  124     }
//  125 
//  126     return status;
//  127 }
//  128 #endif // defined ( MT_NWK_FUNC )
//  129 
//  130 /*********************************************************************
//  131  * @fn      MT_NwkCommandProcessing
//  132  *
//  133  * @brief
//  134  *
//  135  *   Process all the NWK commands that are issued by test tool
//  136  *
//  137  * @param   cmd_id - Command ID
//  138  * @param   len    - Length of received SPI data message
//  139  * @param   pData  - pointer to received SPI data message
//  140  *
//  141  * @return  void
//  142  */

        RSEG BANKED_CODE:CODE:NOROOT(0)
//  143 void MT_NwkCommandProcessing( uint16 cmd_id , byte len , byte *pData )
MT_NwkCommandProcessing:
        CFI Block cfiBlock0 Using cfiCommon0
        CFI Function MT_NwkCommandProcessing
//  144 {
        FUNCALL MT_NwkCommandProcessing, NLME_PermitJoiningRequest
        LOCFRAME ISTACK, 0, STACK
        LOCFRAME PSTACK, 0, STACK
        LOCFRAME XSTACK, 10, STACK
        LOCFRAME IOVERLAY, 0, STATIC
        LOCFRAME DOVERLAY, 0, STATIC
        ARGFRAME ISTACK, 0, STACK
        ARGFRAME PSTACK, 0, STACK
        ARGFRAME XSTACK, 10, STACK
        ARGFRAME IOVERLAY, 0, STATIC
        ARGFRAME DOVERLAY, 0, STATIC
        MOV     A,#-0xa
        LCALL   ?BANKED_ENTER_XDATA
        CFI DPH0 load(1, XDATA, add(CFA_XSP16, literal(-1)))
        CFI DPL0 load(1, XDATA, add(CFA_XSP16, literal(-2)))
        CFI ?BRET_EXT load(1, XDATA, add(CFA_XSP16, literal(-3)))
        CFI ?RET_HIGH load(1, XDATA, add(CFA_XSP16, literal(-4)))
        CFI ?RET_LOW load(1, XDATA, add(CFA_XSP16, literal(-5)))
        CFI R7 load(1, XDATA, add(CFA_XSP16, literal(-6)))
        CFI V1 load(1, XDATA, add(CFA_XSP16, literal(-7)))
        CFI V0 load(1, XDATA, add(CFA_XSP16, literal(-8)))
        CFI VB load(1, XDATA, add(CFA_XSP16, literal(-9)))
        CFI R6 load(1, XDATA, add(CFA_XSP16, literal(-10)))
        CFI CFA_SP SP+0
        CFI CFA_XSP16 add(XSP16, 10)
        ; Saved register size: 10
        ; Auto size: 0
//  145   byte ret;
//  146 #if defined ( MT_NWK_FUNC )
//  147   uint8 dummyExPANID[Z_EXTADDR_LEN] = { 0xFF, 0xFF, 0xFF, 0xFF, 0xFF, 0xFF, 0xFF, 0xFF };
//  148   uint16 dstAddr;
//  149 #endif
//  150 #if defined ( MT_NWK_FUNC )  //NWK commands
//  151   byte attr;
//  152   byte index;
//  153   byte dataLen;
//  154   byte *dataPtr;
//  155   uint32 channelList;
//  156   byte databuf[SPI_RESP_LEN_NWK_DEFAULT + NWK_DEFAULT_GET_RESPONSE_LEN];
//  157 #if defined( ZDO_COORDINATOR )
//  158 	uint16 panId;
//  159 #else
//  160   byte i,j;
//  161 #endif
//  162 #endif // MT_NWK_FUNC
//  163 
//  164   len = SPI_0DATA_MSG_LEN + SPI_RESP_LEN_NWK_DEFAULT;
//  165 	ret = (byte)ZSuccess;
//  166 
//  167   switch (cmd_id)
        MOV     ?V0 + 0,R2
        MOV     ?V0 + 1,R3
        MOV     R0,#?V0 + 0
        LCALL   ?US_SWITCH_DENSE
`?<Jumptable for MT_NwkCommandProcessing>_0`:
        DATA
        DW        259
        DB        0
        DW        ??MT_NwkCommandProcessing_0
        DW        ??MT_NwkCommandProcessing_1
        CODE
//  168   {
//  169 #if defined( RTR_NWK )
//  170     case SPI_CMD_NLME_PERMIT_JOINING_REQ:
//  171       //The only information is PermitDuration
//  172       ret = (byte)NLME_PermitJoiningRequest( *pData );
??MT_NwkCommandProcessing_1:
        ; Setup parameters for call to function NLME_PermitJoiningRequest
        MOV     DPL,R4
        MOV     DPH,R5
        MOVX    A,@DPTR
        MOV     R1,A
        LCALL   ??NLME_PermitJoiningRequest?relay
//  173       break;
//  174 #endif
//  175 
//  176 #if defined ( MT_NWK_FUNC )  //NWK commands
//  177     case SPI_CMD_NWK_INIT:
//  178       nwk_init( NWK_TaskID );
//  179       break;
//  180 
//  181     case SPI_CMD_NLDE_DATA_REQ:
//  182       //First read the DstAddr
//  183       dstAddr = BUILD_UINT16( pData[1], pData[0] );
//  184       pData += sizeof( dstAddr );
//  185 
//  186       //Get the NSDU details
//  187       dataLen = *pData++;
//  188       dataPtr = pData;
//  189 
//  190       /* For now, skip a length of ZTEST_DEFAULT_DATA_LEN, instead of dataLen.
//  191          In future ZTOOL releases the data buffer will be only as long as dataLen */
//  192 
//  193       //pData += dataLen;
//  194       pData += ZTEST_DEFAULT_DATA_LEN;
//  195 
//  196       /* pData[0] = NSDUHandlde
//  197          pData[1] = NSDUHandleOptions
//  198          pData[3] = SecurityEnable
//  199          pData[4] = DiscoverRoute
//  200          pData[5] = RadiusCounter */
//  201 
//  202       ret = (byte)MT_Nwk_DataRequest( dstAddr, dataLen, dataPtr, pData[0],
//  203                                       BUILD_UINT16( pData[2], pData[1] ),
//  204                                       pData[3], pData[4], pData[5]);
//  205       break;
//  206 
//  207 #if defined( ZDO_COORDINATOR )
//  208     case SPI_CMD_NLME_INIT_COORD_REQ:
//  209 			panId = BUILD_UINT16( pData[1], pData[0] );
//  210 			
//  211 			MT_ReverseBytes( &pData[2], 4 );
//  212 			channelList = osal_build_uint32( &pData[2], 4 );
//  213 
//  214 			ret = (byte)NLME_NetworkFormationRequest( panId, channelList, pData[6], pData[7],
//  215                                                       pData[8], pData[9] );
//  216       break;
//  217 #endif  // ZDO
//  218 
//  219 #if defined( RTR_NWK )
//  220     case SPI_CMD_NLME_START_ROUTER_REQ:
//  221       // NOTE: first two parameters are not used, see NLMEDE.h for details
//  222       ret = (byte)NLME_StartRouterRequest( pData[0], pData[1], pData[2] );
//  223     break;
//  224 #endif  // RTR
//  225 
//  226     case SPI_CMD_NLME_JOIN_REQ:
//  227 		  ret = (byte)NLME_JoinRequest( dummyExPANID, BUILD_UINT16( pData[1], pData[0] ), pData[2], pData[3] );
//  228       if ( pData[3] & CAPINFO_RCVR_ON_IDLE )
//  229       {
//  230         // The receiver is on, turn network layer polling off.
//  231         NLME_SetPollRate( 0 );
//  232         NLME_SetQueuedPollRate( 0 );
//  233         NLME_SetResponseRate( 0 );
//  234       }
//  235       break;
//  236 
//  237     case SPI_CMD_NLME_LEAVE_REQ:
//  238       {
//  239         NLME_LeaveReq_t req;
//  240         // if extAddr is all zeros, it means null pointer..
//  241         for( index = 0; ( ( index < Z_EXTADDR_LEN ) &&
//  242                         ( pData[index] == 0 ) ) ; index++ );
//  243         if ( index == Z_EXTADDR_LEN )
//  244         {
//  245           req.extAddr = NULL;
//  246         }
//  247         else
//  248         {
//  249           MT_ReverseBytes( pData, Z_EXTADDR_LEN );
//  250           req.extAddr = pData;
//  251         }
//  252         pData += Z_EXTADDR_LEN;
//  253 
//  254         req.removeChildren = FALSE;
//  255         req.rejoin         = FALSE;
//  256         req.silent         = FALSE;
//  257         ret = (byte)NLME_LeaveReq( &req );
//  258       }
//  259       break;
//  260 
//  261     case SPI_CMD_NLME_RESET_REQ:
//  262       //Its a direct call to reset NWK
//  263       ret = (byte)NLME_ResetRequest();
//  264       break;
//  265 
//  266     case SPI_CMD_NLME_GET_REQ:
//  267       attr = *pData++;
//  268       index = *pData;
//  269 			databuf[0] = (byte)NLME_GetRequest( (ZNwkAttributes_t )attr, index, &databuf[1] );
//  270       len = SPI_0DATA_MSG_LEN + SPI_RESP_LEN_NWK_DEFAULT + NWK_DEFAULT_GET_RESPONSE_LEN;
//  271       MT_BuildAndSendZToolResponse( len, (SPI_RESPONSE_BIT | SPI_CMD_NLME_GET_REQ),
//  272             (SPI_RESP_LEN_NWK_DEFAULT + NWK_DEFAULT_GET_RESPONSE_LEN), databuf );
//  273       return;   // Don't return to this function
//  274 
//  275     case SPI_CMD_NLME_SET_REQ:
//  276       ret = (byte)NLME_SetRequest( (ZNwkAttributes_t)pData[0], pData[1], &pData[2] );
//  277       osal_start_timerEx( ZDAppTaskID, ZDO_NWK_UPDATE_NV, 1000 );
//  278       break;
//  279 
//  280     case SPI_CMD_NLME_NWK_DISC_REQ:
//  281       MT_ReverseBytes( pData, 4 );
//  282       ret = (byte)NLME_NetworkDiscoveryRequest( osal_build_uint32( pData, 4 ), pData[4] );
//  283       break;
//  284 
//  285 #if !defined( ZDO_COORDINATOR )
//  286     case SPI_CMD_NLME_ORPHAN_JOIN_REQ:
//  287       // Channel list bit mask
//  288       MT_ReverseBytes( pData, 4 );
//  289       channelList = osal_build_uint32( pData, 4 );
//  290 
//  291       // Count number of channels
//  292       j = attr = 0;
//  293       for ( i = 0; i < ED_SCAN_MAXCHANNELS; i++ )
//  294       {
//  295         if ( channelList & (1 << i) )
//  296         {
//  297            j++;
//  298            attr = i;
//  299         }
//  300       }
//  301 
//  302       // If only one channel specified...
//  303       if ( j == 1 )
//  304       {
//  305         _NIB.scanDuration = pData[4];
//  306         _NIB.nwkLogicalChannel = attr;
//  307         _NIB.channelList = channelList;
//  308         if ( !_NIB.CapabilityInfo )
//  309           _NIB.CapabilityInfo = ZDO_Config_Node_Descriptor.CapabilityFlags;
//  310 
//  311         devState = DEV_NWK_ORPHAN;
//  312         ret = (byte)NLME_OrphanJoinRequest( channelList, pData[4] );
//  313       }
//  314       else
//  315         ret = ZNwkInvalidParam;
//  316       break;
//  317 #endif  // !ZDO
//  318 	
//  319 #if defined (RTR_NWK)
//  320     case SPI_CMD_NLME_ROUTE_DISC_REQ:
//  321       ret = (byte)NLME_RouteDiscoveryRequest( BUILD_UINT16( pData[1], pData[0] ), pData[2] );
//  322       break;
//  323 			
//  324     case SPI_CMD_NLME_DIRECT_JOIN_REQ:
//  325       MT_ReverseBytes( pData, 8 );
//  326       ret = (byte)NLME_DirectJoinRequest( pData, pData[8] );
//  327     break;
//  328 #endif	// RTR
//  329 
//  330 #endif // MT_NWK_FUNC
//  331 
//  332     default:
//  333       ret = (byte)ZUnsupportedMode;
//  334       break;
//  335   }
//  336 
//  337 #if defined ( MT_NWK_FUNC )
//  338 	MT_SendSPIRespMsg( ret, cmd_id, len, SPI_RESP_LEN_NWK_DEFAULT );
//  339 #endif	
//  340   (void)len;
//  341   (void)ret;
//  342 }
??MT_NwkCommandProcessing_0:
        MOV     R7,#0x2
        LJMP    ?BANKED_LEAVE_XDATA
        CFI EndBlock cfiBlock0

        RSEG BANK_RELAYS:CODE:REORDER:NOROOT(0)
??MT_NwkCommandProcessing?relay:
        LCALL   ?BDISPATCH
        DATA
        DC24    MT_NwkCommandProcessing

        END
//  343 
//  344 #if defined ( MT_NWK_CB_FUNC )             //NWK callback commands
//  345 /*********************************************************************
//  346  * @fn          nwk_MTCallbackSubDataConfirm
//  347  *
//  348  * @brief       Process the callback subscription for NLDE-DATA.confirm
//  349  *
//  350  * @param       nsduHandle  - APS handle
//  351  * @param       Status      - result of data request
//  352  *
//  353  * @return      none
//  354  */
//  355 void nwk_MTCallbackSubDataConfirm(byte nsduHandle, ZStatus_t status )
//  356 {
//  357   byte buf[2];
//  358 
//  359   buf[0] = nsduHandle;
//  360   buf[1] = (byte)status;
//  361 
//  362   MT_BuildAndSendZToolCB( SPI_CB_NLDE_DATA_CNF, 2, buf );
//  363 }
//  364 
//  365 /*********************************************************************
//  366  * @fn          nwk_MTCallbackSubDataIndication
//  367  *
//  368  * @brief       Process the callback subscription for NLDE-DATA.indication
//  369  *
//  370  * @param       SrcAddress      - 16 bit address
//  371  * @param       nsduLength      - Length of incoming data
//  372  * @param       nsdu            - Pointer to incoming data
//  373  * @param       LinkQuality     - Link quality measured during
//  374  *                                reception.
//  375  * @param       SecuritySuite   - Security Suite Applied
//  376  * @param       SecurityStatus  - MLDE_SUCCESS if security process
//  377  *                                successfull, MLDE_FAILURE if not.
//  378  *
//  379  * @return      none
//  380  */
//  381 void nwk_MTCallbackSubDataIndication( uint16 SrcAddress, int16 nsduLength,
//  382                                       byte *nsdu, byte LinkQuality )
//  383 {
//  384   byte *msgPtr;
//  385   byte *msg;
//  386   byte msgLen;
//  387 
//  388   msgLen = sizeof( uint16 ) + sizeof( uint8 ) + ZTEST_DEFAULT_DATA_LEN
//  389             + sizeof( byte);
//  390 
//  391   msgPtr = osal_mem_alloc( msgLen );
//  392   if ( msgPtr )
//  393   {
//  394     //Fill up the data bytes
//  395     msg = msgPtr;
//  396 
//  397     //First fill in details
//  398     *msg++ = HI_UINT16( SrcAddress );
//  399     *msg++ = LO_UINT16( SrcAddress );
//  400 
//  401     //Since the max packet size is less than 255 bytes, a byte is enough
//  402     //to represent nsdu length
//  403     *msg++ = ( uint8 ) nsduLength;
//  404 
//  405     osal_memset( msg, NULL, ZTEST_DEFAULT_DATA_LEN ); // Clear the mem
//  406     osal_memcpy( msg, nsdu, nsduLength );
//  407     msg += ZTEST_DEFAULT_DATA_LEN;
//  408 
//  409     *msg++ = LinkQuality;
//  410 
//  411     MT_BuildAndSendZToolCB( SPI_CB_NLDE_DATA_IND, msgLen, msgPtr );
//  412 
//  413     osal_mem_free( msgPtr );
//  414   }
//  415 }
//  416 
//  417 /*********************************************************************
//  418  * @fn          nwk_MTCallbackSubInitCoordConfirm
//  419  *
//  420  * @brief       Process the callback subscription for NLME-INIT-COORD.confirm
//  421  *
//  422  * @param       Status - Result of NLME_InitCoordinatorRequest()
//  423  *
//  424  * @return      none
//  425  */
//  426 void nwk_MTCallbackSubInitCoordConfirm( ZStatus_t Status )
//  427 {
//  428 #if defined( ZDO_COORDINATOR )
//  429   MT_BuildAndSendZToolCB( SPI_CB_NLME_INITCOORD_CNF,
//  430                                     sizeof( byte ), (byte*)&Status );
//  431 #endif  // ZDO_COORDINATOR
//  432 }
//  433 
//  434 /*********************************************************************
//  435  * @fn          nwk_MTCallbackSubStartRouterConfirm
//  436  *
//  437  * @brief       Process the callback subscription for NLME-START-ROUTER.confirm
//  438  *
//  439  * @param       Status - Result of NLME_StartRouterRequest()
//  440  *
//  441  * @return      none
//  442  */
//  443 void nwk_MTCallbackSubStartRouterConfirm( ZStatus_t Status )
//  444 {
//  445   MT_BuildAndSendZToolCB( SPI_CB_NLME_START_ROUTER_CNF,
//  446                                         sizeof( byte ), (byte*)&Status );
//  447 }
//  448 
//  449 /*********************************************************************
//  450  * @fn          nwk_MTCallbackSubJoinConfirm
//  451  *
//  452  * @brief       Process the callback subscription for NLME-JOIN.confirm
//  453  *
//  454  * @param       Status - Result of NLME_JoinRequest()
//  455  *
//  456  * @return      none
//  457  */
//  458 void nwk_MTCallbackSubJoinConfirm(  uint16 PanId, ZStatus_t Status )
//  459 {
//  460   byte msg[Z_EXTADDR_LEN + 3];
//  461 
//  462   // This device's 64-bit address
//  463   ZMacGetReq( ZMacExtAddr, msg );
//  464   MT_ReverseBytes( msg, Z_EXTADDR_LEN );
//  465 
//  466   msg[Z_EXTADDR_LEN + 0] = HI_UINT16( PanId );
//  467   msg[Z_EXTADDR_LEN + 1] = LO_UINT16( PanId );
//  468   msg[Z_EXTADDR_LEN + 2] = (byte)Status;
//  469 
//  470   MT_BuildAndSendZToolCB( SPI_CB_NLME_JOIN_CNF, Z_EXTADDR_LEN + 3, msg );
//  471 }
//  472 /*********************************************************************
//  473  * @fn          nwk_MTCallbackSubNetworkDiscoveryConfirm
//  474  *
//  475  * @brief       Process the callback subscription for NLME-NWK_DISC.confirm
//  476  *
//  477  * @param       ResultCount			- number of networks discovered
//  478  * @param				NetworkList			- pointer to list of network descriptors
//  479  *
//  480  * @return      void
//  481  */
//  482 void nwk_MTCallbackSubNetworkDiscoveryConfirm( byte ResultCount, networkDesc_t *NetworkList )
//  483 {
//  484 	byte len;
//  485 	byte *msgPtr;
//  486 	byte *msg;
//  487 	byte i;
//  488 
//  489         // The message cannot be bigger then SPI_TX_BUFF_MAX.  Reduce resultCount if necessary
//  490         if (ResultCount * sizeof(networkDesc_t) > SPI_TX_BUFF_MAX - (1 + SPI_0DATA_MSG_LEN))
//  491         {
//  492           ResultCount = (SPI_TX_BUFF_MAX - (1 + SPI_0DATA_MSG_LEN)) / sizeof(networkDesc_t);
//  493         }
//  494 
//  495 	len = 1 + ResultCount * sizeof(networkDesc_t);
//  496   msgPtr = osal_mem_alloc( len );
//  497 	if ( msgPtr )
//  498 	{
//  499 	 //Fill up the data bytes
//  500     msg = msgPtr;
//  501 
//  502 		*msg++ = ResultCount;
//  503 
//  504 		for ( i = 0; i < ResultCount; i++ )
//  505 		{
//  506 		  *msg++ = HI_UINT16( NetworkList->panId );
//  507 		  *msg++ = LO_UINT16( NetworkList->panId );
//  508 		  *msg++ = NetworkList->logicalChannel;
//  509 		  *msg++ = NetworkList->beaconOrder;
//  510 		  *msg++ = NetworkList->superFrameOrder;
//  511 		  *msg++ = NetworkList->routerCapacity;
//  512 		  *msg++ = NetworkList->deviceCapacity;
//  513 		  *msg++ = NetworkList->version;
//  514 		  *msg++ = NetworkList->stackProfile;
//  515 		  //*msg++ = NetworkList->securityLevel;
//  516 		
//  517 			NetworkList = (networkDesc_t*)NetworkList->nextDesc;
//  518 		}
//  519 
//  520     MT_BuildAndSendZToolCB( SPI_CB_NLME_NWK_DISC_CNF, len, msgPtr );
//  521 
//  522     osal_mem_free( msgPtr );
//  523 	}
//  524 }
//  525 /*********************************************************************
//  526  * @fn          nwk_MTCallbackSubJoinIndication
//  527  *
//  528  * @brief       Process the callback subscription for NLME-INIT-COORD.indication
//  529  *
//  530  * @param       ShortAddress - 16-bit address
//  531  * @param       ExtendedAddress - IEEE (64-bit) address
//  532  * @param       CapabilityInformation - Association Capability Information
//  533  *
//  534  * @return      ZStatus_t
//  535  */
//  536 void nwk_MTCallbackSubJoinIndication( uint16 ShortAddress, byte *ExtendedAddress,
//  537                                       byte CapabilityInformation )
//  538 {
//  539   byte *msgPtr;
//  540   byte *msg;
//  541   byte len;
//  542 
//  543   len = sizeof( uint16 ) + Z_EXTADDR_LEN + sizeof( byte );
//  544   msgPtr = osal_mem_alloc( len );
//  545 
//  546   if ( msgPtr )
//  547   {
//  548     //Fill up the data bytes
//  549     msg = msgPtr;
//  550 
//  551     //First fill in details
//  552     *msg++ = HI_UINT16( ShortAddress );
//  553     *msg++ = LO_UINT16( ShortAddress );
//  554 
//  555     osal_cpyExtAddr( msg, ExtendedAddress );
//  556     MT_ReverseBytes( msg, Z_EXTADDR_LEN );
//  557     msg += Z_EXTADDR_LEN;
//  558 
//  559     *msg = CapabilityInformation;
//  560 
//  561     MT_BuildAndSendZToolCB( SPI_CB_NLME_JOIN_IND, len, msgPtr );
//  562 
//  563     osal_mem_free( msgPtr );
//  564   }
//  565 }
//  566 
//  567 /*********************************************************************
//  568  * @fn          nwk_MTCallbackSubLeaveConfirm
//  569  *
//  570  * @brief       Process the callback subscription for NLME-LEAVE.confirm
//  571  *
//  572  * @param       DeviceAddress - IEEE (64-bit) address
//  573  * @param       Status - Result of NLME_LeaveRequest()
//  574  *
//  575  * @return      none
//  576  */
//  577 void nwk_MTCallbackSubLeaveConfirm( byte *DeviceAddress, ZStatus_t Status )
//  578 {
//  579   byte *msgPtr;
//  580   byte *msg;
//  581 
//  582   msgPtr = osal_mem_alloc( Z_EXTADDR_LEN + sizeof( byte ) );
//  583   if ( msgPtr )
//  584   {
//  585     //Fill up the data bytes
//  586     msg = msgPtr;
//  587 
//  588     //First fill in details
//  589     osal_cpyExtAddr( msg, DeviceAddress );
//  590     MT_ReverseBytes( msg, Z_EXTADDR_LEN );
//  591     msg += Z_EXTADDR_LEN;
//  592 
//  593     *msg = (byte)Status;
//  594 
//  595     MT_BuildAndSendZToolCB( SPI_CB_NLME_LEAVE_CNF,
//  596                                   Z_EXTADDR_LEN + sizeof( byte ), msgPtr );
//  597 
//  598     osal_mem_free( msgPtr );
//  599   }
//  600 }
//  601 /*********************************************************************
//  602  * @fn          nwk_MTCallbackSubLeaveIndication
//  603  *
//  604  * @brief       Process the callback subscription for NLME-LEAVE.indication
//  605  *
//  606  * @param       DeviceAddress - IEEE (64-bit) address
//  607  *
//  608  * @return      NULL
//  609  */
//  610 void nwk_MTCallbackSubLeaveIndication( byte *DeviceAddress )
//  611 {
//  612   byte msg[Z_EXTADDR_LEN+1];
//  613 
//  614   //First fill in details
//  615   if ( DeviceAddress )
//  616   {
//  617     osal_cpyExtAddr( msg, DeviceAddress );
//  618     MT_ReverseBytes( msg, Z_EXTADDR_LEN );
//  619   }
//  620   else
//  621     osal_memset( msg, 0, Z_EXTADDR_LEN );
//  622   msg[Z_EXTADDR_LEN] = 0;  // Status, assume good if we get this far
//  623 
//  624   MT_BuildAndSendZToolCB( SPI_CB_NLME_LEAVE_IND, Z_EXTADDR_LEN+1, msg );
//  625 }
//  626 /*********************************************************************
//  627  * @fn          nwk_MTCallbackSubSyncIndication
//  628  *
//  629  * @brief       Process the callback subscription for NLME-SYNC.indication
//  630  *
//  631  * @param       none
//  632  *
//  633  * @return      none
//  634  */
//  635 void nwk_MTCallbackSubSyncIndication( void )
//  636 {
//  637   MT_BuildAndSendZToolCB( SPI_CB_NLME_SYNC_IND, 0, NULL );
//  638 }
//  639 
//  640 /*********************************************************************
//  641  * @fn          nwk_MTCallbackSubPollConfirm
//  642  *
//  643  * @brief       Process the callback subscription for NLME-POLL.confirm
//  644  *
//  645  * @param       status - status of the poll operation
//  646  *
//  647  * @return      none
//  648  */
//  649 void nwk_MTCallbackSubPollConfirm( byte status )
//  650 {
//  651   byte msg = status;
//  652   MT_BuildAndSendZToolCB( SPI_CB_NLME_POLL_CNF, 1, &msg );
//  653 }
//  654 
//  655 #endif /*NWK Callback commands*/
//  656 
//  657 /*********************************************************************
//  658 *********************************************************************/
//  659 
// 
// 35 bytes in segment BANKED_CODE
//  6 bytes in segment BANK_RELAYS
//  2 bytes in segment XDATA_Z
// 
// 41 bytes of CODE  memory
//  2 bytes of XDATA memory
//
//Errors: none
//Warnings: none
