#

##

##

    礦ision2 Build Log
    Project:
    D:\My Documents\桌面\单片机\485+51通信仿真\接收\receive_data.uv2
    Project File Date:  02/06/2014

    Output:
    Build target 'Target 1'
    assembling STARTUP.A51...
    compiling 接收文件.c...
    linking...
    Program Size: data=13.0 xdata=0 code=78
    creating hex file from "receive_data"...
    "receive_data" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling STARTUP.A51...
    compiling 接收文件.c...
    linking...
    Program Size: data=13.0 xdata=0 code=78
    creating hex file from "receive_data"...
    "receive_data" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling STARTUP.A51...
    compiling 接收文件.c...
    linking...
    Program Size: data=13.0 xdata=0 code=82
    creating hex file from "receive_data"...
    "receive_data" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling STARTUP.A51...
    compiling 接收文件.c...
    linking...
    Program Size: data=13.0 xdata=0 code=87
    creating hex file from "receive_data"...
    "receive_data" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling STARTUP.A51...
    compiling 接收文件.c...
    linking...
    Program Size: data=13.0 xdata=0 code=87
    creating hex file from "receive_data"...
    "receive_data" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling STARTUP.A51...
    compiling 接收文件.c...
    linking...
    Program Size: data=13.0 xdata=0 code=87
    creating hex file from "receive_data"...
    "receive_data" - 0 Error(s), 0 Warning(s).
    Build target 'Target 1'
    assembling STARTUP.A51...
    compiling 接收文件.c...
    linking...
    Program Size: data=13.0 xdata=0 code=78
    creating hex file from "receive_data"...
    "receive_data" - 0 Error(s), 0 Warning(s).