--A1L47 is disp_select~923
A1L47_p0_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & date_disp_select[5];
A1L47_p1_out = time_disp_select[5] & Stopwatch_EN;
A1L47_p2_out = time_disp_select[5] & Timepiece_EN;
A1L47_p3_out = time_disp_select[5] & TimeSet_EN;
A1L47_p4_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & alarmclock_disp_select[5] & Alarmclock_EN;
A1L47_or_out = A1L47_p0_out # A1L47_p1_out # A1L47_p2_out # A1L47_p3_out # A1L47_p4_out;
A1L47 = A1L47_or_out;


--A1L57 is disp_select~924
A1L57_p0_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & date_disp_select[4];
A1L57_p1_out = time_disp_select[4] & Stopwatch_EN;
A1L57_p2_out = time_disp_select[4] & Timepiece_EN;
A1L57_p3_out = time_disp_select[4] & TimeSet_EN;
A1L57_p4_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & alarmclock_disp_select[4] & Alarmclock_EN;
A1L57_or_out = A1L57_p0_out # A1L57_p1_out # A1L57_p2_out # A1L57_p3_out # A1L57_p4_out;
A1L57 = A1L57_or_out;


--A1L67 is disp_select~925
A1L67_p0_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & date_disp_select[3];
A1L67_p1_out = time_disp_select[3] & Stopwatch_EN;
A1L67_p2_out = time_disp_select[3] & Timepiece_EN;
A1L67_p3_out = time_disp_select[3] & TimeSet_EN;
A1L67_p4_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & alarmclock_disp_select[3] & Alarmclock_EN;
A1L67_or_out = A1L67_p0_out # A1L67_p1_out # A1L67_p2_out # A1L67_p3_out # A1L67_p4_out;
A1L67 = A1L67_or_out;


--A1L77 is disp_select~926
A1L77_p0_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & date_disp_select[2];
A1L77_p1_out = time_disp_select[2] & Stopwatch_EN;
A1L77_p2_out = time_disp_select[2] & Timepiece_EN;
A1L77_p3_out = time_disp_select[2] & TimeSet_EN;
A1L77_p4_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & alarmclock_disp_select[2] & Alarmclock_EN;
A1L77_or_out = A1L77_p0_out # A1L77_p1_out # A1L77_p2_out # A1L77_p3_out # A1L77_p4_out;
A1L77 = A1L77_or_out;


--A1L87 is disp_select~927
A1L87_p0_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & date_disp_select[1];
A1L87_p1_out = time_disp_select[1] & Stopwatch_EN;
A1L87_p2_out = time_disp_select[1] & Timepiece_EN;
A1L87_p3_out = time_disp_select[1] & TimeSet_EN;
A1L87_p4_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & alarmclock_disp_select[1] & Alarmclock_EN;
A1L87_or_out = A1L87_p0_out # A1L87_p1_out # A1L87_p2_out # A1L87_p3_out # A1L87_p4_out;
A1L87 = A1L87_or_out;


--A1L97 is disp_select~928
A1L97_p0_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & date_disp_select[0];
A1L97_p1_out = time_disp_select[0] & Stopwatch_EN;
A1L97_p2_out = time_disp_select[0] & Timepiece_EN;
A1L97_p3_out = time_disp_select[0] & TimeSet_EN;
A1L97_p4_out = !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & alarmclock_disp_select[0] & Alarmclock_EN;
A1L97_or_out = A1L97_p0_out # A1L97_p1_out # A1L97_p2_out # A1L97_p3_out # A1L97_p4_out;
A1L97 = A1L97_or_out;


--A1L01 is Data~2814
A1L01 = EXP(!Stopwatch_EN & !Timepiece_EN & !TimeSet_EN);


--A1L6 is Data~2798
A1L6_p0_out = A1L01 & time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & hour1[3];
A1L6_p1_out = A1L01 & second1[3] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0];
A1L6_p2_out = A1L01 & !time_disp_select[5] & !time_disp_select[3] & time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute0[3];
A1L6_p3_out = A1L01 & !time_disp_select[5] & time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute1[3];
A1L6_p4_out = A1L01 & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & time_disp_select[4] & !time_disp_select[0] & hour0[3];
A1L6_or_out = A1L31 # A1L6_p0_out # A1L6_p1_out # A1L6_p2_out # A1L6_p3_out # A1L6_p4_out;
A1L6 = A1L6_or_out;


--A1L7 is Data~2800
A1L7_p0_out = A1L01 & time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & hour1[0];
A1L7_p1_out = A1L01 & second1[0] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0];
A1L7_p2_out = A1L01 & !time_disp_select[5] & !time_disp_select[3] & time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute0[0];
A1L7_p3_out = A1L01 & !time_disp_select[5] & time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute1[0];
A1L7_p4_out = A1L01 & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & time_disp_select[4] & !time_disp_select[0] & hour0[0];
A1L7_or_out = A1L61 # A1L7_p0_out # A1L7_p1_out # A1L7_p2_out # A1L7_p3_out # A1L7_p4_out;
A1L7 = A1L7_or_out;


--A1L8 is Data~2802
A1L8_p0_out = A1L01 & time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & hour1[2];
A1L8_p1_out = A1L01 & second1[2] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0];
A1L8_p2_out = A1L01 & !time_disp_select[5] & !time_disp_select[3] & time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute0[2];
A1L8_p3_out = A1L01 & !time_disp_select[5] & time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute1[2];
A1L8_p4_out = A1L01 & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & time_disp_select[4] & !time_disp_select[0] & hour0[2];
A1L8_or_out = A1L91 # A1L8_p0_out # A1L8_p1_out # A1L8_p2_out # A1L8_p3_out # A1L8_p4_out;
A1L8 = A1L8_or_out;


--A1L9 is Data~2804
A1L9_p0_out = A1L01 & time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & hour1[1];
A1L9_p1_out = A1L01 & second1[1] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0];
A1L9_p2_out = A1L01 & !time_disp_select[5] & !time_disp_select[3] & time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute0[1];
A1L9_p3_out = A1L01 & !time_disp_select[5] & time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & !time_disp_select[0] & minute1[1];
A1L9_p4_out = A1L01 & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & time_disp_select[4] & !time_disp_select[0] & hour0[1];
A1L9_or_out = A1L22 # A1L9_p0_out # A1L9_p1_out # A1L9_p2_out # A1L9_p3_out # A1L9_p4_out;
A1L9 = A1L9_or_out;


--A1L37 is disp_select[5]$latch~10
A1L37_p1_out = A1L47 & A1L53;
A1L37_p2_out = A1L37 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L37_p3_out = A1L47 & A1L37;
A1L37_or_out = A1L37_p1_out # A1L37_p2_out # A1L37_p3_out;
A1L37 = A1L37_or_out;


--A1L17 is disp_select[4]$latch~10
A1L17_p1_out = A1L57 & A1L53;
A1L17_p2_out = A1L17 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L17_p3_out = A1L57 & A1L17;
A1L17_or_out = A1L17_p1_out # A1L17_p2_out # A1L17_p3_out;
A1L17 = A1L17_or_out;


--A1L96 is disp_select[3]$latch~10
A1L96_p1_out = A1L67 & A1L53;
A1L96_p2_out = A1L96 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L96_p3_out = A1L67 & A1L96;
A1L96_or_out = A1L96_p1_out # A1L96_p2_out # A1L96_p3_out;
A1L96 = A1L96_or_out;


--A1L76 is disp_select[2]$latch~10
A1L76_p1_out = A1L77 & A1L53;
A1L76_p2_out = A1L76 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L76_p3_out = A1L77 & A1L76;
A1L76_or_out = A1L76_p1_out # A1L76_p2_out # A1L76_p3_out;
A1L76 = A1L76_or_out;


--A1L56 is disp_select[1]$latch~10
A1L56_p1_out = A1L87 & A1L53;
A1L56_p2_out = A1L56 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L56_p3_out = A1L87 & A1L56;
A1L56_or_out = A1L56_p1_out # A1L56_p2_out # A1L56_p3_out;
A1L56 = A1L56_or_out;


--A1L36 is disp_select[0]$latch~10
A1L36_p1_out = A1L97 & A1L53;
A1L36_p2_out = A1L36 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L36_p3_out = A1L97 & A1L36;
A1L36_or_out = A1L36_p1_out # A1L36_p2_out # A1L36_p3_out;
A1L36 = A1L36_or_out;


--A1L5 is Data[3]~2844
A1L5_p1_out = A1L6 & A1L53;
A1L5_p2_out = A1L5 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L5_p3_out = A1L6 & A1L5;
A1L5_or_out = A1L5_p1_out # A1L5_p2_out # A1L5_p3_out;
A1L5 = A1L5_or_out;


--A1L2 is Data[0]~2848
A1L2_p1_out = A1L7 & A1L53;
A1L2_p2_out = A1L2 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L2_p3_out = A1L7 & A1L2;
A1L2_or_out = A1L2_p1_out # A1L2_p2_out # A1L2_p3_out;
A1L2 = A1L2_or_out;


--A1L4 is Data[2]~2852
A1L4_p1_out = A1L8 & A1L53;
A1L4_p2_out = A1L4 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L4_p3_out = A1L8 & A1L4;
A1L4_or_out = A1L4_p1_out # A1L4_p2_out # A1L4_p3_out;
A1L4 = A1L4_or_out;


--A1L3 is Data[1]~2856
A1L3_p1_out = A1L9 & A1L53;
A1L3_p2_out = A1L3 & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN;
A1L3_p3_out = A1L9 & A1L3;
A1L3_or_out = A1L3_p1_out # A1L3_p2_out # A1L3_p3_out;
A1L3 = A1L3_or_out;


--A1L011 is reduce_or~1064
A1L011_p1_out = A1L4 & !A1L3;
A1L011_p2_out = A1L3 & A1L5;
A1L011_or_out = A1L011_p1_out # A1L011_p2_out # A1L2;
A1L011 = !(A1L011_or_out);


--A1L111 is reduce_or~1070
A1L111_p1_out = !A1L2 & !A1L4 & A1L3;
A1L111_p2_out = A1L4 & A1L5;
A1L111_p3_out = A1L3 & A1L5;
A1L111_or_out = A1L111_p1_out # A1L111_p2_out # A1L111_p3_out;
A1L111 = !(A1L111_or_out);


--A1L211 is reduce_or~1076
A1L211_p1_out = A1L5 & A1L3;
A1L211_p2_out = A1L5 & A1L4;
A1L211_p3_out = !A1L3 & A1L4 & A1L2;
A1L211_p4_out = A1L3 & A1L4 & !A1L2;
A1L211_or_out = A1L211_p1_out # A1L211_p2_out # A1L211_p3_out # A1L211_p4_out;
A1L211 = !(A1L211_or_out);


--A1L311 is reduce_or~1082
A1L311_p1_out = A1L2 & !A1L5 & !A1L4;
A1L311_p2_out = A1L5 & A1L4;
A1L311_p3_out = A1L2 & A1L3;
A1L311_p4_out = !A1L4 & A1L3;
A1L311_or_out = A1L311_p1_out # A1L311_p2_out # A1L311_p3_out # A1L311_p4_out;
A1L311 = !(A1L311_or_out);


--A1L411 is reduce_or~1088
A1L411_p1_out = A1L5 & !A1L4 & !A1L3;
A1L411_p2_out = !A1L5 & !A1L4 & A1L3;
A1L411_p3_out = !A1L5 & A1L4 & !A1L2;
A1L411_p4_out = !A1L5 & A1L4 & !A1L3;
A1L411_or_out = A1L411_p1_out # A1L411_p2_out # A1L411_p3_out # A1L411_p4_out;
A1L411 = A1L411_or_out;


--A1L511 is reduce_or~1093
A1L511_p1_out = A1L2 & A1L4 & !A1L5;
A1L511_p2_out = !A1L2 & !A1L4 & !A1L5;
A1L511_p3_out = !A1L4 & A1L5 & !A1L3;
A1L511_p4_out = !A1L5 & A1L3;
A1L511_or_out = A1L511_p1_out # A1L511_p2_out # A1L511_p3_out # A1L511_p4_out;
A1L511 = A1L511_or_out;


--A1L611 is reduce_or~1099
A1L611_p0_out = A1L4 & A1L2 & A1L3;
A1L611_p1_out = A1L4 & !A1L2 & !A1L3;
A1L611_p2_out = !A1L4 & A1L2 & !A1L3 & !A1L5;
A1L611_p3_out = A1L3 & A1L5;
A1L611_p4_out = A1L4 & A1L5;
A1L611_or_out = A1L611_p0_out # A1L611_p1_out # A1L611_p2_out # A1L611_p3_out # A1L611_p4_out;
A1L611 = !(A1L611_or_out);


--A1L11 is Data~2858
A1L11_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second0[3] & !TimeSet_EN;
A1L11_p2_out = Timepiece_EN & second0[3] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L11_p3_out = second0[3] & TimeSet_EN & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L11 = A1L11_p1_out # A1L11_p2_out # A1L11_p3_out;


--A1L21 is Data~2860
A1L21_p0_out = alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour1[3];
A1L21_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second1[3] & !TimeSet_EN;
A1L21_p2_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute0[3];
A1L21_p3_out = !alarmclock_disp_select[5] & alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute1[3];
A1L21_p4_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour0[3];
A1L21 = A1L11 # A1L21_p0_out # A1L21_p1_out # A1L21_p2_out # A1L21_p3_out # A1L21_p4_out;


--A1L31 is Data~2866
A1L31_p0_out = Stopwatch_EN & second0[3] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L31_p1_out = day0[3] & !Alarmclock_EN & !date_disp_select[5] & date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN;
A1L31_p2_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & day1[3];
A1L31_p3_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month0[3];
A1L31_p4_out = !Alarmclock_EN & date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month1[3];
A1L31 = A1L21 # A1L31_p0_out # A1L31_p1_out # A1L31_p2_out # A1L31_p3_out # A1L31_p4_out;


--A1L41 is Data~2872
A1L41_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second0[0] & !TimeSet_EN;
A1L41_p2_out = Timepiece_EN & second0[0] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L41_p3_out = second0[0] & TimeSet_EN & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L41 = A1L41_p1_out # A1L41_p2_out # A1L41_p3_out;


--A1L51 is Data~2874
A1L51_p0_out = alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour1[0];
A1L51_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second1[0] & !TimeSet_EN;
A1L51_p2_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute0[0];
A1L51_p3_out = !alarmclock_disp_select[5] & alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute1[0];
A1L51_p4_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour0[0];
A1L51 = A1L41 # A1L51_p0_out # A1L51_p1_out # A1L51_p2_out # A1L51_p3_out # A1L51_p4_out;


--A1L61 is Data~2880
A1L61_p0_out = Stopwatch_EN & second0[0] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L61_p1_out = day0[0] & !Alarmclock_EN & !date_disp_select[5] & date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN;
A1L61_p2_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & day1[0];
A1L61_p3_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month0[0];
A1L61_p4_out = !Alarmclock_EN & date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month1[0];
A1L61 = A1L51 # A1L61_p0_out # A1L61_p1_out # A1L61_p2_out # A1L61_p3_out # A1L61_p4_out;


--A1L71 is Data~2886
A1L71_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second0[2] & !TimeSet_EN;
A1L71_p2_out = Timepiece_EN & second0[2] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L71_p3_out = second0[2] & TimeSet_EN & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L71 = A1L71_p1_out # A1L71_p2_out # A1L71_p3_out;


--A1L81 is Data~2888
A1L81_p0_out = alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour1[2];
A1L81_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second1[2] & !TimeSet_EN;
A1L81_p2_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute0[2];
A1L81_p3_out = !alarmclock_disp_select[5] & alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute1[2];
A1L81_p4_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour0[2];
A1L81 = A1L71 # A1L81_p0_out # A1L81_p1_out # A1L81_p2_out # A1L81_p3_out # A1L81_p4_out;


--A1L91 is Data~2894
A1L91_p0_out = Stopwatch_EN & second0[2] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L91_p1_out = day0[2] & !Alarmclock_EN & !date_disp_select[5] & date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN;
A1L91_p2_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & day1[2];
A1L91_p3_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month0[2];
A1L91_p4_out = !Alarmclock_EN & date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month1[2];
A1L91 = A1L81 # A1L91_p0_out # A1L91_p1_out # A1L91_p2_out # A1L91_p3_out # A1L91_p4_out;


--A1L02 is Data~2900
A1L02_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second0[1] & !TimeSet_EN;
A1L02_p2_out = Timepiece_EN & second0[1] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L02_p3_out = second0[1] & TimeSet_EN & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L02 = A1L02_p1_out # A1L02_p2_out # A1L02_p3_out;


--A1L12 is Data~2902
A1L12_p0_out = alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour1[1];
A1L12_p1_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & second1[1] & !TimeSet_EN;
A1L12_p2_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute0[1];
A1L12_p3_out = !alarmclock_disp_select[5] & alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & !alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & minute1[1];
A1L12_p4_out = !alarmclock_disp_select[5] & !alarmclock_disp_select[3] & !alarmclock_disp_select[2] & !alarmclock_disp_select[1] & alarmclock_disp_select[4] & !alarmclock_disp_select[0] & Alarmclock_EN & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & hour0[1];
A1L12 = A1L02 # A1L12_p0_out # A1L12_p1_out # A1L12_p2_out # A1L12_p3_out # A1L12_p4_out;


--A1L22 is Data~2908
A1L22_p0_out = Stopwatch_EN & second0[1] & !time_disp_select[5] & !time_disp_select[3] & !time_disp_select[2] & !time_disp_select[1] & !time_disp_select[4] & time_disp_select[0];
A1L22_p1_out = day0[1] & !Alarmclock_EN & !date_disp_select[5] & date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN;
A1L22_p2_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & day1[1];
A1L22_p3_out = !Alarmclock_EN & !date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month0[1];
A1L22_p4_out = !Alarmclock_EN & date_disp_select[5] & !date_disp_select[2] & !date_disp_select[1] & !date_disp_select[0] & !date_disp_select[4] & !date_disp_select[3] & !Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & month1[1];
A1L22 = A1L12 # A1L22_p0_out # A1L22_p1_out # A1L22_p2_out # A1L22_p3_out # A1L22_p4_out;


--A1L53 is always0~45sexp
A1L53 = EXP(!Stopwatch_EN & !Timepiece_EN & !TimeSet_EN & !Alarmclock_EN & !Date_EN & !DateSet_EN);


--Timepiece_EN is Timepiece_EN
--operation mode is input

Timepiece_EN = INPUT();


--TimeSet_EN is TimeSet_EN
--operation mode is input

TimeSet_EN = INPUT();


--Stopwatch_EN is Stopwatch_EN
--operation mode is input

Stopwatch_EN = INPUT();


--time_disp_select[5] is time_disp_select[5]
--operation mode is input

time_disp_select[5] = INPUT();


--time_disp_select[4] is time_disp_select[4]
--operation mode is input

time_disp_select[4] = INPUT();


--time_disp_select[3] is time_disp_select[3]
--operation mode is input

time_disp_select[3] = INPUT();


--time_disp_select[2] is time_disp_select[2]
--operation mode is input

time_disp_select[2] = INPUT();


--time_disp_select[1] is time_disp_select[1]
--operation mode is input

time_disp_select[1] = INPUT();


--time_disp_select[0] is time_disp_select[0]
--operation mode is input

time_disp_select[0] = INPUT();


--Alarmclock_EN is Alarmclock_EN
--operation mode is input

Alarmclock_EN = INPUT();


--alarmclock_disp_select[5] is alarmclock_disp_select[5]
--operation mode is input

alarmclock_disp_select[5] = INPUT();


--alarmclock_disp_select[4] is alarmclock_disp_select[4]
--operation mode is input

alarmclock_disp_select[4] = INPUT();


--alarmclock_disp_select[3] is alarmclock_disp_select[3]
--operation mode is input

alarmclock_disp_select[3] = INPUT();


--alarmclock_disp_select[2] is alarmclock_disp_select[2]
--operation mode is input

alarmclock_disp_select[2] = INPUT();


--alarmclock_disp_select[1] is alarmclock_disp_select[1]
--operation mode is input

alarmclock_disp_select[1] = INPUT();


--alarmclock_disp_select[0] is alarmclock_disp_select[0]
--operation mode is input

alarmclock_disp_select[0] = INPUT();


--hour1[3] is hour1[3]
--operation mode is input

hour1[3] = INPUT();


--hour1[2] is hour1[2]
--operation mode is input

hour1[2] = INPUT();


--hour1[1] is hour1[1]
--operation mode is input

hour1[1] = INPUT();


--hour1[0] is hour1[0]
--operation mode is input

hour1[0] = INPUT();


--hour0[3] is hour0[3]
--operation mode is input

hour0[3] = INPUT();


--hour0[2] is hour0[2]
--operation mode is input

hour0[2] = INPUT();


--hour0[1] is hour0[1]
--operation mode is input

hour0[1] = INPUT();


--hour0[0] is hour0[0]
--operation mode is input

hour0[0] = INPUT();


--minute1[3] is minute1[3]
--operation mode is input

minute1[3] = INPUT();


--minute1[2] is minute1[2]
--operation mode is input

minute1[2] = INPUT();


--minute1[1] is minute1[1]
--operation mode is input

minute1[1] = INPUT();


--minute1[0] is minute1[0]
--operation mode is input

minute1[0] = INPUT();


--minute0[3] is minute0[3]
--operation mode is input

minute0[3] = INPUT();


--minute0[2] is minute0[2]
--operation mode is input

minute0[2] = INPUT();


--minute0[1] is minute0[1]
--operation mode is input

minute0[1] = INPUT();


--minute0[0] is minute0[0]
--operation mode is input

minute0[0] = INPUT();


--second1[3] is second1[3]
--operation mode is input

second1[3] = INPUT();


--second1[2] is second1[2]
--operation mode is input

second1[2] = INPUT();


--second1[1] is second1[1]
--operation mode is input

second1[1] = INPUT();


--second1[0] is second1[0]
--operation mode is input

second1[0] = INPUT();


--second0[3] is second0[3]
--operation mode is input

second0[3] = INPUT();


--second0[2] is second0[2]
--operation mode is input

second0[2] = INPUT();


--second0[1] is second0[1]
--operation mode is input

second0[1] = INPUT();


--second0[0] is second0[0]
--operation mode is input

second0[0] = INPUT();


--Date_EN is Date_EN
--operation mode is input

Date_EN = INPUT();


--DateSet_EN is DateSet_EN
--operation mode is input

DateSet_EN = INPUT();


--date_disp_select[5] is date_disp_select[5]
--operation mode is input

date_disp_select[5] = INPUT();


--date_disp_select[4] is date_disp_select[4]
--operation mode is input

date_disp_select[4] = INPUT();


--date_disp_select[3] is date_disp_select[3]
--operation mode is input

date_disp_select[3] = INPUT();


--date_disp_select[2] is date_disp_select[2]
--operation mode is input

date_disp_select[2] = INPUT();


--date_disp_select[1] is date_disp_select[1]
--operation mode is input

date_disp_select[1] = INPUT();


--date_disp_select[0] is date_disp_select[0]
--operation mode is input

date_disp_select[0] = INPUT();


--month1[3] is month1[3]
--operation mode is input

month1[3] = INPUT();


--month1[2] is month1[2]
--operation mode is input

month1[2] = INPUT();


--month1[1] is month1[1]
--operation mode is input

month1[1] = INPUT();


--month1[0] is month1[0]
--operation mode is input

month1[0] = INPUT();


--month0[3] is month0[3]
--operation mode is input

month0[3] = INPUT();


--month0[2] is month0[2]
--operation mode is input

month0[2] = INPUT();


--month0[1] is month0[1]
--operation mode is input

month0[1] = INPUT();


--month0[0] is month0[0]
--operation mode is input

month0[0] = INPUT();


--day1[3] is day1[3]
--operation mode is input

day1[3] = INPUT();


--day1[2] is day1[2]
--operation mode is input

day1[2] = INPUT();


--day1[1] is day1[1]
--operation mode is input

day1[1] = INPUT();


--day1[0] is day1[0]
--operation mode is input

day1[0] = INPUT();


--day0[3] is day0[3]
--operation mode is input

day0[3] = INPUT();


--day0[2] is day0[2]
--operation mode is input

day0[2] = INPUT();


--day0[1] is day0[1]
--operation mode is input

day0[1] = INPUT();


--day0[0] is day0[0]
--operation mode is input

day0[0] = INPUT();


--disp_select[5] is disp_select[5]
--operation mode is output

disp_select[5] = OUTPUT(A1L37);


--disp_select[4] is disp_select[4]
--operation mode is output

disp_select[4] = OUTPUT(A1L17);


--disp_select[3] is disp_select[3]
--operation mode is output

disp_select[3] = OUTPUT(A1L96);


--disp_select[2] is disp_select[2]
--operation mode is output

disp_select[2] = OUTPUT(A1L76);


--disp_select[1] is disp_select[1]
--operation mode is output

disp_select[1] = OUTPUT(A1L56);


--disp_select[0] is disp_select[0]
--operation mode is output

disp_select[0] = OUTPUT(A1L36);


--disp_data[2] is disp_data[2]
--operation mode is output

disp_data[2] = OUTPUT(A1L011);


--disp_data[4] is disp_data[4]
--operation mode is output

disp_data[4] = OUTPUT(A1L111);


--disp_data[5] is disp_data[5]
--operation mode is output

disp_data[5] = OUTPUT(A1L211);


--disp_data[6] is disp_data[6]
--operation mode is output

disp_data[6] = OUTPUT(A1L511);


--disp_data[1] is disp_data[1]
--operation mode is output

disp_data[1] = OUTPUT(A1L311);


--disp_data[0] is disp_data[0]
--operation mode is output

disp_data[0] = OUTPUT(A1L411);


--disp_data[3] is disp_data[3]
--operation mode is output

disp_data[3] = OUTPUT(A1L611);


